SystemSupportAddendum_{PRODUCT NAME: VMS DECwindows/Norsk V2.1}

SSA 26.A2.01-AHARDWARE REQUIREMENTS

Processors Supported:VAX:

VAX 9000 Model 210, VAX 9000 Model 410, VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 6000 Model 400 Series, VAX 4000 Model 300, VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978, VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785.MICROVAX: MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX 3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, MicroVAX 3800, MicroVAX 3900.VAXstation: VAXstation II, VAXstation 2000, VAXstation 3100 Series, VAXstation 3200, VAXstation 3500, VAXstation 3520, VAXstation 3540.VAXserver: VAXserver 3100, VAXserver 3300, VAXserver 3400, VAXserver 3500, VAXserver 3600, VAXserver 3602, VAXserver 3800, VAXserver 3900, VAXserver 6000-210, VAXserver 6000-310, VAXserver 6000-410, VAXserver 6000-420.

Processors Not Supported:

VAX: VAX-11/725, VAX-11/782. MicroVAX: MicroVAX I. VAXstation: VAXstation I, VAXstation 8000.

Processor Restriction:

A TK50 Tape Drive is required for standalone MicroVAX 2000 and VAXstation 2000 systems.

Block Space Requirements (Block Cluster Size = 1)

Disk space required for installation: 8,000 BlocksDisk space required for use (permanent): 8,000 Blocks

These counts refer to the disk space required on the system disk. The sizes are approximate; actual sizes may vary depending on the user’s system environment, con�guration and software options.

Memory Requirements For DECwindows Support

The minimum supported memory for this application running in a standalone DECwindows environment with both the client and server executing on that same system is 6 mb. At least 8 mb is required for use in a VAXcluster.

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and licensed VAXcluster* con�guration without restrictions. The HARDWARE REQUIRE- MENTS sections of this product’s Software Product Description and System Support Addendum detail any special hardware required by this product.

* V5.x VAXcluster con�gurations are fully described in the VAXcluster Software Product Description (29.78.xx) and include CI, Ethernet and Mixed Interconnect con- �gurations.

SOFTWARE REQUIREMENTS

VMS Operating System V5.4 and (necessary components of VMS DECwindows)Note: All VMS DECwindows V2.1 Language Variants run on VMS V5.4 releases only.

Refer to the VMS Operating System Software Product Description (SPD Number 25.01.XX) for availability and versions of required software and for information regarding components of VMS DECwindows.

This product may run in either of the following ways:

Stand-alone execution - Running the X11 display server and the client application on the same machine.

Remote execution - Running the X11 display server and the client application on different machines.October 1990 AE-PBP2B-TE dt

VMS DECwindows/Norsk V2.1 SSA 26.A2.01-A

VMS TAILORING CLASSES

All classes of VMS are required for full functionality of this layered product.

For more information on VMS classes and tailoring refer to the VMS Operating System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

In addition to your own language variant of DECwindows V2.1, the following V2.1 language variants are or will be available:

Dutch VMS DECwindows/Nederlands French VMS DECwindows/Fran�ais French Canadian VMS DECwindows/Canadien-fran�ais German VMS DECwindows/Deutsch Italian VMS DECwindows/Italiano Norwegian VMS DECwindows/Norsk Swedish VMS DECwindows/Svenska Swiss-French VMS DECwindows/Fran�ais/CH Swiss-German VMS DECwindows/Deutsch/CH Swiss-Italian VMS DECwindows/Italiano/CH

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this product may be different from the minimum requirements for the current version.

DISTRIBUTION MEDIA

Tape - TK50 Streaming Tape.

This product is also available as part of the VMS Consolidated Software Distribution on CDROM.

ORDERING INFORMATION

Software Media Q*-YFSNA-** Software Documentation QA-YFSNA-**

* Denotes variant �elds. for additional information on available licenses, services and media refer to the appropriate price book.

The above information is valid at time of release. Please contact your local Digital of�ce for the most up-to-date information.

� X Window System, Version 11 and its derivations (X, X11, X Version 11, X Window System) are trademarks of the Massachusetts Institute of Technology.

2