 

Software
Product
Description

___________________________________________________________________

PRODUCT NAME:  Compaq DECprint Supervisor (DCPS) for OpenVMS,   SPD
44.15.12                Version 2.1

DESCRIPTION

Compaq DECprint Supervisor (DCPS) for OpenVMS is a layered software
application that runs on OpenVMS Alpha and OpenVMS VAX systems to pro-
vide access to selected PostScript[R] Level 1, Level 2 and Level 3 print-
ers.

DCPS drives selected PostScript printers and supports these printers'
special features, such as tray and media selection and two-sided print-
ing. File formats supported include PostScript, ANSI-Compliant DIGITAL
Printing Protocol Level 3 (DEC PPL3) and HP PCL. DCPS also includes
features such as number-up, layup, automatic data type detection and
high speed image printing, plus translators for a number of printer
languages. See the Other Hardware Required section of the SPD for the
list of supported printer models.

DECprint Supervisor software consists of the following components:

o  A print symbiont that processes print requests for the host on which
   it resides.

o  Software to transmit the request and associated data over the fol-
   lowing protocols:

   -  Ethernet via TCP/IP to a printer connected to a print server or
      a terminal server that supports the bidirectional raw TCP/IP socket
      protocol

   -  Ethernet via TCP/IP to a printer with a network interface card
      (NIC) that supports the bidirectional raw TCP/IP socket proto-
      col

                                                          July 2002

 

   -  Ethernet to a PrintServer printer via DECnet or TCP/IP using Com-
      mon Printer Access Protocol (CPAP)

   -  Local Area Transport (LAT)

   -  Serial line

o  Translators to convert various non-PostScript files into the PostScript
   language for printing.

o  Page formatting capabilities such as the ability to print multi-
   ple page images on a single side of a sheet of paper and to spec-
   ify borders, margins and page offsets.

o  A series of PostScript tools for application developers. These in-
   clude a PostScript error handler and Font Encoding Vectors for the
   ISO Latin Alphabet Number 1 (ISO 8859/1) and DIGITAL Multinational
   Character Set for use with all the PostScript text fonts that are
   built into DIGITAL and selected Compaq PostScript printers.

Install DECprint Supervisor software on each node that has print queues
for PostScript printers.

A system running DECprint Supervisor software can transmit print re-
quests to printers on a TCP/IP, DECnet or LAT network. Note that not
all printers support all these protocols.

To communicate with a printer on a TCP/IP network, Compaq TCP/IP Ser-
vices for OpenVMS software, or Process Software MultiNet[R] for OpenVMS
or TCPware[R] for OpenVMS software must be installed on your system.

For DIGITAL PrintServer printers, whether using the TCP/IP or DECnet
protocol, PrintServer Software must be installed on at least one sys-
tem in your network.

Printing Features

o  PostScript printing. The print symbiont passes PostScript files di-
   rectly to the printer. DECprint Supervisor does not interpret or
   translate PostScript files. Therefore, they must be created using
   standard PostScript Level 1, Level 2 or Level 3 operators as de-
   fined within the printer itself.

                                 2

 

o  ANSI (DEC PPL3) printing. DECprint Supervisor translates ANSI files
   into PostScript for printing on the output device. These ANSI files
   may contain ASCII text, sixel graphics and other features of DIGITAL's
   ANSI-compliant Printing Protocol Level 3.

o  Selection of input tray via INPUT_TRAY, SHEET_SIZE, or PAGE_SIZE
   parameters and output tray via OUTPUT_TRAY, within the limitations
   of the printer and the tray-naming conventions to provide such fea-
   tures.

o  Rotation of the page via the PAGE_ORIENTATION parameter for non-
   PostScript files only.

o  Selection of single-sided, double-sided, or tumble printing when
   available on the printer, via the SIDES parameter.

o  Formatting of ANSI text files via the /HEADER, /FORM, /SPACE and
   /FEED qualifiers and the TAB parameter.

o  Control of ANSI file margins, page setup and wrap or truncate op-
   tions as specified by the DEFINE/FORM command.

o  Status and error messages sent to the user's terminal, may be printed
   on the job trailer page or job log page, written to a log file, or
   displayed on the operator's console.

o  Use of device control modules for basic data types via the /SETUP
   qualifier. PostScript modules may contain any PostScript operators
   supported by the printer in the printing context.

o  Collection of accounting information for each print job as follows:
   sheets of paper printed, the number of RMS Gets and the number of
   QIO Writes. All Compaq, DIGITAL and GENICOM printers support this
   feature except where noted in the Other Hardware Required section
   of the SPD. This feature may not be available with other printers.

o  Access to the PCL interpreter native to selected printers. Print-
   ers for which the native PCL interpreter is supported are listed
   in the Other Hardware Required section of the SPD.

o  Support for PrintServer printers on DECnet or TCP/IP interconnects
   using CPAP protocol.

                                 3

 

o  Support for printers via network interface cards, print servers and
   terminal servers that support bidirectional raw TCP/IP socket.

o  Automatic data type detection and switching. The software attempts
   to determine the data type of the file. If successful, it will au-
   tomatically translate, if necessary, and print the file. If it can-
   not determine the file data type, it will use the default data type
   defined by DATA_TYPE=AUTOMATIC.

   If the file is printed using the data type defined by DATA_TYPE=AUTOMATIC,
   the symbiont will look for a switch to PostScript command (%!) and
   continue to process the rest of the file as PostScript. This switch
   may occur only once per file. The switch to PostScript feature is
   not available when DCPS uses a printer's native PCL interpreter to
   process the file.

o  Printing non-PostScript data types on the PostScript printer. Trans-
   lators are provided to translate the following data types into PostScript
   for printing:

   -  DDIF (bitonal Image subset only; requires DECwindows Motif soft-
      ware)

   -  PCL Level 4 (as implemented on the HP[R] LaserJet[R] IID)

   -  IBM[R] Proprinter[R] XL24

   -  ReGIS (monochrome output only)

   -  Tektronix[R] 4010/4014

   -  ASCII LIST translator that formats and numbers ASCII files. This
      translator numbers each line of text, creates alternating bars
      of gray and white in the background and creates a running head
      of the file name and page number.

o  Printing two or more page images on a single side of a sheet via
   the NUMBER_UP parameter.


                                 4

 

o  Specifying page layup features via the LAYUP_DEFINITION parameter.
   Page layup features include Borders, Margins, Margin Alternation,
   Pages Per Sheet, First Page, Page Order and Page Grid. Layup def-
   inition options may be provided directly, as arguments to the LAYUP_
   DEFINITION parameter, or indirectly, as the contents of a file spec-
   ified by that parameter.

o  Specifying a range of pages of the file to be printed via the PAGE_
   LIMIT parameter.

o  Automatically scaling a page created for one paper size so that it
   fits on a different paper size via use of both the PAGE_SIZE and
   SHEET_SIZE parameters on the same print command.

o  Printing multiple uncollated copies of each sheet via the SHEET_
   COUNT parameter.

o  Use of device control modules for all data types via the /SETUP qual-
   ifier. ANSI modules may include control sequences. PCL modules may
   include binary font data.

ANSI (DEC PPL3) Emulation

Printing of ANSI text and sixel graphics is compatible with DIGITAL's
ANSI-compliant PPL3 printers.

Note: PostScript printers differ in the amount of virtual memory they
have available for printing and font storage. Files that require down-
loading of fonts may be printed differently, may print more slowly or
may fail to print on some printers.

INSTALLATION STATEMENT

Compaq recommends that a customer's first purchase of this software
product include Compaq Installation Services. These services provide
for installation of the software product by an experienced Compaq Soft-
ware Specialist.



                                 5

 

For subsequent purchases of this product, only customers with knowl-
edge of OpenVMS generic and execution print queues in clustered and
non-clustered environments and, if operating in a DECserver environ-
ment, knowledge of DECserver management, should attempt installation
of this software product. Compaq recommends that all other customers
purchase Compaq's Installation Services.

These services provide for the installation of the software product
and Compaq PostScript Printer hardware by an experienced Compaq Spe-
cialist.

Before installation of the software by Compaq Installation Services,
the customer must:

o  Obtain, install and demonstrate as operational any equipment and
   facilities necessary to interface to Compaq's communication equip-
   ment.

o  Make available for a reasonable period of time, as mutually agreed
   upon by Compaq and the customer, all hardware, communication fa-
   cilities and terminals that are to be used during installation.

o  For verification of installation and connectivity in a multi-node
   node network, designate and provide access to a host that has pre-
   viously been installed by Compaq.

o  Assure that a valid OpenVMS operating system license is installed.

Delays caused by any failure to meet these responsibilities will be
charged at the then prevailing rate for time and materials.

Installation of DECprint Supervisor software will consist of the fol-
lowing:

o  Verification that all prerequisite software and hardware has been
   installed.

o  Verification that a complete set of DCPS software media and doc-
   umentation has been received.

o  Verification that all hardware and software prerequisites have been
   met and the equipment is operational.

                                 6

 

o  Installation of DCPS software on one system.

o  Verification that DCPS software has been correctly installed by run-
   ning the Installation Verification Procedure (IVP).

o  Modification of the DECnet database or TCP/IP hosts file to add printer
   node names and addresses.

o  Modification of the OpenVMS start-up files to automate the start-
   up of print queues.

HARDWARE REQUIREMENTS

Processors Supported

For information about support processors, refer to the Software Prod-
uct Description for the OpenVMS Operating System for Alpha and VAX (SPD
25.01.xx and 41.87.xx).

Other Hardware Required

At least one PostScript printer, as follows:

o  Apple

      LaserWriter IIg
      LaserWriter IIf [1]
      LaserWriter II NT [1]
      LaserWriter II NTR [1]
      LaserWriter II NTX [1]
      LaserWriter Plus [1]
      LaserWriter Pro 600 [1]
      LaserWriter Pro 630 [1]

o  Compaq

      Laser Printer LN16 [2]
      Laser Printer LN32

____________________

 Printer  does not have native PCL interpreter

 Supported  only when the printer is in PostScript mode

                                 7

 

      Laser Printer LNC02 [3]
      Laser Printer LNM40

o  DIGITAL

      Colormate PS[R] (LF01R) [1]
      Colorwriter LSR 2000 and 2000[+] (LNC01) [1]
      DECcolorwriter 1000 (LF02) [1]
      DEClaser 1150 (LN07R) [1]
      DEClaser 1152 (LN07C) [1]
      DEClaser 2150 (LN05R) [1]
      DEClaser 2250 (LN06R) [1]
      DEClaser 3250 (LN08R) [1]
      DEClaser 3500 (LN14) [4]
      DEClaser 5100 (LN09) [4]
      Laser Printer LN15 [2]
      Laser Printer LN15+ [2]
      Laser Printer LN17+ps
      Laser Printer LN20 [3]
      Laser Printer LN40 [3]
      Laser Printer LNC02 [3]
      LN17ps
      PrintServer 17 (LPS17)
      PrintServer 17/600
      PrintServer 20 (LPS20) [1]
      turbo PrintServer 20 [1]
      PrintServer 32 (LPS32) [1]
      PrintServer 32 plus
      PrintServer 40 (LPS40) [1]
      PrintServer 40 Plus [1]
      ScriptPrinter (LN03R) [1]

o  GENICOM

      Intelliprint cL160
      Intelliprint mL402
____________________

 Does  not support DCPS accounting feature
 Includes  support for direct printing to native PCL interpreter only

  when printer is in autosensing mode

                                 8

 

      Intelliprint mL450
      LN21
      LN28
      LN45
      LNM40
      microLaser 170 [2]
      microLaser 210
      microLaser 280
      microLaser 320
      microLaser 401

o  HP

      Color LaserJet 4500
      Color LaserJet 4550
      Color LaserJet 4600
      LaserJet III with PostScript (Level 1) cartridge [1]
      LaserJet III with PostScript-Plus (Level 2) cartridge [1]
      LaserJet IIID with PostScript (Level 1) cartridge [1]
      LaserJet IIID with PostScript-Plus (Level 2) cartridge [1]
      LaserJet IIISi with PostScript (Level 1) option
      LaserJet IIISi with PostScript (Level 2) option
      LaserJet 4M
      LaserJet 4M Plus
      LaserJet 4ML
      LaserJet 4MP
      LaserJet 4SiMX
      LaserJet 4MV
      LaserJet 5SiMX
      LaserJet 5M (monochrome version)
      LaserJet 2100
      LaserJet 2200
      LaserJet 4000
      LaserJet 4050
      LaserJet 4100
      LaserJet 5000
      LaserJet 8000
      LaserJet 8100
      LaserJet 8150

                                 9

 

      LaserJet 9000
      PaintJet XL300 [1]

o  IBM

      Infoprint 21
      InfoPrint 32
      InfoPrint 40

o  Lexmark

      Optra C710
      Optra C720
      Optra Rt+ [1]
      Optra S 1250
      Optra S 1255
      Optra S 1620
      Optra S 1625
      Optra S 1650
      Optra S 1855
      Optra S 2420
      Optra S 2450
      Optra S 2455
      Optra Se 3455
      Optra T520
      Optra T522
      Optra T610
      Optra T612
      Optra T614
      Optra T616
      Optra T620
      Optra T622
      Optra W810
      Optra W820

o  Tektronix

      Phaser 200e [1]
      Phaser 200i [1]
      Phaser 220e [1]
      Phaser 740 [1]

                                10

 

      Phaser 750 [1]
      Phaser 780 [1]
      Phaser 850 [1]

o  Xerox

      DocuPrint N24
      DocuPrint N32
      DocuPrint N40
      DocuPrint N2025
      DocuPrint N2125
      DocuPrint N2825
      DocuPrint N3225
      DocuPrint N4025

A supported printer must be equipped with one or more of the follow-
ing supported interconnects:

o  EIA-232 (RS-232) serial port

o  EIA-422 (RS-422) serial port

o  Ethernet port or Network Interface Card (NIC) supporting CPAP, LAT
   or bidirectional raw TCP/IP socket protocol

o  Bidirectional Centronics parallel port connected through a print
   server or terminal server

Note: DCPS does not support the following types of printer connections:

 -  A unidirectional connection (for example, a parallel or raw TCP/IP
   port that is unidirectional)

 -  The parallel port on an OpenVMS system

 -  The Telnet or LPD network protocols

The following notes apply when using the above interconnects:

o  EIA-232 serial interfaces are optional with some printers and may
   need to be purchased separately.

o  EIA-422 serial interfaces, such as that employed on the HP Paint-
   Jet XL300, require an EIA-422/EIA-232 converter/adapter.

                                11

 

o  The HP LaserJet 4SiMX is supported for serial communication when
   equipped with the Extend Systems ESI-2633A interface card.

o  Ethernet interfaces may require an adapter to connect the printer's
   Ethernet hardware to that of the local area network.

o  Ethernet protocols supported for certain Desktop and Workgroup print-
   ers (not including PrintServer printers) are raw TCP/IP socket and
   LAT.

o  Ethernet protocols supported for DIGITAL PrintServer printers are
   DECnet CPAP and TCP/IP CPAP.

For Serial Line configurations, the following are required

o  At least one printer listed above

o  Serial interface and cable for EIA-232 or EIA-422 with converter/adapter

o  One of the following serial interfaces or servers:

   -  CVAX serial interface (CXA16, CXB16, CX08, DZQ-11; 9600 baud)

   -  DHV11 (9600 baud; serial interface)

   -  DZQ11 (9600 baud; serial interface)

   -  DLV11 (9600 baud; serial interface)

   -  DHU11 (9600 baud; serial interface)

   -  DMZ32 (4800 baud; serial interface)

   -  DMF32 (9600 baud; serial interface)

   -  DMB32 (9600 baud; serial interface)

   -  DECserver 90L and 90L+ (38.4K baud; LAT)

   -  DECserver 90M (57.6K baud; LAT and raw TCP/IP socket)

   -  DECserver 90TL (57.6K baud; LAT and raw TCP/IP socket)

   -  DECserver 100 (9600 baud; LAT)

   -  DECserver 200/MC (19.2K baud; LAT)

   -  DECserver 250 (19.2K baud; LAT)

                                12

 

   -  DECserver 300 (19.2K baud; LAT

   -  DECserver 500 (9600 baud; LAT)

   -  DECserver 550 (9600 baud; LAT)

   -  DECserver 700 series (115.2K baud; LAT and raw TCP/IP socket)

   -  DECserver 900 series (115.2K baud; LAT and raw TCP/IP socket)

   -  MUXserver 100 (19.2K baud; LAT)

   -  MUXserver 300 (19.2K baud; LAT)

   -  NetRider 90 - see DECserver 90M

   -  NetRider 900 - see DECserver 900 series

   -  LATprint (38.4K baud; LAT)

   -  RapidPrint 200 (115.2K baud; LAT)

A DECserver or NetRider configuration requires DECserver Network Ac-
cess Software (DNAS) V2.0 or later and a minimum of 4 Mbytes of mem-
ory to support raw TCP/IP sockets.

All of the interfaces above support EIA-232 and some support EIA-422.
The customer must select an appropriate combination of host serial in-
terface, cable and printer serial interface. In some cases, an exter-
nal adapter may be required. Also:

o  The printer's communications interface must be set for 8-bit, no
   parity communication.

o  The interface baud rate must be set to a value less than or equal
   to the value specified above for the chosen host interface.

o  Flow control should be set to XON/XOFF for PostScript-only print-
   ers or DTR/CTS (hardware handshake) for PostScript/PCL 5 printers.

For parallel port configurations, the following are required

o  At least one printer (listed above)

o  Bidirectional Centronics parallel port interface

                                13

 

o  One of the following print servers:

   -  DIGITAL RapidPrint 200 (LAT)

   -  DIGITAL RapidPrint 500 (Raw TCP/IP socket and LAT)

   -  GENICOM MPS100 (Raw TCP/IP socket and LAT)

A parallel cable may also be required to connect the printer to the
print server.

For Raw TCP/IP configurations, the following are required

o  At least one printer (listed above)

o  A NIC, print server, or terminal server that provides bidirectional
   raw TCP/IP sockets.

A cable may also be required to connect the printer to a print server
or terminal server.

For PrintServer configurations, the following are required

o  A DIGITAL PrintServer printer

o  An Ethernet Controller Interface for the client system

o  An Ethernet physical channel for the printer, and one of the fol-
   lowing:

   -  Ethernet Transceiver (H4000 or H4004)

   -  Local Network Interconnect (DELNI)

   -  ThinWire Ethernet Station Adapter (DESTA)

   -  ThinWire Interconnect (DEMPR)

Disk Space Requirements:

DECprint Supervisor for
OpenVMS Alpha
Disk space required for      7,400 blocks
installation:                (3.7 Mbytes)

                                14

 


Disk space required for      6,900 blocks
use (permanent):             (3.5 Mbytes)

DECprint Supervisor for
OpenVMS VAX
Disk space required for      5,900 blocks
installation:                (3.0 Mbytes)
Disk space required for      5,500 blocks
use (permanent):             (2.8 Mbytes)

These counts refer to the disk space required on the system disk. The
sizes are approximate; actual sizes may vary depending on the user's
system environment, system disk cluster size, configuration and soft-
ware options.

SOFTWARE REQUIREMENTS

DECprint Supervisor (DCPS) for OpenVMS Version 2.1 software runs on
the following versions of the OpenVMS operating system:

o  OpenVMS Alpha V6.2, V7.2-2, V7.3 and V7.3-1

o  OpenVMS VAX V5.5-2, V7.2 and V7.3

However, only specific versions of networking software are supported
for each version of the operating system. See the following sections
for the supported versions.

Raw TCP/IP Configurations

For Raw TCP/IP configurations, you need one of the following TCP/IP
products:

o  Compaq TCP/IP Services for OpenVMS

o  Process Software MultiNet for OpenVMS



                                15

 

o  Process Software TCPware for OpenVMS

See Table 1 for supported versions.

___________________________________________________________________

Table_1:_Supported_TCP/IP_Versions_________________________________

            TCP/IP
OpenVMS_____Services____MultiNet____TCPware________________________

Alpha       V4.2        V4.0 -      V5.3 - V5.5
V6.2                    V4.4

Alpha       V5.1 -      V4.0 -      V5.3 - V5.5
V7.2-2      V5.3        V4.4

Alpha       V5.1 -      V4.0 -      V5.3 - V5.5
V7.3        V5.3        V4.4

Alpha       V5.3        V4.0 -      V5.3 - V5.5
V7.3-1                  V4.4

VAX         V4.0        V4.0 -      V5.3 - V5.5
V5.5-2                  V4.4

VAX V7.2    V5.0A -     V4.0 -      V5.3 - V5.5
            V5.3        V4.4

VAX V7.3    V5.1 -      V4.0 -      V5.3 - V5.5
____________V5.3________V4.4_______________________________________

PrintServer Printer Configurations

For PrintServer printer configurations, you need a supporting host and
PrintServer Software V4.0 or later.[5] Refer to the PrintServer Soft-
ware SPD 48.09.xx for more information.

You also need one of the following products:

o  DECnet for OpenVMS

o  DECnet-Plus for OpenVMS

____________________

 This  product has been retired.

                                16

 

o  Compaq TCP/IP Services for OpenVMS

o  Process Software MultiNet for OpenVMS

o  Process Software TCPware for OpenVMS

See Table 1 and Table 2 for supported versions.

___________________________________________________________________

Table_2:_Supported_DECnet_Versions_________________________________

OpenVMS_________DECnet______DECnet-Plus____________________________

Alpha V6.2      V6.2        V6.3

Alpha V7.2-2    V7.2-2      V7.2-2

Alpha V7.3      V7.3        V7.3

Alpha V7.3-1    V7.3-1      V7.3-1

VAX V5.5-2      V5.5-2      --

VAX V7.2        V7.2        V7.2

VAX_V7.3________V7.3________V7.3___________________________________

DDIF image printing

o  DECwindows Motif software

SOFTWARE LICENSING

This software is furnished under the licensing provisions of Compaq
Computer Corporation's Standard Terms and Conditions. For more infor-
mation about Compaq's licensing terms and policies, contact your re-
seller, VAR or local Compaq office.

DECprint Supervisor for OpenVMS

The right to use DECprint Supervisor for OpenVMS is included with the
license for the OpenVMS Alpha and OpenVMS VAX operating systems.

                                17

 

This right permits execution of the DECprint Supervisor for OpenVMS
software on any Alpha or VAX processor for purposes of controlling and
providing basic printing features for all PostScript printers controlled
by the licensed node.

The Hardware Requirements section of this SPD lists the supported print-
ers. Supported printers have been tested and verified to work. Compaq
makes no representation relative to the use of this product with PostScript
devices not listed in the SPD. Customers' use of the product with PostScript
devices not listed in the SPD is at their own risk.

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid
and licensed VMScluster[6] configuration without restrictions. The Hard-
ware Requirements section of this product's Software Product Descrip-
tion and System Support Addendum detail any special hardware required
by this product.

OpenVMS Tailoring

The following OpenVMS classes are required for full functionality of
this layered product:

o  OpenVMS Required Saveset

o  Network Support (for PrintServer support) [7]

o  Secure User's Environment

o  Utilities (for support of DECserver connected printers) [7]

o  DECwindows Application Files (for printing DDIF encoded bitonal im-
   ages) [7]

____________________
 VMScluster  configurations are fully described in the VMScluster Soft-
  ware Product Description (42.18.xx) and include CI, Ethernet, DSSI

  and SCSI configurations.
 These  are optional features.  Installations that do not use these fea-

  tures do not need to install the tailoring classes indicated.

                                18

 

For more information on OpenVMS classes and tailoring, refer to the
appropriate OpenVMS Operating System Software Product Description.

OPTIONAL SOFTWARE

o  Distributed Queuing Service for OpenVMS (DQS) (SPD 28.80.xx)

o  DECnet-Plus for OpenVMS Alpha (SPD 50.45.xx) or DECnet-Plus for Open-
   VMS VAX (SPD 25.03.xx) when DECnet is used as the communication pro-
   tocol to PrintServer printers.

o  Compaq TCP/IP Services for OpenVMS (SPD 46.46.xx) when TCP/IP is
   used as the communication protocol to PrintServer printers and to
   printers with NICs and print servers and terminal servers that sup-
   port raw TCP/IP socket protocol.

o  Process Software MultiNet for OpenVMS when TCP/IP is used as the
   communication protocol to PrintServer printers and to printers with
   NICs and print servers and terminal servers that support raw TCP/IP
   socket protocol.

o  Process Software TCPware for OpenVMS when TCP/IP is used as the com-
   munication protocol to PrintServer printers and to printers with
   NICs and print servers and terminal servers that support raw TCP/IP
   socket protocol.

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of
this product may be different from the requirements for the current
version.









                                19

 

DISTRIBUTION MEDIA

DCPS software is available on CD-ROM as described below, and as part
of the OpenVMS Alpha and VAX Software Product Libraries.

DCPS documentation is available on CD-ROM and in hardcopy as described
below, and as part of the OpenVMS Alpha and VAX Online Documentation
Libraries.

ORDERING INFORMATION

Software Documentation:
   QA-09NAA-GZ (hardcopy)

Software Media and Documentation:
   QA-09NAB-H8 (CD-ROM)

This CD-ROM contains DCPS software for Alpha and VAX, and documenta-
tion in various formats.

o  Documentation
   Software Product Description (SPD)
   Release Notes
   Installation Guide
   System Manager's Guide
   User's Guide

o  Formats
   Text
   PostScript (PS)
   Adobe Acrobat[R] Portable Document Format (PDF)
   HyperText Markup Language (HTML)
   Bookreader







                                20

 

SOFTWARE PRODUCT SERVICES

A variety of service options are available from Compaq. For more in-
formation, contact your Compaq reseller or local Compaq office.

SOFTWARE WARRANTY

This software is provided by Compaq with a ninety-day comformance war-
ranty in accordance with the Compaq warranty terms applicable to the
license purchase.

© 2002 Compaq Information Technologies Group, L.P.

Compaq, the Compaq logo, Alpha, DCPS, DECnet, OpenVMS, VAX and VMS are
trademarks of Compaq Information Technologies Group, L.P. in the U.S.
and/or other countries.

All other product names mentioned herin may be trademarks of their re-
spective companies.

Confidential computer software. Valid license from Compaq required for
possession, use, or copying. Consistent with FAR 12.211 and 12.212,
Commercial Computer Software, Computer Software Documentation, and Tech-
nical Data for Commercial Items are licensed to the U.S. Government
under vendor's standard commercial license.

Compaq shall not be liable for technical or editorial errors or omis-
sions contained herein. The information in this document is provided
"as is" without warranty of any kind and is subject to change with-
out notice. The warranties for Compaq products are set forth in the
express limited warranty statements accompanying such products. Noth-
ing herein should be construed as constituting an additional warranty.








                                21

 









































                                22
