AA-N323G-TE

ALL-IN-1

Installation Guide Part 1

Base Installation

digital equipment corporation maynard, massachusetts

AA-N323G-TE First Printing, December 1989

The information in this document is subject to change without notice and should not be construed as a commitment by Digital Equipment Corporation. Digital Equipment Corporation assumes no responsibility for any errors that may appear in this document.

The software described in this document is furnished under a license and may be used or copied only in accordance with the terms of such license.

Digital Equipment Corporation assumes no responsibility for the use or reliability of its software on equipment that is not supplied by Digital.

Restricted Rights: Use, duplication, or disclosure by the U.S. Government is subject to restrictions as set forth in subparagraph (c)(1)(ii) of the Rights in Technical Data and Computer Software clause at DFARS 252.227-7013.

' Digital Equipment Corporation. 1989. All rights reserved.

Please complete the reader’s comments page at the end of the book. It will help us to keep improving our documentation.

The following are trademarks of Digital Equipment Corporation:

ALL-IN-1 MicroVAX VAX DOCUMENT DDIF MicroVMS VAX FMS DEC PDP VAX Grammar Checker DECdx P/OS VAX Notes DECmail Professional VAX RALLY DECmate Rainbow VAX TEAMDATA DECspell RSTS VAX VTX DECtalk RSX VMS DECtalk Mail Access TK50 VT DECUS TOPS-20 Work Processor DECwindows UNIBUS WPS-PLUS DECwriter VAX DIBOL VAXcluster MAILbus VAX DATATRIEVE MASSBUS VAX DECpage dt

Bell is a trademark of Bell telephone companies.

Ethernet is a trademark of Xerox Corporation.

PostScript is a registered trademark of Adobe Systems, Inc.

Vadic is a trademark of Racal-Vadic.

This document was prepared using VAX DOCUMENT, Version 1.2.

Contents

Preface . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . xi

1 Preparing to Install ALL-IN-1 V2.4

1.1 Examining the Distribution Kit . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�3 1.1.1 Magnetic Tape and TK50 Kits . . . . . . . . . . . . . . . . . . . . . . . . . 1�4 1.1.2 Compact Disk Consolidated Software Distribution Kits . . . . . . 1�5 1.2 VMS License Management Facility . . . . . . . . . . . . . . . . . . . . . . . . 1�5 1.3 Required Operating System Components . . . . . . . . . . . . . . . . . . . . 1�6 1.4 Prerequisite Software . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�6 1.4.1 Installed Images . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�6 1.5 Optional Software Products . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�8 1.5.1 Initial DDIF Support . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�10 1.5.2 Integrating VAX DATATRIEVE with ALL-IN-1 . . . . . . . . . . . . 1�11 1.5.3 Integrating Message Router and the Message Router VMSmail Gateway with ALL-IN-1 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�12 1.5.3.1 The Mail Directory and the ALL-IN-1 Directory . . . . . . . . 1�13 1.5.4 Integrating ACMS with ALL-IN-1 . . . . . . . . . . . . . . . . . . . . . . 1�14 1.5.5 Integrating WPS-PLUS with ALL-IN-1 . . . . . . . . . . . . . . . . . . 1�14 1.5.6 Installation Order . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�15 1.5.7 Keeping a Record of the Installation . . . . . . . . . . . . . . . . . . . . 1�15 1.6 Installing ALL-IN-1 on VAXcluster Systems . . . . . . . . . . . . . . . . . 1�16 1.6.1 Installing ALL-IN-1 on a Common-Environment Cluster . . . . . 1�16 1.6.1.1 Running ALL-IN-1 on a Common-Environment Cluster . . 1�16 1.6.2 Installing ALL-IN-1 on a Multiple-Environment Cluster . . . . . 1�17 1.6.2.1 Running ALL-IN-1 on a Multiple-Environment Cluster . . . 1�18 1.6.3 Installing ALL-IN-1 on a Local Area VAXcluster System . . . . . 1�19 1.7 Installing Additional Languages . . . . . . . . . . . . . . . . . . . . . . . . . . 1�20 1.8 Preparing the System for Installation . . . . . . . . . . . . . . . . . . . . . . 1�20iii

1.8.1 Time Needed to Install ALL-IN-1 Version 2.4 . . . . . . . . . . . . . 1�22 1.8.2 Privileges . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�23 1.8.3 Back Up Your System and Target Disks . . . . . . . . . . . . . . . . . 1�23 1.8.4 Ensure No Active Users on the System . . . . . . . . . . . . . . . . . . 1�23 1.8.5 Moving Your Applications to ALL-IN-1 Customization Management . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�23 1.8.5.1 Uncustomized Elements Supported by Customization Management . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�24 1.8.5.2 Customized Elements Supported by Customization Management . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�24 1.8.5.3 Elements Not Supported by Customization Management . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�24 1.8.6 Register the Licenses for the Prerequisite Software . . . . . . . . . 1�25 1.8.7 Ensure Message Router Directory Service is Running . . . . . . . 1�25 1.8.8 Shut Down the OA$FORMATTER Batch Queue . . . . . . . . . . . 1�25 1.8.9 Start the Queue Manager . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�25 1.8.10 Run the Mail Sender and Fetcher . . . . . . . . . . . . . . . . . . . . . . 1�26 1.8.11 Delete the ALL-IN-1 Housekeeping Jobs . . . . . . . . . . . . . . . . . 1�26 1.8.12 Calculate the Values for GBLPAGES, GBLSECTIONS and GBLPAGFIL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�26 1.8.13 Check the System Parameter Values . . . . . . . . . . . . . . . . . . . . 1�29 1.8.14 Changing System Parameter Values with AUTOGEN . . . . . . . 1�31 1.8.15 Process Account Quotas . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�32 1.8.16 Disk Space . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�33 1.8.16.1 Installation Modes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�33 1.8.16.2 ALL-IN-1 Areas . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�34 1.8.17 Deinstall Patches . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�36 1.8.18 Check Your Site-Speci�c Startup Procedures . . . . . . . . . . . . . . 1�36 1.8.19 Considerations for ALL-IN-1 Version 2.4 Group Conferencing . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�37 1.8.20 Checklist of Information Required for Installation . . . . . . . . . . 1�37 1.8.21 License Management Utility Requirements . . . . . . . . . . . . . . . 1�38

2 Accessing the Online Release Notes

2.1 Accessing the Release Notes . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 2�2 iv

3 Installing a New ALL-IN-1 V2.4 System

3.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�1

3.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�1

3.3 Determining the Files and Logical Names Added to the System . . 3�2

3.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 3�2

3.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�2

3.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�2

3.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�3

3.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 3�5

3.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 3�6

4 Installing Additional Languages for ALL-IN-1 V2.4

4.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�1

4.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�2

4.3 Determining the Files and Logical Names Added to the System . . 4�2

4.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 4�2

4.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�2

4.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�3

4.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�3

4.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 4�4

4.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 4�5

5 Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4

5.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�1

5.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�2

5.3 Determining the Files and Logical Names Added to the System . . 5�2

5.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 5�2

5.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�2

5.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�3

5.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�3

5.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 5�5

5.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 5�6

6 Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4

Languages

6.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�1

6.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�2

6.3 Determining the Files and Logical Names Added to the System . . 6�2

6.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 6�2v

6.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�2

6.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�3

6.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�3

6.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 6�4

6.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 6�5

7 Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1

V2.47.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�1

7.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�2

7.3 Determining the Files and Logical Names Added to the System . . 7�2

7.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 7�2

7.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�3

7.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�3

7.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�4

7.8 Stop and Start the OA$FORMATTER Queue . . . . . . . . . . . . . . . . 7�5

7.9 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�5

7.9.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 7�6

8 Upgrading ALL-IN-1 STARTER V1.0 Languages to

ALL-IN-1 V2.4 Languages

8.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�1

8.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�2

8.3 Determining the Files and Logical Names Added to the System . . 8�2

8.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 8�2

8.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�2

8.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�3

8.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�3

8.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�4

8.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 8�5

9 Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4

9.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�1

9.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�2

9.3 Determining the Files and Logical Names Added to the System . . 9�2

9.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 9�2

9.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�2

9.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�3

9.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�3 vi

9.8 Stop and Start the OA$FORMATTER Queue . . . . . . . . . . . . . . . . 9�5

9.9 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�5

9.9.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 9�6

10 Updating ALL-IN-1 STARTER V2.4 Languages to

ALL-IN-1 V2.4 Languages

10.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�1

10.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�2

10.3 Determining the Files and Logical Names Added to the System . . 10�2

10.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 10�2

10.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�2

10.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�3

10.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�3

10.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�4

10.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 10�5

11 Updating an Existing ALL-IN-1 V2.4 System

11.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�1

11.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�1

11.3 Determining the Files and Logical Names Added to the System . . 11�2

11.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 11�2

11.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�2

11.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�2

11.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�3

11.8 Start the OA$FORMATTER Queue . . . . . . . . . . . . . . . . . . . . . . . . 11�4

11.9 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�4

11.9.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 11�5

12 Updating an ALL-IN-1 V2.4 Language

12.1 Before You Start . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�1

12.2 Overview of VMSINSTAL . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�1

12.3 Determining the Files and Logical Names Added to the System . . 12�2

12.4 Running the Installation Veri�cation Procedure (IVP) . . . . . . . . . . 12�2

12.5 Aborting the Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�2

12.6 Warning and Error Messages . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�2

12.7 The Installation Procedure . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�3

12.8 Error Recovery . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�4

12.8.1 Errors Found During the IVP . . . . . . . . . . . . . . . . . . . . . . . . . 12�4vii

13 Steps Required for Installing ALL-IN-1 V2.4

13.1 Installation Steps . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 13�1

14 After Installing ALL-IN-1 V2.4

14.1 Replace the DCLTABLES on VAXcluster Systems . . . . . . . . . . . . . 14�2

14.2 Convert the User Pro�les . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�3

14.3 Update the License Count and Subscriber Count for ALL-IN-1 . . . 14�3

14.4 Delete Files That Are No Longer Required . . . . . . . . . . . . . . . . . . 14�3

14.5 Convert the Format of OA$DATA_SHARE:

SM_USED_UIC.DAT . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�4

14.6 Execute the ALL-IN-1 Startup Command Procedure . . . . . . . . . . . 14�4

14.6.1 After a New Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�4

14.6.2 After an Upgrade Installation . . . . . . . . . . . . . . . . . . . . . . . . . 14�5

14.6.3 Site-Speci�c Startup Procedures . . . . . . . . . . . . . . . . . . . . . . . 14�6

14.6.4 How to Handle Errors Relating to Images Not Installed . . . . . 14�7

14.7 Compile and Install the TXLs . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�7

14.8 Compile and Install Your Form Libraries . . . . . . . . . . . . . . . . . . . . 14�9

14.9 How to Set Up a Remote Message Router . . . . . . . . . . . . . . . . . . . 14�9

14.10 Setting Up the Message Router Transfer Service . . . . . . . . . . . . . . 14�10

14.10.1 Con�guring the VMSmail Gateway . . . . . . . . . . . . . . . . . . . . . 14�11

14.11 Diagnostic Tools . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�11

14.12 Set the Global Buffers . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�12

14.13 Set the Terminal and Queue Characteristics for Printers . . . . . . . 14�13

14.14 Modi�cations Required for VTX . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�13

14.15 Replacing the Help Modules for Your Application . . . . . . . . . . . . . 14�13

14.16 Reschedule the ALL-IN-1 Housekeeping Procedures . . . . . . . . . . . 14�14

14.17 Changes Required if DECmail No Longer In Use . . . . . . . . . . . . . 14�14

14.18 Mail Directory Setup . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�14

14.19 ALL-IN-1 Setup . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�16

14.20 Convert WPS-PLUS/VMS Documents to ALL-IN-1 . . . . . . . . . . . . 14�18

14.21 Determining and Reporting Problems . . . . . . . . . . . . . . . . . . . . . . 14�19

A Files on the ALL-IN-1 V2.4 Distribution Media

A.1 Magnetic Tape and TK50 Kits . . . . . . . . . . . . . . . . . . . . . . . . . . . . A�1

A.2 Compact Disk Consolidated Software Distribution Kits . . . . . . . . . A�2

A.3 List of Files in Each Saveset . . . . . . . . . . . . . . . . . . . . . . . . . . . . . A�4 viii

B Sample Installations

B.1 Sample of a New Installation . . . . . . . . . . . . . . . . . . . . . . . . . . . . . B�1

B.2 Sample of an Upgrade Installation from ALL-IN-1 Version 2.3 . . . B�23

B.3 Sample of an ALL-IN-1 Version 2.4 Update Installation . . . . . . . . B�42

B.4 Additional Language Installation . . . . . . . . . . . . . . . . . . . . . . . . . . B�61

C Files and Logical Names Installed on Your System

C.1 Files Installed in Non-ALL-IN-1 Directories . . . . . . . . . . . . . . . . . C�1

C.2 Logical Names . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . C�2

C.2.1 Logical Names Entered into the System Logical Name

Table . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . C�2

C.2.2 Logical Names Entered into the Language Logical Name

Table . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . C�4

C.3 Directory Structure of an ALL-IN-1 System Installed on Separate

Disks . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . C�5

D Changing the Con�guration of ALL-IN-1 V2.4

D.1 Change to Using VAX DATATRIEVE . . . . . . . . . . . . . . . . . . . . . . . D�1

D.2 Change to Using WPS-PLUS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . D�2

D.3 Change to Using VAX ACMS . . . . . . . . . . . . . . . . . . . . . . . . . . . . . D�2

D.4 Change the Location of an ALL-IN-1 Version 2.4 Area . . . . . . . . . D�2

D.5 Moving ALL-IN-1 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . D�3

Index

FiguresC�1 Directory Structure of the ALL-IN-1 Manager’s Account . . . . . . . . C�6

C�2 Directory Structure for the Library Files . . . . . . . . . . . . . . . . . . . . C�7

C�3 Directory Structure for the Language Files . . . . . . . . . . . . . . . . . . C�8

C�4 Directory Structure for the Data Files . . . . . . . . . . . . . . . . . . . . . . C�8

C�5 Directory Structure for Mail Area E . . . . . . . . . . . . . . . . . . . . . . . C�8

C�6 Directory Structure for the Shared Directories . . . . . . . . . . . . . . . C�9ix

Tables1�1 Section Reference Chart . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 1�3

1�2 Actions to Complete Before Installing ALL-IN-1 . . . . . . . . . . . . . . 1�21

1�3 Required System Parameter Values . . . . . . . . . . . . . . . . . . . . . . . . 1�30

1�4 Process Account Quotas for the Installing Account . . . . . . . . . . . . 1�32

1�5 Disk Space Requirements for the ALL-IN-1 Areas . . . . . . . . . . . . . 1�35

3�1 Steps Required to Install a New ALL-IN-1 Version 2.4 System . . . 3�4

4�1 Steps Required for an ALL-IN-1 V2.4 Language Installation . . . . . 4�3

5�1 Steps Required to Upgrade ALL-IN-1 V2.3 to ALL-IN-1 V2.4 . . . . 5�4

6�1 Steps Required for Upgrading an ALL-IN-1 V2.3 Language . . . . . 6�3

7�1 Steps Required to Upgrade your ALL-IN-1 STARTER V1.0 System to ALL-IN-1 V2.4 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 7�4

8�1 Steps Required for Upgrading an ALL-IN-1 STARTER V1.0

Language . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 8�3

9�1 Steps Required to Update your ALL-IN-1 STARTER V2.4 System to ALL-IN-1 V2.4 . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 9�4

10�1 Steps Required for Updating an ALL-IN-1 STARTER V2.4

Language . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 10�3

11�1 Steps Required for Updating an Existing ALL-IN-1 V2.4

System . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 11�3

12�1 Steps Required for Updating an Existing ALL-IN-1 V2.4

Language . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 12�3

14�1 Section Reference Chart . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�1

14�2 Global Buffer Allocations . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 14�12 x

Preface

Product: ALL-IN-1 Version 2.4

Purpose of This Guide

This guide is Part 1 of three parts. See the section on Document Structure.

This part describes how to:

1 Prepare the VMS system for the installation of ALL-IN-1

2 Install ALL-IN-1

3 Set up ALL-IN-1 so that the ALL-IN-1 manager can log in to ALL-IN-1 and use ALL-IN-1 locally

All other tasks required to complete the set up of ALL-IN-1, and for ongoing management, are described in the ALL-IN-1 Management Guide and ALL-IN-1

Mail Management Guide, for example:

Printer set up

Creating accounts

Setting up Message Router and Message Router VMSmail Gateway, if mail messages need to be sent to other systems or VMS users

AudienceThis guide is primarily intended for:

Managers who want to install ALL-IN-1 Version 2.4 and set it up for use

Managers who want to upgrade to ALL-IN-1 Version 2.4 from either

ALL-IN-1 Version 2.3 or ALL-IN-1 STARTER Version 1.0 xi

Managers who want to update their current ALL-IN-1 STARTER Version

2.4 system to ALL-IN-1 Version 2.4

Managers who want to update their existing ALL-IN-1 Version 2.4 system

How To Use This Guide

Use this guide as follows:

1 Carry out the steps described in Chapter 2 to access the Release Notes.

You must print and read the Release Notes before starting the installation as they may contain information which applies to installation.

2 Read Chapter 1 which describes the tasks you must do before installing

ALL-IN-1.

3 Read the chapter corresponding to the type of installation you are going to perform, (see Chapters 3 to 12). The chapter lists the steps required to perform the installation.

4 Carry out the steps required for the type of installation you are going to perform. These steps are described in Chapter 13.

5 Read Chapter 14 which describes the tasks required to set up ALL-IN-1 so that the usual management and mail management tasks can be performed

(for example, creating user accounts) to allow your users to use ALL-IN-1.

Books in the Management Documentation Set

The following documents make up the ALL-IN-1 Management documentation set:ALL-IN-1 Installation Guide Part 1 Base Installation

This part describes the steps required to install ALL-IN-1 and contains information speci�c to the base component. Although it is a large book, you need only refer to the chapters relating to the type of installation that you are going to perform.

ALL-IN-1 Installation Guide Part 2 Language Installation

This part contains information speci�c to the language that you are installing; a version is supplied with each language component. Refer to this part as indicated in the ALL-IN-1 Installation Guide Part 1 Base

Installation. xii

ALL-IN-1 Installation Guide Part 3 Market Installation

This part contains information speci�c to your market component. Refer to this part as indicated in the ALL-IN-1 Installation Guide Part 1

Base Installation. Note that this document may not exist for all market components.

ALL-IN-1 Release Notes Part 1 Language

This part contains information about problems in the ALL-IN-1 Version 2.4 international base component and about problems that are speci�c to the language component that you install. Where possible, workarounds to the problems are also described.

ALL-IN-1 Release Notes Part 2 Market

This part contains information about problems that are speci�c to the

ALL-IN-1 Version 2.4 market component. Note that this document may not exist for all market components.

Differences Between ALL-IN-1 Version 2.3 and ALL-IN-1 Version 2.4

This document introduces the new and changed functionality, and describes the problems that have been �xed, in ALL-IN-1 Version 2.4. In addition, there are answers to some common questions about the new version, and details of packaging, software requirements, and changes to the documentation.

ALL-IN-1 Management Guide

This guide describes the tasks for setting up and managing an ALL-IN-1 system, so that it operates ef�ciently. The guide also explains how to improve performance, how to incorporate customizations, and how the

ALL-IN-1 �les are organized within VMS.

ALL-IN-1 Mail Management Guide

This guide describes how to manage an ALL-IN-1 mail system. The major management concern is to ensure that all messages sent to and from local

ALL-IN-1 users are delivered.

ALL-IN-1 Administration Guide

This guide describes the ALL-IN-1 administration tasks, which include maintaining ALL-IN-1 on a day-to-day basis and supporting users. The administration tasks are de�ned by the ALL-IN-1 manager, and are available from the Administration menu.

ALL-IN-1 Modifying Printer Tables

This guide describes the use of printer tables, and teaches you how to use the printer table utility to customize existing printer tables to meet your needs. xiii

Related Books

In addition to the ALL-IN-1 Management documentation set, your ALL-IN-1 kit contains a user documentation set and a programming documentation set.

The user documentation set contains:

ALL-IN-1 Getting Started

ALL-IN-1 Quick Lookup

ALL-IN-1 User’s Reference

ALL-IN-1 User Changes

ALL-IN-1 Keyboard Reference Cards

ALL-IN-1 Keyboard Diagram Cards

WPS-PLUS Quick Lookup

WPS-PLUS Editor Functions

WPS-PLUS List and Sort Processing

The programming documentation set contains:

ALL-IN-1 Application Programming: Getting Started

ALL-IN-1 Application Programming: Guide

ALL-IN-1 Application Programming: Mini-Reference

ALL-IN-1 Application Programming: Reference Volume 1

ALL-IN-1 Application Programming: Reference Volume 2

ALL-IN-1 Application Programming: User Interface Standards

ALL-IN-1 Application Programming: Index

WPS-PLUS Accessing External Applications

You may also need to refer to the documentation on the following products:

VAX FMS Version 2.4

ALL-IN-1 Version 2.4 Group Conferencing

ALL-IN-1 Voice Messaging Support Version 1.0

VAX Message Router Version 3.1

VAX Datatrieve Version 5.0

VAX Application Control and Management System Version 3.1

VAX DECpage Version 3.1

DECtalk Mail Access Version 1.1

VAX VTX Version 4.0

VAX TEAMDATA Version 1.3

VAX RALLY Version 2.0

DECdx/VMS Version 1.1 xiv

You may need to refer to the VMS books for the version of VMS running on your system.

Document Structure

ALL-IN-1 Installation Guide Part 1 Base Installation

This part describes the installation of ALL-IN-1 Version 2.4.

Chapter 1 Preparing to Install ALL-IN-1 V2.4

This chapter describes the steps to complete before beginning the installation, including how to prepare the system if you want to integrate ALL-IN-1 with optional software products.

Chapter 2 Accessing the Online Release Notes

This chapter describes how to access and print the online Release

Notes

Chapter 3 Installing a New ALL-IN-1 V2.4 System

This chapter describes the steps to perform to install a new

ALL-IN-1 Version 2.4 system.

Chapter 4 Installing Additional Languages for ALL-IN-1 V2.4

This chapter describes the steps to perform to install additional languages for ALL-IN-1 Version 2.4.

Chapter 5 Upgrading Your ALL-IN-1 V2.3 System to ALL-IN-1 V2.4

This chapter describes the steps to perform to upgrade from

ALL-IN-1 Version 2.3 to ALL-IN-1 Version 2.4.

Chapter 6 Upgrading ALL-IN-1 V2.3 Additional Languages to ALL-IN-1 V2.4

Additional Languages

This chapter describes the steps to perform to upgrade ALL-IN-1

Version 2.3 additional languages to ALL-IN-1 Version 2.4 additional languages.

Chapter 7 Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4

ALL-IN-1 STARTER Version 1.0 to ALL-IN-1 Version 2.4.

Chapter 8 Upgrading ALL-IN-1 STARTER V1.0 Additional Languages to

ALL-IN-1 V2.4 Additional Languages

STARTER Version 1.0 additional languages to ALL-IN-1 Version 2.4 additional languages.

Chapter 9 Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4

This chapter describes the steps to perform to update ALL-IN-1

STARTER Version 2.4 to ALL-IN-1 Version 2.4. xv

Chapter 10 Updating ALL-IN-1 STARTER V2.4 Additional Languages to

ALL-IN-1 V2.4 Additional Languages

This chapter describes the steps to perform to update ALL-IN-1

STARTER Version 2.4 additional languages to ALL-IN-1 Version 2.4 languages.

Chapter 11 Updating an Existing ALL-IN-1 V2.4 System

This chapter describes the steps to perform to update your existing

ALL-IN-1 Version 2.4 system. You can update your ALL-IN-1

Version 2.4 system if you decide to change the con�guration, or an

ALL-IN-1 component is revised by Digital.

Chapter 13 Steps Required for Installing ALL-IN-1 V2.4

This chapter contains a complete list of the steps required for installing ALL-IN-1 Version 2.4.

Chapter 14 After Installing ALL-IN-1 V2.4

This chapter describes the tasks to complete so that ALL-IN-1 can be run by users.

Appendix A Files on the ALL-IN-1 V2.4 Distribution Media

This appendix lists the �les contained on the distribution media.

Appendix B Sample Installation

This appendix contains computer listings of a new ALL-IN-1 Version

2.4 installation, an upgrade installation from ALL-IN-1 Version 2.3, and an additional language installation.

Appendix C Files and Logical Names Installed on Your System

This appendix lists the directories, and the �les in each directory, of an installed ALL-IN-1 Version 2.4 system.

Appendix D Changing the Con�guration of ALL-IN-1 V2.4

This appendix describes how to change the con�guration of an installed ALL-IN-1 Version 2.4 system.

ALL-IN-1 Installation Guide Part 2 Language Installation

This part contains language-speci�c information, for the language you are installing. There is a version of this part for each language supported by

ALL-IN-1 Version 2.4. Your ALL-IN-1 Version 2.4 kit contains a version of this part for each language included with the kit.

ALL-IN-1 Installation Guide Part 3 Market Installation

This part contains market-speci�c information, where a market may be speci�c to a single country. Your ALL-IN-1 Version 2.4 kit contains the version speci�c to your market. xvi

ConventionsThe following conventions are used throughout this document:

Messages Indicates prompts and messages from the computer.

Red Print Indicates entries you make at the terminal.

lowercase Lowercase text in an ALL-IN-1 function call, or in a DCL command or command procedure, indicates that you substitute a valid expression in that place.

[ ] Brackets in an ALL-IN-1 function, or in a DCL command or command procedure, indicate an optional entry, or a DCL directory speci�cation.

. . . Horizontal ellipses indicate that additional data or text can be entered.

. Vertical ellipses indicate that the example can or does contain more data or text than is shown.

123 Marks the order of the steps to complete a procedure.

a.b.c. Marks steps within a major step in a procedure.

Press Indicates that you make one keystroke with an editing or command key. For example, press RETURN.

Enter Means type a command or response, or type information into a menu or form, and then press a terminator key such as RETURN.

UPPERCASE Indicates keyboard keys and GOLD functions.

< > Indicates a display that is variable.

CTRL/z Indicates that you hold down the CTRL key while pressing the other key (z).

GOLD x Means press the GOLD key, labeled PF1 on some keyboards, then press the key for the function. For example, GOLD TOP.

STEP n Indicates step n of the ALL-IN-1 installation procedure.

step n Indicates step n of a pre-installation or post-installation task.

ALL-IN-1 Means ALL-IN-1� of�ce automation system

DECnet Means DECnet� software

Message Router Means Message Router� software

WPS-PLUS Means WPS-PLUS� software xvii

1 Preparing to Install ALL-IN-1 V2.4

You install ALL-IN-1 Version 2.4 using VMSINSTAL, from the SYSTEM account. VMSINSTAL is a command procedure used to install optional software products on the VMS operating system.

You can install ALL-IN-1 Version 2.4 if you are not currently running

ALL-IN-1, or you can upgrade your ALL-IN-1 Version 2.3 system to

ALL-IN-1 Version 2.4. You must also upgrade your languages to the corresponding ALL-IN-1 Version 2.4 languages.

You can also install additional languages, or update the language(s) currently being used by your ALL-IN-1 Version 2.4 system.

If you are currently running ALL-IN-1 STARTER Version 1.0, you can upgrade to ALL-IN-1 Version 2.4 (see Chapter 7). You must also upgrade your languages to the corresponding ALL-IN-1 Version 2.4 languages.

If you are currently running ALL-IN-1 STARTER Version 2.4, you can update to ALL-IN-1 Version 2.4 (see Chapter 9).

If you decide to change the con�guration of your existing ALL-IN-1 Version

2.4 system, or an ALL-IN-1 component is revised by Digital, you can update your ALL-IN-1 Version 2.4 system.

If you are currently using WPS-PLUS/VMS, and you do not have a previous version of ALL-IN-1, you can install ALL-IN-1 Version 2.4 and optionally convert your WPS-PLUS/VMS users to ALL-IN-1. See Section 14.20 for details.

If you are currently running ALL-IN-1 Version 2.2, ALL-IN-1/BEV Version

2.1 or ALL-IN-1 Version 2.1, you must �rst upgrade to ALL-IN-1 Version

2.3 and then upgrade to ALL-IN-1 Version 2.4 as described later. Note that you must read the ALL-IN-1 Version 2.3 Release Notes and ALL-IN-1

Installation Guide before installing ALL-IN-1 Version 2.4.Preparing to Install ALL-IN-1 V2.4 1�1

For certain changes to your existing ALL-IN-1 Version 2.4 system you need not perform an update installation (for example, if you want to recon�gure

ALL-IN-1 to use VAX DATATRIEVE). These changes are described in

Appendix D.

To prepare for installation:

1 Check that the distribution kit is complete and correct according to the bill of materials included with the kit. See Section 1.1.

2 Make sure that your system has the prerequisite software. See Section 1.4.

3 Determine what other products you need to install before installing

ALL-IN-1. See Section 1.5.

4 If you are intending to install ALL-IN-1 on a VAXcluster, see Section 1.6.

5 If you are intending to install additional languages, see Section 1.7.

6 Set up your system so that it is ready for the installation. See Section 1.8.

7 Complete the checklist of information appropriate to the type of installation you are going to perform. See Section 1.8.20.

8 If you are unfamiliar with ALL-IN-1, see the �rst chapter of the ALL-IN-1

User’s Reference before starting installation.

Table 1�1 indicates the sections that you need to refer to in this chapter for the type of installation that you are going to perform.

1�2 Preparing to Install ALL-IN-1 V2.4

Table 1�1 Section Reference Chart

Installation Type

Sections 1.1 1.2 1.3 1.4 1.5 1.6 1.7 1.8

New ALL-IN-1

V2.4 installation

* * * * * * *

New additional language installation * * * * * * *

Upgrade from

ALL-IN-1 V2.3

Upgrade of an language * * * * * * *

ALL-IN-1

STARTER V1.0 * * * * * * *

Upgrade of an ALL-IN-1

STARTER V1.0

Update from

STARTER V2.4 * * * * * * *

Update of

STARTER V2.4

ALL-IN-1 V2.4

Update of an additional

* Indicates that you need to refer to this section

1.1 Examining the Distribution Kit

To make sure that you have a complete kit, check the contents of the kit against the bill of materials.

If your kit is damaged or if you �nd that parts of it are missing, contact your

Digital representative. Preparing to Install ALL-IN-1 V2.4 1�3

1.1.1 Magnetic Tape and TK50 Kits

All full ALL-IN-1 Version 2.4 kits (that is, as opposed to an additional language kit) should contain:

Three magnetic tapes or TK50 cartridges containing all the �les listed in Appendix A of this book, the ALL-IN-1 Installation Guide Part 2

Language Installation and the ALL-IN-1 Installation Guide Part 3 Market

Installation. The VAX FMS Version 2.4 software is also contained on the tape or TK50 cartridge labeled:

ALL-IN-1 V2.4 BASE BIN media_type

INTERNATIONAL BASE

(c) 1989 Digital Equipment Corp.

media_type is 16MT9 for tape or TK50 for a TK50 cartridge.

One magnetic tape or TK50 cartridge containing the Message Router

VMSmail Gateway Version 3.1 kit. The kit contains Message Router

Version 3.1 and Message Router VMSmail Gateway Version 3.1.

One magnetic tape or TK50 cartridge containing the Release Notes Part 1

Language, for the language component supplied with your kit.

One magnetic tape or TK50 cartridge containing the Release Notes Part 2

Market, for the market component supplied with your kit. (This document may not exist for all market components.)

A Software Product Description (SPD).

A System Support Addendum.

The ALL-IN-1 Installation Guide Part 1 Base Installation (this book)

The ALL-IN-1 Installation Guide Part 2 Language Installation, for the language component supplied with your kit.

The ALL-IN-1 Installation Guide Part 3 Market Installation, for the market component supplied with your kit.

If you are installing an additional language you should have:

A magnetic tape or TK50 cartridge containing the �les for the language that you are installing (see Appendix A of the ALL-IN-1 Installation Guide

Part 2 Language Installation)

A magnetic tape or TK50 cartridge containing the Release Notes Part 1

Language, for the additional language additional language

1�4 Preparing to Install ALL-IN-1 V2.4

1.1.2 Compact Disk Consolidated Software Distribution Kits

All full ALL-IN-1 Version 2.4 kits (that is, as opposed to an additional language kit) should contain one compact disk (CD) containing all the �les listed in

Appendix A of this book.

The CD also contains VAX FMS Version 2.4, and Message Router VMSmail

Gateway Version 3.1 which contains Message Router Version 3.1 and Message

Router VMSmail Gateway Version 3.1.

The following documentation (in ASCII text format) is also included on the CD:

A Read Me First

The ALL-IN-1 Installation Guide Part 1 Base Installation (this book)

The ALL-IN-1 Installation Guide Part 2 Language Installation, for the language component supplied with your kit.

The ALL-IN-1 Installation Guide Part 3 Market Installation, for the market component supplied with your kit.

A Software Product Description (SPD)

A System Support Addendum (SSA)

A Software Warranty Addendum (SWA)

If you are installing an additional language you should have a CD containing the �les for the language that you are installing (see Appendix A of the

ALL-IN-1 Installation Guide Part 2 Language Installation).

The CD also includes (in ASCII text format):

additional language

1.2 VMS License Management Facility

The VMS License Management Facility (LMF) is available with Version 5.1 of the VMS operating system. If you are installing ALL-IN-1 Version 2.4 on a

VMS V5.1 (or higher) system, you must register your software license.

The license registration information you need is contained in the Product

Authorization Key (PAK) that comes with ALL-IN-1 Version 2.4. The PAK is a paper certi�cate that contains information about the license you must have in order to run a particular piece of software.

You must register your ALL-IN-1 Version 2.4 license before you perform the installation. During the installation, you are asked if you have registered the

ALL-IN-1 Version 2.4 license and loaded the appropriate authorization key.

Preparing to Install ALL-IN-1 V2.4 1�5

To register a license under VMS V5.1, �rst log in to the system manager’s account, SYSTEM. You then have a choice of two ways to perform the registration:

Invoke the SYS$UPDATE:VMSLICENSE.COM procedure. When it prompts you for information, respond with data from your Product

Authorization Key (PAK).

Issue the DCL command, LICENSE REGISTER, together with the appropriate quali�ers that correspond to information on the PAK.

For complete information on using LMF, see the manual on the License

Management Utility in the VMS V5.1 documentation set.

1.3 Required Operating System Components

For VMS Version 5.1, or higher, systems, ALL-IN-1 Version 2.4 requires that your system is running a full, untailored VMS system.

1.4 Prerequisite Software

The following software must be installed on your system:

VMS Version 5.1, or higher

VAX Forms Management System (FMS) Version 2.4.

Note ALL-IN-1 must have the form driver (FDVSHR) installed as a known shareable image. See Section 1.4.1.

See the VAX FMS Installation Guide and Release Notes for details of installing VAX FMS. (If you want to run the sample programs supplied with VAX FMS you must have at least one compiler installed on your system.)

Digital does not recommend the use of any earlier version of FMS with

ALL-IN-1 Version 2.4.

If you install VAX FMS from the kit supplied with ALL-IN-1 Version

2.4, you must register the license before you can run FMS. FMS must be running before you install ALL-IN-1.

1.4.1 Installed Images

Make sure that the following shareable image and message �les are installed on your system before installing ALL-IN-1:

SYS$MESSAGE:FDVMSG.EXE

SYS$SHARE:CONVSHR.EXE

SYS$SHARE:FDLSHR.EXE

1�6 Preparing to Install ALL-IN-1 V2.4

SYS$SHARE:FDVSHR.EXE

SYS$SHARE:LBRSHR.EXE

SYS$SHARE:MTHRTL.EXE

SYS$SHARE:NMLSHR.EXE

SYS$SHARE:PASRTL.EXE

SYS$SHARE:SCNRTL.EXE

SYS$SHARE:SCRSHR.EXE

SYS$SHARE:VMSRTL.EXE

SYS$SHARE:VAXCRTL.EXE

To check whether or not these images are installed on your system, enter the following:

$ INSTALL

INSTALL> LIST image image is the image to be checked. For example, SYS$SHARE:CONVSHR.

If the Install Utility cannot �nd an entry for an image, install the image as follows:

INSTALL> CREATE image /OPEN /SHARED /HEADER_RES

INSTALL> EXIT

Note If the images FDVMSG.EXE and FDVSHR.EXE are not installed, edit the command procedure SYS$MANAGER:FMSTARTUP.COM, remove the EXIT command before the entry RUN SYS$SYSTEM:INSTALL, and then execute the command procedure.

If there is an entry for the image, check that the display shows the following information:

imagename.EXE Open Hdr Shar imagename is the name of the image. For example, CONVSHR.

If the display does not show this information, change the way that the image is installed as follows:

INSTALL> REPLACE image /OPEN /SHARED /HEADER_RES

For details of installing shareable image �les, see the VMS manual describing the Install Utility. Preparing to Install ALL-IN-1 V2.4 1�7

Note that the following images are temporarily installed during the installation of ALL-IN-1:

If you integrated WPS-PLUS:

- SYS$SHARE:LNGSPLCOM.EXE

- SYS$SHARE:LNGOSENVR.EXE

- SYS$SHARE:LNGSPLMSG.EXE

- SYS$SHARE:LNGSPLlang.EXE, for all languages with DECspell support (see the ALL-IN-1 Installation Guide Part 2 Language

Installation)

- SYS$SHARE:LNGSPLSHR.EXE

If standalone DECspell is installed on your system:

- SYS$SYSTEM:LNGSPLCOR.EXE

- SYS$SYSTEM:LNGSPLNDX.EXE

- SYS$SYSTEM:LNGSPLFOR.EXE

The ALL-IN-1 startup command procedure A1V24START.COM installs all these as known images at system startup. This command procedure is in

SYS$MANAGER.

1.5 Optional Software Products

The following products can be purchased separately and integrated with

ALL-IN-1:

VAX DATATRIEVE Version 5.0 or higher. See Section 1.5.2.

Digital does not recommend the use of any earlier version of VAX

DATATRIEVE with ALL-IN-1 Version 2.4.

VAX Application Control and Management System (ACMS) Version 3.1 or higher. See Section 1.5.4

Digital does not recommend the use of any earlier version of ACMS with

ALL-IN-1 Version 2.4.

Message Router Version 3.1 is supplied with ALL-IN-1 Version 2.4 (see

Section 1.5.3). If you want to use Mail directory addressing you must install

Message Router Version 3.1 on the same node as ALL-IN-1. Digital does not recommend the use of any earlier version of Message Router with ALL-IN-1

Version 2.4.

1�8 Preparing to Install ALL-IN-1 V2.4

Message Router VMSmail Gateway (MRGATE) Version 3.1 is supplied with

ALL-IN-1 Version 2.4 (see Section 1.5.3). If you want to install Message Router on the same node as ALL-IN-1, Digital does not recommend the use of any earlier version of MRGATE with ALL-IN-1 Version 2.4.

Note If you install Message Router and Message Router VMSmail Gateway from the kit supplied with ALL-IN-1 Version 2.4, you must register the licenses for both products before you can run them. Message Router and, if installed, Message

Router VMSmail Gateway must be running before you install ALL-IN-1.

If you want to use any of these products with ALL-IN-1, see the order of installation listed in Section 1.5.6.

In addition, the following products can be integrated with ALL-IN-1:

ALL-IN-1 Version 2.4 Group Conferencing

ALL-IN-1 Version 2.4 Group Conferencing is an option that you install separately. ALL-IN-1 Version 2.4 Group Conferencing provides an interface, from within ALL-IN-1, to VAX Notes conferences.

VAX DECpage Version 3.1

DECpage is an ALL-IN-1 option that you install separately. When VAX

DECpage Version 3.1 is installed after ALL-IN-1, it is accessible from the

Word and Document Processing (WP) menu within ALL-IN-1. It is not necessary to link the VAX DECpage software to ALL-IN-1.

VAX VTX Version 4.0

VTX is an ALL-IN-1 option that you install separately. When VAX VTX

Version 3.1 is installed after ALL-IN-1, it is accessible from the Information

Management (IM) menu within ALL-IN-1. It is not necessary to link VAX

VTX software to ALL-IN-1.

VAX TEAMDATA Version 1.3

VAX RALLY Version 2.0

Language and Specialized Lexicons. See the ALL-IN-1 Installation Guide

Part 2 Language Installation for the language and specialized lexicons supported. (The language and specialized lexicons are only available for certain languages.)

DECtalk Mail Access Version 1.1.

DECdx/VMS Version 1.1

DECdx/VMS is required only to allow users to transfer DX documents between Digital’s mainframe computers (in conjunction with DECdx/RSTS,

DECdx/RSX and DECdx/TOPS-20) Preparing to Install ALL-IN-1 V2.4 1�9

DECnet/VAX Version 5.1 can be purchased separately. If you want to exchange mail with other systems and use the Time Management scan option you must install DECnet/VAX Version 5.1 on your system.

If you are upgrading to ALL-IN-1 Version 2.4, and you are currently running any ALL-IN-1 layered products, you may need to prepare the layered product(s) before you install ALL-IN-1 Version 2.4 (see your layered product documentation).

1.5.1 Initial DDIF Support

ALL-IN-1 provides users with the ability to manipulate Digital Document

Interchange Format (DDIF) documents, for example, documents produced by

DECwrite. You can:

Send or forward DDIF documents by mail as attachments between

ALL-IN-1 users on the same or remote nodes

You can store the DDIF documents directly in the ALL-IN-1 File Cabinet and read them (display on the screen) using the Word and document processing Read (WP R) option.

When in the ALL-IN-1 File Cabinet you can manipulate the DDIF documents using any of the File Cabinet (FC) functions such as Delete and Archive.

Edit DDIF documents by using either the EDT or WPS-PLUS editors

Print DDIF documents either on PostScript capable printers or on ASCII printers

Export DDIF documents from the ALL-IN-1 File Cabinet to VMS where they reside as VMS �les

Convert DDIF documents to ASCII, DX, WPS-PLUS, or Alternate Format

Syntax (AFS)

Create DDIF documents by converting documents in ASCII, DX,

WPS-PLUS, or AFS to DDIF

The following software must be installed, before you can use DDIF with

ALL-IN-1.

DECwindows Version 1.0, or higher

The installation checks to see if the logical name CDA$LIBRARY is de�ned.

Compound Document Architecture Converter Library Version 1.0

The installation checks to see if the following �les are present:

- DDIF$READ_DX.EXE

- DDIF$READ_DFX.EXE

1�10 Preparing to Install ALL-IN-1 V2.4

- DDIF$WRITE_AFS.EXE

The �les for DDIF support are installed during the installation of ALL-IN-1

Version 2.4. However, your users will be unable to convert DDIF documents to

ALL-IN-1 until the prerequisite software is installed.

1.5.2 Integrating VAX DATATRIEVE with ALL-IN-1

If you integrate VAX DATATRIEVE Version 5.0 with ALL-IN-1, you can use the ALL-IN-1 DTR function to make VAX DATATRIEVE applications available from ALL-IN-1. See ALL-IN-1 Application Programming: Reference Volume 2 for details.

The ALL-IN-1 installation procedure asks if you want to integrate VAX

DATATRIEVE with ALL-IN-1.

You must install the following images before you install ALL-IN-1 if you want

ALL-IN-1 to integrate with VAX DATATRIEVE:

SYS$SHARE:DTRSHR.EXE

SYS$SHARE:CDDSHR.EXE

SYS$MESSAGE:CDDEXC.EXE

SYS$MESSAGE:DTRMSGS.EXE

If these images are not installed, ALL-IN-1 cannot link with the VAX

DATATRIEVE software.

In addition, if you are integrating with VAX DATATRIEVE software, and if

VAX DATATRIEVE links against any of the images in the following list (see the VAX Datatrieve Installation Guide), you must install them before installing

ALL-IN-1:

SYS$MESSAGE:DBMMSG.EXE

SYS$SHARE:RDBSHR.EXE

SYS$SHARE:RDMSHR.EXE

SYS$SHARE:SORTSHR.EXE

SYS$SHARE:EDTSHR.EXE

SYS$SHARE:SECURESHR.EXE

SYS$MESSAGE:RDBBMSGS.EXE

SYS$MESSAGE:RDBMSGS.EXE

SYS$MESSAGE:SHRIMGMSG.EXE Preparing to Install ALL-IN-1 V2.4 1�11

Also, all the SYS$SHARE:*RTL.EXE images must be installed. If you are not sure whether or not any of these images are installed on your system, enter the following commands from the VMS system manager’s account:

$ INSTALL

INSTALL> LIST image image is the image to be checked, for example, SYS$SHARE:DBMSHR.

If the Install utility cannot �nd an entry for an image, install the image as follows:

INSTALL> CREATE image /OPEN /SHARED /HEADER_RES

INSTALL> EXIT

If there is an entry for the image, check that the display shows the following information:

imagename.EXE Open Hdr Shar imagename is the name of the image, for example, DBMSHR.

If the display does not show this information, change the way that the image is installed as follows:

INSTALL> REPLACE image /OPEN /SHARED /HEADER_RES

For details of installing shareable image �les, see the VMS manual describing the Install Utility.

1.5.3 Integrating Message Router and the Message Router

VMSmail Gateway with ALL-IN-1

The ALL-IN-1 installation procedure asks if you want to send and receive remote mail.

Install and con�gure Message Router before you install ALL-IN-1, if you want to send and receive remote mail

Install and con�gure Message Router and the Message Router VMSmail

Gateway before you install ALL-IN-1, if you want to send mail to VMSmail users, either on the local system or remotely

If you want to install Message Router on the local system (that is, the system on which you are installing ALL-IN-1) then you must install

Message Router Version 3.1. The Message Router on the local system is referred to as a local Message Router. Both Message Router Version 3.1 and the Message Router VMSmail Gateway Version 3.1 are provided in the

ALL-IN-1 kit.

If you want to use the Message Router Directory Service (referred to as the

Mail directory), you must install Message Router Version 3.1 on the local system before you install ALL-IN-1.

1�12 Preparing to Install ALL-IN-1 V2.4

If you already have Message Router Version 3.1 installed on your system, make sure that it is con�gured before you install ALL-IN-1 Version 2.4.

If ALL-IN-1 Version 2.4 is already installed, and you want to install

Message Router on the local system, you must install and con�gure

Message Router Version 3.1 and then perform an update installation of

ALL-IN-1 Version 2.4.

You can also integrate ALL-IN-1 with Message Router on a remote system

(that is, a system other than the one on which you are installing ALL-IN-1).

See Section 14.9 for more information. You may want to do this if you do not have enough space on your own system to install Message Router. However, the Mail directory is not available when Message Router is remote, so you cannot use Mail directory addressing (see Section 1.5.3.1). The Message Router on the remote system is referred to as a remote Message Router.

When you install Message Router the exception reporting routines for the

ALL-IN-1 Electronic Messaging subsystem are installed. If you want to run the exception reporting routines, you must con�gure exception reporting for the ALL-IN-1 Electronic Messaging subsystem.

See Section 1.6 for information on using ALL-IN-1 and Message Router on

VAXcluster systems.

For more information on installing and using Message Router and Message

Router VMSmail Gateway, refer to the Message Router and Message Router

VMSmail Gateway books, and the ALL-IN-1 Mail Management Guide.

Before you install ALL-IN-1, read the chapter on planning in the ALL-IN-1

Mail Management Guide, to decide how to set up the mail system.

1.5.3.1 The Mail Directory and the ALL-IN-1 Directory

The Mail directory and the ALL-IN-1 directory are directories of users in the network. These directories hold the names and electronic mail addresses of users in the network.

The Mail directory is provided by the Directory Service component of Message

Router.

Before deciding whether or not to use the Mail directory, see the Planning chapter in the ALL-IN-1 Mail Management Guide.Preparing to Install ALL-IN-1 V2.4 1�13

1.5.4 Integrating ACMS with ALL-IN-1

ACMS is a software tool that makes online applications easier to develop.

If you want to integrate ACMS with ALL-IN-1, you must install the �le

ACMSHR.EXE. If you are not sure whether ACMSHR.EXE is installed on your system, enter the following commands from the VMS system manager’s account:

$ INSTALL

INSTALL> LIST SYS$SHARE:ACMSHR

If the Install utility cannot �nd an entry for ACMSHR.EXE, install it as follows:

INSTALL> CREATE SYS$SHARE:ACMSHR /OPEN /SHARED /HEADER_RES

INSTALL> EXIT

If there is an entry for ACMSHR.EXE, check that the display shows the following information:

ACMSHR.EXE Open Hdr Shar

If the display does not show this information, change the way that

ACMSHR.EXE is installed as follows:

INSTALL> REPLACE SYS$SHARE:ACMSHR /OPEN /SHARED /HEADER_RES

1.5.5 Integrating WPS-PLUS with ALL-IN-1

You can integrate WPS-PLUS Version 3.1 when you install ALL-IN-1. An installation question asks whether you want to integrate WPS-PLUS. If you choose to integrate WPS-PLUS it is fully integrated with ALL-IN-1 and is available as the default editor. You do not need additional software to integrate

WPS-PLUS, as everything required is provided in the ALL-IN-1 kit. After installation there are a number of tasks you must perform before users can use WPS-PLUS, for example, setting terminal and queue characteristics (see

Section 14.13 and the ALL-IN-1 Management Guide for details).

If WPS-PLUS/VMS already exists on your system, you can still integrate and use WPS-PLUS with ALL-IN-1 (see Section 14.20 for details).

If you integrate WPS-PLUS with ALL-IN-1, you may be able to use various spell-checking lexicons. See the ALL-IN-1 Installation Guide Part 2 Language

Installation for the spell-checking lexicon that is supplied with your kit, and for any other optional products.

Note Lexicons are only available for certain language versions of ALL-IN-1 Version

2.4.

1�14 Preparing to Install ALL-IN-1 V2.4

1.5.6 Installation Order

The following installation order is recommended:

1 Register the licenses for VAX FMS Version 2.4, Message Router Version 3.1,

Message Router VMSmail Gateway Version 3.1, CDA Converter Library

Version 1.0 and VAX Notes Version 2.0.

2 Install VAX FMS Version 2.4, if it is not already installed on your system.

3 Install ACMS Version 3.1, or higher, if you want to incorporate it with

ALL-IN-1 Version 2.4.

4 Install VAX DATATRIEVE Version 5.0, or higher, if you want to incorporate it with ALL-IN-1 Version 2.4.

5 Install Message Router Version 3.1, if you want to send and receive messages to and from other systems, or you want to use Mail directory addressing, or you want to send mail to VMSmail users, either on the local system or to remote systems.

6 Con�gure Message Router Version 3.1, if it is installed and not yet con�gured.

7 Install Message Router VMSmail Gateway Version 3.1, if you want to send mail to VMSmail users, either on the local system or remotely.

8 Con�gure Message Router VMSmail Gateway Version 3.1, if it is installed and not yet con�gured.

9 Install CDA Converter Library Version 1.0.

10 Install ALL-IN-1 Version 2.4.

11 Con�gure exception reporting routines for ALL-IN-1 Version 2.4 Electronic

Messaging subsystem.

12 Install VAX Notes Version 2.0.

13 Install ALL-IN-1 Version 2.4 Group Conferencing.

Note WPS-PLUS is supplied with ALL-IN-1. If you choose to integrate WPS-PLUS with ALL-IN-1, it is available as the default editor in ALL-IN-1.

1.5.7 Keeping a Record of the Installation

When you install ALL-IN-1 Version 2.4, Digital recommends that you use a hard-copy terminal, so that you have a permanent record of the installation.

Alternatively, you can keep a record of the installation in a log �le if you enter the command:

$ SET HOST /LOG=filename 0 Preparing to Install ALL-IN-1 V2.4 1�15

where �lename is the name of the log �le. For example, you might use

ALLIN1_INSTALL.LOG. The default is SETHOST.LOG, if �lename is omitted.

The log �le is created in the directory where you entered the command. For example, if you enter the command in the directory

SYS$SYSDEVICE:[SYSTEM.FRED] then this directory will contain the log �le.

To use the SET HOST command, DECnet must be running on your system.

Make a note of the directory where you entered the SET HOST command.

If you decide to keep a record of the installation in a log �le, you need to allow at least 200 blocks, in addition to the space required for ALL-IN-1 (see

Section 1.8.16).

If you have a VAXcluster system, and you are running the VAXcluster Console

System (VCS), you can use this to record the installation of ALL-IN-1 Version

2.4. This does not require DECnet to be running, does not use any disk space on the system where the installation is performed, and does not echo any passwords that you enter during the installation. See the manual for the

VAXcluster Console System.

1.6 Installing ALL-IN-1 on VAXcluster Systems

ALL-IN-1 Version 2.4 can be installed on a common-environment cluster, a multiple-environment cluster or Local Area VAXcluster.

1.6.1 Installing ALL-IN-1 on a Common-Environment Cluster

In a common-environment cluster, the operating environment is identical on each member node, because the nodes are run from the same system �les. The nodes are set up with identical user accounts, the same known images (such as the ALL-IN-1 image) are installed, the same logical names are de�ned, and mass storage devices and queues are shared. In effect, users in a commonenvironment cluster can log in to any node and work in the same operating environment. For example, ALL-IN-1 will be installed on one node only, but will be available to users on all nodes.

1.6.1.1 Running ALL-IN-1 on a Common-Environment Cluster

When running ALL-IN-1 on a common-environment cluster:

You must run the ALL-IN-1 startup command procedure,

SYS$MANAGER:A1V24START.COM, on all nodes in the cluster on which you want to run ALL-IN-1. (See Section 14.6 of this guide.)

Note ALL-IN-1 Version 2.4 does not support rolling upgrades; that is, mixed

VMS Version 4.7 and Version 5.0 clusters. All nodes in the cluster must be running VMS Version 5.1, or higher, before you install ALL-IN-1 Version

2.4.You can spread the ALL-IN-1 areas around your VAXcluster disks, just as you would for a single-node system (see Section 1.8.16).

1�16 Preparing to Install ALL-IN-1 V2.4

You must check the VMS system parameters, as described in Section 1.8, on each node in the VAXcluster on which you are going to run ALL-IN-1.

The housekeeping procedure which creates new shared directories has to de�ne new system logical names on each node in a VAXcluster. You must ensure that the new names are de�ned on every node in the cluster for which the new shared directories will be created. Use the Manage node speci�c batch queues (MNQ) option on the Manage Mail Areas menu to do this. See the ALL-IN-1 Management Guide for details.

The default value of the logical name OA$PRIMARY_NODE is set by

A1V24START.COM after the installation has completed, as follows:

- If you are using a remote Message Router, OA$PRIMARY_NODE is set to the name of the node on which the Message Router is resident.

- If you are installing ALL-IN-1 on a VAXcluster, and cluster aliasing is enabled, OA$PRIMARY_NODE is set to the cluster alias.

- If you are using a local Message Router and cluster aliasing is not enabled, OA$PRIMARY_NODE is the name of the node on which the

Message Router is resident.

The node name represented by this logical name is used in ALL-IN-1 directory addressing as the node name for all users on the cluster. It is also used by Electronic Messaging in the return address for all mail sent to other computer systems via Message Router.

For further information about clusters, see the VMS VAXcluster documentation.1.6.2 Installing ALL-IN-1 on a Multiple-Environment Cluster

In a multiple-environment cluster, the environment varies from node to node, and users can work in environments that are speci�c to the node that they are logged in to. A multiple-environment cluster is effective when you want to share data among member nodes, but when you want certain nodes to serve specialized needs. A multiple-environment cluster can be considered as having different parts, each part providing a different environment.

For example, you might want to set up a three-node cluster in which ALL-IN-1 can be used on two nodes, while the third node is set up exclusively for batch processing of large inventory jobs. In this case, the nodes from which

ALL-IN-1 is available are set up with a common environment, sharing users, queues, and access to mass storage devices, while the the third node runs in its own restricted environment and ALL-IN-1 is unavailable.

However, you must run the ALL-IN-1 startup command procedure,

SYS$MANAGER:A1V24START.COM, on all the nodes in the part of the cluster with the common environment. Preparing to Install ALL-IN-1 V2.4 1�17

Another con�guration might have four nodes split into two parts (two nodes in each part), with both parts providing distinct common environments. If you want to run ALL-IN-1 on all four nodes, you must install ALL-IN-1 in each part. However, the ALL-IN-1 system on one part is available only to users logged in to that part of the cluster. The two ALL-IN-1 systems are managed separately.

1.6.2.1 Running ALL-IN-1 on a Multiple-Environment Cluster

When running ALL-IN-1 on a multiple-environment cluster:

You must check the VMS system parameters, as described in Section 1.8, on each node in the part of the cluster on which you are going to run

ALL-IN-1.

ALL-IN-1 is only available to users that are logged in to the part on which

ALL-IN-1 is installed. If a part of the cluster does not have ALL-IN-1 installed, users logged in to a node in that part of the cluster cannot use

ALL-IN-1. Therefore, users (including batch jobs) of an ALL-IN-1 system must make sure that they are running on the part of the cluster containing the ALL-IN-1 system that they want to use.

The ALL-IN-1 housekeeping procedures must be assigned to a batch queue.

You must use a queue speci�c to the part of the cluster on which the

ALL-IN-1 system is running. If your system has a cluster-wide generic queue which points to all queues in the cluster you must not use that queue.

The housekeeping procedure which creates new shared directories has to de�ne new system logical names on each node in a VAXcluster. You must ensure that the new names are de�ned on every node in the part of the cluster containing the ALL-IN-1 system for which the new shared directories will be created. Use the Manage node speci�c batch queues

(MNQ) option on the Manage Mail Areas menu to do this. See the

ALL-IN-1 Management Guide for details.

You must install Message Router, if you want to send and receive remote mail.

If you want to use Mail directory addressing, you must install Message

Router Version 3.1 on the same part of the cluster on which you are going to install the ALL-IN-1 system. In this case, Message Router is referred to as a local Message Router.

Note Mail directory addressing can only be used on certain multiple-environment cluster con�gurations. See the Message Router Installation Guide for details.

1�18 Preparing to Install ALL-IN-1 V2.4

You can use Message Router on another part of the cluster, or on another system, if you do not have enough disk space on the part that you are going to install ALL-IN-1. In this case, Message Router is referred to as a remote

Message Router. You cannot use Mail directory addressing with a remote

Message Router.

The main points to remember when running ALL-IN-1 in a multipleenvironment cluster are:

Users must log in to the right part of the cluster to use ALL-IN-1.

Batch queue names should be speci�c to the part of the cluster running

ALL-IN-1.

You must run A1V24START.COM on every node in the part of the cluster running ALL-IN-1. This command procedure is in SYS$MANAGER.

To use the Mail directory, you must install Message Router Version 3.1 in the same part as ALL-IN-1. However, the Mail directory can only be used on certain multiple-environment cluster con�gurations (see the Message

Router Installation Guide for details). You can use a remote Message

Router, but you cannot use the Mail directory.

For further information about clusters, see the VMS VAXcluster documentation.1.6.3 Installing ALL-IN-1 on a Local Area VAXcluster System

You can install ALL-IN-1 Version 2.4 on a local area VAXcluster system. A local area VAXcluster system consists of a boot node (a VAX system or MicroVAX system containing all the disks from which ALL-IN-1 is run) connected by

Ethernet to a number of satellite nodes, usually MicroVAX systems.

If you are using a local area VAXcluster system, Digital recommends that you install ALL-IN-1 on the boot node. This node is likely to be the only node where disk space is available to run ALL-IN-1. The satellite nodes are for the individual work groups only, and they use the boot node to access ALL-IN-1

�les.You must check the VMS system parameters as described in Section 1.8, on each node in the local area VAXcluster system on which you are going to run

ALL-IN-1.

Note If you intend to install ALL-IN-1 on a local area VAXcluster system, Digital recommends that you contact your local Software Services representative.

Preparing to Install ALL-IN-1 V2.4 1�19

1.7 Installing Additional Languages

Your basic ALL-IN-1 Version 2.4 kit is supplied with a speci�c language component for your market. You can use other languages with your ALL-IN-1

Version 2.4 system, in addition to the one supplied with your kit. If you want to install additional languages, you must have speci�ed that you wanted to build a multi-language system when you installed the original language. See the System Support Addendum for a list of the languages supported by your

ALL-IN-1 Version 2.4 system.

If, during the installation of the original language, you answered NO to the prompt Do you want to build a multi-language system?, you must re-link

ALL-IN-1 Version 2.4 and answer YES to this prompt. See the ALL-IN-1

Management Guide for details on linking the ALL-IN-1 image.

You can install the languages (if available), including the one supplied with your kit, in any order. However, the language that you install when the main ALL-IN-1 Version 2.4 kit is installed is the default language. That is, it is the language indicated in the language �eld of the user’s account details, and is used by ALL-IN-1 if you do not use the /LANGUAGE quali�er

(see Section 14.6) when logging in to ALL-IN-1. You install other laguages separately by performing an additional language installation (see Chapter 4).

These languages are additional to the default language.

See the ALL-IN-1 Installation Guide Part 2 Language Installation of the language you want to install for:

The language name used for language-speci�c �le, directory, and logical names.

The size of the ALL-IN-1 Version 2.4 language component. You need this information to determine the disk space required for installing that language (see Section 1.8.16).

1.8 Preparing the System for Installation

To prepare your system for the installation of ALL-IN-1 Version 2.4, carry out the steps listed in Table 1�2, and mark off each action as you complete it, before starting the installation. You must carry out these actions from a privileged SYSTEM account.

Note Digital recommends using logical names wherever possible. For example, assign logical names to your disks. The logical names must not start with

A1$ or OA$. For example, you must not use A1$DEVICE. If your system uses logical names with pre�xes A1$ or OA$, other than those de�ned by the ALL-IN-1 installation (see Appendix C), you must rename them.

1�20 Preparing to Install ALL-IN-1 V2.4

ALL-IN-1 must not be used by any batch jobs or users during the installation, or the installation will fail. Therefore, you must remove the mail Sender and Fetcher from the batch queue if you are going to perform an upgrade installation.

The values for the various system parameters and quotas given in Table 1�2 are those speci�c to ALL-IN-1 and are acceptable for most systems. The

ALL-IN-1 Management Guide describes how to set system parameters for

ALL-IN-1. Also, see the VMS books for guidelines on the setting of system parameters.

Table 1�2 Actions to Complete Before Installing ALL-IN-1

Step Section Action Completed

1 1.8.3 Backup the system disk

1 1.8.3 Backup any target disks (if applicable)

2 1.8.4 Make sure that there are no active users on the system

3 1.8.6 Register and load the licenses for the prerequisite software

4 1.8.7 Ensure that the Message Router Directory Service is running if you want to use the Mail directory

5 1.8.5 Move your applications to ALL-IN-1 Customization

Management (Ug, Ud)

6 1.8.8 Stop the OA$FORMATTER queue (Ug, Ud)

7 1.8.9 Ensure the queue manager is started

8 1.8.10 Run the mail Sender and Fetcher (Ug, Ud)

9 1.8.11 Remove the ALL-IN-1 housekeeping jobs from the batch queue (Ug, Ud)

10 1.8.12 Check for adequate:global pages global sections global page �le sections

11 1.8.13 Check system parameter values:

LOCKIDTBL 340

MAXBUF 5000

PIOPAGES 350

PQL_DENQLM 150

PQL_MENQLM 150

� The values for WSEXTENT and WSQUOTA must be greater than the WSDEFAULT value.

Ug Upgrade installations

Ud Update installations (continued on next page)

Preparing to Install ALL-IN-1 V2.4 1�21

Table 1�2 (Cont.) Actions to Complete Before Installing ALL-IN-1

Step Section Action Completed

PROCSECTCNT 45

RESHASHTBL 85

RMS_DFMBC 16

RMS_DFMBFIDX 2

STARTUP_P1 null

TTY_TYPAHDSZ 1500

VIRTUALPAGECNT 16385

12 1.8.14 Recompute system parameters

13 1.8.15 Check process quotas:

ASTLM 100

BIOLM 50

BYTLM 36000

DIOLM 50

ENQLM 200

FILLM 100

JTQUOTA 1024

PGFLQUOTA 20000

PRCLM 10

TQELM 50

WSDEFAULT 600�

WSEXTENT 2048

WSQUOTA 800

14 1.8.16 Check disk space

15 1.8.17 Deinstall patches (Ug)

16 1.8.18 Check your site-speci�c startup procedures (Ug)

17 1.8.19 Considerations for ALL-IN-1 Version 2.4 Group

Conferencing

18 1.8.20 Complete checklist

19 1.8.21 Check the License Management Utility requirements

� The values for WSEXTENT and WSQUOTA must be greater than the WSDEFAULT value.

Ug Upgrade installations

Ud Update installations

1.8.1 Time Needed to Install ALL-IN-1 Version 2.4

The installation of ALL-IN-1 Version 2.4 can take from two to �ve hours, depending on the con�guration of your system. For example, the installation will take longer on a MicroVAX system than on a VAX system. This does not include the time taken to install and con�gure Message Router and to set up your system.

The installation of an additional language takes approximately 1 to 2.5 hours.

1�22 Preparing to Install ALL-IN-1 V2.4

1.8.2 Privileges

Install ALL-IN-1 Version 2.4 from the VMS system manager’s account, with full privileges.

Note that the VMSINSTAL turns off the BYPASS privilege at the start of the installation.

1.8.3 Back Up Your System and Target Disks

If possible, back up your system disk and use this backup copy for installation.

If you are going to install ALL-IN-1 Version 2.4 on more than one disk, back up those disks that are to be used during the installation.

Do this because:

If a system failure occurs at a critical point during installation, some �les could be left in an inconsistent state

You can verify that the backup copy contains a working system image and then replace the system disk with it

There is more contiguous free space, which may be needed for installation

1.8.4 Ensure No Active Users on the System

Ensure that there are no active users on the system.

Ask users currently on the system to log off and disable logins, by entering the following:

$ SET LOGINS /INTERACTIVE=0

1.8.5 Moving Your Applications to ALL-IN-1 Customization

Management

If you have an application that that was not created using the ALL-IN-1

Customization Management subsystem, and you want to move the application to ALL-IN-1 Customization Management, you must save the appropriate elements as customizations. There are three situations to consider:

Elements that are supported by customization management and have not yet been customized. See Section 1.8.5.1

Elements that are supported by customization management and have been customized. See Section 1.8.5.2

Elements that are not supported by customization management. See

Section 1.8.5.3 Preparing to Install ALL-IN-1 V2.4 1�23

1.8.5.1 Uncustomized Elements Supported by Customization Management

If your application contains uncustomized elements, do the following:

1 From the Customization Management menu of ALL-IN-1 Version 2.3, select the Access DIGITAL Elements (ADE) option to display the Access DIGITAL

Elements menu.

2 Press SELECT and enter the name of the element that you want to move, and the type of the element.

3 Use the Copy to development area (CO) option to copy the selected element to the development area.

4 If the element is a form, enter EXIT. The following prompt is displayed:

Do you want to save this form? (Y/N)

Enter Y to exit the editing session without making any changes.

If the element is not a form, press EXIT to exit the editing session without making any changes.

In both cases, the Customization Management Site Modi�cation Log is now displayed. Enter the details of the element.

1.8.5.2 Customized Elements Supported by Customization Management

Any elements that have been customized using Customization Management, are already in the SITE areas, and therefore you need not carry out any special steps.

1.8.5.3 Elements Not Supported by Customization Management

Certain elements cannot be customized using Customization Management.

These elements are the help �les in OAHELP.HLB, various messages in

OAMESS.MSG and OASYMMSG.MAR.

Save these elements as follows:

1 Edit the elements that contain message symbols, using the ALL-IN-1

Version 2.3 Customization Management subsystem, and replace the symbols with the appropriate text. These symbols are de�ned in the message �les OAMESS.MSG, and OASYMMSG.MAR.

2 Extract the help text from the help library, OA$BUILD:HLPSOURCE.HLB as follows:

$ LIBRARY/EXTRACT=module_name/HELP -

_$ /OUT=OA$SITE_DEV:module_name.RNO OA$BUILD:HLPSOURCE.HLB where module_name is the name of the help module for your application.

Section 14.15 describes how to replace these modules after ALL-IN-1

Version 2.4 is installed.

1�24 Preparing to Install ALL-IN-1 V2.4

1.8.6 Register the Licenses for the Prerequisite Software

If you install VAX FMS, Message Router and Message Router VMSmail

Gateway, CDA Converter Library, and VAX Notes from the kits supplied with

ALL-IN-1, register the licenses for these products as follows:

1 Invoke VMSINSTAL:

$ SET DEFAULT SYS$UPDATE

$ @VMSINSTAL A1024 device:

where device: is the device on which the distribution media are to be mounted. You can use either a physical or logical device name. Logical device names must not begin with either A1$, OA$ or OA1$.

2 If your system is running VMS Version 5.1, answer YES to the prompt:

%VMSINSTAL-W-DECNET, Your DECnet network is up and running.

* Do you want to continue anyway [NO]?

3 Answer YES to the prompt:

* Are you satisfied with the backup of your system disk [YES]?

4 VMSINSTAL subsequently displays a list of installation types. Enter 7 at the prompt:

* What type of installation do you wish to perform [1]:

VMSINSTAL checks the licenses, and if necessary installs and loads the appropriate licenses. VMSINSTAL then exits.

1.8.7 Ensure Message Router Directory Service is Running

If you want to use Mail directory addressing (see Section 1.5.3.1), make sure that the Message Router Directory Service is running.

If you are installing ALL-IN-1 on a multiple-environment cluster, the Message

Router Directory Service must be running on the part on which you are installing ALL-IN-1 (see Section 1.6.2.1).

1.8.8 Shut Down the OA$FORMATTER Batch Queue

If you are performing an upgrade or update installation, shut down the

OA$FORMATTER batch queue using the following command:

$ STOP /QUEUE /NEXT OA$FORMATTER

1.8.9 Start the Queue Manager

If your queue manager is not running, start it by entering the following command:

$ START /QUEUE /MANAGER Preparing to Install ALL-IN-1 V2.4 1�25

1.8.10 Run the Mail Sender and Fetcher

If you are performing an upgrade or update installation, run the mail Sender and Fetcher to read all the mail:

1 Enter the ALL-IN-1 manager’s ALL-IN-1 account:

$ ALLIN1 /USERNAME=MANAGER

2 Enter MGT to display the ALL-IN-1 Management menu.

3 Enter MM to display the Manage Messaging menu.

4 Enter RF (Run Fetcher) to run the Fetcher to fetch all received messages from the queue.

5 Enter RS (Run Sender) to run the Sender to clear all messages that are waiting to be sent from the queue.

6 Enter EXIT to exit the ALL-IN-1 manager’s account.

1.8.11 Delete the ALL-IN-1 Housekeeping Jobs

If you are performing an upgrade or update installation, you must delete all the ALL-IN-1 houskeeping jobs from the batch queue. Do this as follows:

2 Enter the following command to �nd out the entry numbers of the housekeeping jobs:

$ SHOW QUEUE/BATCH

Make a note of the entry numbers.

3 Enter the following command to delete each of the ALL-IN-1 housekeeping jobs:

$ DELETE/ENTRY=entry_number queue_name where entry_number is the entry number of each housekeeping job, and queue_name is the name of the batch queue running the housekeeping jobs.

1.8.12 Calculate the Values for GBLPAGES, GBLSECTIONS and

GBLPAGFIL

Make sure that you have enough global pages, global sections, and global page �le sections available. Also, follow the steps described in this section to check that certain system parameters are set to adequate values. For more information on SYSGEN parameters refer to the VMS manual describing the

SYSGEN utility.

1�26 Preparing to Install ALL-IN-1 V2.4

Note If you are running a VAXcluster system, you must ensure that these parameters are large enough on each node in the cluster on which you are going to run

ALL-IN-1.

These checks only ensure that the system is adequately con�gured for ALL-IN-1, and do not allow for the requirements of any other layered product.

1 Run the Install Utility and display the currently active values for the system parameters GBLSECTIONS and GBLPAGES:

$ INSTALL

INSTALL> LIST /GLOBAL /SUMMARY

A message similar to the following will be displayed:

160 global sections used, 9867/985 global pages used/unused

The number of unused global pages required for the different installations is:GBLPAGES (Global Pages Unused) for a new installation 9000 for an upgrade installation

5000

If the number of unused global pages shown in the display is less than the required amount, increase it as follows:

a Calculate the value of GBLPAGES as follows:

If you install ALL-IN-1 Version 2.4 but do not install Message

Router, the number of global pages is:

9000 + the allowance for global buffers

For each system �le, calculate the allowance for global buffers as follows:

number of global buffers� maximum bucket size

See the chapter on ALL-IN-1 tuning in the ALL-IN-1 Management

Guide for the formulas used to determine the global buffer counts.

On a default system, the ATTENDEE.DAT �le has a bucket size of 2. Other system �les have a bucket size of 4. Thus, for an installation that uses these default values, the formula for calculating the allowance for global buffers is as follows:

4(n+1) + 4(n+1) + 4(n+1) + 2(n+1) + 4(5) n is the number of ALL-IN-1 users. For example, for an installation using the default values on a system with 100 users, the number of global pages is: Preparing to Install ALL-IN-1 V2.4 1�27

9000 + 4(101) + 4(101) + 4(101) + 2(101) + 20

= 9000 + 404 + 404 + 404 + 202 + 20

= 10434

If you install Message Router as well as ALL-IN-1, add an extra

3500 blocks to the result of this calculation b Edit the �le SYS$SYSTEM:MODPARAMS.DAT, and include the following line:

ADD_GBLPAGES = increase-value increase-value is the amount by which you want to increase the setting of this parameter.

For example, if you want to increase the value by 60, enter:

ADD_GBLPAGES = 60

2 Exit from the Install Utility as follows:

INSTALL> EXIT

3 Run the System Generation Utility as follows:

$ RUN SYS$SYSTEM:SYSGEN

4 Display the current value of global sections as follows:

SYSGEN> USE CURRENT

SYSGEN> SHOW GBLSECTIONS

The system displays the current value of global sections in the �rst column.

To �nd the number of unused global sections, subtract the number of global sections used (as shown by the Install Utility) from the current value (as shown by the System Generation Utility).

The number of global sections required for the different installations is:

for a new installation 45 for an upgrade installation 30

To increase the value of global sections, edit the �le

SYS$SYSTEM:MODPARAMS.DAT, and include the following line:

ADD_GBLSECTIONS = increase-value increase-value is the amount by which you want to increase the setting of this parameter.

For example, if you want to increase the value by 10, enter:

ADD_GBLSECTIONS=10

5 Check the number of global page-�le sections as follows:

SYSGEN> SHOW GBLPAGFIL

1�28 Preparing to Install ALL-IN-1 V2.4

The current value for GBLPAGFIL should be high enough to allow for the maximum number of global buffers allocated on the system.

It is not possible to display the current value for GBLPAGFIL. The value displayed by entering the SHOW command is the value at the last reboot.

If the value of GBLPAGFIL is not high enough, it causes the Fetcher and

Sender jobs of Electronic Messaging, or other parts of ALL-IN-1, to fail.

If the Sender and Fetcher jobs fail, the following error message is placed in the Sender and Fetcher log �le:

System Service $CRMPSC failed to map global buffers

If other parts of ALL-IN-1 fail, this error message may be displayed on your screen.

To increase the value of GBLPAGFIL, edit the �le

SYS$SYSTEM:MODPARAMS.DAT and include the following line:

ADD_GBLPAGFIL = increase-value increase-value is the amount by which you want to increase the setting of this parameter.

For example, if you want to increase the value by 60, enter:

ADD_GBLPAGFIL = 60

1.8.13 Check the System Parameter Values

Display the current system parameter settings using the following command:

SYSGEN> SHOW /ALL

Alternatively, show each system parameter setting separately using the following command:

SYSGEN> SHOW parameter parameter is the parameter you want to examine. Table 1�3 lists the minimum required system parameter values for the installation. Depending on the kinds of programs and applications running at your site, you might need higher values for some settings. If necessary, modify the parameters (as described in

Step 2 or 3 of this section) to at least these values.Preparing to Install ALL-IN-1 V2.4 1�29

Table 1�3 Required System Parameter Values

System Parameter Value

LOCKIDTBL 340

MAXBUF (D) 5000

PIOPAGES 350

PQL_DENQLM (D) 150

PQL_MENQLM (D) 150

PROCSECTCNT 45

RESHASHTBL 85

RMS_DFMBC (D) 16

RMS_DFMBFIDX (D) 2

STARTUP_P1 null

TTY_TYPAHDSZ 1500

VIRTUALPAGECNT 16385

(D) Dynamic system parameters

You must ensure that the system parameter STARTUP_P1 is null before installing ALL-IN-1 Version 2.4.

You need not modify the MAXBUF parameter at this point. If this parameter is too low, the installation displays an appropriate message and then continues.

However, you must set MAXBUF to at least the value given in Table 1�3 before

ALL-IN-1 is used.

Note If you integrate any other software with ALL-IN-1, you must increase the

SYSGEN parameter PROCSECTCNT by at least �ve. This makes sure that shared images are accessible during installation.

1 Press CTRL/Z to leave SYSGEN.

2 Modify the following parameters as necessary:

PQL_DENQLM

PQL_MENQLM

RMS_DFMBC

RMS_DFMBFIDX

TTY_TYPAHDSZ

To modify these system parameters edit the �le

SYS$SYSTEM:MODPARAMS.DAT and specify new parameter values. Use assignment statements of the form:

parameter = parameter-value parameter is the name of the parameter you want to change and parameter-value is the setting you want to change it to.

1�30 Preparing to Install ALL-IN-1 V2.4

For example, if RMS_DFMBFIDX is currently set to 1, which is not suf�cient for running ALL-IN-1, you must increase it as follows:

RMS_DFMBFIDX = 2

3 Change the the following parameters, as necessary:

LOCKIDTBL

MAXBUF

PIOPAGES

PROCSECTCNT

RESHASHTBL

VIRTUALPAGECNT

To modify these system parameters edit the �le

SYS$SYSTEM:MODPARAMS.DAT. Include a line of the following format for each parameter to be changed:

ADD_parameter = increase-value parameter is the name of the parameter you want to change increase-value is the amount by which you want to increase the setting of this parameter.

For example, if you want to increase the value of LOCKIDTBL by 60, enter:

ADD_LOCKIDTBL=60

1.8.14 Changing System Parameter Values with AUTOGEN

If you have changed only dynamic system parameters, you need not reboot your system. In this case, do the following:

1 Run AUTOGEN as follows:

$ @SYS$UPDATE:AUTOGEN SAVPARAMS SETPARAMS

2 Write the changes to the current system:

$ @SYS$SYSTEM:SYSGEN

SYSGEN> USE CURRENT

SYSGEN> WRITE ACTIVE

If you changed the values of any of your non-dynamic system parameters in the previous steps, do the following:

1 Set AGEN$SHUTDOWN_TIME to a value greater than

SHUTDOWN$MINIMUM_MINUTES:

$ DEFINE/SYSTEM/EXECUTIVE_MODE AGEN$SHUTDOWN_TIME shutdown_time

2 Run AUTOGEN to recompute the system parameters:

$ @SYS$UPDATE:AUTOGEN SAVPARAMS REBOOT

Preparing to Install ALL-IN-1 V2.4 1�31

AUTOGEN performs an automatic shutdown and reboot when it has

�nished. See the VMS manual describing the Autogen Utility.

Note The system must have been running at least 24 hours for these commands to work. If your system has been running for less than 24 hours add the parameter

NOFEEDBACK at the end of each AUTOGEN command.

1.8.15 Process Account Quotas

Ensure that process quotas are adequate.

The account you use to install ALL-IN-1 Version 2.4 must have suf�cient quotas to allow you to perform the installation. Table 1�4 summarizes the process quotas required to perform the installation.

Table 1�4 Process Account Quotas for the Installing Account

Account Quota Value

ASTLM 100

BIOLM 50

BYTLM 36000

DIOLM 50

ENQLM 200

FILLM 100

JTQUOTA 1024

PGFLQUOTA 20000

PRCLM 10

TQELM 50

WSDEFAULT 600�

WSEXTENT 2048

WSQUOTA 800

� The values for WSEXTENT and WSQUOTA must be greater than the WSDEFAULT value.

When you create user accounts for ALL-IN-1 Version 2.4 the process quotas are set to the appropriate values. See the ALL-IN-1 Management Guide for details.

If you are upgrading from ALL-IN-1 Version 2.3, you must set the process quotas to at least the values listed in Table 1�4 for all the users on your current ALL-IN-1 system.

To increase the process account quotas use the Authorize Utility.

Note If you integrate any other software with ALL-IN-1, you must increase the quota values according to the requirements of the software.

1�32 Preparing to Install ALL-IN-1 V2.4

You can change the process quotas for an account even if a user is logged in to the account. However, if a user is logged in, that user must log out and log back in again for the process quotas to become active.

1.8.16 Disk Space

Installing ALL-IN-1 Version 2.4 requires a certain amount of free storage space during the installation. Once ALL-IN-1 Version 2.4 is installed, less storage space is required.

The amount of disk space available on the system disk determines the mode of installation. The installation runs in either Safety or Non-Safety mode (see

Section 1.8.16.1).

The minimum disk space required on the system disk during installation depends on whether you are installing ALL-IN-1 Version 2.4 on the system disk only, or across several disks. To determine the minimum disk space required on the system disk, add together the values given in the ALL-IN-1

Installation Guide Part 2 Language Installation and ALL-IN-1 Installation

Guide Part 3 Market Installation.

1.8.16.1 Installation Modes

The installation runs in one of two modes, depending on how many blocks are available on the system disk:

Safety mode

If you have a minimum of 65,000 free blocks on your system disk, the installation is performed in Safety mode. All the �les are transferred from the media to a working area on the system disk before they are moved to their target directories. If you are performing a system disk installation, the installation is always carried out in Safety mode.

If a failure occurs before the �les start to be moved to target directories,

VMSINSTAL deletes the working area so that you can restart the installation.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

Non-Safety mode

In Non-Safety mode each �le is transferred from the media to a working directory on the system disk. After each �le is transferred it is moved to its target directory, before the next �le is transferred.

If a failure occurs during a Non-Safety mode installation, some �les have already been copied to their target directories. Therefore, cleaning up the target disks involves more work than for Safety mode.Preparing to Install ALL-IN-1 V2.4 1�33

1.8.16.2 ALL-IN-1 Areas

To ease the management of ALL-IN-1 you can choose to split ALL-IN-1 across several disks; each disk containing an ALL-IN-1 area. The ALL-IN-1 areas are:ALL-IN-1 manager’s account. This account includes the IVPUSER, MGR,

POSTMASTE, TRANSFER_INCOMING and TRANSFER_OUTGOING directories

Shared library �les

Shared data �les

Language �les

Mail area shared document attributes �le SDAF �le

OA$SHARE:OA$DAF_E.DAT. Mail area E is created during a new installation.

Shared directories SHAREnnnn, where nnnn is a number in the range

1 to 9999. Shared directories for Mail area E are created during a new

An example of the directory structure for a multiple-disk ALL-IN-1 system is given in Appendix C.

Space is provided in Table 1�5 for you to enter the disk space requirements of each ALL-IN-1 area. See the ALL-IN-1 Installation Guide Part 3 Market

Installation for the disk space required by all areas except for the language

�les. See the ALL-IN-1 Installation Guide Part 2 Language Installation for the disk space required by the language �les.

Note The ALL-IN-1 Installation Guide Part 2 Language Installation and

ALL-IN-1 Installation Guide Part 3 Market Installation also give the disk space requirements if WPS-PLUS is incorporated and if WPS-PLUS is not incorporated.

If you want more than one area on the same disk, the disk space required is the total for those areas.

1�34 Preparing to Install ALL-IN-1 V2.4

Table 1�5 Disk Space Requirements for the ALL-IN-1 Areas

ALL-IN-1 Area

Disk Space Requirements (blocks) New Upgrade Update

ALL-IN-1

V2.4

ALL-IN-1 STARTER V1.0

ALL-IN-1 V2.3

ALL-IN-1 STARTER V2.4

System �les*

Manager’s account�

Shared library �les

Shared data �les

Mail area SDAF �le 1,000

Shared directories n x 1000

Language �les�:

(1)(2)(3)(4)(5)(6)(7)(8)(9)

(10)* These are the �les that are installed in the SYS$MANAGER, SYS$LIBRARY, SYS$MESSAGE and SYS$HELP directories (see Appendix C)

� This �gure includes the [.IVPUSER], [.MGR], [.POSTMASTE], [.TRANSFER_INCOMING] and

[.TRANSFER_OUTGOING] directories.

n is the number of shared directories speci�ed during the installation.

� See the ALL-IN-1 Installation Guide Part 2 Language Installation for the language(s) that you are installingIf you decide to keep a record of the installation in a log �le, add at least 200

blocks to the disk space determined in steps 1 to 3.

If you are installing an additional language you need the minimum amount of free blocks given in the ALL-IN-1 Installation Guide Part 2 Language

Installation for that language. Preparing to Install ALL-IN-1 V2.4 1�35

If you want more than one ALL-IN-1 area on the same disk, the minimum disk space required is the total for those areas.

Note If you only have the minimum amount of recommended free space, and your system crashes during installation, or if the installation fails, the software will be only partially installed. For this reason, Digital recommends that you back up your system disk, and all target disks for a multiple disk installation, before installing ALL-IN-1 Version 2.4.

If all areas of ALL-IN-1 are going to be installed on the system disk, ensure that there are enough free blocks on the system disk by issuing the SHOW

DEVICE command, for example:

$ SHOW DEVICE SYS$SYSDEVICE

If the areas of ALL-IN-1 are to be installed on a disk or disks other than the system disk, ensure that these disks have enough free blocks by issuing the

SHOW DEVICE command. For example:

$ SHOW DEVICE disk where disk is the name of the disk that will hold the ALL-IN-1 areas.

1.8.17 Deinstall Patches

If you have an ALL-IN-1 Version 2.3 system that has patches installed, you must deinstall the patches before you upgrade to ALL-IN-1 Version 2.4.

Contact your Digital support center for further details.

1.8.18 Check Your Site-Speci�c Startup Procedures

If you are upgrading from ALL-IN-1 Version 2.3, and you have created site-speci�c startup procedures (that is, A1V23_SITE_START.COM and

OA$SITE_language_START.COM), do the following:

1 Check your site-speci�c startup command procedure(s) for any commands that change the con�guration of ALL-IN-1. You may wish to change the con�guration during the installation of ALL-IN-1 Version 2.4, for example, if you re-link ALL-IN-1 to incorporate VAX DATATRIEVE, and so on.

2 If you want to keep your site-speci�c startup command procedure

A1V23_SITE_START.COM, you must rename it to

A1V24_SITE_START.COM after the installation (see Section 14.6.3).

1�36 Preparing to Install ALL-IN-1 V2.4

1.8.19 Considerations for ALL-IN-1 Version 2.4 Group

Conferencing

ALL-IN-1 Version 2.4 Group Conferencing is supplied with ALL-IN-1 Version

2.4. ALL-IN-1 Version 2.4 Group Conferencing is installed separately, after ALL-IN-1 Version 2.4 is installed. However, you must not make any customizations to the images OAGBL.EXE and OASYMMSG.EXE before

ALL-IN-1 Version 2.4 Group Conferencing is installed. This is because the installation of ALL-IN-1 Version 2.4 Group Conferencing replaces these images and any customizations will be lost.

If you are upgrading from ALL-IN-1 Version 2.3, and you have already customized these images, copy the images to the OA$SITE_BUILD_SHARE directory, upgrade to ALL-IN-1 Version 2.4 as described in Chapter 5 and then install ALL-IN-1 Version 2.4 Group Conferencing. After ALL-IN-1 Version 2.4

Group Conferencing is installed, you can apply your customizations to the new

OAGBL.EXE and OASYMMSG.EXE images.

1.8.20 Checklist of Information Required for Installation

Before you install ALL-IN-1 Version 2.4 you should know what answers you are going to give to the questions asked during the installation. Refer to the table of steps in the chapter appropriate to the installation you are going to perform. This table indicates which steps are required for that installation.

Full descriptions of the steps are described in Chapter 13. Place a tick in the box for each of the steps required by your installation and enter your answer to the prompt(s) in that step in the space provided.

If you are installing ALL-IN-1 Version 2.4, and you do not have any other version of ALL-IN-1, see Chapter 3

If you are installing an additional language, see Chapter 4

If you are upgrading your ALL-IN-1 Version 2.3 system to ALL-IN-1

Version 2.4, see Chapter 5

If you are upgrading an ALL-IN-1 Version 2.3 additional language to an

ALL-IN-1 Version 2.4 additional language, see Chapter 6

If you are upgrading your ALL-IN-1 STARTER Version 1.0 system to

ALL-IN-1 Version 2.4, see Chapter 7

If you are upgrading an ALL-IN-1 STARTER Version 1.0 additional language to an ALL-IN-1 Version 2.4 additional language, see Chapter 8

If you are updating your ALL-IN-1 STARTER Version 2.4 system to

ALL-IN-1 Version 2.4, see Chapter 9

If you are updating an ALL-IN-1 STARTER Version 2.4 additional language to an ALL-IN-1 Version 2.4 additional language, see Chapter 10

Preparing to Install ALL-IN-1 V2.4 1�37

If you are updating your existing ALL-IN-1 Version 2.4 system, see

Chapter 11

If you are updating an ALL-IN-1 Version 2.4 additional language, see

Chapter 12

1.8.21 License Management Utility Requirements

You must register and load your license for ALL-IN-1 Version 2.4 before you start the installation in order to install ALL-IN-1 Version 2.4.

For more information on the VMS License Management Facility, see the VMS

License Management Facility documentation.

1�38 Preparing to Install ALL-IN-1 V2.4

2 Accessing the Online Release Notes

ALL-IN-1 Version 2.4 provides online Release Notes. The Release Notes contain information that was unavailable before the books went to print. It is important to read the Release Notes, because they may contain information relating to the installation.

Note The ALL-IN-1 Release Notes Part 1 Language also contains the release notes for ALL-IN-1 Version 2.4 Group Conferencing.

There are two parts to the Release Notes:

Release Notes Part 1 Language

This part contains the release notes speci�c to the ALL-IN-1 Version 2.4 international base component and to the language being installed, and is on the tape labeled:

ALL-IN-1 V2.4 language BIN media_type

Release Notes Part 1

(c) 1989 Digital Equipment Corp.

language is the name of the ALL-IN-1 Version 2.4 language component to be installed, and media_type is 16MT9 for tape and TK50 for a TK50 cartridge.

Release Notes Part 2 Market

This part contains the release notes speci�c to your ALL-IN-1 Version 2.4 market component, and is on the tape labeled:

ALL-IN-1 V2.4 market BIN media_type

Release Notes Part 2

(c) 1989 Digital Equipment Corp. Accessing the Online Release Notes 2�1

market is the name of the ALL-IN-1 Version 2.4 Market component to be installed.

Note This document may not exist for all market components.

2.1 Accessing the Release Notes

To access the Release Notes:

1 Log in to the privileged VMS system manager’s account.

2 Establish the following default directory:

$ SET DEFAULT SYS$UPDATE

3 Enter the following command:

$ @VMSINSTAL product device: OPTIONS N product is the product code:

A1LRlang024 for the Release Notes Part 1 Language orA1CRmarket024 for the Release Notes Part 2 Market device is the device on which the tape containing the appropriate version of the Release Notes is mounted.

The following message is displayed:

VAX/VMS Software Product Installation Procedure V<version>.

It is <dd-mmm-yyyy> at <hh:mm>.

<dd-mmm-yyy> and <hh:mm> are the current date and time, and

<version> is the version of VMS that your system is running.

Enter a question mark (?) at any time for help.

4 If your system is running VMS Version 5.1, and your DECnet network is running, the following message is displayed:

%VMSINSTAL-W-DECNET, your DECnet network is up and running.

* Do you want to continue anyway [NO]?

Enter YES and press RETURN.

5 If other users are accessing the system, the following message appears:

%VMSINSTAL-W-ACTIVE,The following processes are still active

<process_name>

   .

<process_name> refers to the process name of a user logged in to the system.

2�2 Accessing the Online Release Notes

As you are only printing the Release Notes, it is safe to continue. Enter

YES and press RETURN.

6 VMSINSTAL displays:

* Are you satisfied with the backup of your system disk [YES]?

As you are only printing the Release Notes, it is safe to continue, so press

RETURN.

7 VMSINSTAL then prompts you to mount the distribution media:

Please mount the first volume of the set on <device>:

where <device> is the device you speci�ed.

The Release Notes are in two parts, one part on each of the distribution media labeled as follows:

ALL-IN-1 V2.4 language BIN media_type

Release Notes Part 1

(c) 1989 Digital Equipment Corp. and ALL-IN-1 V2.4 market BIN media_type

Release Notes Part 2 where language is the name of the ALL-IN-1 Version 2.4 language component to be installed, market is the name of the ALL-IN-1 Version 2.4

Market component to be installed, and media_type is 16MT9 for tape and

TK50 for a TK50 cartridge.

If you are performing an additional language installation, you need only print the ALL-IN-1 Release Notes Part 1 Language that is supplied with your kit.

VMSINSTAL displays:

* Are you ready?

At this prompt, mount the �rst volume of the distribution medium. (If you are unfamiliar with the loading of media, refer to the VMS software intsallation documentation.)

When you have mounted the volume, enter YES and press RETURN.

VMSINSTAL tries to mount the distribution volume. If it succeeds, a message is displayed, for example:

%MOUNT-I-MOUNTED, A1<n>024 mounted on <device>:

where <n> is 3 for the ALL-IN-1 Release Notes Part 1 Language and 2 for the ALL-IN-1 Release Notes Part 2 Market, and <device> is the device where the media is mounted. Accessing the Online Release Notes 2�3

The following message is then displayed:

The following products will be processed:

<name> V2.4

Beginning installation of <name> V2.4 at <hh:mm> where <hh:mm> is the current time and <name> is:

A1LRlanguage for the ALL-IN-1 Release Notes Part 1 Language

A1CRmarket for the ALL-IN-1 Release Notes Part 2 Market

8 VMSINSTAL displays:

%VMSINSTAL-I-RESTORE, Restoring product saveset A...

Release Notes Options:

1 Display Release Notes

2 Print Release Notes

3 Both 1 and 2

4 Copy release notes to SYS$HELP

5 Do not display, print, or copy the release notes

* Select option [3]:

Enter the number of the option that you require.

If you enter 2, or 3, to print the Release Notes, the following message is displayed:

* Queue name [SYS$PRINT]:

Press RETURN if you want to print the Release Notes on SYS$PRINT. If you do not want to print on SYS$PRINT, enter the name of the printer queue you want to use.

* Do you want to continue the installation [N]?

Press RETURN to accept the default answer of NO.

The following messages are displayed:

%VMSINSTAL-I-RELMOVED, The product Release Notes have been

    successfully moved to SYS$HELP.

Installation of <name> V2.4 completed at <hh:mm>

VMSINSTAL procedure done at <hh:mm>

If you have accessed only one part of the Release Notes, repeat steps 3 to 8 for the other part.

2�4 Accessing the Online Release Notes

If you chose to print the Release Notes, or copy them to SYS$HELP, the following �les are placed in SYS$HELP:

A1LRlang024.RELEASE_NOTES, for the Release Notes Part 1 Language

A1CRmarket024.RELEASE_NOTES, for the Release Notes Part 2 Market

Note It is important to read the Release Notes before installing ALL-IN-1.

Accessing the Online Release Notes 2�5

3 Installing a New ALL-IN-1 V2.4 System

This chapter explains how to install ALL-IN-1 Version 2.4 if you are installing

ALL-IN-1 as a new system.

3.1 Before You Start

Before you start the installation procedure:

1 Make sure that you have made all the necessary preparations (see

Section 1.8).

2 Complete the checklist of information required for installation (see

Section 1.8.20). Refer to this checklist during the installation.

You must have the base, language, and market components to install ALL-IN-1

Version 2.4.

3.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.

The name of the device where the distribution media are to be mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution media and that command procedure controls the rest of the installation.Installing a New ALL-IN-1 V2.4 System 3�1

3.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

3.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

3.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

3.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

%UAF-E-RDBADDERRU, unable to add A1$XFER_IN value:

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

3�2 Installing a New ALL-IN-1 V2.4 System

%UAF-E-RDBADDERRU, unable to add A1$XFER_OUT value

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

ALL-IN-1 Version 2.4 can be installed only on systems running VMS Version

5.1, or higher. If your system does not have the correct version of VMS an error message is displayed as follows:

$A1-F-V50VMS-1, Incorrect VMS version. Please upgrade to VMS

      Version 5.1

$A1-F-V50VMS-2, before installing ALL-IN-1 version 2.4.

Upgrade your system to VMS Version 5.1, or higher, before installing ALL-IN-1

Version 2.4.

3.7 The Installation Procedure

Table 3�1 lists the steps required for a new installation of ALL-IN-1 Version

2.4. Installing a New ALL-IN-1 V2.4 System 3�3

Table 3�1 Steps Required to Install a New ALL-IN-1 Version 2.4 System

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

7 Load the Distribution Media - Sequence 2

8 Specify the market code required by this installation

9 Specify the language code required by this installation

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

12 Indicate whether or not you want to incorporate DATATRIEVE

13 Indicate whether or not you want to incorporate WPS-PLUS

14 Indicate whether or not you want to incorporate ACMS

15 Check to see if the CDA Converter Library is installed

16 Indicate whether or not you want to build a multi-language system

17 Select the date format to use with ALL-IN-1

18 Specify the greatest number of simultaneous ALL-IN-1 users

19 Specify the batch queue to run the Sender and Fetcher

20 Indicate whether or not you want to send and receive messages to and from other systems

21 Indicate whether the Message Router you want ALL-IN-1 to use is on this node or another node

22 Specify the node whose Message Router you want to use

23 Specify the level of use of the Mail directory

24 Specify the password for the ALL-IN-1 Message Router mailbox

25 Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

26 Check the mandatory and optional software prerequisites

27 Specify the device to hold the ALL-IN-1 shared library �les

28 Specify the device to hold the ALL-IN-1 shared data �les

29 Specify the device to hold the ALL-IN-1 language �les

30 Specify the device to use for the ALL-IN-1 mail area SDAF �le

31 Indicate how many shared directories you would like

32 Specify a device for each shared directory

33 Identify or create the VMS account for ALL-IN-1 (continued on next page)

3�4 Installing a New ALL-IN-1 V2.4 System

Table 3�1 (Cont.) Steps Required to Install a New ALL-IN-1 Version 2.4

System

STEP Title

35 Specify the password for the ALL-IN-1 manager’s VMS account

36 Specify the password for the ALL-IN-1 transfer user accounts

37 Specify the UIC for the ALL-IN-1 manager’s VMS account

38 Specify the device and directory for the ALL-IN-1 manager’s VMS account

39 Specify the UICs for the ALL-IN-1 transfer user accounts

40 Specify the directory to hold the shared library �les, in OA$LIB

41 Specify the directory to hold the shared data �les, in OA$DATA

42 Specify the directory to hold the language �les

43 Specify the directory to hold the mail area SDAF �le

OA$DATA:OA$DAF_E.DAT

44 Specify the directory to hold the shared directories, OA$SHAREnnn

45 Indicate whether or not you want to run the IVPs

46 Load the Distribution Media - Sequence 3

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

3.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1 V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1 V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in useInstalling a New ALL-IN-1 V2.4 System 3�5

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

3.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command �le

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL is compiled and installed successfully and recompile it if you received any error messages when the startup command �le was run.

Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

3�6 Installing a New ALL-IN-1 V2.4 System

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide. Installing a New ALL-IN-1 V2.4 System 3�7

4 Installing Additional Languages for

ALL-IN-1 V2.4

This chapter explains how to install a new additional language.

4.1 Before You Start

Before you start the installation procedure:

1 Print and read the ALL-IN-1 Release Notes Part 1 Language (see

Section 2.1)

2 Make sure that you have made all the necessary preparations (see

Section 1.8).

3 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command �le

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You need only the required language component to install an additional

ALL-IN-1 Version 2.4 language.Installing Additional Languages for ALL-IN-1 V2.4 4�1

4.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.

The name of the device where the distribution medium is mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution medium and that command procedure controls the rest of the installation.

4.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

4.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

4.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

4�2 Installing Additional Languages for ALL-IN-1 V2.4

4.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

4.7 The Installation Procedure

Table 4�1 lists the steps required for an additional language installation.

Table 4�1 Steps Required for an ALL-IN-1 V2.4 Language Installation

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

17 Select the date format to use with ALL-IN-1

29 Specify the device to hold the ALL-IN-1 language �les(continued on next page)

Installing Additional Languages for ALL-IN-1 V2.4 4�3

Table 4�1 (Cont.) Steps Required for an ALL-IN-1 V2.4 Language

Installation

STEP Title

34 Indicate the existing VMS username for the ALL-IN-1 account

42 Specify the directory to hold the language �les

45 Indicate whether or not you want to run the IVPs

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

4.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1L<lang> V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1L<lang> V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

where <lang> is the name of the language being installed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

4�4 Installing Additional Languages for ALL-IN-1 V2.4

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

4.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP /LANGUAGE=lang

Installing Additional Languages for ALL-IN-1 V2.4 4�5

where lang is the name of the language being installed.

Manually execute each IVP as described in the ALL-IN-1 Management

Guide.

Note The IVP runs in the language context of the current optional language being installed and also tests the international base system.

Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

4�6 Installing Additional Languages for ALL-IN-1 V2.4

5 Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4

This chapter explains how to upgrade your ALL-IN-1 Version 2.3 system to

ALL-IN-1 Version 2.4.

5.1 Before You Start

Before you start the installation procedure:

1 Make sure that you have made all the necessary preparations (see

Section 1.8).

2 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

3 If you run any ALL-IN-1 layered products, you may need to prepare the layered product(s) before you install ALL-IN-1 Version 2.4 (see your layered product documentation).

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V23START.COM) before you start the installation.

You must have the base, language, and market components to upgrade your

ALL-IN-1 Version 2.3 system to ALL-IN-1 Version 2.4.

Note Upgrading to ALL-IN-1 Version 2.4 also upgrades your default language. If you have a multi-language ALL-IN-1 system, you will be unable to use your additional languages until you have upgraded them; you can still use your default language. In this case, you must run only the IVP for the default language. Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4 5�1

5.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed

The name of the device where the distribution media are to be mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution media and that command procedure controls the rest of the installation.

5.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

5.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

5.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

5�2 Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4

5.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

%UAF-E-RDBADDERRU, unable to add A1$XFER_IN value:

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

%UAF-E-RDBADDERRU, unable to add A1$XFER_OUT value:

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

ALL-IN-1 Version 2.4 can be installed only on systems running VMS Version

5.1, or higher. If your system does not have the correct version of VMS an error message is displayed as follows:

$A1-F-V50VMS-1, Incorrect VMS version. Please upgrade to VMS

    Version 5.1

$A1-F-V50VMS-2, before installing ALL-IN-1 version 2.4.

Upgrade your system to VMS Version 5.1, or higher, before installing ALL-IN-1 version 2.4.

5.7 The Installation Procedure

Table 5�1 lists the steps required to upgrade your ALL-IN-1 Version 2.3 system to ALL-IN-1 Version 2.4. Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4 5�3

Table 5�1 Steps Required to Upgrade ALL-IN-1 V2.3 to ALL-IN-1 V2.4

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

7 Load the Distribution Media - Sequence 2

8 Specify the market code required by this installation

9 Specify the language code required by this installation

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

12 Indicate whether or not you want to incorporate DATATRIEVE

13 Indicate whether or not you want to incorporate WPS-PLUS

14 Indicate whether or not you want to incorporate ACMS

15 Check to see if the CDA Converter Library is installed

16 Indicate whether or not you want to build a multi-language system

17 Select the date format to use with ALL-IN-1

18 Specify the greatest number of simultaneous ALL-IN-1 users

19 Specify the batch queue to run the Sender and Fetcher

20 Indicate whether or not you want to send and receive messages to and from other systems

21 Indicate whether the Message Router you want ALL-IN-1 to use is on this node or another node

22 Specify the node whose Message Router you want to use

23 Specify the level of use of the Mail directory

24 Specify the password for the ALL-IN-1 Message Router mailbox

25 Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

36 Specify the password for the ALL-IN-1 transfer user accounts

39 Specify the UICs for the ALL-IN-1 transfer user accounts

45 Indicate whether or not you want to run the IVPs

46 Load the Distribution Media - Sequence 3

47 Wait for the installation to complete

48 Complete installation

5�4 Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

You must now upgrade any additional languages that were installed with your

(ALL-IN-1) Version 2.3 system. A separate installation is required for each of the additional languages on your system (see Chapter 6).

5.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1 V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1 V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4 5�5

5.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP

Manually execute each IVP as described in the ALL-IN-1 Management

Guide.

Note Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

5�6 Upgrading ALL-IN-1 V2.3 to ALL-IN-1 V2.4

6 Upgrading ALL-IN-1 V2.3 Languages to

ALL-IN-1 V2.4 Languages

This chapter explains how to upgrade an ALL-IN-1 Version 2.3 additional language to an ALL-IN-1 Version 2.4 additional language

6.1 Before You Start

Before you start the installation procedure:

1 Print and read the ALL-IN-1 Release Notes Part 1 Language (see

Section 2.1)

2 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

3 Make sure that you have made all the necessary preparations (see

Section 1.8).

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You need only the required language component to upgrade an ALL-IN-1

Version 2.3 additional language to an ALL-IN-1 Version 2.4 additional language.

Note You must upgrade your main ALL-IN-1 Version 2.3 system to ALL-IN-1 Version

2.4 before upgrading the languages. See Chapter 5.

Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages 6�1

6.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.

The name of the device where the distribution medium is mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution medium and that command procedure controls the rest of the installation.

6.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

6.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

6.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

6�2 Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages

6.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

6.7 The Installation Procedure

Table 6�1 lists the steps required for updating an ALL-IN-1 Version 2.3 additional language to an ALL-IN-1 Version 2.4 additional language.

Table 6�1 Steps Required for Upgrading an ALL-IN-1 V2.3 Language

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation(continued on next page)

Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages 6�3

Table 6�1 (Cont.) Steps Required for Upgrading an ALL-IN-1 V2.3

Language

STEP Title

17 Select the date format to use with ALL-IN-1

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

6.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1L<lang> V2.4 has failed.

where <lang> is the name of the language being installed.

If the IVP fails, the following messages are displayed:

The A1L<lang> V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

6�4 Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

6.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP /LANGUAGE=lang

Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages 6�5

where lang is the name of the language being installed.

Manually execute each IVP as described in the ALL-IN-1 Management

Guide.

Note The IVP runs in the language context of the current optional language being installed and also tests the international base system.

Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

6�6 Upgrading ALL-IN-1 V2.3 Languages to ALL-IN-1 V2.4 Languages

7 Upgrading from ALL-IN-1 STARTER V1.0 to

ALL-IN-1 V2.4

This chapter explains how to upgrade from ALL-IN-1 STARTER Version 1.0 to

ALL-IN-1 Version 2.4.

7.1 Before You Start

Before you start the installation procedure:

1 Make sure that you have made all the necessary preparations (see

Section 1.8).

2 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

3 If you have carried out any permitted modi�cations (for example, to template �les) to your ALL-IN-1 STARTER Version 1.0 system, save the modi�cations in an area that is not used by ALL-IN-1.

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 Run the following command procedure to set up the correct environment for the upgrade installation:

SYS$MANAGER:AS010_PRE_V23UPGRADE.COM

6 Modify the ALL-IN-1 manager’s account details to include access to

OA$LIB:CM as follows:

a Create a script, for example STARTER_MODIFY.SCP, containing the following:

WRITE CHANGE PROFIL USER=’MANAGER’, -

FRMLIB=’OA$LIB:MANAGER,OA$LIB:ADMIN,OA$LIB:CM’

Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4 7�1

b Enter the ALL-IN-1 STARTER manager’s account, and enter the following command:

<DO directory:STARTER_MODIFY where directory is the directory containing STARTER_MODIFY.SCP.

c Exit ALL-IN-1.

You must have the base, language, and market components to upgrade your

ALL-IN-1 STARTER Version 1.0 system to ALL-IN-1 Version 2.4.

Note Upgrading to ALL-IN-1 Version 2.4 also upgrades your default language. If you have a multi-language ALL-IN-1 system, you will be unable to use your additional languages until you have upgraded them; you can still use your default language. In this case, you must run only the IVP for the default language.

7.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed

The name of the device where the distribution media are to be mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution media and that command procedure controls the rest of the installation.

7.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

7.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

7�2 Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

7.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

7.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

%UAF-E-RDBADDERRU, unable to add A1$XFER_IN value:

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

%UAF-E-RDBADDERRU, unable to add A1$XFER_OUT value:

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4 7�3

7.7 The Installation Procedure

Table 7�1 lists the step required to upgrade your ALL-IN-1 STARTER Version

1.0 system to ALL-IN-1 Version 2.4.

Table 7�1 Steps Required to Upgrade your ALL-IN-1 STARTER V1.0 System to ALL-IN-1 V2.4

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

7 Load the Distribution Media - Sequence 2

8 Specify the market code required by this installation

9 Specify the language code required by this installation

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

12 Indicate whether or not you want to incorporate DATATRIEVE

13 Indicate whether or not you want to incorporate WPS-PLUS

14 Indicate whether or not you want to incorporate ACMS

15 Check to see if the CDA Converter Library is installed

16 Indicate whether or not you want to build a multi-language system

17 Select the date format to use with ALL-IN-1

18 Specify the greatest number of simultaneous ALL-IN-1 users

19 Specify the batch queue to run the Sender and Fetcher

20 Indicate whether or not you want to send and receive messages to and from other systems

21 Indicate whether the Message Router you want ALL-IN-1 to use is on this node or another node

22 Specify the node whose Message Router you want to use

23 Specify the level of use of the Mail directory

24 Specify the password for the ALL-IN-1 Message Router mailbox

25 Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

26 Check the mandatory and optional software prerequisites

(continued on next page)

7�4 Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4

Table 7�1 (Cont.) Steps Required to Upgrade your ALL-IN-1 STARTER V1.0

System to ALL-IN-1 V2.4

STEP Title

34 Indicate the existing VMS username for the ALL-IN-1 account

36 Specify the password for the ALL-IN-1 Transfer User accounts

39 Specify the UICs for the ALL-IN-1 transfer user accounts

45 Indicate whether or not you want to run the IVPs

46 Load the Distribution Media - Sequence 3

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

You must now upgrade any additional languages that were installed with your

(ALL-IN-1) STARTER Version 1.0 system. A separate installation is required for each of the additional languages on your system (see Chapter 8).

7.8 Stop and Start the OA$FORMATTER Queue

You must stop and restart the OA$FORMATTER queue by entering the following commands:

$ STOP /QUEUE /NEXT OA$FORMATTER

$ START /QUEUE OA$FORMATTER

7.9 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1 V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1 V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4 7�5

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

7.9.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

7�6 Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

Upgrading from ALL-IN-1 STARTER V1.0 to ALL-IN-1 V2.4 7�7

8 Upgrading ALL-IN-1 STARTER V1.0

Languages to ALL-IN-1 V2.4 Languages

This chapter explains how to upgrade an ALL-IN-1 STARTER Version 1.0 additional language to an ALL-IN-1 Version 2.4 additional language

8.1 Before You Start

Before you start the installation procedure:

1 Print and read the ALL-IN-1 Release Notes Part 1 Language (see

Section 2.1)

2 Make sure that you have made all the necessary preparations (see

Section 1.8).

3 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You need only the required language component to upgrade an ALL-IN-1

STARTER Version 1.0 additional language to an ALL-IN-1 Version 2.4 additional language.

Note You must upgrade your main ALL-IN-1 STARTER Version 1.0 system to

ALL-IN-1 Version 2.4 before upgrading the languages. See Chapter 7.

Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages 8�1

8.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.

The name of the device where the distribution medium is mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution medium and that command procedure controls the rest of the installation.

8.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

8.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

8.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

8�2 Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages

8.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

8.7 The Installation Procedure

Table 8�1 lists the steps required for upgrading an ALL-IN-1 STARTER

Version 1.0 additional language to an ALL-IN-1 Version 2.4 additional language.

Table 8�1 Steps Required for Upgrading an ALL-IN-1 STARTER V1.0

Language

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform(continued on next page)

Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages 8�3

Table 8�1 (Cont.) Steps Required for Upgrading an ALL-IN-1 STARTER V1.0

Language

STEP Title

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

17 Select the date format to use with ALL-IN-1

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

8.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1L<lang> V2.4 has failed.

If the IVP fails, the following messages are displayed:

        The A1L<lang> V2.4 Installation Verification Procedure failed.

        %VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

The A1L<lang> V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

where <lang> is the name of the language being installed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

8�4 Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

8.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages 8�5

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP /LANGUAGE=lang where lang is the name of the language being installed.

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note The IVP runs in the language context of the current optional language being installed and also tests the international base system.

Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

8�6 Upgrading ALL-IN-1 STARTER V1.0 Languages to ALL-IN-1 V2.4 Languages

9 Updating ALL-IN-1 STARTER V2.4 to

ALL-IN-1 V2.4

This chapter explains how to upgrade from ALL-IN-1 STARTER Version 2.4 to

ALL-IN-1 Version 2.4.

9.1 Before You Start

Before you start the installation procedure:

1 Make sure that you have made all the necessary preparations (see

Section 1.8).

2 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

3 If you have carried out any permitted modi�cations (for example, to template �les) to your ALL-IN-1 STARTER Version 2.4 system, save the modi�cations in an area that is not used by ALL-IN-1.

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 Run the following command procedure to set up the correct environment for the upgrade installation:

SYS$MANAGER:AS024_PREV24_UPGRADE.COM

You must have the base, language, and market components to update your

ALL-IN-1 STARTER Version 2.4 system to ALL-IN-1 Version 2.4.

Note Updating to ALL-IN-1 Version 2.4 also updates your default language. If you have a multi-language ALL-IN-1 system, you will be unable to use your additional languages until you have updated them; you can still use your

Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4 9�1

default language. In this case, you must run only the IVP for the default language.

9.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed

The name of the device where the distribution media are to be mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution media and that command procedure controls the rest of the installation.

9.3 Determining the Files and Logical Names Added to the

System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

9.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

9.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

9�2 Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4

9.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

%UAF-E-RDBADDERRU, unable to add A1$XFER_IN value:

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

%UAF-E-RDBADDERRU, unable to add A1$XFER_OUT value:

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

9.7 The Installation Procedure

Table 9�1 lists the step required to update your ALL-IN-1 STARTER Version

2.4 system to ALL-IN-1 Version 2.4.Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4 9�3

Table 9�1 Steps Required to Update your ALL-IN-1 STARTER V2.4 System to

ALL-IN-1 V2.4

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

7 Load the Distribution Media - Sequence 2

8 Specify the market code required by this installation

9 Specify the language code required by this installation

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

12 Indicate whether or not you want to incorporate DATATRIEVE

13 Indicate whether or not you want to incorporate WPS-PLUS

14 Indicate whether or not you want to incorporate ACMS

16 Indicate whether or not you want to build a multi-language system

17 Select the date format to use with ALL-IN-1

18 Specify the greatest number of simultaneous ALL-IN-1 users

19 Specify the batch queue to run the Sender and Fetcher

20 Indicate whether or not you want to send and receive messages to and from other systems

21 Indicate whether the Message Router you want ALL-IN-1 to use is on this node or another node

22 Specify the node whose Message Router you want to use

23 Specify the level of use of the Mail directory

24 Specify the password for the ALL-IN-1 Message Router mailbox

25 Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

46 Load the Distribution Media - Sequence 3

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

9�4 Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4

You must now update any additional languages that were installed with your

(ALL-IN-1) STARTER Version 2.4 system. A separate installation is required for each of the additional languages on your system (see Chapter 10).

9.8 Stop and Start the OA$FORMATTER Queue

You must stop and restart the OA$FORMATTER queue by entering the following commands:

$ STOP /QUEUE /NEXT OA$FORMATTER

$ START /QUEUE OA$FORMATTER

9.9 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1 V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1 V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4 9�5

9.9.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

9�6 Updating ALL-IN-1 STARTER V2.4 to ALL-IN-1 V2.4

10 Updating ALL-IN-1 STARTER V2.4

Languages to ALL-IN-1 V2.4 Languages

This chapter explains how to update an ALL-IN-1 STARTER Version 2.4 additional language to an ALL-IN-1 Version 2.4 additional language.

10.1 Before You Start

Before you start the installation procedure:

1 Print and read the ALL-IN-1 Release Notes Part 1 Language (see

Section 2.1)

2 Make sure that you have made all the necessary preparations (see

Section 1.8).

3 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You need only the required language component to update an ALL-IN-1

STARTER Version 2.4 additional language to an ALL-IN-1 Version 2.4 additional language.

Note You must update your main ALL-IN-1 STARTER Version 2.4 system to

ALL-IN-1 Version 2.4 before updating the languages. See Chapter 9.

Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages 10�1

10.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.

The name of the device where the distribution medium is mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution medium and that command procedure controls the rest of the installation.

10.3 Determining the Files and Logical Names Added to the System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

10.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

10.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

10�2 Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages

10.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

10.7 The Installation Procedure

Table 10�1 lists the steps required for updating an ALL-IN-1 STARTER

Version 2.4 additional language to an ALL-IN-1 Version 2.4 additional language.

Table 10�1 Steps Required for Updating an ALL-IN-1 STARTER V2.4

Language

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform(continued on next page)

Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages 10�3

Table 10�1 (Cont.) Steps Required for Updating an ALL-IN-1 STARTER V2.4

Language

STEP Title

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

17 Select the date format to use with ALL-IN-1

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

10.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1L<lang> V2.4 has failed.

If the IVP fails, the following messages are displayed:

The A1L<lang> V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

where <lang> is the name of the language being installed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

10�4 Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

10.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedurewas run.

Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP /LANGUAGE=lang where lang is the name of the language being installed.

Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages 10�5

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note The IVP runs in the language context of the current optional language being installed and also tests the international base system.

Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

10�6 Updating ALL-IN-1 STARTER V2.4 Languages to ALL-IN-1 V2.4 Languages

11 Updating an Existing ALL-IN-1 V2.4 System

This chapter explains how to update your existing ALL-IN-1 Version 2.4 system. You can update your ALL-IN-1 Version 2.4 system if you decide to change the con�guration, or an ALL-IN-1 component is revised by Digital.

11.1 Before You Start

Before you start the installation procedure:

1 Make sure that you have made all the necessary preparations (see Section

Section 1.8).

2 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

3 Complete the checklist of information required for installation given in

Section Section 1.8.20. Refer to this checklist during the installation.

4 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You must have the base, language, and market components to update ALL-IN-1

Version 2.4.

11.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installedUpdating an Existing ALL-IN-1 V2.4 System 11�1

The name of the device where the distribution media are to be mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution media and that command procedure controls the rest of the installation.

11.3 Determining the Files and Logical Names Added to the System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

11.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

11.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press

CTRL/Y, and the installation is being performed in Safety mode (see Section

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

11.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

%SYSTEM-E-NOSUCHSEC, no such (global) section

11�2 Updating an Existing ALL-IN-1 V2.4 System

%UAF-E-RDBADDERRU, unable to add A1$XFER_IN value:

[000001,000100] to RIGHTSLIST.DAT

-SYSTEM-F-DUPIDENT, duplicate identifier

%UAF-E-RDBADDERRU, unable to add A1$XFER_OUT value:

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

11.7 The Installation Procedure

Table 11�1 lists the step required to update your existing ALL-IN-1 Version 2.4 system.

Table 11�1 Steps Required for Updating an Existing ALL-IN-1 V2.4 System

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

7 Load the Distribution Media - Sequence 2

8 Specify the market code required by this installation

9 Specify the language code required by this installation

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

12 Indicate whether or not you want to incorporate DATATRIEVE(continued on next page)

Updating an Existing ALL-IN-1 V2.4 System 11�3

Table 11�1 (Cont.) Steps Required for Updating an Existing ALL-IN-1 V2.4

System

STEP Title

13 Indicate whether or not you want to incorporate WPS-PLUS

14 Indicate whether or not you want to incorporate ACMS

16 Indicate whether or not you want to build a multi-language system

17 Select the date format to use with ALL-IN-1

18 Specify the greatest number of simultaneous ALL-IN-1 users

19 Specify the batch queue to run the Sender and Fetcher

20 Indicate whether or not you want to send and receive messages to and from other systems

21 Indicate whether the Message Router you want ALL-IN-1 to use is on this node or another node

22 Specify the node whose Message Router you want to use

23 Specify the level of use of the Mail directory

25 Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

46 Load the Distribution Media - Sequence 3

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps.

11.8 Start the OA$FORMATTER Queue

The OA$FORMATTER queue is restarted if you elected to run the IVP during the installation. If you did not elect to run the IVP, you must restart the

OA$FORMATTER queue by entering the following command:

$ START /QUEUE OA$FORMATTER

11.9 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

11�4 Updating an Existing ALL-IN-1 V2.4 System

If the IVP fails, the following messages are displayed:

The A1 V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1 V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

11.9.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run. Updating an Existing ALL-IN-1 V2.4 System 11�5

Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.

11�6 Updating an Existing ALL-IN-1 V2.4 System

12 Updating an ALL-IN-1 V2.4 Language

This chapter explains how to update an ALL-IN-1 Version 2.4 language.

12.1 Before You Start

Before you start the installation procedure:

1 Print and read the ALL-IN-1 Release Notes Part 1 Language (see

Section 2.1)

2 Make sure that you have made all the necessary preparations (see

Section 1.8).

3 Make sure that no ALL-IN-1 logical names point to system root directories, for example, OA$LIB must not be de�ned as

SYS$SYSROOT:[ALLIN1.LIB].

4 Complete the checklist of information required for installation given in

Section 1.8.20. Refer to this checklist during the installation.

5 If you have rebooted your system prior to starting the installation, make sure that you have run the ALL-IN-1 startup command procedure

(SYS$MANAGER:A1V24START.COM) before you start the installation.

You need only the required language component to update an ALL-IN-1 Version

2.4 additional language.

12.2 Overview of VMSINSTAL

VMSINSTAL is a DCL command procedure that is used to install optional software products on the VMS operating system. VMSINSTAL requires at least two parameters:

The name of the product(s) being installed.Updating an ALL-IN-1 V2.4 Language 12�1

The name of the device where the distribution medium is mounted or loaded. You can use either a physical or logical device name.

VMSINSTAL invokes a command procedure on the distribution medium and that command procedure controls the rest of the installation.

12.3 Determining the Files and Logical Names Added to the System

A list of the �les, and their directories, of an installed ALL-IN-1 Version 2.4 system is given in Appendix C.

A list of the logical names added to your system is given in Appendix C.

12.4 Running the Installation Veri�cation Procedure (IVP)

The Installation Veri�cation Procedure (IVP) for ALL-IN-1 Version 2.4 veri�es the installation. During the installation, you are asked if you want to run the

IVP as part of the installation. If you respond YES, VMSINSTAL runs the IVP.

Digital recommends that you run the IVP to ensure that ALL-IN-1 Version 2.4 is installed correctly.

After ALL-IN-1 Version 2.4 is installed, you can run the IVP independently to verify that the software is available on your system. You might also want to run the IVP after a system failure to ensure that users can access ALL-IN-1

Version 2.4. Instructions on running the IVP are given in the ALL-IN-1

Management Guide.

12.5 Aborting the Installation

To abort the installation procedure at any time, press CTRL/Y. When you press CTRL/Y, and the installation is being performed in Safety mode (see

Section 1.8.16.1), the installation procedure deletes all �les it has created up to that point and exits. You must restart the installation from the beginning.

Note VMSINSTAL does not delete any accounts or directory structures that are created.

12.6 Warning and Error Messages

The following warning and error messages may be displayed during the installation:

%INSTALL-W-NOPREV, no previous entry exists - new entry created for

<filename> where <�lename> is the full �le speci�cation for the image that is to be created.

12�2 Updating an ALL-IN-1 V2.4 Language

%SYSTEM-E-NOSUCHSEC, no such (global) section

These messages can be ignored.

The following informational and error messages are displayed when the IVP is run:%OA-I-LNF, Error opening form library "THIS_IS_A_TEST"

-RMS-E-FNF, file not found

%OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

%OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form
library

These messages are due to various tests being performed by the IVP.

12.7 The Installation Procedure

Table 12�1 lists the steps required for updating an existing language.

Table 12�1 Steps Required for Updating an Existing ALL-IN-1 V2.4

Language

STEP Title

1 Invoke VMSINSTAL

2 DECnet status

3 Active processes

4 System backup

5 Load the distribution media - Sequence 1

6 Indicate which type of installation you wish to perform

10 Indicate whether you have registered and loaded your ALL-IN-1 Product

Authorization Key

11 Indicate whether or not you want to purge �les replaced by the installation

17 Select the date format to use with ALL-IN-1

26 Check the mandatory and optional software prerequisites

34 Indicate the existing VMS username for the ALL-IN-1 account

45 Indicate whether or not you want to run the IVPs

47 Wait for the installation to complete

48 Complete installation

The steps are described in Chapter 13. Before starting the installation, indicate the steps required for your installation by placing a tick in the box for each of the steps. Updating an ALL-IN-1 V2.4 Language 12�3

12.8 Error Recovery

If errors occur during the installation itself or when the IVP is running,

VMSINSTAL displays failure messages. If the installation fails, the following message is displayed:

%VMSINSTAL-E-INSFAIL, The installation of A1L<lang> V2.4 has failed.

where <lang> is the name of the language being installed.

If the IVP fails, the following messages are displayed:

The A1L<lang> V2.4 Installation Verification Procedure failed.

%VMSINSTAL-E-IVPFAIL, The IVP for A1L<lang> V2.4 has failed.

Errors can occur during the installation if any of the following conditions exist:

The operating system version is incorrect

A prerequisite software version is incorrect

Quotas necessary for successful installation are insuf�cient

System parameter values for successful installation are insuf�cient

The VMS help library is currently in use

The product is not properly licensed

SYS$LIBRARY:IMAGELIB.OLB and SYS$LIBRARY:STARLET.OLB are not present. These �les are removed if you tailor VMS.

For descriptions of the error messages generated by these conditions, see the VMS books on system messages, recovery procedures, and VMS software installation. If you are noti�ed that any of these conditions exist, you should take the appropriate action as described in the message. (You might need to change a system parameter or increase an authorized quota value.) For information on installation requirements, see Chapter 1.

Note If the installation fails, you must restart the installation from the beginning.

12.8.1 Errors Found During the IVP

If any error messages occur during the IVP, do the following:

Check the log of the installation for any errors that may have occurred during installation.

Check the �le ALLIN1_IVP.LOG. This �le does not contain the results of the IVP, but the results of invoking ALL-IN-1 when running the

IVPs. This �le is in the directory where you run the installation, usually

SYS$MANAGER.

12�4 Updating an ALL-IN-1 V2.4 Language

Make sure you have executed the startup command procedure

SYS$MANAGER:A1V24START.COM so that all image �les, logical names and form libraries have been successfully installed.

Make sure that the ALL-IN-1 TXL and your site-speci�c TXL, if there is one, were compiled and installed successfully and recompile them if you received any error messages when the startup command procedure was run.Check that you have not run out of quota on the disk(s) containing the

OA$SHAREnnnn directories (refer to the manual describing VMS utilities).

Check that the details for the IVP account are completed correctly, as follows:All the ALL-IN-1 privileges are set to YES.

The IVP user directory points to the disk and subdirectory that you speci�ed for the ALL-IN-1 manager’s account. For example, using the installation defaults would give:

SYS$SYSDEVICE:[ALLIN1.IVPUSER]

The ALL-IN-1 account, IVP, is accessed from the ALL-IN-1 manager’s

VMS account.

Run ALL-IN-1 and try to use those areas that failed during the IVP to �nd more information on the error.

Log in to the ALL-IN-1 manager’s IVP account:

$ ALLIN1 /USERNAME=IVP /LANGUAGE=lang where lang is the name of the language being installed.

Manually execute each IVP test as described in the ALL-IN-1 Management

Guide.

Note The IVP runs in the language context of the current optional language being installed and also tests the international base system.

Most IVPs are designed to exercise and test ALL-IN-1 at a level which is normally customization independent. However, if you have customized the Phone Directory subsystem of ALL-IN-1, the display graphics (IDG) procedure may fail. This is a demonstration test used to exercise the terminal graphics as a typical application.Updating an ALL-IN-1 V2.4 Language 12�5

13 Steps Required for Installing ALL-IN-1 V2.4

This chapter contains a complete list of the steps required for installing

ALL-IN-1 Version 2.4. The steps required depend on the type of installation you are performing (see the chapter for the type of installation you are going to perform (Chapters 3 to 12).

Indicate the steps required for your type of installation by placing a tick in the box for each of those steps.

For those steps that require you to input information, enter the information in the space provided, before you start the installation.

13.1 Installation Steps

During the installation procedure a number of cautionary messages and general information messages, which are not documented here, are displayed.

Read all messages carefully and follow the advice they offer.

Each question in the installation is marked with an asterisk (*) at the beginning of the line. If you are unsure how to answer a question, enter a question mark (?). The installation procedure displays explanatory text.

Note If the installation fails, you must restart the installation from the beginning.

STEP 1: Invoke VMSINSTALTo start the installation, log in to the privileged VMS system

manager’s account, and enter the following command:

$ SET DEFAULT SYS$UPDATE

If you are performing a new, upgrade, or update installation, enter:

Steps Required for Installing ALL-IN-1 V2.4 13�1

$ @VMSINSTAL A1024 device:

If you are installing an additional language, or upgrading or updating an existing language, enter:

$ @VMSINSTAL A1Llang024 device:

device is the device on which the distribution media are to be mounted. You can use either a physical or logical device name. Logical device names must not begin with A1$ or OA$.

A1024, is the product identi�er for the full ALL-IN-1 Version 2.4 system.

A1Llang024 is the product identi�er for the language to be installed.

For example, enter the following command if you are performing a new, upgrade or update installation:

$ @VMSINSTAL A1024 TAPE0

Note Do not use the command @VMSINSTAL * device:, since this causes

VMSINSTAL to install the products from the kit in the incorrect order.

If you omit these items, you are prompted for the product identi�er and device.

The following messages are displayed:

        VAX/VMS Software Product Installation Procedure V<version>

It is <dd-mmm-yyyy> at <hh:mm>
Enter a question mark (?) at any time for help.

<version> is the version of VMS that you are running on your system

<dd-mmm-yyyy> and <hh:mm> are the current date and time

If your system is running VMS Version 5.2, or higher, and any users are logged in to your system, VMSINSTAL goes to STEP 3.

If your system is running VMS Version 5.2, or higher, and no users are logged in to your system, VMSINSTAL goes to STEP 4.

STEP 2: DECnet status

If your system is running VMS Verison 5.1, and your DECnet network is running, the following message is displayed:

%VMSINSTAL-W-DECNET, Your DECnet network is up and running.
* Do you want to continue anyway [NO]?

Enter YES to continue.

13�2 Steps Required for Installing ALL-IN-1 V2.4

If you want to use a local Message Router and it is not running, press RETURN. VMSINSTAL aborts. Start the Message Router and restart the installation.

Note If you want to use Mail directory addressing, make sure that the Message

Router Directory Service is running on your system. If you are installing ALL-IN-1 on a multiple-environment cluster, the Message Router Directory Service must be running on the part on which you are installing ALL-IN-1 (see Section 1.6.2.1).

STEP 4: System Backup

VMSINSTAL displays:

* Are you satisfied with the backup of your system disk [YES]?

If you are not satis�ed, enter NO, carry out a disk backup and restart the installation.

If you are satis�ed, press RETURN.Steps Required for Installing ALL-IN-1 V2.4 13�3

STEP 5: Load the distribution media�Sequence 1

If you did not specify a device when invoking VMSINSTAL, the following message is displayed:

* Where will the distribution volumes be mounted:

Enter the device on which the media are to be mounted. You can use either a physical or logical device name. Logical device names must not begin with A1$ or OA$.

If you did not specify the product identi�er when invoking VMSINSTAL, the following message is displayed:

Enter the products to be processed from the first distribution volume set:
* Products:

If you are performing a new, upgrade or update installation, enter the product identi�er, A1024.

If you are installing an additional language, or upgrading or updating an existing language, enter the product identi�er, A1Llang024.

If your system is running VMS Version 5.1, VMSINSTAL displays:

* Options:

If your system is running VMS Version 5.2 (or higher), VMSINSTAL displays:

* Enter installation options you wish to use (none):

Press RETURN to continue.

If you are installing ALL-IN-1 Version 2.4 from magnetic tape or TK50 cartridge, VMSINSTAL displays:

Please mount the first volume of the set on <device>:
* Are you ready?

where <device>: is the device you speci�ed.

Mount the �rst volume of the distribution media.

For a new, upgrade or update installation, this is the volume labeled: ALL-IN-1 V2.4 BASE BIN media_type INTERNATIONAL BASE (c) 1989 Digital Equipment Corp.

For an additional language installation, or an update of an existing language, this is the volume labeled:

13�4 Steps Required for Installing ALL-IN-1 V2.4

ALL-IN-1 V2.4 language BIN media_type LANGUAGE COMPONENT (c) 1989 Digital Equipment Corp.

media_type is 16MT9 for tape and TK50 for a TK50 cartridge. (If you are unfamiliar with the loading of media, refer to the VMS software installation documentation.)

When you have mounted the volume, enter YES. VMSINSTAL tries to mount the distribution volume. If it succeeds, the following messages are displayed:

If you are performing a new, upgrade or update installation:

                    %MOUNT-I-MOUNTED, A11024 mounted on <device>:

The following products will be processed:
  A1 V2.4

        Beginning installation of A1 V2.4 at <hh:mm>

%VMSINSTAL-I-RESTORE, Restoring product saveset A...
%VMSINSTAL-I-RELMOVED, The product’s release notes have been successfully
     moved to SYS$HELP.

This is LOCAL ALL-IN-1 V2.4 BASE kit

<hh:mm> is the current time.

If you are installing an additional language, upgrading or updating an existing language:

                    %MOUNT-I-MOUNTED, A13024 mounted on <device>:

The following products will be processed:
  A1L<lang> V2.4

        Beginning installation of A1L<lang> V2.4 at <hh:mm>

%VMSINSTAL-I-RESTORE, Restoring product saveset A...
%VMSINSTAL-I-RELMOVED, The product’s release notes have been successfully
     moved to SYS$HELP.

This is the LOCAL ALL-IN-1 V2.4 LANGUAGE-only kit

<hh:mm> is the current time.

The installation continues at STEP 7. However, if you are upgrading or updating from a multilingual system, you can use only the language that is being installed at this time. You must upgrade or update the remaining languages before you can use them. Also, you cannot run the Installation Veri�cation Procedure for the additional languages until you have upgraded or updated them. Enter 7 to register the licenses. This option registers and loads the licenses for VAX FMS Version 2.4, Message Router Version 3.1, Message Router VMSmail Gateway Version 3.1, CDA Converter Library Version 1.0, and VAX Notes Version 2.0. VMSINSTAL displays:

%A1-I-CHKSWLIC, Checking licenses for prerequisite software
%A1-I-CONFLICENSE. All necessary licenses are installed and loaded
%VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
directories...
        Installation of A1 V2.4 completed at <hh:mm>

        VMSINSTAL procedure done at <hh:mm>

VMSINSTAL exits after registering the licenses. Before you install ALL-IN-1 Version 2.4, make sure that FMS, and if necessary, Message Router and Message Router VMSmail Gateway are running.

If you are performing an additional language installation or updating an existing language, VMSINSTAL displays:

   Using the LANGUAGE only ALL-IN-1 V2.4 KIT, the following types of
   installation can be performed :-

        (1) Installation of an additional language
        (2) Upgrade of an additional existing ALL-IN-1 V2.3 language
        (3) Update of an existing ALL-IN-1 V2.4 language

* What type of installation do you wish to perform [1]:

Press RETURN to indicate an additional language installation. Otherwise, enter 2 to upgrade an existing ALL-IN-1 Version 2.3 additional language, or enter 3 to update an existing ALL-IN-1 Version 2.4 language. If you are upgrading an ALL-IN-1 STARTER language to an ALL-IN-1 Version 2.4 language, enter:

2 To upgrade an ALL-IN-1 STARTER Version 1.0 language

3 To update an ALL-IN-1 STARTER Version 2.4 language

If you are performing an upgrade or update installation, VMSINSTAL searches for the default ALL-IN-1 image, OA$LIB_SHARE:OA$MAIN.EXE. If it does not �nd this image (because you have renamed the image), VMSINSTAL displays: Steps Required for Installing ALL-IN-1 V2.4 13�7

The main ALL-IN-1 image OA$MAIN.EXE cannot be found using its default
    specification

* Can you provide the full file specification of the main ALL-IN-1 image [YES]?

Press RETURN if you know the full �le speci�cation of the main ALL-IN-1 image. VMSINSTAL displays:

* What is the full file specification of the main ALL-IN-1 image:

Enter the full �le speci�cation of the image (including the device and directory).

If you do not know the full �le speci�cation, enter NO. VMSINSTAL exits. Find out the full �le speci�cation of your ALL-IN-1 image and start the installation again.

If you are installing a full ALL-IN-1 Version 2.4 system, or are upgrading or updating an existing ALL-IN-1 system, you may be prompted to enter a market code at this point if you are installing ALL-IN-1 from disk. If you see this prompt go to STEP 8.

If you are installing an additional language, you may be prompted to enter a language code at this point if you are installing the ALL-IN-1 language from disk. If you see this prompt go to STEP 9.

If you are updating an existing language, you may be prompted to enter a language code at this point if you are installing the ALL-IN-1 language from disk. If you see this prompt go to STEP 9.

STEP 7: Load the distribution media�Sequence 2

Mount the second volume of the distribution media. This is the volume labeled:

ALL-IN-1 V2.4 market BIN media_type MARKET COMPONENT (c) 1989 Digital Equipment Corp.

market is the market name

media_type is 16MT9 for tape and TK50 for a TK50 cartridge.

See the ALL-IN-1 Installation Guide Part 3 Market Installation.

The following messages are displayed:

Media <device>:A11024 dismounted. (MEDIA CHANGE REQUIRED):
Dismounted media labeled A11024. Please mount the MARKET kit media which
is labeled A12024 and reply to the prompt below. (Answer NO to exit).

* Type YES when correct media mounted, NO to terminate installation?

13�8 Steps Required for Installing ALL-IN-1 V2.4

When you have mounted the volume, enter YES. VMSINSTAL tries to mount the distribution volume. If the distribution volume is mounted, the following messages are displayed:

%MOUNT-I-MOUNTED, A12024 mounted on <device>:
%A1C<market>-I-RECOUK, Restoring the MARKET kit savesets.
%VMSINSTAL-I-RESTORE, Restoring product saveset B . . .

where <market> is the market code (see the ALL-IN-1 Installation Guide Part 3 Market Installation).

Mount the third volume of the distribution media. This is the volume labeled:

ALL-IN-1 V2.4 language BIN media_type LANGUAGE COMPONENT (c) 1989 Digital Equipment Corp.

language is the language name

media_type is 16MT9 for tape and TK50 for a TK50 cartridge

See the ALL-IN-1 Installation Guide Part 2 Language Installation.

The following messages are displayed:

Media <device>:A12024 dismounted. (MEDIA CHANGE REQUIRED):
Dismounted media labeled A12024. Please mount the LANGUAGE kit media which is
labeled A13024 and reply to the prompt below. (Answer NO to exit).

* Type YES when correct media mounted, NO to terminate installation?

When you have mounted the volume, enter YES. VMSINSTAL tries to mount the distribution volume. If the distribution volume is mounted, the following messages are displayed:

%MOUNT-I-MOUNTED, A13024 mounted on <device>:
%A1L<lang>-I-RELANK, Restoring the LANGUAGE kit savesets.
%VMSINSTAL-I-RESTORE, Restoring product saveset B . . .

This is the <lang> version of ALL-IN-1 V2.4

where <lang> is the language being installed (see the ALL-IN-1 Installation Guide Part 2 Language Installation).

VMSINSTAL goes to STEP 10. Steps Required for Installing ALL-IN-1 V2.4 13�9

STEP 8: Specify the market code required by this installation

Market code: ......................

VMSINSTAL displays:

* Enter market code for this installation (up to 3 characters) [US]:

Press RETURN to accept the default, US. Otherwise, enter the market code required for your installation (see the ALL-IN-1 Installation Guide Part 3 Market Installation).

VMSINSTAL displays the following:

%A1C<market>-I-RECOUK, Restoring the MARKET kit savesets.
%VMSINSTAL-I-RESTORE, Restoring product saveset B . . .

STEP 10: Indicate whether you have registered and loaded your ALL-IN-1 Product Authorization Key

Have you registered and loaded the PAK? .........

If you are installing ALL-IN-1 for the �rst time, or updating or upgrading a an ALL-IN-1 system, you must have a capacity or personal (subscriber) license registered

13�10 Steps Required for Installing ALL-IN-1 V2.4

If you have a capacity (ALLIN1) license, and you want to install, update or upgrade an additional language, you must also have a language-speci�c capacity license, ALLIN1-UI-language, where language is the name of the language you want to install

If you have a personal (ALLIN1-PERSONAL) license, you can install, update or upgrade an additional language, without a language-speci�c license

VMSINSTAL displays:

* Does this product have an authorization key registered and loaded [YES]?

If you have not registered and loaded your product authorization key, you must answer NO to this question. VMSINSTAL then exits.

A successful installation of ALL-IN-1 depends on a product authorization key being registered and loaded. Please be certain that this has been completed before proceeding with the installation.

Press RETURN if you have a product authorization key registered and loaded for ALL-IN-1 Version 2.4.

If the appropriate licenses are registered and loaded, VMSINSTAL displays:

%LMF-I-GOTLICENSE, An <licence> license is installed and loaded

where <license> is:

ALLIN1 or ALLIN1-PERSONAL if you are installing ALL-IN-1 for the �rst time, or you are updating or upgrading a previous version of ALL-IN-1.

ALLIN1-PERSONAL or ALLIN1-UI-language if you are installing, updating, or upgrading an additional language

VMSINSTAL then checks for all prerequisite software licenses:

%LMF-I-CHKSWLIC, Checking licenses for prerequisite software

If a license already exists, and the installation updates the license with a more up-to-date version, the following message is displayed:

%LICENSE-I-ALREADYLOADED, <license> has already been loaded

<license> is the name of the license that has been updated.

If a license is not found, the license is registered then loaded, and the following message is displayed:

%LICENSE-I-LOADED, <license> was successfully loaded with <n> units

<license> is the name of the license that has been updated and <n> is the number of units for the license. Steps Required for Installing ALL-IN-1 V2.4 13�11

STEP 11: Indicate whether or not you want to purge �les replaced by this installation

Do you want to purge �les? .........

You can choose to have the �les of your existing ALL-IN-1 system purged to save space on the disk(s) on which ALL-IN-1 Version 2.4 is being installed.

If you are performing an upgrade or update installation, VMSINSTAL displays:

* Do you want to purge files replaced by this installation?

This installation creates new copies of ALL-IN-1 language �les. You can purge the old copies of these �les.

Enter YES if you want to purge the old copies of these �les. Otherwise, enter

NO.

If you are upgrading or updating an existing language, VMSINSTAL goes to STEP 17.

13�12 Steps Required for Installing ALL-IN-1 V2.4

STEP 13: Indicate whether or not you want to incorporate WPS-PLUS

Do you want to incorporate WPS-PLUS? ..........

VMSINSTAL displays:

        If you wish to have the WPS-PLUS editor available then answer YES
        to the following question. If you answer NO, then your users will
        not be able to access the WPS-PLUS editor. Note this will also
        impact SPELL and MERGE functions.

   NOTE: You will be able to link WPS-PLUS in at a later time, should you
   choose not to link it now.

* Do you want to incorporate WPS-PLUS [YES]?Steps Required for Installing ALL-IN-1 V2.4 13�13

If you want to incorporate WPS-PLUS (see Section 1.5.5), press RETURN. Otherwise, enter NO.

Note If you decide not to incorporate WPS-PLUS at this time, you can incorporate WPS-PLUS at a later date by performing an update installation (see Appendix D for details).

STEP 14: Indicate whether or not you want to incorporate ACMS

Do you want to incorporate ACMS? ..........

VMSINSTAL displays:

   If you wish to interface with ACMS, then answer YES to the following
   questions.

   NOTE:

            o ACMS needs to be installed before ALL-IN-1.

            o If the user answers yes and the relevant ACMS files are
              present then the interface will get built. If they are not
              then the default is to abort the link, in order to remedy it.

* Do you want to incorporate ACMS [NO]?

If you do not want to incorporate ACMS (see Section 1.5.4), press RETURN. Otherwise, enter YES.

STEP 16: Indicate whether or not you want to build a multilingual system

Do you want to build a multilingual system? ..........

You can install an additional language to build a multilingual ALL-IN-1 system. See Section 1.7 for details.

VMSINSTAL displays:

        If you answer YES to this then you will produce TWO images -
   OA$MAIN.EXE and OA$LLVlanguage.EXE. This will allow more than one
   language to be installed.

* Do you want to build a MULTI-LANGUAGE system [NO]?

Press RETURN if you do not want to install other languages. Otherwise, enter YES. You install each additional language after ALL-IN-1 Version 2.4 is installed, by performing an additional language installation (see Chapter 4).

If you elect to build a multilingual system, the installation creates a languagespeci�c image �le, SYS$LIBRARY:OA$LLVlang.EXE, in addition to the OA$LIB_SHARE:OA$MAIN.EXE image �le.

Note The performance of ALL-IN-1 will suffer slightly if you con�gure ALL-IN-1 as

a multilingual system (that is, if you enter YES at the prompt). If you are not sure whether or not you want to run a multilingual ALL-IN-1 system, you can choose to install ALL-IN-1 Version 2.4 as a single language system, and relink the ALL-IN-1 image at a later date for multilingual operation (see the ALL-IN-1 Management Guide for details). Steps Required for Installing ALL-IN-1 V2.4 13�15

STEP 17: Select the date format to use with ALL-IN-1

Date format to use with ALL-IN-1: ..........

VMSINSTAL displays:

   ALL-IN-1 allows you to select a default date format for each language
   you have installed. This will become the default ALL-IN-1 date format
   for each user (on a per language basis). This may be changed by user
   through the Set Working Conditions option.

            Alphanumeric Date Numeric Date

        1 DD-MMM-YYYY MM/DD/YY (Standard Default)
        2 DD-MMM-YYYY DD/MM/YY
        3 DD-MMM-YYYY YY/MM/DD
        4 YYYY-MMM-DD MM/DD/YY
        5 YYYY-MMM-DD DD/MM/YY
        6 YYYY-MMM-DD YY/MM/DD

* Which date format do you require [1]:

Press RETURN to select the default date format DD-MMM-YYYY MM/DD/YY. Otherwise, enter the number of the desired date format. See the ALL-IN-1 Installation Guide Part 3 Market Installation.

If you are performing an additional language installation, VMSINSTAL goes to STEP 26.

STEP 19: Specify the batch queue to run the Sender and Fetcher

Batch queue for sending and receiving mail: ..........................

VMSINSTAL displays:

* Which batch queue would you like to use for sending/receiving mail
    [SYS$BATCH]:

If you are installing ALL-IN-1 on a multiple-environment cluster you must use a batch queue that runs only on the part of the cluster on which you are installing ALL-IN-1 (see Section 1.6.2).

ALL-IN-1 uses one of your system batch queues to run the mail Sender and Fetcher. Press RETURN to use SYS$BATCH. Otherwise, specify the name of another batch queue that exists already or that you will create before you run ALL-IN-1. If your system runs a local Message Router, you may consider using the Message Router queue MB$BATCH.

Note Digital recommends that you use a dedicated batch queue for the mail Sender

and Fetcher. Steps Required for Installing ALL-IN-1 V2.4 13�17

STEP 20: Indicate whether or not you want to send and receive messages to and from other systems

Do you want to send and receive messages to and from other systems? ..........

See Section 1.5.3 to help you decide whether or not to integrate ALL-IN-1 with Message Router.

VMSINSTAL displays:

* Do you want to use Message Router to send/receive messages to/from other
    systems [NO]?

Press RETURN if you do not want to send and receive electronic messages to and from other computer systems, or by way of the Message Router VMSmail Gateway to and from VMSmail. Otherwise, enter YES.

If you respond NO to this prompt, VMSINSTAL goes to STEP 26.

STEP 22: Specify the node whose Message Router you want to useMessage Router node name: ....................................

If you want to use a Message Router on another system, VMSINSTAL displays:

* What node is the Message Router on:

Enter the node name of the computer system whose Message Router you want to use. The following message is displayed:

The Message Router mailbox name has been set up to be <mailbox>.
If you wish to change the name you must create the file :

     OA$SITE_BUILD_SHARE:A1V24_SITE_START.COM

Change the definition of the logical name OA$MTI_MAILBX and then
when you run the MRMAN utility use this new name to define the
mailbox.

where <mailbox> is the name of ALL-IN-1 Message Router mailbox (usually A1).

VMSINSTAL goes to STEP 25.

Enter 0 if you do not want to use Mail directory addressing. VMSINSTAL goes to STEP 24.

Enter 1 if you want to use ALL-IN-1 directory addressing as the primary directory. The Mail directory can still be accessed from the Message Header menu.

Enter 2 if you want to use Mail directory addressing as the primary directory. ALL-IN-1 directory addressing can still be accessed from the Message Header menu.

If you are performing an update installation, and your ALL-IN-1 system currently uses a local Message Router with Mail directory support (that is, OA$DDS_PRIME is set to 1 or 2), VMSINSTAL displays the following message, and then continues at STEP 24:

As this is an update you will not be asked for a Mail directory password

If you are performing a new installation, or your ALL-IN-1 system currently uses a local Message Router without Mail directory support (that is, OA$DDS_PRIME is set to 0), VMSINSTAL displays:

* Enter password for the Mail directory user agent account:

Enter the password for the Mail directory user agent entry (minimum six characters, maximum eight characters).

VMSINSTAL asks you to con�rm the password:

* Please confirm the Mail directory password specified:

Enter the password again.

STEP 25: Indicate whether or not you want to translate outgoing WPS-PLUS and DX messages to ASCII

Translate outgoing WPS-PLUS and DX messages to ASCII? ............

VMSINSTAL displays:

* Do you want to translate outgoing WPS-PLUS and DX messages to ASCII [NO]?

Enter YES if:

Your users will be sending messages to DECmail. However, if your users send messages to DECmail users occasionally, you may want to enter NO, and ask your users to use EDT to send to DECmail if necessary. If you answer YES to this prompt, all messages will be translated to ASCII, whether or not they are sent to DECmail users. or: Your users will be sending messages to VMSmail through Version 2.0 or an earlier version of the Message Router VMSmail Gateway. This situation may occur if you are using a remote Message Router VMSmail Gateway.

ALL-IN-1 will then convert any outgoing messages to ASCII.

Steps Required for Installing ALL-IN-1 V2.4 13�21

If your users will not be sending messages to DECmail, or your ALL-IN-1 system will use Version 2.1 of the Message Router VMSmail Gateway, or higher, press RETURN. ALL-IN-1 will then exchange any messages in the same form in which they were created.

If the OA$ADMIN identi�er exists, and you are performing a new installation, VMSINSTAL displays information relating to OA$ADMIN, together with the prompt:

* Do you want to use the existing general identifier OA$ADMIN [YES]?

Enter NO if your existing OA$ADMIN identi�er is used for something other than ALL-IN-1. In this case, the installation will fail after all other checks have been made.

Press RETURN if you are sure that:

The OA$ADMIN identi�er is created only for ALL-IN-1

There are no holders of this identi�er outside ALL-IN-1

This identi�er is not speci�ed in any Access Control List (ACL) outside ALL-IN-1

If the OA$PRVAPP identi�er exists, and you are performing an upgrade or update installation, VMSINSTAL displays:

%A1L<lang>-I-GENIDOK, General identifier OA$PRVAPP will be used from the
    previous installation.

If the OA$PRVAPP identi�er exists, and you are performing a new installation, VMSINSTAL displays information relating to OA$PRVAPP, together with the prompt:

* Do you want to use the existing general identifier OA$PRVAPP [YES]?

Enter NO if your existing OA$PRVAPP identi�er is used for something other than ALL-IN-1. In this case, the installation will fail after all other checks have been made.

Press RETURN if you are sure that:

The OA$PRVAPP identi�er is created only for ALL-IN-1

There are no holders of this identi�er outside ALL-IN-1

This identi�er is not speci�ed in any ACL outside ALL-IN-1

If you are not installing an additional language, VMSINSTAL displays:

%A1L<lang>-I-CHKTRAC, Checking ALL-IN-1 transfer accounts

If you are performing an installation, and the accounts A1$XFER_IN and A1$XFER_OUT already exist, the following is displayed:

Steps Required for Installing ALL-IN-1 V2.4 13�23

VMS account named A1$XFER_IN, which should be used for ALL-IN-1
purposes only, was already created before this installation.

You have two options:

 1. Answer YES if you want the existing A1$TRANSFER account to be used
    for ALL-IN-1 pruposes ONLY. Note that in this case, some characterists
    of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
    the installation.
 2. Answer NO to stop the installation, correct the problem and then start
    again.

* Do you want to use the existing A1$XFER_IN account [NO]?

Press RETURN if you do not want to use the existing TRANSFER_INCOMING account.

Enter YES to continue. VMSINSTAL displays:

VMS account named A1$XFER_OUT, which should be used for ALL-IN-1
purposes only, was already created before this installation.

You have two options:

 1. Answer YES if you want the existing A1$TRANSFER account to be used
    for ALL-IN-1 pruposes ONLY. Note that in this case, some characterists
    of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
    the installation.
 2. Answer NO to stop the installation, correct the problem and then start
    again.

* Do you want to use the existing A1$XFER_OUT account [NO]?

Press RETURN if you do not want to use the existing TRANSFER_OUTGOING account.

Enter YES to continue. VMSINSTAL displays:

%A1L<lang>-I-CHKVMSV, Checking VAX/VMS version
%A1L<lang>-I-CHKLIBS, Checking required shareable libraries are installed
%A1L<lang>-I-CHKFMSV, Checking VAX/FMS version
%A1L<lang>-I-CHKMROV, Checking Message Router version

For all installations, VMSINSTAL displays:

%A1L<lang>-I-CHKPARA, Checking system parameters

If no errors are detected, the installation continues.

If you are upgrading your current ALL-IN-1 system to ALL-IN-1 Version 2.4, VMSINSTAL goes to STEP 34.

If you are updating your existing ALL-IN-1 Version 2.4 system, or ALL-IN-1 STARTER Version 2.4 system to ALL-IN-1 Version 2.4, VMSINSTAL goes to STEP 34.

If you are performing an additional language installation, VMSINSTAL goes to STEP 29.

13�24 Steps Required for Installing ALL-IN-1 V2.4

If any software checks fail, VMSINSTAL displays:

During the check phase following <n> errors are discovered:

        SHAREABLE LIBRARY FILES:

Shareable library file <filename> is NOT installed.
   .
   .
   .

        MESSAGE FILES:

Message file <filename> is NOT installed.
   .
   .
   .

   This installation will fail due to mismatched software
   prerequisites. However, you may continue and check the DISK SPACE
   requirements before the installation procedure terminates.
   Otherwise, stop the installation here and correct the reported
   problems before starting again.

* Do you want to continue [YES]?

<n> is the number of sofware errors detected, and <�lename> is the name of the �le that is not installed.

Press RETURN to continue to check the disk space requirements. VMSINSTAL goes to STEP 29, after which VMSINSTAL aborts.

Enter NO if you do not want to continue. VMSINSTAL displays:

%A1L<lang>-E-RETRY1, Please correct any reported problem(s) before attempting
%A1L<lang>-E-RETRY2, to install ALL-IN-1.

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

        VMSINSTAL procedure done at <hh:mm>

You must correct the error(s) and install ALL-IN-1 Version 2.4 again. Check the prerequisites given in Chapter 1.

STEP 28: Specify the device to hold the ALL-IN-1 shared data �lesDevice to hold shared data �les: ..................................

VMSINSTAL displays:

* Which device will hold the ALL-IN-1 shared data files [<device>:]:

Enter the logical name of the device to hold the ALL-IN-1 shared data �les in OA$DATA. Press RETURN to accept the default device which you speci�ed at STEP 27.

13�26 Steps Required for Installing ALL-IN-1 V2.4

You can use either a physical or logical device name. Digital recommends that you use a logical name for the device as users do not have to be concerned with the physical location of the volumes. Do not use a logical name that points to a search list. For example, do not use SYS$SYSROOT, SYS$SPECIFIC, or SYS$COMMON. Also, logical device names must not begin with A1$ or OA$.

If you enter an incorrect device speci�cation, the following prompt is displayed:

%A1L<lang>-W-NODEVICE, That device doesn’t exist on your system
* Do you want to select another device to hold the ALL-IN-1 DATA_SHARE
    files ? [NO]?

Enter YES to select another device. VMSINSTAL displays:

* Which device will hold the ALL-IN-1 shared data files :

Enter the logical name of the device to hold the ALL-IN-1 shared data �les in OA$DATA.

If there is insuf�cient disk space for the shared data �les, VMSINSTAL displays:

There is NOT enough diskspace on <device>: to provide DATA_SHARE files.
Please provide AT LEAST <nnnn> free blocks more on <device>: and restart
the installation, or choose another device to transfer DATA_SHARE files.

* Do you want to select another device to hold the ALL-IN-1 DATA_SHARE
    files ? [NO]?

Enter YES to select another device. VMSINSTAL prompts you to enter the logical name of the device.

Press RETURN if you do not want to select another device.

You can use either a physical or logical device name. Digital recommends that you use a logical name for the device as users do not have to be concerned with the physical location of the volumes. Do not use a logical name that points to a search list. For example, do not use SYS$SYSROOT, SYS$SPECIFIC, or SYS$COMMON. Also, logical device names must not begin with A1$ or OA$.

If you enter an incorrect device speci�cation, the following prompt is displayed:

%A1L<lang>-W-NODEVICE, That device doesn’t exist on your system
* Do you want to select another device to hold the ALL-IN-1 LLV files ? [NO]?

Enter YES to select another device. VMSINSTAL displays:

* Which device will hold the ALL-IN-1 <lang> language files :

Enter the logical name of the device to hold the ALL-IN-1 language �les for the language being installed.

If you are performing an additional language installation, VMSINSTAL goes to STEP 34.

If there is insuf�cient disk space for the language �les, VMSINSTAL displays:

There is NOT enough diskspace on <device>: to provide LLV files.
Please provide AT LEAST <nnnn> free blocks more on <device>: and restart
the installation, or choose another device to transfer LLV files.

* Do you want to select another device to hold the ALL-IN-1 LLV files ? [NO]?

Enter YES to select another device. VMSINSTAL prompts you to enter the logical name of the device.

Press RETURN if you do not want to select another device.

STEP 31: Indicate how many shared directories you would like

Number of shared directories: ...............

If you want to create more than 10 shared directories, Digital recommends that you select the default of 1. You can create the remaining number of shared directories after ALL-IN-1 Version 2.4 is installed (see the chapter on managing mail areas in the ALL-IN-1 Management Guide). The reason for this is that it is much quicker to create additional shared directories using the option provided in the management subsystem of ALL-IN-1 Version 2.4.

Note that the number of shared directories cannot exceed 9999. ALL-IN-1 uses the shared directories in rotation.

VMSINSTAL displays:

* How many shared directories do you want to create [1]:

Steps Required for Installing ALL-IN-1 V2.4 13�29

Enter the number of shared directories you would like to create. If you want to use only one directory, press RETURN.

If there is insuf�cient disk space for the shared directories, VMSINSTAL displays:

There is NOT enough diskspace on <device>: to create shared area SHARE<n>
please provide AT LEAST <nnnn> free blocks more on <device>: and restart
the installation, or choose another device to create shared area SHARE<n>.

* Do you want to select another device to create shared file cabinet
    SHARE<n> [NO]?

Enter YES to select another device. VMSINSTAL prompts you to enter the logical name of the device.

Press RETURN if you do not want to select another device.

If all disk space prerequisites are satis�ed, VMSINSTAL displays:

NO missing DISK SPACE prerequisites discovered.

If any errors were found during the software checks (STEP 26), VMSINSTAL displays:

%A1L<lang>-E-RETRY1, Please correct any reported problem(s) before attempting
%A1L<lang>-E-RETRY2, to install ALL-IN-1.

%VMSINSTAL-E-INSFAIL, The installation of A1 V2.4 has failed.

        VMSINSTAL procedure done at <hh:mm>

STEP 34: Indicate the existing VMS username for the ALL-IN-1 account

If you are performing an upgrade or update installation, or an additional language installation, VMSINSTAL displays:

* What is the existing VMS username for the ALL-IN-1 account [ALLIN1]:

Press RETURN to use the default name ALLIN1.

Otherwise, enter the name you want to use. Refer to the VMS manual describing the Authorize Utility for a list of valid characters that can be used for the user name.

Details of the ALL-IN-1 account are displayed if you are:

Performing a new installation and the account already exists

Performing an upgrade installation

Performing an update installation

Installing an additional language

Updating an existing language

The details displayed are as follows:

OWNER = <owner>
USERNAME = <username>
UIC = <UIC>
ACCOUNT = <account>
PRIVS = <privileges>
PRIORITY = <priority>
DIRECTORY = <device:[directory]>

13�32 Steps Required for Installing ALL-IN-1 V2.4

Also, the following prompt is displayed:

* Are you sure all the specified account’s characteristics are correct? [YES]?

Press RETURN if you want to use this account. VMSINSTAL:

Goes to STEP 36 if you are performing a new installation, and you created an ALL-IN-1 account before starting the installation

Goes to STEP 36 if you are performing an upgrade installation

Goes to STEP 45 if you are performing an update installation

Goes to STEP 42 if you are installing an additional language

Goes to STEP 45 if you are updating an existing language

Enter NO if you do not want to use this account. VMSINSTAL prompts you again for the username.

Enter the username.

accounts

Two VMS accounts, A1$XFER_IN and A1$XFER_OUT, are created. These accounts are used for transferring users to other systems. ALL-IN-1 logs in to these accounts, which are on the same disk as the ALL-IN-1 manager’s account. Steps Required for Installing ALL-IN-1 V2.4 13�33

STEP 37: Specify the UIC for the ALL-IN-1 manager’s VMS account

UIC: [ , ]

VMSINSTAL displays:

* What UIC do you want to use for the account <account_name>:

where <account_name> is the name of the ALL-IN-1 manager’s VMS account that you speci�ed in STEP 33.

You must enter a unique UIC, with a system group number.

Note All the ALL-IN-1 shared library �les, shared data �les, and shared documents

are owned by this UIC. Therefore, if disk quota checking is enabled on any of the devices used for ALL-IN-1 areas, this UIC must have a suitably large quota.

If you enter an invalid UIC, VMSINSTAL displays:

To be classified as a System UIC group member, the ALL-IN-1 manager’s account

must have the group number in the range 1 through <max_sys_group>.

If you do not want to continue with this installation then answer NO to the
next question.

* Do you want to select another UIC value:

where <max_sys_group> is the maximum group number for a system UIC (MAXSYSGROUP) de�ned on your system. The default is 10.

Enter NO if you do not want to enter another UIC value. VMSINSTAL aborts.

Enter YES if you want to enter another UIC value. VMSINSTAL prompts you to enter another UIC.

13�34 Steps Required for Installing ALL-IN-1 V2.4

A1$XFER_IN UIC: [ , ]

A1$XFER_OUT UIC: [ , ]

If the transfer user accounts do not exist, VMSINSTAL displays:

* What UIC do you want for the A1$XFER_IN account?:

Enter a non-system UIC for the account.

VMSINSTAL displays:

* What UIC do you want for the A1$XFER_OUT account?:

Enter a non-system UIC for the account.

The UIC for each of these accounts need not have the same system group number.

If the transfer user accounts already exist, the UICs of the transfer user accounts are checked. If the UICs are system UICs, the following prompt is displayed: Steps Required for Installing ALL-IN-1 V2.4 13�35

STEP 40: Specify the directory to hold the shared library �les, in OA$LIB

Directory for the shared library �les: ..............................

VMSINSTAL asks you for the name of the directory to hold the shared library �les:

* Enter ALL-IN-1 top-level directory required for the shared library files
    [<directory>]:

Press RETURN to use the default directory <directory>, where <directory> is the name of the ALL-IN-1 account you speci�ed at STEP 38. Otherwise, enter the name of the directory.

STEP 42: Specify the directory to hold the language �les

Directory for the language �les: ..................................

VMSINSTAL asks you for the name of the directory to hold the language �les, where <language> is the language that you are installing.

If you are performing a new installation, VMSINSTAL displays:

* Enter ALL-IN-1 top-level directory required for all <lang> language
    files [<directory>]:

Press RETURN to use the default directory which you speci�ed at STEP 41. Otherwise, enter the name of the directory.

If you are performing an additional language installation, VMSINSTAL displays:

* Enter ALL-IN-1 sub-directory required for the <lang> language files
    [<directory>]:

Press RETURN to use the default directory [ALLIN1]. Otherwise, enter the name of the directory. VMSINSTAL goes to STEP 45.

STEP 45: Indicate whether or not you want to run the IVPs

Do you want to run the IVPs? ..........

VMSINSTAL displays:

* Do you want to run the IVP after the installation [YES]?

Enter NO if you do not want to run the IVP after the installation.

Press RETURN if you want to run the IVP after the installation. The IVP is run automatically at the end of the installation. Any messages output by the IVP are either printed on your hardcopy terminal or inserted into the log �le, depending on your choice of media for the log of the installation.

Note Digital recommends that you run the IVP after installation.

VMSINSTAL displays the following message:

%A1L<lang>-I-ASKDONE, All questions have now been completed.
%A1L<lang>-I-SOMTIME, The installation will now continue for some time.
    No further action is required.

13�38 Steps Required for Installing ALL-IN-1 V2.4

If you are upgrading from ALL-IN-1 Version 2.3 or ALL-IN-1 STARTER Version 1.0, and the installation is being performed in Safety mode, the following message is displayed:

File [.DATA_SHARE]PROFILE.DAT prepared to be renamed to
    [.DATA_SHARE]V23_PROFILE.DAT

The ALL-IN-1 Version 2.3 �le, PROFILE.DAT, is renamed to V23_PROFILE.DAT at a later stage of the installation.

If you are upgrading from ALL-IN-1 Version 2.3 or ALL-IN-1 STARTER Version 1.0, and the installation is being performed in Non-Safety mode, the ALL-IN-1 Version 2.3 �le, PROFILE.DAT, is renamed to V23_PROFILE.DAT and the following message is displayed:

File [.DATA_SHARE]PROFILE.DAT renamed to [.DATA_SHARE]V23_PROFILE.DAT

If you were asked to enter a language code (see STEP 10), VMSINSTAL goes to STEP 47.

If you are installing an additional language, or upgrading or updating an existing language, VMSINSTAL goes to STEP 47.

When you have mounted the volume, enter YES. VMSINSTAL tries to mount the distribution volume. If it succeeds, the following message is displayed:

%MOUNT-I-MOUNTED, A11024 mounted on <device>:
%A1-I-MEDEXCH, Media changed from A1L<lang>024, to A1024
%VMSINSTAL-I-RESTORE, Restoring product saveset B . . .
   .
   .
   .

where <lang> is the language being installed.

STEP 48: Complete installation

When VMSINSTAL has �nished installing ALL-IN-1, it displays:

Installation of A1 V2.4 completed at <hh:mm>

If you invoked VMSINSTAL without specifying any parameters (see STEP 1), VMSINSTAL displays:

Enter the products to be processed from the next distribution volume set.
* Products:

        VMSINSTAL procedure done at <hh:mm>

<hh:mm> is the current time.

13�40 Steps Required for Installing ALL-IN-1 V2.4

Enter EXIT, or press CTRL/Z to exit from VMSINSTAL.

Note that VMSINSTAL deletes or changes entries in the process symbol tables during the installation. Therefore, if you are going to continue using the system manager’s account and you want to restore these symbols, you must log out and log in again.

Carry out the tasks described in Chapter 14 to set up ALL-IN-1 ready for use.

Steps Required for Installing ALL-IN-1 V2.4 13�41 14 After Installing ALL-IN-1 V2.4

This chapter describes the tasks to complete so that ALL-IN-1 can be run by users.

Table 14�1 indicates the sections that you need to refer to in this chapter for the type of installation that you are performing.

Table 14�1 Section Reference Chart

Installation Type

Sub-sections

1 2,3 4 5 6,7 & 8 9,10 11 12,13 14 15,16 17 18 19,20� 21

New ALL-IN-1 V2.4 installation

* * * * * * * *

ALL-IN-1 V2.4 additional language installation * * *

Upgrade from ALL-IN-1 V2.3

* * * * * * * * * * * * *

Upgrade of an

language

* * * ALL-IN-1 STARTER V1.0

* * * * * * * * * * * * Indicates that you need to refer to this section � refer to this section if your users are currently using WPS-PLUS/VMS (continued on next page)

After Installing ALL-IN-1 V2.4 14�1

Enter the location of the file A1CONFIG.DAT:

Enter the location of the ALL-IN-1 Version 2.4 con�guration �le, A1CONFIG.DAT. Refer to the log of the installation for the location of A1CONFIG.DAT.

Note If you are running ALL-IN-1 on a VAXcluster system, you must execute the

ALL-IN-1 startup command procedure on each node in the cluster. Therefore, you must modify the entry in the startup command procedure on each node. You must also edit OA$BUILD_SHARE: OA$FORMATTER_START.COM, as speci�ed in the command �le itself.

14.6.2 After an Upgrade Installation

If you are upgrading from ALL-IN-1 Version 2.3 or ALL-IN-1 STARTER Version 1.0, or updating an ALL-IN-1 STARTER Version 2.4 system, make sure that the ALL-IN-1 environment is established after the system is shut down by replacing the following entries in the VMS system manager’s site startup procedure:

$ @SYS$MANAGER:A1V23START.COM location for ALL-IN-1 V2.3

$ @SYS$MANAGER:A1S010START.COM location for ALL-IN-1 STARTER V1.0

$ @SYS$MANAGER:A1S024START.COM location for ALL-IN-1 STARTER V2.4

Change the entry to:

$ @SYS$MANAGER:A1V24START.COM device:[directory.DATA_SHARE]

where device:[directory.DATA_SHARE] is the location of the ALL-IN-1 Version 2.4 con�guration �le:

device is the device that you speci�ed for the ALL-IN-1 data �les

directory is the top-level directory that you speci�ed for the ALL-IN-1 data �les

The location of A1CONFIG.DAT, is given in the log of the installation. You must include the location as part of the command.

This entry must be entered after the SYS$MANAGER:STARTNET.COM and SYS$MANAGER:MB$CONTROL START=(DDS,TS,...,ER) entries.

If you run A1V24START.COM from the DCL prompt, you need not enter the location. In this case you are prompted for the location as follows:

Enter the location of the file A1CONFIG.DAT:

Enter the location of the ALL-IN-1 Version 2.4 con�guration �le, A1CONFIG.DAT. Refer to the log of the installation for the location of A1CONFIG.DAT. After Installing ALL-IN-1 V2.4 14�5

Note If you are running ALL-IN-1 on a VAXcluster system, you must execute the

ALL-IN-1 startup command procedure on each node in the cluster. Therefore, you must modify the entry in the startup command procedure on each node.

One of the tasks performed by the startup command procedure is to start the mail Sender and Fetcher.

14.6.3 Site-Speci�c Startup Procedures

You must not edit the ALL-IN-1 startup command procedure A1V24START.COM. Instead, you must create your own startup command procedures:

A1V24_SITE_START.COM This is the site-speci�c startup command procedure and must be placed in the OA$SITE_BUILD_SHARE directory. This command procedure is called by A1V24START.COM after all language-speci�c startup command procedures, if any. If you are upgrading from ALL-IN-1 Version 2.3, and you have a sitespeci�c startup command procedure that you want to keep, rename it from A1V23_SITE_START.COM to A1V24_SITE_START.COM (see Section 1.8.18). You may also need to check the command procedure to ensure that it re�ects the con�guration of your ALL-IN-1 Version 2.4 system.

OA$SITE_language_START.COM This is the language-speci�c startup command procedure and must be placed in the directory device:[directory.SITE.SOURCES_language] for the language concerned, where device is the device containing the language �les, and directory is the name of the top-level directory of your ALL-IN-1 Version 2.4 system. If you are running a multilingual ALL-IN-1 system, you can have one of these command procedures for each language installed.

Note You can specify the directory for your default language using the logical

name OA$SITE_BUILD_LLV. If you are upgrading from ALL-IN-1 Version 2.3, you may also need to check the command procedure to ensure that it re�ects the con�guration of your ALL-IN-1 Version 2.4 system.

These command procedures, if present, are executed by the ALL-IN-1 startup command procedure, A1V24START.COM.

14�6 After Installing ALL-IN-1 V2.4

14.6.4 How to Handle Errors Relating to Images Not Installed

On startup, if any error messages are displayed relating to images that are not installed, use the Install Utility to install those images before executing this procedure again. For example:

$ INSTALL
INSTALL> ADD SYS$SHARE:RDBSHR /OPEN /HEAD_RES /SHARED

The images that you must install in this way are those referenced by optional products that you have integrated with the ALL-IN-1 image. Examples are RDBSHR or ACMSHR, which may be referenced by DATATRIEVE and ACMS.

For more details of the Install Utility, see the VMS manual describing the Install Utility.

ALL-IN-1 can now be run with the ALLIN1 command quali�ers as follows:

$ ALLIN1[/qualifier[=argument][/qualifier[=argument]] ...]

There are a number of command-line quali�ers that you can use with the ALLIN1 command. These are described in the ALL-IN-1 Management Guide.

If you have installed an additional language, run ALL-IN-1 using the quali�er /LANGUAGE, where language is the name of the language that you have just installed (see the ALL-IN-1 Installation Guide Part 2 Language Installation for this language).

14.7 Compile and Install the TXLs

A text library (TXL) contains the most frequently used scripts and document templates. The TXL is installed as a VMS global section. This makes access faster and uses memory more ef�ciently. After installing ALL-IN-1, you must compile and install the ALL-IN-1 TXL and site-speci�c TXL.

If you chose to run the IVPs automatically after installation, and the IVPs complete successfully, the ALL-IN-1 TXL (and site-speci�c TXL) is already compiled and installed on the node that you used to install ALL-IN-1. If you installed ALL-IN-1 on a VAXcluster system, you must install the TXLs on the remaining nodes in the cluster.

If you need to compile and install the ALL-IN-1 TXL, do the following:

1 Enter the DCL command:

$ DIRECTORY /SECURITY OA$LIB:A1TXL.TXL

If the �le does not exist carry out steps 2 to 5. Check that the protection of the TXL is set to:

SYSTEM:RWED, OWNER:RWED, GROUP:RE, WORLD:RE

If the protection is not set to this, use the SET FILE /PROTECTION command to change the protection. After Installing ALL-IN-1 V2.4 14�7

2 Log in to the VMS account belonging to the ALL-IN-1 manager.

3 Enter the following commands:

$ ALLIN1 /NOINITIALIZE /LANGUAGE=language
Enter CMD: DO OA$LIB:CM_CTX

where language is the language associated with the TXL to be compiled. The following prompt is displayed:

Do you really want to compile the ALL-IN-1 TXL? [Y/N]?

If you want to compile and install the TXL, enter YES. The following message is subsequently displayed:

ALL-IN-1 TXL compiled and installed.

If you do not want to compile and install the TXL, enter NO.

4 When the script has �nished, enter:

Enter CMD: EXIT

5 Check the protection of the TXL as described in step 1.

If you are upgrading from a customized ALL-IN-1 Version 2.3 system, you need to create a site-speci�c TXL. Compile and install it as follows:

1 Enter the ALL-IN-1 manager’s ALL-IN-1 account:

$ ALLIN1 /USERNAME=MANAGER /LANGUAGE=language

2 Enter MGT to display the ALL-IN-1 Management menu.

3 Press NEXT SCREEN to display the second screen of the Management

menu.

4 Enter CSZ to display the System Customization Management menu.

5 Enter CCM to compile the site-speci�c TXL.

ALL-IN-1 displays the following prompt:

Do you really want to compile the CDS TXL? [Y/N]

Enter YES. The following message is subsequently displayed:

CDS TXL compiled and installed.

6 Exit ALL-IN-1 and set the protection of the site-speci�c TXL,

OA$SITE_LIB_language:CMTXL.TXL, to the following: SYSTEM:RWED OWNER:RWED GROUP:RE WORLD:RE

7 If you want the site-speci�c TXL installed in memory, repeat steps 1 to 5

and then answer Y to both prompts.

14�8 After Installing ALL-IN-1 V2.4

You can use the Trace Utility in one of two ways, as follows:

1 Within ALL-IN-1 press GOLD TRACE. The Trace Flag Argument Form

is displayed. See the Application Programming books for details.

2 Within ALL-IN-1 use the OA$TRA_SET function. See the Application

Programming books for details.

The keys are de�ned in the ALL-IN-1 Management Guide.

14.12 Set the Global Buffers

During the installation of ALL-IN-1 Version 2.4, global buffers are allocated to the data �les shown in Table 14�2:

Table 14�2 Global Buffer Allocations

System File Number of Global Buffers

OA$DATA:PROFILE.DAT n + 1

OA$SHARE:OA$DAF_E.DAT n + 1

OA$DATA:MEETING.DAT 5

OA$DATA:ATTENDEE.DAT n + 1

OA$DATA:PENDING.DAT n + 1

n is the maximum number of users

During the installation of ALL-IN-1 Version 2.4, the number you enter at the prompt "What will be the greatest number of simultaneous ALL-IN-1 users" is used to calculate initial values for these global buffers. If you later increase this value, you should recalculate the global buffers using the table; change them using the DCL command:

$ SET FILE /GLOBAL_BUFFER filename

Note ALL-IN-1 must be shut down �rst.

To save these values permanently edit the appropriate FDL �les for these �les. You may also need to increase values of certain SYSGEN parameters, notably GBLPAGFIL and GBLPAGES. GBLPAGES is calculated as described in Section 1.8.

14�12 After Installing ALL-IN-1 V2.4

14.13 Set the Terminal and Queue Characteristics for

Printers

For most of the supported system printers, you can use the default VMS queue characteristics. However, if you have one or more LQP02, LQP03, or LN03 printers on your system, you must set the terminal and queue characteristics for each of these printers.

Note If you have DECpage on your system, see the DECpage Installation Guide for

the printer settings required for DECpage.

See the ALL-IN-1 Management Guide for details of how to set up the printers.

14.14 Modi�cations Required for VTX

If you have upgraded from ALL-IN-1 Version 2.3 or ALL-IN-1 STARTER Version 1.0, you must change the foreground function for the VTX entry in the Printer Types Master �le as follows:

1 From ALL-IN-1, enter MGT MPR PT. The Manage Printer Types menu is

displayed

2 Press SELECT and enter VTX

3 Enter E to edit the Printer Types Master �le for VTX. The Printer Types

Master form is displayed

4 Move the cursor to the Foreground function �eld and press

ERASE LINE

5 Enter DO VTXOUT

6 Press RETURN to complete the entry

14.15 Replacing the Help Modules for Your Application

If you are upgrading or updating ALL-IN-1, and you had an application that was not created using the Customization Management subsystem, you must now replace the help modules in the appropriate help libraries:

1 Format the module with RUNOFF:

$ RUNOFF module_name

2 Replace both the source text and the formatted text in the appropriate

libraries:

$ LIBRARY/HELP/REPLACE OA$LIB:OAHELP.HLB module_name.MEM

$ LIBRARY/HELP/REPLACE OA$BUILD:HLPSOURCE.HLB module_name.RNO

After Installing ALL-IN-1 V2.4 14�13

14.16 Reschedule the ALL-IN-1 Housekeeping Procedures

If you are performing an upgrade or update installation, you must reschedule your ALL-IN-1 housekeeping procedures. See the the chapter on ALL-IN-1 housekeeping in the ALL-IN-1 Management Guide.

14.17 Changes Required if DECmail No Longer In Use

ALL-IN-1 Version 2.4 does not provide an interface to DECmail. Therefore, if you upgraded from ALL-IN-1 Version 2.3, the DECmail interface is no longer available to your users. Any users that used DECmail may receive error messages when they log in to ALL-IN-1. The error messages will be received if: The �eld MAIL_MENU is set to EMD

The �eld START is set to either EMD or EMD1

To remove this problem, enter the command:

<DO OA$LIB:EMEMD_PROFIL_UPDATE.SCP

This script:

1 Checks each user’s account details and, if the �elds MAIL_MENU and

START are set as described above, changes the �elds to EMC.

2 Checks to see if the �les CNVDMI., MIGRATE.EXE, MIGRATE.COM,

MIGRATE.BAS and MIGRATE.OBJ exist, and if so, deletes them.

14.18 Mail Directory Setup

If you chose to use either the ALL-IN-1 directory (that is, OA$DDS_PRIME equal to 1) or the Mail directory (that is, OA$DDS_PRIME equal to 2) as the primary mail directory, then after installation you have:

A user agent entry name and password. The user agent entry name is OA$node$ALLIN1 for a new or upgrade installation, where node is either the node name or the cluster alias for the system on which you are installing ALL-IN-1. For example, OA$LYNX$ALLIN1. The user agent entry password is the Mail directory password that you entered during the installation (see STEP 23 in Chapter 13).

A subscriber entry for the ALL-IN-1 manager. The proxy attribute of the subscriber entry is the name of the local ALL-IN-1 user agent entry (OA$node$ALLIN1). This attribute gives ALL-IN-1 proxy access to the manager’s entry, so that ALL-IN-1 can update and access the entry.

UAPASSWRD.DAT which contains the name of the user agent object and the user agent password, from the �rst item in this list.

14�14 After Installing ALL-IN-1 V2.4

Before you can use the Mail directory you must perform the actions described in the following steps:

1 If area routing is in use at your site, you need to know the area code

for use at step 3. Run the MAILbus Con�guration Procedure to display the current Transfer Service settings in use at your site. Enter the DCL command:

$ @SYS$MANAGER:MB$CONFIG

To list the current settings of the con�guration parameters, enter:

MBC> SHOW TS

The area code is displayed, along with other settings, as follows:

   .
   .
   .
Transfer Service uses area routing
Area Code : <area_code>
   .
   .
   .

<area_code> is the area code in use at your site. Enter EXIT, or press CTRL/Z, to exit from the MAILbus Con�guration Procedure. For more details of this command, see the Message Router books.

2 Log in to the ALL-IN-1 manager’s ALL-IN-1 account as follows:

$ ALLIN1 /USERNAME=MANAGER

3 Enter the following commands from ALL-IN-1:

<GET #ORGNAME="orgname"
<GET #LOCATION="location"

where:

orgname is the name of your company or organization

location is the location of your users If area routing is in use at your site, you must also enter:

<GET #AREA="area_code"

area_code is the area code (obtained at step 1) for the area that includes your system.

4 Enter the following command:

<DO OA$LIB:USERAGENT_POST After Installing ALL-IN-1 V2.4 14�15

10 To convert your User De�ned Process [.UDP] �les, do the following:

a From the Word and Document Processing menu, enter $.

ALL-IN-1 places you in the subprocess.

b Enter the following command:

$ COPY /LOG [username.WPSPLUS.UDP]*.UDP [.UDP]*.*

where username is the user’s top-level VMS directory, as recorded in the SYS$SYSTEM:SYSUAF.DAT �le.

c When the copying is �nished, press EXIT to return to ALL-IN-1.

Note If you want to use the converted documents when using ALL-IN-1, your default

editor must be WPS-PLUS.

14.21 Determining and Reporting Problems

If you �nd an error in the ALL-IN-1 Version 2.4 books, you should �ll out and submit the Reader’s Comments form at the back of the document in which the error was found. Include the section and page number where the error was found.

If an error occurs while ALL-IN-1 Version 2.4 is being used and you believe that the error is caused by a problem with ALL-IN-1 Version 2.4, take one of the following actions:

Contact your Customer Support Center, if you have a System Support Agreement or are covered by warranty (see your Software Warranty Addendum)

If you think the problem is caused by a software error, you can submit a Software Performance Report (SPR) After Installing ALL-IN-1 V2.4 14�19 A Files on the ALL-IN-1 V2.4 DistributionMedia

This appendix contains a list of the �les on the ALL-IN-1 distribution media.

A.1 Magnetic Tape and TK50 Kits

The ALL-IN-1 �les are supplied on three pieces of media, one for each component of ALL-IN-1 (that is, base, language and market). The media are labeled as follows:

ALL-IN-1 V2.4 BASE BIN media_type INTERNATIONAL BASE (c) 1989 Digital Equipment Corp. This contains save sets A1024.A to A1024.E. A list of the �les in these save sets is given in Section A.3.

ALL-IN-1 V2.4 market BIN media_type MARKET COMPONENT (c) 1989 Digital Equipment Corp. This contains save sets A1Ccode024.A and A1Ccode024.B, where market is the name of your market and code is the market code (up to three characters). A list of the �les in these save sets is given in the ALL-IN-1 Installation Guide Part 3 Market Installation.

ALL-IN-1 V2.4 language BIN media_type LANGUAGE COMPONENT (c) 1989 Digital Equipment Corp. This contains save sets A1Llang024.A to A1Llang024.H, where language is the name of the language and lang is the language code of the language being installed (up to nine characters). A list of the �les in these save sets is given in the ALL-IN-1 Installation Guide Part 2 Language Installation.

Files on the ALL-IN-1 V2.4 Distribution Media A�1

media_type is 16MT9 for tape and TK50 for a TK50 cartridge

Note *.ELE �les are used by the installation procedure to transfer the �les to the

correct place. These �les are removed when the installation is completed.

Each saveset has a unique kit revision identi�er, <revision>. For example, A1024BASEA.REV_A.

A.2 Compact Disk Consolidated Software Distribution Kits

The compact disk (CD) for your market contains directories of the form [A1lang024], where lang is the ALL-IN-1 language available to you. For example, [A1ENGLISH024]. This directory contains two subdirectories; one containing the save sets for the ALL-IN-1 Version 2.4 kit, the other containing various documentation (in ASCII text format).

All the save sets required to install the base, language, and market components for your kit are in the directory [A1lang024.KIT]. The documentation is in the directory [A1lang024.LINE_DOCS].

The save sets of the base component are:

A1024.A A1024.B A1024.C A1024.D A1024.E

A list of the �les in these save sets is given in Section A.3.

The save sets of the language component are:

A1Llang024.A A1Llang024.B A1Llang024.C A1Llang024.D A1Llang024.E A1Llang024.F A1Llang024.G A1Llang024.H A1LRlang024.A (Release Notes Part 1 Language)

A list of the �les in these save sets is given in the ALL-IN-1 Installation Guide Part 2 Language Installation.

A list of the �les in these save sets is given in Section A.3.

The save sets of the market component are:

A1Cmarket024.A A1Cmarket024.B

A�2 Files on the ALL-IN-1 V2.4 Distribution Media

A1CRmarket024.A (Release Notes Part 2 Market)

A list of the �les in these save sets is given in the ALL-IN-1 Installation Guide Part 3 Market Installation.

This directory also contains the following:

VAX Forms Management System (FMS) Version 2.4

FMS024.A FMS024.B

Message Router Version 3.1

MR031.A MR031.B

Message Router VMSmail Gateway Version 3.1

MRGATE031.A MRGATE031.B

Compound Document Architecture Converter Library Version 1.0

CDACVTLIB010.A CDACVTLIB010.B

The documentation directory contains the following:

The ALL-IN-1 Installation Guide:

A1024_INSTALL_GUIDE.TXT A1Llang024_INSTALL_GUIDE.TXT A1Cmarket024_INSTALL_GUIDE.TXT

The Read Me First:

A1024_READ_ME_FIRST.TXTFiles on the ALL-IN-1 V2.4 Distribution Media A�3

MUA_MOVEDISK_INTER.COM;1 MUA_NOMINATE.COM;1
MUA_NOMINATE_INTER.COM;1 MUA_PAT.COM;1
MUA_PAT_ARCHIVE.SCP;1 MUA_PAT_FIND_ACCOUNT.SCP;1
MUA_PAT_INTER.COM;1 MUA_PAT_SELECT_FILE.FDL;1
MUA_REMOVE_ADMIN.COM;1 MUA_REMOVE_ADMIN_INTER.COM;1
MUA_RENAME.COM;1 MUA_RENAME_INTER.COM;1
MUA_RENAME_PENDING.EXE;1 MUA_SAVE_UNREAD_MAIL.SCP;1
MUA_SWITCH_APP_PRV.COM;1 MUA_TRANSFER.FDL;1
MUA_UTILITY.FDL;1 MUA_VMS_CHK.SCP;1 MUA_XFER_DOCLIST.FDL;1
NAME_CONVERT.COM;1 NETWORK.FDL;1 NETWORKB.BLP;1
NEWDOCDB.COM;1 NEXTLIST.SCP;1 NICKNAMES.FDL;1
OA$APPL_INTMENU.SCP;1 OA$APPL_SPMENU.SCP;1
OA$FORMATTER_START.COM;1 OA$PRINTERS.FDL;1
OA$PRINTERTYPES.FDL;1 OA$SAM_BALANCE_SHARED_DIRS.EXE;1
OA$SAM_BALANCE_USERS.EXE;1 OA$SAM_CHECK_MAIL_AREA_DELETE.EXE;1
OA$SHARE_DEVICE_MASTER.FDL;1 OA$SM_FCVR.EXE;1
OA$SM_FCVR_PRE_PHASE1.EXE;1 OA$SM_RECOG_MAIL_AREA.SCP;1
OA$SUBMIT.OBJ;1 OACMSV.OBJ;1 OADDIF_DIRCHK.COM;1
OADDIF_INSTALL.SCP;1 OAFCV.EXE;1
OAFORMATTER.OBJ;1 OAFORMATTERX.OBJ;1 OAINI.COM;1
OALNM.COM;1 OASHRBLD.EXE;1 OASYMMSG.MAR;1
PARANUM.SCP;1 PDAF.FDL;1 PENDING.FDL;1
PERPHONE.FDL;1 PFCONTROL.SCP;1 PFCREATE.SCP;1
PFSQ.COM;1 PFVMPRINT.COM;1 PHALLB.BLP;1
PHPERB.BLP;1 POSTMASTE.A1CAL;1 POSTMASTE.PST;1
PRINTER_TYPESB.BLP;1 PRINT_DDIF.COM;1
PRINT_PS.SCP;1 PROFILE.FDL;1 PROFILE_PRINT.FDL;1
PROVIDE_DATA_CBI_FILES.SCP;1 PROVIDE_DATA_FILES.SCP;1
PROVIDE_DATA_FILES_2.SCP;1 PROVIDE_DATA_LLV_FILES.SCP;1
PROVIDE_DATA_WPS_FILES.SCP;1 PTU.EXE;1
QUOTA.COM;1 QUOTA.EXE;1 QUOTA_CHECK.COM;1
REMOVEND.EXE;1 RENAME.FDL;1 REORDER.COM;1
RMSANLZ.COM;1 SA_CHANGE_PASSWORDS.SCP;1
SA_DELETE_ACCOUNT.SCP;1 SA_MULT_DELETE_ACCOUNT.SCP;1
SA_PREPARE_MAS_NETWORK.COM;1 SA_PREPARE_MAS_TAPE.COM;1
SA_PROFILEB.BLP;1 SDAF.FDL;1 SELECTIONLIST.BLP;1
SELECTIONLIST1.BLP;1 SELECTIONLIST_RFA.BLP;1
SENDCHECK.EXE;1 SHARED_DOC.BLP;1 SITE_PRINTERSB.BLP;1
SM$SHARE$SCROLL$PREPOP.SCP;1 SMA1.EXE;1
SMBKUSER.COM;1 SMJACKET.SCP;1 SMNETINIT.COM;1
SMNETINIT.SCP;1 SMNETPRGE.COM;1 SMNETPRGE.EXE;1
SMNETUPDT.EXE;1 SMNETUPDT.SCP;1 SMONOFF.COM;1
SMREORG.SCP;1 SMREORG_DEPT.SCP;1 SMSREORG.COM;1
SMTRLU.SCP;1 SMUNSHARE.SCP;1 SM_CHANGE_PASSWORDS.SCP;1
SM_DELETE_ACCOUNT.SCP;1 SM_MULT_DELETE_ACCOUNT.SCP;1
SM_PAT_VALIDATE_NODE.COM;1 SM_PAT_VALIDATE_TAPE.COM;1
SM_PLM_AVAIL.SCP;1 SM_PLM_COUNT.SCP;1 SM_POLICIES_PREPOP.SCP;1
SM_PREPARE_MAS_NETWORK.COM;1 SM_PREPARE_MAS_TAPE.COM;1
SM_RESTART.COM;1 SM_RESTART_INTER.COM;1
SM_SKEDSCRIPT_DEFAULT.SCP;1 SM_TPL_CLEAR_SYMBOLS.SCP;1
SM_TPL_GLOBAL_EDIT.SCP;1 SM_USED_UIC.FDL;1
SPECIAL.COM;1 SPELL.CLD;1 SPFILE.SCP;1
SPNULL.TXT;1 SPSEND.SCP;1 START_TM_SERVER.COM;1
SUBSCRIBER.SCP;1 SUBSCRIBER_ADD.SCP;1
SUBSCRIBER_ADD_INTERACTIVE.SCP;1 SUBSCRIBER_CHANGE.SCP;1

Files on the ALL-IN-1 V2.4 Distribution Media A�7

SUBSCRIBER_CHANGE_INTERACTIVE.SCP;1 SUBSCRIBER_DELETE.SCP;1
SYMBOLS.PST;1 TAG.COM;1 TAG.EXE;1
TEMPLATE_PRINT.FDL;1 TIME_DIFF.EXE;1
TM.SCP;1 TMAA.SCP;1 TMAIC.SCP;1
TMAISEL.SCP;1 TMAPC.SCP;1 TMAPD.SCP;1
TMAPE.SCP;1 TMAPMEC.SCP;1 TMAPMECSCAN.SCP;1
TMAPMED.SCP;1 TMAPMEE.SCP;1 TMAPMEP.SCP;1
TMAPMER.SCP;1 TMAPMESEL.SCP;1 TMAPSEL.SCP;1
TMCREREM.SCP;1 TMCRETD.SCP;1 TMDAYSCH.SCP;1
TMEDIT.SCP;1 TMEV.SCP;1 TMEVSEL_RECOG.SCP;1
TMEV_TIMEVAL.SCP;1 TMINITFORM.SCP;1 TMINIT_GET.SCP;1
TMJOUD.SCP;1 TMJOUE.SCP;1 TMMDCAL.SCP;1
TMMEC.SCP;1 TMMED.SCP;1 TMMEDUI.SCP;1
TMMEE.SCP;1 TMMENU.SCP;1 TMMENU_VALID.SCP;1
TMMERA.SCP;1 TMMESEL.SCP;1 TMMESTRIP.SCP;1
TMMONTH3.SCP;1 TMNEXT.SCP;1 TMPRINT.SCP;1
TMRA.SCP;1 TMRA_VALID.SCP;1 TMREPRINT.SCP;1
TMRESEL.SCP;1 TMRFA.SCP;1 TMRFA_RECOG.SCP;1
TMRFA_VALID.SCP;1 TMSCAN.SCP;1 TMSCAN_DATEVAL.SCP;1
TMSCAN_DURATION.SCP;1 TMSET_CONTEXT.SCP;1
TMSEVC.SCP;1 TMSEVD.SCP;1 TMSEVE.SCP;1
TMSEVI.SCP;1 TMSEVP.SCP;1 TMSEVR.SCP;1
TMSEVXD.SCP;1 TMSEVXP_METER.SCP;1 TMSEVXR.SCP;1
TMSEV_APSYM.SCP;1 TMSEV_ATTSYM.SCP;1 TMSEV_CLEANSYM.SCP;1
TMSEV_MESYM.SCP;1 TMSRE.SCP;1 TMSREPOST.SCP;1
TMSTC.SCP;1 TMSTCL.SCP;1 TMSTD.SCP;1
TMSTE.SCP;1 TMSTI.SCP;1 TMSTP.SCP;1
TMSTR.SCP;1 TMSTXCL.SCP;1 TMSTXD.SCP;1
TMSTXP_METER.SCP;1 TMTASKCRE.SCP;1 TMTCL.SCP;1
TMTD.SCP;1 TMTDDEL.SCP;1 TMTE.SCP;1
TMTMSDOWN.SCP;1 TMTMSPRE.SCP;1 TMTMXTPRE.SCP;1
TMTP.SCP;1 TMTR.SCP;1 TMTSEL.SCP;1
TMXSELAPR.SCP;1 TM_CAM_NONO.SCP;1 TM_FLAG.SCP;1
TM_LIST.SCP;1 TM_REPLY.SCP;1 TM_SETOWN.SCP;1
TM_TWOCAL.SCP;1 TRACESET.SCP;1 TRIM.CLD;1
TRIM.EXE;1 UDP_SCRIPT.SCP;1 USER.FLB;1
USERAGENT_POST.SCP;1 V.COM;1
VAXMAIL.COM;1 VMNXTLIST.SCP;1 VMSMAIL.COM;1
VTX.SCP;1 VTXOUT.SCP;1 WEEK_DAYS.SCP;1
WPCOPYCAB.BLP;1 WPCOPYDX.BLP;1 X400COUNTRY_CODES.FDL;1
XPORTMSG.EXE;1

Total of 521 files.

A�8 Files on the ALL-IN-1 V2.4 Distribution Media

Save Set: A1024.C

A1024BASEC.REV_<revision>;1 ACMSA1MSG.MSG;1
DIRBASEC.ELE;1 FINDFILE.OBJ;1 IMAGEID.OPT;1
OA$CNV_TIMEZONE_CONVERT.SCP;1 OA$SM_CHECK_CLUSTER.COM;1
OA$SM_DEFINE_SHARED_LOGICALS.COM;1 OA$SM_DEFINE_SHARED_LOGICALS.SCP;1
OA$SM_FCVR_PRE_PHASE1_SCHEDULE.COM;1 OA$SM_FCVR_PRE_PHASE1_SCHEDULE.SCP;1
OA$SM_FCVR_SCHEDULE.COM;1 OA$SM_FCVR_SLAVE1.COM;1
OA$SM_FIELD_OFFSETS.COM;1 OA$SM_SAM_BA_SCHEDULE.COM;1
OA$SM_SAM_BSD_SCHEDULE.COM;1 OA$SM_SAM_SCHEDULE.SCP;1
OA$SM_SET_WRITE_WINDOW.COM;1 OA$SM_SHARED_DAF_MASTER.SCP;1
OA$SM_UTILITY_MASTER.FDL;1 OA$SM_UTIL_SCHEDULE.FDL;1
OA$SM_WRITE_DIR_MASTER_INSTALL.SCP;1 OA.BLI;1
OAET.MAR;1 OAGBL.BLI;1 OALIBR.OLB;1
OAMAC.REQ;1 OASDF.BLI;1 SCPTABLE.TXT;1
SYSTEM_PST.COM;1 SYSTEM_PST.FDL;1 WPDELETE.SCP;1
WPDOUDP.SCP;1 WPDUMPUDP.SCP;1 WPEDADDMEN.SCP;1
WPEDIT.SCP;1 WPFCFDROP.SCP;1 WPFCFOLD.SCP;1
WPFOLDER.SCP;1 WPLIST.SCP;1 WPMDMP.SCP;1
WPNEXTL.SCP;1 WPNEXTNUM.SCP;1 WPPAFOLDER.SCP;1
WPPALTERN.SCP;1 WPPBGFORMAT.SCP;1 WPPFILE.SCP;1
WPPOUTDOC.SCP;1 WPPPORT.SCP;1 WPPRINT.SCP;1
WPPSCRPD.SCP;1 WPPSYSTEM.SCP;1 WPPTERMIN.SCP;1
WPPTYPEIT.SCP;1 WPSLPS.SCP;1 WPSMAIL.COM;1
WPSTSTSPC.SCP;1 X400.CMU;1

Total of 58 files.

Save Set: A1024.D

A1024BASED.REV_<revision>;1 ACMSALLIN1.OLB;1
DIRBASED.ELE;1 DMPLUS.OLB;1 DXLIB.OLB;1
KOAVMS.OLB;1 KOFORM.OLB;1 MRMIS.OLB;1
MRVMS.OLB;1 MRVMS4.OLB;1 MTILIB.OLB;1
OATALKLIB.OLB;1 OAVOICE.OLB;1 SIL.OLB;1
TMSERVER.OLB;1 WPADOC.OLB;1 WPADSA.OLB;1
WPAPRINT.OLB;1 WPARVMS.OLB;1 XPORT.L32;1
XPORT.OLB;1 XPORT.REQ;1

Total of 22 files.

Save Set: A1024.E

A1024BASEE.REV_<revision>;1 DIRBASEE.ELE;1
LNGOSENVR.EXE;1 LNGSPLCOM.EXE;1 LNGSPLCRE.SCP;1
LNGSPLCSY.SCP;1 LNGSPLFMT.SCP;1 LNGSPLFOR.EXE;1
LNGSPLIST.SCP;1 LNGSPLMNU.SCP;1 LNGSPLMSG.EXE;1
LNGSPLSC2.SCP;1 LNGSPLSEL.SCP;1 LNGSPLSHR.EXE;1
LOADTCS.TXT;1 PTU.OBJ;1 PTULIB.OLB;1
SPLMSGREF.OBJ;1 WPABASE.OLB;1 WPAEDIT.OLB;1
WPALIPS.OLB;1 WPAPECO.OLB;1 WPASORT.OLB;1
WPCOPY.SCP;1 WPDECDX.COM;1 WPPRTEXIT.SCP;1
WPPRUNOFF.COM;1 WPPSPEC.COM;1 WPSDECGET.SCP;1
WPSDECWRT.SCP;1 WPSDEF.WPL;1 WPSFNATT.SCP;1
WPSFNPOS.SCP;1 WPSFNSEPS.SCP;1 Files on the ALL-IN-1 V2.4 Distribution Media A�9

                    Total of 34 files.

A�10 Files on the ALL-IN-1 V2.4 Distribution Media

        If you answer YES to this then you will produce TWO images -
   OA$MAIN.EXE and OALLVlanguage.EXE. This will allow more than one
   image to be installed.

* Do you want to build a MULTI-LANGUAGE system [NO]? NO
%A1LENGLISH-I-NOMLLINK, ALL-IN-1 will be linked as a single language system

   ALL-IN-1 allows you to select a default date format for each language
   you have installed. This will become the default ALL-IN-1 date format
   for each user (on a per language basis). This may be changed by user
   through the Set Working Conditions option.

            Alphanumeric Date Numeric Date

        1 DD-MMM-YYYY MM/DD/YY (Standard Default)
        2 DD-MMM-YYYY DD/MM/YY
        3 DD-MMM-YYYY YY/MM/DD
        4 YYYY-MMM-DD MM/DD/YY
        5 YYYY-MMM-DD DD/MM/YY
        6 YYYY-MMM-DD YY/MM/DD

* Which date format do you require [1]: 1
%A1LENGLISH-I-DATEFORMAT, Date format DD-MMM-YYYY and MM/DD/YY (1) has been
selected

* What will be the greatest number of simultaneous ALL-IN-1 users: 5
* Which batch queue would you like to use for sending/receiving mail
[SYS$BATCH]: SYS$BATCH
* Do you want to use Message Router to send/receive messages to/from other
systems [NO]? YES

* Do you want to use a Message Router on another node [NO]? NO
* What level of Mail directory support do you want [0/1/2] [0]: 1

* Enter password for the Mail directory user agent account: A1MAIL

* Please confirm the Mail directory password specified: A1MAIL

* What password do you want to use for the ALL-IN-1 Message Router mailbox:
LYNX_A1

* Please confirm the password you have specified: LYNX_A1

* Do you want to translate outgoing WPS-PLUS and DX messages to ASCII [NO]?
NO

%A1LENGLISH-I-CHKSWPR, Checking MANDATORY and OPTIONAL SW prerequisites

%A1LENGLISH-I-CHKQUOT, Checking process quotas for the current process
%A1LENGLISH-I-CHKIDNT, Checking ALL-IN-1 general identifiers
%A1LENGLISH-I-CHKTRAC, Checking ALL-IN-1 transfer accounts
%A1LENGLISH-I-CHKVMSV, Checking VAX/VMS version
%A1LENGLISH-I-CHKLIBS, Checking required shareable libraries are installed
%A1LENGLISH-I-CHKFMSV, Checking VAX/FMS version
%A1LENGLISH-I-CHKMROV, Checking Message Router version
%A1LENGLISH-I-CHKPARA, Checking system parameters

B�4 Sample Installations

        All software checks have been successful.
        Installation will continue.

%A1LENGLISH-I-CHKDISK, Checking DISK SPACE

* Which device will hold the ALL-IN-1 shared library files [SYS$SYSDEVICE:]:
SYS$SYSDEVICE
* Which device will hold the ALL-IN-1 shared data files [SYS$SYSDEVICE:]:
SYS$SYSDEVICE
* Which device will hold the ALL-IN-1 ENGLISH language files
[SYS$SYSDEVICE:]: SYS$SYSDEVICE
* Which device will hold the ALL-IN-1 mail area SDAF file [SYS$SYSDEVICE:]:
SYS$SYSDEVICE
* How many shared directories do you want to create [1]: 3
* Which device will hold the ALL-IN-1 shared directory SHARE1
[SYS$SYSDEVICE:]: SYS$SYSDEVICE
* Which device will hold the ALL-IN-1 shared directory SHARE2
[SYS$SYSDEVICE:]: SYS$SYSDEVICE
* Which device will hold the ALL-IN-1 shared directory SHARE3
[SYS$SYSDEVICE:]: SYS$SYSDEVICE

        NO missing DISK SPACE prerequisites discovered.
        The installation will continue.

* What VMS username do you want to use for ALL-IN-1 manager’s account
[ALLIN1]: ALLIN1

* What password do you want to use for this account: LYNX_SAMPLE

* Please confirm the password you have specified: LYNX_SAMPLE

* What UIC do you want to use for account ALLIN1: 1,100
* What default device you want to use for ALL-IN-1 manager’s account
[SYS$SYSDEVICE:]: SYS$SYSDEVICE
* What default directory do you want to use for ALL-IN-1 manager’s account?
[ALLIN1]: ALLIN1

A DISKQUOTA entry will be added for UIC [1,100] on SYS$SYSDEVICE:.
The DISKQUOTA entry has been added, with a PERMANENT quota of 10000
and an OVERDRAFT quota of 1000.

A DISKQUOTA entry on SYS$SYSDEVICE: for UIC [1,100] will now be modified.
The DISKQUOTA entry has been modified to: PERMANENT quota of 62500
and OVERDRAFT quota of 5000.
%VMSINSTAL-I-SYSDISK, This product creates system disk directory
SYS$SYSDEVICE:[ALLIN1].
%VMSINSTAL-I-ACCOUNT, This installation creates an account named ALLIN1.
%UAF-I-ADDMSG, user record successfully added
%UAF-I-RDBADDMSGU, identifier ALLIN1 value: [000001,000100] added to
RIGHTSLIST.DAT
%VMSINSTAL-I-ACCOUNT, This installation updates an account named ALLIN1.
%UAF-I-MDFYMSG, user record(s) updated

* What UIC do you want for the A1$XFER_IN account?: [500,1]
* What UIC do you want for the A1$XFER_OUT account?: [500,2]

%VMSINSTAL-I-ACCOUNT, This installation creates an ACCOUNT named A1$XFER_IN.
%UAF-I-ADDMSG, user record successfully added Sample Installations B�5

                    %UAF-I-RDBADDMSGU, identifier A1$XFER_IN value [00500,000001] added to
                        RIGHTSLIST

                    A DISKQUOTA entry will be added for UIC [500,1] on SYS$SYSDEVICE:.
                    The DISKQUOTA entry has been added, with a PERMANENT quota of 50000
                    and an OVERDRAFT quota of 5000

                    %VMSINSTAL-I-ACCOUNT, This installation creates an ACCOUNT named
                        A1$XFER_OUT.
                    %UAF-I-ADDMSG, user record successfully added

                    %UAF-I-RDBADDMSGU, identifier A1$XFER_OUT value [00500,000002] added to
                        RIGHTSLIST

                    A DISKQUOTA entry will be added for UIC [500,2] on SYS$SYSDEVICE:.
                    The DISKQUOTA entry has been added, with a PERMANENT quota of 50000
                    and an OVERDRAFT quota of 5000

                    %A1LENGLISH-I-CREATID, Create ALL-IN-1 RIGHTS identifiers ...

                    A DISKQUOTA entry will be added for UIC OA$PRVAPP on SYS$SYSDEVICE:.
                    The DISKQUOTA entry has been added, with a PERMANENT quota of 1000
                    and an OVERDRAFT quota of 1000.

                    A DISKQUOTA entry on SYS$SYSDEVICE: for UIC OA$PRVAPP will now be modified.
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 1000
                    and OVERDRAFT quota of 1000.
                    %A1LENGLISH-I-GRANTID, Grant ALL-IN-1 general identifiers to UIC [1,100] ...

                    * Enter ALL-IN-1 top-level directory required for the shared library files
                    [ALLIN1]: ALLIN1
                    * Enter ALL-IN-1 top-level directory required for the shared data files
                    [ALLIN1]: ALLIN1
                    * Enter ALL-IN-1 top-level directory required for all ENGLISH language files
                    [ALLIN1]: ALLIN1
                    * Enter ALL-IN-1 top-level directory required for the mail area SDAF file
                    [ALLIN1]: ALLIN1
                    * What directory will hold the shares directories on SYS$SYSDEVICE:
                    [ALLIN1]: ALLIN1
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.MSG].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.UDP].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC0].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC1].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC2].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC3].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC4].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory

B�6 Sample Installations

                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC5].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC6].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC7].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC8].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.MGR.DOC9].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.MSG].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.UDP].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC0].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC1].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC2].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC3].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC4].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC5].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC6].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC7].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC8].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.POSTMASTE.DOC9].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.MSG].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.UDP].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC0].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC1].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC2].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC3].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC4].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1.IVPUSER.DOC5].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directorySample Installations B�7

                SYSTEM finished using ALL-IN-1 at 8-Dec-1989 11:40

%OA-I-LASTLINE, "ALL-IN-1 running -- compiling form libraries..."
%OA-I-LASTLINE, "ALL-IN-1 running -- compiling OAFORM..."
%OA-I-LASTLINE, "ALL-IN-1 running -- compiling MEMRES..."
%OA-I-LASTLINE, "ALL-IN-1 running -- compiling SITEOAFORM..."
%OA-I-LASTLINE, "ALL-IN-1 running -- compiling SITEMEMRES..."
%OA-I-LASTLINE, "ALL-IN-1 running -- form libraries compiled"
%OA-I-LASTLINE, "ALL-IN-1 running -- data file and form processing complete"

                SYSTEM finished using ALL-IN-1 at 8-Dec-1989 11:44

%A1-I-SETACL, Setting ACL’s
%A1-I-SETACL, Setting global buffers

The installation procedure for ALL-IN-1 V2.4 has now completed
%VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
    directories...

    The IVP for ALL-IN-1 V2.4 takes about 30 minutes to run. This will
 vary according to the system that it is running on.

       It will first of all run SYS$MANAGER:A1V24START to initialise
 ALL-IN-1 logical names and to install the various images required. It
 also will clear the VMS account name associated with the ALL-IN-1 IVP
 account. Should the IVPs fail to reset the VMS username in the PROFILE,
 then please reset it to the same as the MANAGER vms username as soon as
 possible, by doing the following:

   $ALLIN1/NOINIT
   Enter CMD: WRITE CHANGE PROFIL USER="IVP",VMSUSR="ALLIN1"

    If the IVPs fail then please investigate the log files found in
 OA$IVP. There is an additional log file in SYS$MANAGER called
 ALLIN1IVP.LOG containing the messages from running ALL-IN-1 IVPs.
 This may sometimes prove useful, for instance if ALL-IN-1 fails to
 run, it can be seen in this file. To run the IVPs again type:

   $SET PROC/PRIV=(NOBYPASS,ALL)
   $ALLIN1/USER=IVP

    Use the various options on the menu that is presented to run parts
 of the IVP or all of it. The "ALL" option is what is run during the
 installation phase IVPs. See the System Management Guide for more
 details.

   As an aid to finding problems then please read IVPHINTS.MEM in
 OA$IVP:

%A1IVP-I-IVPSTART,Running startup for ALL-IN-1 . Sample Installations B�11

                            Starting ALL-IN-1
                            Installing ALL-IN-1 images
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<SYS0.SYSCOMMON.SYSLIB>LNGSPLCOM.EXE
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<SYS0.SYSCOMMON.SYSLIB>LNGOSENVR.EXE
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<ALLIN1.LIB_SHARE>MAILCOUNT.EXE
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<ALLIN1.LIB_SHARE>OA$MAIN.EXE
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<ALLIN1.LIB_SHARE>OA$SUBMIT.EXE
                            Defining language independent logical names
                            Defining ENGLISH language logical names
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<SYS0.SYSCOMMON.SYSLIB>OA$LLVENGLISH.EXE
                    %INSTALL-W-NOPREV, no previous entry exists - new entry created for
                    SYS$SYSDEVICE:<SYS0.SYSCOMMON.SYSLIB>LNGSPLENG.EXE

                            Running ALL-IN-1 to install the ENGLISH FORM LIBRARIES

                    %OA-I-LASTLINE, "" ALL-IN-1 is RUNNING""

                            Running ALL-IN-1 to define SHARED AREA logicals

                    %OA-I-LASTLINE, "" ALL-IN-1 is RUNNING""

                            Starting the TM SERVER
                            Starting OA$FCV
                            Starting the MAIL Sender and Fetcher
                            ALL-IN-1 startup procedure completed

                    %A1IVP-I-IVPFINISH,Finished running startup for ALL-IN-1 .
                    %A1IVP-I-IVPSTART,Running IVPs for ALL-IN-1 .

                    %A1IVP-I-IVPFINISH,The IVPs for ALL-IN-1 have finished .

                    Log File for ALL option
                    -----------------------
                    ! Starting verification of interface with VMS.
                    !
                    ! Starting verification of form library compilation.
                    ! Checksum of FLC should be (6D4C620C).
                    ! Test of form library compilation has passed.
                    ! IVP checksum of form library = 6D4C620C.
                    ! Finished verifying form library compilation.
                    !
                    ! Starting verification of CLI interface.
                    ! CLI symbol ivpclistatus = ALL-IN-1 V2.4.
                    ! verification of CLI interface has passed.
                    ! Finished verifying CLI interface.
                    !
                    ! Verification of interface with VMS has PASSED.
                    !
                    ! Verification of interface with VMS has finished.

B�12 Sample Installations

%OAIVP-I-PASSED, File check for ALL-IN-1 has passed. Sample Installations B�13

                    0 ! "Running editor check"
                    23 ! "EDT/WPS test."
                    252 ! " first address line check"
                    258 ! " second address line check"
                    265 ! " third address line check"
                    270 ! " fourth address line check"
                    275 ! " date check"
                    282 ! " day check"
                    286 ! " ALL-IN-1 username check"
                    289 ! " job title check"
                    293 ! "EDT/WPS check PASSED."
                    498 ! "WPS-PLUS check starting."
                    935 ! "WPS-PLUS check finished."
                    ! Merged list checksum is 805719118
                    ! Correct checksum is 805719118
                    951 ! "WPS-PLUS check PASSED"
                    955 ! "Editor check PASSED."
                    960 ! "Editor check finished."

B�14 Sample Installations

                                                      OA Sales Department,
                                                  Digital Equip. Corp.,
                                                    DECpark,
                                                     Worton Grange,
                                                            Reading,Berks.
                                                  (0734) 868711
Susie Coggles,
Art Equipment Ltd,
69 London Rd,
Reading.
(0734) 696969.
Dear Susie,
  As a user of ALL-IN-1 V2.1/BEV on your VAX/VMS 8650, you may be interested
  to know that Digital’s OA engineering group has just announced the
  availability of ALL-IN-1 V2.3 - a huge step forward for the future of
  office automation. It’s many *NEW* features include multiple select
  options for the File Cabinet, forward and backward scrolling on Read,
  as well as the capacity for multiple languages. All this together with
  the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
  1989.
        Phone NOW for a demonstration - on (0734) 868711
   Yours faithfully,
        Alain M. Cleaner,
           Office Products Manager.

B�18 Sample Installations

                                                      OA Sales Department,
                                                  Digital Equip. Corp.,
                                                    DECpark,
                                                     Worton Grange,
                                                            Reading,Berks.
                                                  (0734) 868711
Jenny Dagleish,
Art Equipment Ltd,
31 Reading Gardens,
Reading.
(0734) 251017.
Dear Jenny,
  As a user of ALL-IN-1 V2.2 on your VaxStation 2000, you may be interested
  to know that Digital’s OA engineering group has just announced the
  availability of ALL-IN-1 V2.3 - a huge step forward for the future of
  office automation. It’s many *NEW* features include multiple select
  options for the File Cabinet, forward and backward scrolling on Read,
  as well as the capacity for multiple languages. All this together with
  the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
  1989.
        Phone NOW for a demonstration - on (0734) 868711
   Yours faithfully,
        Alain M. Cleaner,
           Office Products Manager. Sample Installations B�19

                                                                         OA Sales Department,
                                                                      Digital Equip. Corp.,
                                                                        DECpark,
                                                                         Worton Grange,
                                                                               Reading,Berks.
                                                                      (0734) 868711
                    Ruth Calladine ,
                    Nutters Catering Compnay,
                    73 Watlington Street,
                    Reading.
                    (0734) 956435.
                    Dear Ruth,
                      As a user of ALL-IN-1 V2.1/BEV on your VaxStation/GPX, you may be
                        interested
                      to know that Digital’s OA engineering group has just announced the
                      availability of ALL-IN-1 V2.3 - a huge step forward for the future of
                      office automation. It’s many *NEW* features include multiple select
                      options for the File Cabinet, forward and backward scrolling on Read,
                      as well as the capacity for multiple languages. All this together with
                      the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
                      1989.
                            Phone NOW for a demonstration - on (0734) 868711)
                       Yours faithfully,
                            Alain M. Cleaner,
                               Office Products Manager.

B�20 Sample Installations

                    %OAIVP-I-INST, SYS$SYSDEVICE:[ALLIN1.LIB_SHARE]OA$MAIN.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$SYSDEVICE:[ALLIN1.LIB_SHARE]OA$SUBMIT.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSEXE]OA$FORMATTER.EXE;25 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]FDVMSG.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]DPEMSG.EXE;17 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]XPORTMSG.EXE;74 is installed.

                    %OAIVP-I-PASSED, Message check for ALL-IN-1 has passed.

                    LOG OF THE VERIFICATION OF ALL-IN-1 MESSAGES:
                    ---------------------------------------------

                    This should contain the string V2.4...

                    Enter CMD: VERSION
                    %OA-I-VERSION, ALL-IN-1 Version 2.4 8-Dec-1989

                     This should produce an Informational level message,
                     and an RMS-E-FNF error

                    Enter CMD: OA$FLO_OPEN THIS_IS_A_TEST
                    %OA-I-LNF, Error opening form library "THIS_IS_A_TEST"
                    -RMS-E-FNF, file not found
                    %OA-I-LNF, Error opening form library "THIS_IS_A_TEST"
                    -RMS-E-FNF, file not found

                     This should produce a Warning level message...

                    Enter CMD: OA$SYM_GET_SYMBOL THIS_IS_A_TEST
                    %OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

                     This should produce a Error level message...

                    Enter CMD: OA$FBT_WRITE_LIBRARY THIS_IS_A.TEST
                    %OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form library

                     FATAL level error messages cause the image to stop,
                      so they are not tested. Sample Installations B�21

* Type YES when correct media mounted, NO to terminate installation? YES

%MOUNT-I-MOUNTED, A13024 mounted on _LYNX$TAPE0:
%A1LENGLISH-I-RELANK, Restoring the LANGUAGE kit savesets.
%VMSINSTAL-I-RESTORE, Restoring product saveset B...

   This is the ENGLISH version of ALL-IN-1 V2.4

* Does this product have an authorization key registered and loaded [YES]?
YES
%LMF-I-GOTLICENSE, An ALLIN1 license is installed and loaded
%LMF-I-CHKSWLIC, Checking licenses for prerequisite software
%LMF-I-CONFLICENSE, All necessary licenses are installed and loaded

* Do you want to purge files replaced by this installation? YES

If DATATRIEVE is only occasionally used within ALL-IN-1 it is suggested that
you answer NO to the next question. You will still be able to use DATATRIEVE
within ALL-IN-1, but you will avoid the overhead of having it physically
linked with the ALL-IN-1 image. If you need to use a DATATRIEVE image other
than SYS$SHARE:DTRSHR.EXE then you MUST answer YES to the following
    question.

* Do you want to incorporate DATATRIEVE [NO]? NO
%A1LENGLISH-I-DTRNOLINK, DATATRIEVE will not be linked with ALL-IN-1

        If you wish to have the WPS-PLUS editor available then answer YES
        to the following question. If you answer NO, then your users will
        not be able to access the WPS-PLUS editor. Note this will also
        impact SPELL and MERGE functions.

   NOTE: You will be able to link WPS-PLUS in at a later time, should you
   choose not to link it now.

* Do you want to incorporate WPS-PLUS [YES]? YES
%A1LENGLISH-I-WPSLINK, The WPS-PLUS editor will be linked with ALL-IN-1

   If you wish to interface with ACMS, then answer YES to the following
   questions.

   NOTE:

        o ACMS needs to be installed before ALL-IN-1.

        o If the user answers yes and the relavent ACMS files are
          present then the interface will get built. If they are not
          then the default is to abort the link, in order to remedy it.

* Do you want to incorporate ACMS [NO]? YES
%A1LENGLISH-I-ACMSLINK, ACMS will be linked with ALL-IN-1

%A1LENGLISH-I-DDIF, Checking CDA support software prerequisites
%A1LENGLISH-I-DDIF, CDA integration will be supported

        If you answer YES to this then you will produce TWO images -
   OA$MAIN.EXE and OALLVlanguage.EXE. This will allow more than one
   image to be installed.

* Do you want to build a MULTI-LANGUAGE system [NO]? YES
%A1LENGLISH-I-MLLINK, ALL-IN-1 will be linked as a multi-language system

Sample Installations B�25

   ALL-IN-1 allows you to select a default date format for each language
   you have installed. This will become the default ALL-IN-1 date format
   for each user (on a per language basis). This may be changed by user
   through the Set Working Conditions option.

            Alphanumeric Date Numeric Date

        1 DD-MMM-YYYY MM/DD/YY (Standard Default)
        2 DD-MMM-YYYY DD/MM/YY
        3 DD-MMM-YYYY YY/MM/DD
        4 YYYY-MMM-DD MM/DD/YY
        5 YYYY-MMM-DD DD/MM/YY
        6 YYYY-MMM-DD YY/MM/DD

* Which date format do you require [1]: 1
%A1LENGLISH-I-DATEFORMAT, Date format DD-MMM-YYYY and MM/DD/YY (1) has been
selected

* What will be the greatest number of simultaneous ALL-IN-1 users: 5
* Which batch queue would you like to use for sending/receiving mail
[SYS$BATCH]: SYS$BATCH
* Do you want to use Message Router to send/receive messages to/from other
systems [NO]? YES

* Do you want to use a Message Router on another node [NO]? NO
* What level of Mail directory support do you want [0/1/2] [0]: 1

* Enter password for the Mail directory user agent account: A1MAIL

* Please confirm the Mail directory password specified: A1MAIL

* What password do you want to use for the ALL-IN-1 Message Router mailbox:
LYNX_A1

* Please confirm the password you have specified: LYNX_A1

* Do you want to translate outgoing WPS-PLUS and DX messages to ASCII [NO]?
NO

%A1LENGLISH-I-CHKSWPR, Checking MANDATORY and OPTIONAL SW prerequisites

%A1LENGLISH-I-CHKQUOT, Checking process quotas for the current process
%A1LENGLISH-I-CHKIDNT, Checking ALL-IN-1 general identifiers
%A1LENGLISH-I-CHKTRAC, Checking ALL-IN-1 transfer accounts

VMS account named A1$XFER_IN, which should be used for ALL-IN-1
purposes only, was already created before this installation.

You have two options:

 1. Answer YES if you want the existing A1$TRANSFER account to be used
    for ALL-IN-1 purposes ONLY. Note that in this case, some characteristics
    of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
    the installation.
 2. Answer NO to stop the installation, correct the problem and then start
    again.

B�26 Sample Installations

* Do you want to use the existing A1$XFER_IN account [NO]? YES

VMS account named A1$XFER_OUT, which should be used for ALL-IN-1
purposes only, was already created before this installation.

You have two options:

 1. Answer YES if you want the existing A1$TRANSFER account to be used
    for ALL-IN-1 purposes ONLY. Note that in this case, some characteristics
    of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
    the installation.
 2. Answer NO to stop the installation, correct the problem and then start
    again.

* Do you want to use the existing A1$XFER_OUT account [NO]? YES

%A1LENGLISH-I-CHKVMSV, Checking VAX/VMS version
%A1LENGLISH-I-CHKLIBS, Checking required shareable libraries are installed
%A1LENGLISH-I-CHKFMSV, Checking VAX/FMS version
%A1LENGLISH-I-CHKMROV, Checking Message Router version
%A1LENGLISH-I-CHKPARA, Checking system parameters

        All software checks have been successful.
        Installation will continue.

%A1LENGLISH-I-CHKDISK, Checking DISK SPACE

        NO missing DISK SPACE prerequisites discovered.
        The installation will continue.

* What is the existing VMS username for the ALL-IN-1 manager’s account
    [ALLIN1]: ALLIN1

            OWNER = ALLIN1
            USERNAME = ALLIN1
            UIC = [000001,000100]
            ACCOUNT = ALLIN1
            PRIVS =
            PRIORITY =
            DIRECTORY = [ALLIN1]

* Are you sure all the specified account’s characteristics are correct
    [YES]? YES

* What password do you want to use for the ALL-IN-1 TRANSFER accounts:
A1TRANSFER

* Please confirm the password you have specified: A1TRANSFER

A DISKQUOTA entry will be added for UIC [1,100] on SYS$SYSDEVICE:.
The DISKQUOTA entry has been added, with a PERMANENT quota of 10000
and an OVERDRAFT quota of 1000. Sample Installations B�27

                    A DISKQUOTA entry on SYS$SYSDEVICE: for UIC [1,100] will now be modified.
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 62500
                    and OVERDRAFT quota of 5000.
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[ALLIN1].
                    %VMSINSTAL-I-ACCOUNT, This installation creates an ACCOUNT named ALLIN1.
                    %UAF-I-ADDMSG, user record successfully added
                    %UAF-I-RDBADDMSGU, identifier ALLIN1 value: [000001,000100] added to
                    RIGHTSLIST.DAT
                    %VMSINSTAL-I-ACCOUNT, This installation updates an ACCOUNT named ALLIN1.
                    %UAF-I-MDFYMSG, user record(s) updated

                    * What UIC do you want for the A1$XFER_IN account?: [500,1]
                    * What UIC do you want for the A1$XFER_OUT account?: [500,2]

                    %VMSINSTAL-I-ACCOUNT, This installation creates an account named A1$XFER_IN.
                    %UAF-I-ADDMSG, user record successfully added

                    A DISKQUOTA on SYS$SYSDEVICE: for UIC [500,1] will now be modified.
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 50000
                    and OVERDRAFT quota of 5000

                    %VMSINSTAL-I-ACCOUNT, This installation creates an account named
                        A1$XFER_OUT.
                    %UAF-I-ADDMSG, user record successfully added

                    A DISKQUOTA on SYS$SYSDEVICE: for UIC [500,2] will now be modified.
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 50000
                    and OVERDRAFT quota of 5000

                    %A1LENGLISH-I-CREATID, Create ALL-IN-1 RIGHTS identifiers ...

                    A DISKQUOTA entry will be added for UIC OA$PRVAPP on SYS$SYSDEVICE:.
                    The DISKQUOTA entry has been added, with a PERMANENT quota of 1000
                    and an OVERDRAFT quota of 1000.

                    A DISKQUOTA entry on SYS$SYSDEVICE: for UIC OA$PRVAPP will now be modified.
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 1000
                    and OVERDRAFT quota of 1000.
                    %A1LENGLISH-I-GRANTID, Grant ALL-IN-1 general identifiers to UIC [1,100] ...

                    * Do you want to run the IVP after the installation [YES]? YES
                    %A1LENGLISH-I-KITREVS, The following items will be installed:

                    %A1LENGLISH-I-BASEREV, ALL-IN-1 BASE kit - Revision <rev>
                    %A1LENGLISH-I-CTRYREV, ALL-IN-1 US MARKET kit - Revision <rev>
                    %A1LENGLISH-I-LANGREV, ALL-IN-1 ENGLISH LANGUAGE kit - Revision <rev>
                    %A1LENGLISH-I-ASKDONE, All questions have now been completed.
                    %A1LENGLISH-I-ONEMEDEX, One more media change required before installation
                    can continue unaided.
                    VMSINSTAL-I-RESTORE, Restoring product saveset C...
                    VMSINSTAL-I-RESTORE, Restoring product saveset D...
                    VMSINSTAL-I-RESTORE, Restoring product saveset E...
                    VMSINSTAL-I-RESTORE, Restoring product saveset F...
                    VMSINSTAL-I-RESTORE, Restoring product saveset G...
                    VMSINSTAL-I-RESTORE, Restoring product saveset H...

B�28 Sample Installations

%OAIVP-I-PASSED, File check for ALL-IN-1 has passed.

B�32 Sample Installations

0 ! "Running editor check"
23 ! "EDT/WPS test."
252 ! " first address line check"
258 ! " second address line check"
265 ! " third address line check"
270 ! " fourth address line check"
275 ! " date check"
282 ! " day check"
286 ! " ALL-IN-1 username check"
289 ! " job title check"
293 ! "EDT/WPS check PASSED."
498 ! "WPS-PLUS check starting."
935 ! "WPS-PLUS check finished."
! Merged list checksum is 805719118
! Correct checksum is 805719118
951 ! "WPS-PLUS check PASSED"
955 ! "Editor check PASSED."
960 ! "Editor check finished." Sample Installations B�33

                    IWP output files follow...

B�34 Sample Installations

                    Text created by EDT/WPS check
                    -----------------------------
                                                                      DECPARK,
                                                                      WORTON GRANGE,
                                                                      READING,
                                                                      BERKSHIRE.
                                                                   Thursday, 28-Jul-1989.
                    Dear IVP user,
                            This is a test of the integration of EDT with ALL-IN-1.
                            If the address,day,date, and name and job title have been
                            substituted with the values of the IVP account then ALL-IN-1
                            and EDT are interacting correctly.
                            Yours Sincerely,
                                    IVP USER,
                                        INSTALLATION VERIFICATION Sample Installations B�35

                                                      OA Sales Department,
                                                  Digital Equip. Corp.,
                                                    DECpark,
                                                     Worton Grange,
                                                            Reading,Berks.
                                                  (0734) 868711
Ruth Calladine ,
Nutters Catering Compnay,
73 Watlington Street,
Reading.
(0734) 956435.
Dear Ruth,
  As a user of ALL-IN-1 V2.1/BEV on your VaxStation/GPX, you may be
    interested
  to know that Digital’s OA engineering group has just announced the
  availability of ALL-IN-1 V2.3 - a huge step forward for the future of
  office automation. It’s many *NEW* features include multiple select
  options for the File Cabinet, forward and backward scrolling on Read,
  as well as the capacity for multiple languages. All this together with
  the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
  1989.
        Phone NOW for a demonstration - on (0734) 868711
   Yours faithfully,
        Alain M. Cleaner,
           Office Products Manager. Sample Installations B�39

                    %OAIVP-I-INST, SYS$SYSDEVICE:[ALLIN1.LIB_SHARE]OA$MAIN.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$SYSDEVICE:[ALLIN1.LIB_SHARE]OA$SUBMIT.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSEXE]OA$FORMATTER.EXE;25 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]FDVMSG.EXE;1 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]DPEMSG.EXE;17 is installed.

                    %OAIVP-I-INST, SYS$COMMON:[SYSMSG]XPORTMSG.EXE;74 is installed.

                    %OAIVP-I-PASSED, Message check for ALL-IN-1 has passed.

                    LOG OF THE VERIFICATION OF ALL-IN-1 MESSAGES:
                    ---------------------------------------------

                    This should contain the string V2.4...

                    Enter CMD: VERSION
                    %OA-I-VERSION, ALL-IN-1 Version 2.4 8-Dec-1989

                     This should produce an Informational level message,
                     and an RMS-E-FNF error

                    Enter CMD: OA$FLO_OPEN THIS_IS_A_TEST
                    %OA-I-LNF, Error opening form library "THIS_IS_A_TEST"
                    -RMS-E-FNF, file not found
                    %OA-I-LNF, Error opening form library "THIS_IS_A_TEST"
                    -RMS-E-FNF, file not found

                     This should produce a Warning level message...

                    Enter CMD: OA$SYM_GET_SYMBOL THIS_IS_A_TEST
                    %OA-W-INVGET, Symbol "THIS_IS_A_TEST" not found

                     This should produce a Error level message...

                    Enter CMD: OA$FBT_WRITE_LIBRARY THIS_IS_A.TEST
                    %OA-E-BADLIB, Error occurred while pre-compiling THIS_IS_A.TEST form library

                     FATAL level error messages cause the image to stop,
                      so they are not tested.

B�40 Sample Installations

! Demonstrating directory application.
! Verifying directory application.
! Demonstration of application has passed.
! Finished demonstrating application
                        Personal Phone Directory Full Listing
Date: 07/28/88 Page:1
   .
   .
   .

! Running create account check
3801 ! "Running create account check"
4105 ! "Flushing unread mail "
4111 ! "Deleting profile and template "
4114 ! "Deleted profile and template"
4114 ! "Deleting VMS account and identifier"
4118 ! "Deleted VMS account"
4122 ! "Account is clean"
4138 ! "Creating account"
! Batch job creating account has finished
4809 ! "Finished creating account"
4810 ! "Starting mail send check"
! The user agent is unknown in the mail directory
5694 ! "Sent message checksum: 1835745907"
5696 ! "Received message checksum: 1835745907"
! Account create check has passed, checksums match
5704 ! "Account create check has passed, checksums match"
5799 ! "Deleting account"
6022 ! "Finished deleting account"
6030 ! "Create account check finished"
! Create account check finished
! Verifying Mail directory
! ALL-IN-1 Mail directory useragent name should be OA$LYNX$ALLIN1
! The following Mail directory useragent entries exist:
! ( DIGITAL MBMAN MASTER OBJECT )
! ( OA$LYNX$ALLIN1 )
! The Mail directory useragent entry for ALL-IN-1 which matched is
OA$LYNX$ALLIN1
! Mail directory verification has PASSED.
! Starting MR verification.
! MR verification has PASSED.
!
! Both tests have passed.
Verifying ALL-IN-1’s interface with Message Router.
---------------------------------------------------
Lowest valid version of MR is V3.
Your current version of MR is MR V3.0-044.
MR version correct.
MR Mailbox entry for ALL-IN-1 verified to be A1.
Message Router IVP has PASSED.
End of Message Router IVP.
! Finished verifying Mail directory and MR. Sample Installations B�41

                    ! Running electronic mail check
                    6592 ! "Running electronic mail check"
                    7115 ! " Sent message checksum: 1835680371 "
                    7117 ! " Received message checksum: 1835680371 "
                    7123 ! "Electronic mail check has PASSED, checksums match."
                    7193 ! "Electronic mail check finished."
                    ! Electronic mail check finished.

                    %A1IVP-I-IVPPASS,The IVPs for ALL-IN-1 V2.4 have passed.
                            Installation of A1 V2.4 completed at 12:34

                    Enter the products to be processed from the next distribution volume set.
                    * Products:

                            VMSINSTAL procedure done at 12:35

B.3 Sample of an ALL-IN-1 Version 2.4 Update Installation

This section contains a sample listing of all the output and input when a multilingual ALL-IN-1 Version 2.4 system was updated, on a system running VMS Version 5.2. The update installation was performed to include Message Router Version 3.1 and Message Router VMSmail Gateway Version 3.1. The ALL-IN-1 Version 2.4 system had WPS-PLUS and VAX DATATRIEVE integrated. The installer chose to:

Install ALL-IN-1 from magnetic tape

Integrate WPS-PLUS and ACMS

Use the ALL-IN-1 directory as the primary directory

Run the IVPs automatically at the end of the installation

The revision identi�er, <rev>, indicates the revision of your ALL-IN-1 Version 2.4 kit.

Username: SYSTEM
Password:
        Welcome to VAX/VMS Version V5.2 on node LYNX
    Last interactive login on Monday, 7-DEC-1989 08:47
    Last non-interactive login on Monday, 7-DEC-1989 08:25

$ set default sys$update
$ @vmsinstal

        VAX/VMS Software Product Installation Procedure V5.1

It is 8-DEC-1989 at 10:26.
Enter a question mark (?) at any time for help.

* Are you satisfied with the backup of your system disk [YES]? YES
* Where will the distribution volumes be mounted: TAPE0

B�42 Sample Installations

    You have two options:

  1. Answer YES if you want the existing A1$TRANSFER account to be used
      for ALL-IN-1 purposes ONLY. Note that in this case, some characteristics
      of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
      the installation.
  2. Answer NO to stop the installation, correct the problem and then start
      again.

 * Do you want to use the existing A1$XFER_IN account [NO]? yes

  VMS account named A1$XFER_OUT, which should be used for ALL-IN-1
    purposes only, was already created before this installation.

    You have two options:

  1. Answer YES if you want the existing A1$TRANSFER account to be used
      for ALL-IN-1 purposes ONLY. Note that in this case, some characteristics
      of the account (e.g. UIC, PASSWORD, ACCESS type) may be changed during
      the installation.
  2. Answer NO to stop the installation, correct the problem and then start
      again.

 * Do you want to use the existing A1$XFER_OUT account [NO]? yes

%A1LENGLISH-I-CHKVMSV, Checking VAX/VMS version
%A1LENGLISH-I-CHKLIBS, Checking required shareable libraries are installed
%A1LENGLISH-I-CHKFMSV, Checking VAX/FMS version
%A1LENGLISH-I-CHKMROV, Checking Message Router version
%A1LENGLISH-I-CHKPARA, Checking system parameters

        All software checks have been successful.
        Installation will continue.

%A1LENGLISH-I-CHKDISK, Checking DISK SPACE

        NO missing DISK SPACE prerequisites discovered.
        The installation will continue.

* What is the existing VMS username for the ALL-IN-1 manager’s account
    [ALLIN1]: ALLIN1

            OWNER = ALLIN1
            USERNAME = ALLIN1
            UIC = [000001,000100]
            ACCOUNT = ALLIN1
            PRIVS =
            PRIORITY =
            DIRECTORY = [ALLIN1]

* Are you sure all the specified account’s characteristics are correct
    [YES]? YES

B�46 Sample Installations

A DISKQUOTA entry on SYS$SYSDEVICE: for UIC [1,100] will now be modified.
The DISKQUOTA entry has been modified to: PERMANENT quota of 62500
and OVERDRAFT quota of 5000.
%VMSINSTAL-I-ACCOUNT, This installation update an ACCOUNT named ALLIN1.
%UAF-I-MDFYMSG, user record(s) updated
%VMSINSTAL-I-ACCOUNT, This installation updates an ACCOUNT named ALLIN1.
%UAF-I-MDFYMSG, user record(s) updated

%A1LENGLISH-I-CREATID, Create ALL-IN-1 RIGHTS identifiers ...
%A1LENGLISH-I-GRANTID, Grant ALL-IN-1 general identifiers to UIC [1,100] ...

* Do you want to run the IVP after the installation [YES]? YES
%A1LENGLISH-I-KITREVS, The following items will be installed:

%A1LENGLISH-I-BASEREV, ALL-IN-1 BASE kit - Revision <rev>
%A1LENGLISH-I-CTRYREV, ALL-IN-1 US MARKET kit - Revision <rev>
%A1LENGLISH-I-LANGREV, ALL-IN-1 ENGLISH LANGUAGE kit - Revision <rev>
%A1LENGLISH-I-ASKDONE, All questions have now been completed.
%A1LENGLISH-I-ONEMEDEX, One more media change required before installation
can continue unaided.
VMSINSTAL-I-RESTORE, Restoring product saveset C...
VMSINSTAL-I-RESTORE, Restoring product saveset D...
VMSINSTAL-I-RESTORE, Restoring product saveset E...
VMSINSTAL-I-RESTORE, Restoring product saveset F...
VMSINSTAL-I-RESTORE, Restoring product saveset G...
VMSINSTAL-I-RESTORE, Restoring product saveset H...

Tape TAPE0:A13024 dismounted. (MEDIA CHANGE REQUIRED ) :
Dismounted tape labeled A13024. Please mount the BASE kit tape which
is labeled A11024 and reply to the prompt below (Answer NO to exit).

* Type YES when correct tape mounted, NO to terminate installation? YES

%MOUNT-I-MOUNTED, A11024 mounted on _LYNX$TAPE0:
%A1-I-REMBKSS, Restoring any remaining BASE kit savesets.
%VMSINSTAL-I-RESTORE, Restoring product saveset B...
%VMSINSTAL-I-RESTORE, Restoring product saveset C...
%VMSINSTAL-I-RESTORE, Restoring product saveset D...
%VMSINSTAL-I-RESTORE, Restoring product saveset E...
%A1-I-A1LINK, Starting to link images

Building shared image modules
Shared image modules built
Linking the OA$MAIN image
   .
   .
   .
%A1-I-A1LINKED, Finished linking images

 During the installation, a file called A1V24START.COM has been added
 to SYS$MANAGER:

 A document outlining the changes affecting your users has been added
 to the MANAGER’S directory. Please distribute USERCHANGES.WPL to your
 users after installation. Sample Installations B�47

                    ****************************************************************************
                    ****************************************************************************
                    * *
                    *The VMS site-dependent start-up file should have the following line added:*
                    * *
                    * $ @SYS$MANAGER:A1V24START SYS$SYSDEVICE:[ALLIN1.DATA_SHARE] *
                    * *
                    * where SYS$SYSDEVICE:[ALLIN1.DATA_SHARE] is the location of the*
                    * ALL-IN-1 configuration file -- A1CONFIG.DAT *
                    * *
                    *This procedure must be invoked before users can successfully use ALL-IN-1 *
                    * *
                    ****************************************************************************
                    ****************************************************************************

                    During the installation, a second file called A1WPSPLUS_LOGIN.COM,

                    has been added to SYS$MANAGER.

                    This file must be run at system login time OR from each user’s LOGIN.COM.
                    Please refer to the Installation Guide for details.

                    %OA-I-LASTLINE, "ALL-IN-1 running -- removing form libraries & TXL"
                    %OA-E-NOSUCHSEC, no such (global) section
                    %OA-E-NOSUCHSEC, no such (global) section

                             SYSTEM finished using ALL-IN-1 at 8-Dec-1989 11:38

                    %A1-I-RNEPROF, Running command procedure EPROFIL.CA1
                    %OA-I-LASTLINE, "ALL-IN-1 running -- opening form libraries"
                    %OA-I-LASTLINE, "ALL-IN-1 running -- updating A1CONFIG data file"

                             SYSTEM finished using ALL-IN-1 at 8-Dec-1989 11:40

                    %OA-I-LASTLINE, "ALL-IN-1 running -- compiling form libraries..."
                    %OA-I-LASTLINE, "ALL-IN-1 running -- compiling OAFORM..."
                    %OA-I-LASTLINE, "ALL-IN-1 running -- compiling MEMRES..."
                    %OA-I-LASTLINE, "ALL-IN-1 running -- compiling SITEOAFORM..."
                    %OA-I-LASTLINE, "ALL-IN-1 running -- compiling SITEMEMRES..."
                    %OA-I-LASTLINE, "ALL-IN-1 running -- form libraries compiled"
                    %OA-I-LASTLINE, "ALL-IN-1 running -- data file and form processing complete"

                             SYSTEM finished using ALL-IN-1 at 8-Dec-1989 11:44

                    %A1-I-CREMBX, Creating mailbox entry A1
                            This is MRMAN V3.1
                    %Added A1, Owner=ALLIN1 Complete_Messages Ignore_Sender
                    Grant_Id Service_Messages
                    %A1-I-DDSUA, Creating DDS UA entry for OA$LYNX$ALLIN1
                     MBMAN V3.1 (BL5.10)
                     Name : OA$LYNX$ALLIN1
                     Master copy owning node : LYNX

B�48 Sample Installations

                    %A1-I-DDSSUB, Creating DDS subscriber entry for MANAGER
                     MBMAN V3.1 (BL5.10)
                     Surname : MANAGER
                     Name : MANAGER
                     Unique subscriber identifier : OA$LYNX$ALLIN1
                     Proxy user agent : OA$LYNX$ALLIN1
                     Master copy owning node : LYNX

                    When the VMSINSTAL procedure terminates, remember to attend to the
                    POST-INSTALLATION tasks described in the Installation guide.

                    Failure to do this will result in ALL-IN-1 not working correctly

                    The installation procedure for ALL-IN-1 V2.4 has now completed
                    %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
                        directories...

                        The IVP for ALL-IN-1 V2.4 takes about 30 minutes to run. This will
                     vary according to the system that it is running on.

                           It will first of all run SYS$MANAGER:A1V24START to initialise
                     ALL-IN-1 logical names and to install the various images required. It
                     also will clear the VMS account name associated with the ALL-IN-1 IVP
                     account. Should the IVPs fail to reset the VMS username in the PROFILE,
                     then please reset it to the same as the MANAGER vms username as soon as
                     possible, by doing the following:

                       $ALLIN1/NOINIT
                       Enter CMD: WRITE CHANGE PROFIL USER="IVP",VMSUSR="ALLIN1"

                        If the IVPs fail then please investigate the log files found in
                     OA$IVP. There is an additional log file in SYS$MANAGER called
                     ALLIN1IVP.LOG containing the messages from running ALL-IN-1 IVPs.
                     This may sometimes prove useful, for instance if ALL-IN-1 fails to
                     run, it can be seen in this file. To run the IVPs again type:

                       $SET PROC/PRIV=(NOBYPASS,ALL)
                       $ALLIN1/USER=IVP

                        Use the various options on the menu that is presented to run parts
                     of the IVP or all of it. The "ALL" option is what is run during the
                     installation phase IVPs. See the System Management Guide for more
                     details.

                       As an aid to finding problems then please read IVPHINTS.MEM in
                     OA$IVP:

                    %A1IVP-I-IVPSTART,Running startup for ALL-IN-1 . Sample Installations B�49

IWP output files follow... Sample Installations B�53

                    Text created by EDT/WPS check
                    -----------------------------
                                                                      DECPARK,
                                                                      WORTON GRANGE,
                                                                      READING,
                                                                      BERKSHIRE.
                                                                   Thursday, 28-Jul-1989.
                    Dear IVP user,
                            This is a test of the integration of EDT with ALL-IN-1.
                            If the address,day,date, and name and job title have been
                            substituted with the values of the IVP account then ALL-IN-1
                            and EDT are interacting correctly.
                            Yours Sincerely,
                                    IVP USER,
                                        INSTALLATION VERIFICATION

B�54 Sample Installations

Text created by WPS-PLUS check
------------------------------
                                                      OA Sales Department,
                                                  Digital Equip. Corp.,
                                                    DECpark,
                                                     Worton Grange,
                                                            Reading,Berks.
                                                  (0734) 868711
Kate Jelly,
Office Equipment Ltd,
666 London Rd,
Reading.
(0734) 663666.
Dear Kate,
  As a user of ALL-IN-1 V2.2 on your VAX/VMS 8800, you may be interested
  to know that Digital’s OA engineering group has just announced the
  availability of ALL-IN-1 V2.3 - a huge step forward for the future of
  office automation. It’s many *NEW* features include multiple select
  options for the File Cabinet, forward and backward scrolling on Read,
  as well as the capacity for multiple languages. All this together with
  the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
  1989.
        Phone NOW for a demonstration - on (0734) 868711
   Yours faithfully,
        Alain M. Cleaner,
           Office Products Manager. Sample Installations B�55

                                                                         OA Sales Department,
                                                                      Digital Equip. Corp.,
                                                                        DECpark,
                                                                         Worton Grange,
                                                                               Reading,Berks.
                                                                      (0734) 868711
                    Susie Coggles,
                    Art Equipment Ltd,
                    69 London Rd,
                    Reading.
                    (0734) 696969.
                    Dear Susie,
                      As a user of ALL-IN-1 V2.1/BEV on your VAX/VMS 8650, you may be interested
                      to know that Digital’s OA engineering group has just announced the
                      availability of ALL-IN-1 V2.3 - a huge step forward for the future of
                      office automation. It’s many *NEW* features include multiple select
                      options for the File Cabinet, forward and backward scrolling on Read,
                      as well as the capacity for multiple languages. All this together with
                      the advanced WP Grammer Checker option, make this THE OFFICE PRODUCT OF
                      1989.
                            Phone NOW for a demonstration - on (0734) 868711
                       Yours faithfully,
                            Alain M. Cleaner,
                               Office Products Manager.

B�56 Sample Installations

! Demonstrating directory application.
! Verifying directory application.
! Demonstration of application has passed.
! Finished demonstrating application
                        Personal Phone Directory Full Listing
Date: 07/28/88 Page:1
   .
   .
   .

! Running create account check
3801 ! "Running create account check"
4105 ! "Flushing unread mail "
4111 ! "Deleting profile and template "
4114 ! "Deleted profile and template"
4114 ! "Deleting VMS account and identifier"
4118 ! "Deleted VMS account"
4122 ! "Account is clean"
4138 ! "Creating account"
! Batch job creating account has finished
4809 ! "Finished creating account"
4810 ! "Starting mail send check"
! The user agent is unknown in the mail directory
5694 ! "Sent message checksum: 1835745907"
5696 ! "Received message checksum: 1835745907"
! Account create check has passed, checksums match
5704 ! "Account create check has passed, checksums match"
5799 ! "Deleting account"
6022 ! "Finished deleting account"
6030 ! "Create account check finished"
! Create account check finished
! Verifying Mail directory
! ALL-IN-1 Mail directory useragent name should be OA$LYNX$ALLIN1
! The following Mail directory useragent entries exist:
! ( DIGITAL MBMAN MASTER OBJECT )
! ( OA$LYNX$ALLIN1 )
! The Mail directory useragent entry for ALL-IN-1 which matched is
OA$LYNX$ALLIN1
! Mail directory verification has PASSED.
! Starting MR verification.
! MR verification has PASSED.
!
! Both tests have passed.
Verifying ALL-IN-1’s interface with Message Router.
---------------------------------------------------
Lowest valid version of MR is V3.
Your current version of MR is MR V3.0-044.
MR version correct.
MR Mailbox entry for ALL-IN-1 verified to be A1.
Message Router IVP has PASSED.
End of Message Router IVP.
! Finished verifying Mail directory and MR.

B�60 Sample Installations

! Running electronic mail check
6592 ! "Running electronic mail check"
7115 ! " Sent message checksum: 1835680371 "
7117 ! " Received message checksum: 1835680371 "
7123 ! "Electronic mail check has PASSED, checksums match."
7193 ! "Electronic mail check finished."
! Electronic mail check finished.

%A1IVP-I-IVPPASS,The IVPs for ALL-IN-1 V2.4 have passed.
        Installation of A1 V2.4 completed at 12:34

Enter the products to be processed from the next distribution volume set.
* Products:

        VMSINSTAL procedure done at 12:35

B.4 Additional Language Installation

This section contains a sample listing of all the output and input when the GERMAN language was installed as an additional language on a system running VMS Version 5.2. The ALL-IN-1 Version 2.4 system has WPS-PLUS and ACMS integrated. The installer chose to install the additional language from magnetic tape.

Username: SYSTEM
Password:
        Welcome to VAX/VMS Version V5.2 on node LYNX
    Last interactive login on Monday, 15-DEC-1989 08:47
    Last non-interactive login on Monday, 15-DEC-1989 08:25

$ set default sys$update
$ @vmsinstal

        VAX/VMS Software Product Installation Procedure V5.2

It is 15-DEC-1989 at 09:11.
Enter a question mark (?) at any time for help.

* Are you satisfied with the backup of your system disk [YES]? YES
* Where will the distribution volumes be mounted: TAPE0

Enter the products to be processed from the first distribution volume set.
* Products: A1LGERMAN024
* Enter installation options you wish to use (none):
Please mount the first volume of the set on TAPE0:.
* Are you ready? YES
%MOUNT-I-MOUNTED, A13024 mounted on _LYNX$TAPE0:

The following products will be processed:

  A1LGERMAN V2.4

        Beginning installation of A1LGERMAN V2.4 at 09:11

%VMSINSTAL-I-RESTORE, Restoring product saveset A...

This is a LOCAL ALL-IN-1 V2.4 LANGUAGE-only kit (GERMAN)Sample Installations B�61

                    Using the LANGUAGE only ALL-IN-1 V2.4 kit, the following types of
                        installation
                    can be performed :-

                            (1) Installation of an additional language
                            (2) Upgrade of an additional existing ALL-IN-1 V2.3 language
                            (3) Update of an existing ALL-IN-1 V2.4 language

                    * Do you want to continue [YES]? YES
                    * What type of installation do you wish to perform [1]: 1

                    This is the GERMAN Additional Language installation

                    %A1LGERMAN-I-RELANK, Restoring the LANGUAGE kit savesets.
                    %VMSINSTAL-I-RESTORE, Restoring product saveset B...

                       This is the GERMAN version of ALL-IN-1 V2.4

                    * Does this product have an authorization key registered and loaded [YES]?
                    YES
                    %LMF-I-GOTLICENSE, An ALLIN1-UI-GERMAN license is installed and loaded
                    %LMF-I-CHKSWLIC, Checking licenses for prerequisite software
                    %LMF-I-CONFLICENSE, All necessary licenses are installed and loaded

                            During your first language installation you elected to install
                            ALL-IN-1 without DATATRIEVE, so this tool will NOT is available from
                        your
                            GERMAN ALL-IN-1.

                            During your first language installation you elected to integrate
                            WPS-PLUS. It means that you can access WPS-PLUS as an additional
                            editor from your GERMAN ALL-IN-1 as well.

                            During your first language installation you elected to install
                            ALL-IN-1 with ACMS, so this tool will be available from your
                            GERMAN ALL-IN-1.

                    %A1LGERMAN-I-CHKSWPR, Checking MANDATORY SW prerequisites

                    %A1LGERMAN-I-CHKMROV, Checking the existence of ALL-IN-1 logical names
                    %A1LGERMAN-I-CHKPARA, Checking system parameters

                            All S/W checks have been successful.
                            Installation will continue.

                    %A1LGERMAN-I-CHKDISK, Checking DISK SPACE

                       ALL-IN-1 allows you to select a default date format for each language
                       you have installed. This will become the default ALL-IN-1 date format
                       for each user (on a per language basis). This may be changed by user
                       through the Set Working Conditions option.

                                Alphanumeric Date Numeric Date

                            1 DD-MMM-YYYY MM/DD/YY (Standard Default)
                            2 DD-MMM-YYYY DD/MM/YY
                            3 DD-MMM-YYYY YY/MM/DD
                            4 YYYY-MMM-DD MM/DD/YY
                            5 YYYY-MMM-DD DD/MM/YY
                            6 YYYY-MMM-DD YY/MM/DD

B�62 Sample Installations

                    * Which date format do you require [1]: 1
                    %A1LGERMAN-I-DATEFORMAT, Date format DD-MMM-YYYY and DD/MM/YY (2) has been
                    selected

                    * Which device will hold the ALL-IN-1 GERMAN language files
                    [SYS$SYSDEVICE:]: SYS$SYSDEVICE

                            NO missing DISK SPACE prerequisites discovered.
                            The installation will continue.

                    * What is the existing VMS username for the ALL-IN-1 account [ALLIN1]:
                    ALLIN1
                                    OWNER =
                                    USERNAME = ALLIN1
                                    UIC = [1,100]
                                    ACCOUNT =
                                    PRIVS = All
                                    PRIORITY = 4
                                    DIRECTORY = SYS$SYSDEVICE:[ALLIN1]

                    * Are you sure all the specified account’s characteristics are correct
                    [YES]? YES

                    A DISKQUOTA entry on SYS$SYSDEVICE: for UIC [1,100] will now be modified.
                    %DISKQ-I-INUSE, [000001,000100] has 96395 blocks in use
                    The DISKQUOTA entry has been modified to: PERMANENT quota of 87904
                    and OVERDRAFT quota of 5000.
                    * Enter ALL-IN-1 top-level directory required for all GERMAN files [GERMAN]:
                    GERMAN
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.BLP_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.CBI_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.DATA_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.DO_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.IVP_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.LIB_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.LLV_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.SCP_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.SITE].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.SITE.DATA_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.SITE.LIB_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directory
                    SYS$SYSDEVICE:[GERMAN.SITE.DO_GERMAN].
                    %VMSINSTAL-I-SYSDISK, This product creates system disk directorySample Installations B�63

DX$PRINT
FAC$COMMON
KOA$HEAP_SIZE
KOA$PRINT_DIR
KOA$PRINT_SHARE
OA$ADMIN_DATA
OA$BLP
OA$BLP_lang
OA$BLP_LLV
OA$BLP_SHARE
OA$BUILD
OA$BUILD_SHARE
OA$DATA
OA$DATA_LLV
OA$DATA_SHARE
OA$DDS_PRIME
OA$DEFAULT_LANGUAGE
OA$DO
OA$DO_lang
OA$DO_LLV
OA$DO_SHARE
OA$IMAGE
OA$LIB
OA$LIB_lang
OA$LIB_LLV
OA$LIB_SHARE
OA$LLV
OA$LOADUSER
OA$LOG
OA$MAIL_NUM_ADDRESSES
OA$MTI_AREA
OA$MTI_DATA
OA$MTI_ERR
OA$MTI_LOG
OA$MTI_MAILBX
OA$MTI_MR_NODE (If you are using a remote Message Router)
OA$MTI_OPER
OA$MTI_QUEUE
OA$MTI_TRNS
OA$PRIMARY_NODE
OA$SCP
OA$SCP_lang
OA$SCP_LLV
OA$SCP_SHARE
OA$SHARE (The logical names OA$SHARE* refer to Mail area
                   E which is created during the installation of
                   ALL-IN-1 Version 2.4)
OA$SHAREn (n is from 1 to the number of shared directories
                   specified during the installation)
OA$SHARE_HIGH
OA$SHARE_LOW
OA$SITE_BLP_lang
OA$SITE_BLP_LLV
OA$SITE_BLP_SHARE Files and Logical Names Installed on Your System C�3

                           OA$SITE_BUILD_LLV
                           OA$SITE_BUILD_SHARE
                           OA$SITE_DATA
                           OA$SITE_DATA_LLV
                           OA$SITE_DATA_SHARE
                           OA$SITE_DEV
                           OA$SITE_DEV_lang
                           OA$SITE_DEV_LLV
                           OA$SITE_DEV_SHARE
                           OA$SITE_DO_lang
                           OA$SITE_DO_LLV
                           OA$SITE_DO_SHARE
                           OA$SITE_LIB
                           OA$SITE_LIB_lang
                           OA$SITE_LIB_LLV
                           OA$SITE_LIB_SHARE
                           OA$SITE_SCP_lang
                           OA$SITE_SCP_LLV
                           OA$SITE_SCP_SHARE
                           OA$SUBMIT_IMAGE
                           OA$SUBSCRIBER_MAIL
                           OA$SYSTEM_LISTS
                           OA$TRANSFER

C.2.2 Logical Names Entered into the Language Logical Name Table

The following logical names are entered into a language-speci�c logical name table for the language installed, OA$lang_TABLE. The same logical names are used for all languages although their de�nitions are different.

Note Copies of all logical names that end in _LLV exist in both the system logical

name table and the logical name table for the default language.

OA$BLP_LLV
OA$DATA_LLV
OA$DO_LLV
OA$LIB_LLV
OA$LLV
OA$SCP_LLV
OA$SITE_BLP_LLV
OA$SITE_BUILD_LLV
OA$SITE_DATA_LLV
OA$SITE_DEV_LLV
OA$SITE_DO_LLV
OA$SITE_LIB_LLV
OA$SITE_SCP_LLV

C�4 Files and Logical Names Installed on Your System

C.3 Directory Structure of an ALL-IN-1 System Installed on

Separate Disks

Figures C�1 to C�6 show the directory structure of an ALL-IN-1 Version 2.4 system installed on the system disk and disks DISK0 to DISK4. Each area of ALL-IN-1 (see Section 1.8.16) was installed on a different disk, with a different directory speci�ed for each area:

The ALL-IN-1 manager’s account was installed on the system disk SYS$SYSDEVICE: using the account name MANAGER.

The shared library �les were installed on disk DISK0 using the directory name LIBRARY.

The language �les were installed on disk DISK1 using the directory name LANGUAGE.

The shared data �les were installed on disk DISK2 using the directory name DATA.

The mail area SDAF �le was installed on disk DISK3 using the directory name MAIL.

The shared directories were installed on disk DISK4 using the directory name SHARED.

If you want to move an ALL-IN-1 area to another disk, copy the directories in that area as shown in Figures C�1 to C�5 (the shared directories cannot be moved once they are created). See Appendix D for details.

Files and Logical Names Installed on Your System C�5

Figure C�1 Directory Structure of the ALL-IN-1 Manager’s Account

[.IVPUSER] [.DOC0]

[.DOC9]

[.MSG]

[.UDP]

[.DOC0]

[.DOC9]

[.MSG]

[.UDP]

[.DOC0]

[.DOC9]

[.MSG]

[.UDP]

. . .

SYS$SYSDEVICE:[MANAGER]

[.TRANSFER_INCOMING]

[.TRANSFER_OUTGOING]

[.MGR] . . .

[.POSTMASTE] . . .

Figure C�2 Directory Structure for the Library Files

[.ADMIN_DATA]

[.BLP_SHARE]

[.DO_SHARE]

[.LIB_SHARE]

[.LOG]

[.PRINT]

[SCP_SHARE]

[.USER]

DISK0:[LIBRARY]

[.BLP_SHARE]

[.DEV_SHARE]

[.DO_SHARE]

[.LIB_SHARE]

[.SCP_SHARE]

[.SOURCES_SHARE]

[.SITE]

[.SOURCES]

[.SYSTEM_LISTS]

Figure C�4

Directory Structure for the Data Files

[.DATA_SHARE]

DISK2:[DATA]

[.DATA_SHARE]

[.SITE]

DISK3:[MAIL] [.SHARE_E]

C�8 Files and Logical Names Installed on Your System

Figure C�6 Directory Structure for the Shared Directories

[.SHARED1]

[.SHARED2]

[.SHARED3]

DISK4:[SHARED]

Files and Logical Names Installed on Your System C�9 D Changing the Con�guration of ALL-IN-1V2.4

This appendix describes changes to the con�guration of ALL-IN-1 Version 2.4 that do not require an update installation to be performed. You can:

Change the con�guration to incorporate VAX DATATRIEVE with ALL-IN-1

Change the con�guration to incorporate WPS-PLUS with ALL-IN-1

Change the con�guration to incorporate VAX Application Control and Management System (ACMS) with ALL-IN-1

Change the location of the ALL-IN-1 Version 2.4 areas

CAUTION This task involves modifying the ALL-IN-1 Version 2.4 con�guration

database. This database is crucial to the operation of ALL-IN-1 and changes must be made with extreme care. Digital recommends that you take a backup copy of OA$DATA_SHARE:A1CONFIG.DAT before making any changes.

If you want to change to using WPS-PLUS or Message Router for the �rst time, you must perform an update installation (see Chapter 11).

D.1 Change to Using VAX DATATRIEVE

If you want to incorporate VAX DATATRIEVE with ALL-IN-1 , do the following:

1 Install VAX DATATRIEVE Version 5.0 (see the VAX DATATRIEVE

Installation Guide)

2 Relink ALL-IN-1 (see the ALL-IN-1 Management Guide) and answer YES to

the question "Do you want to incorporate DATATRIEVE?"

Changing the Con�guration of ALL-IN-1 V2.4 D�1

D.2 Change to Using WPS-PLUS

If you installed ALL-IN-1 Version 2.4 without incorporating WPS-PLUS, the WPS-PLUS �les were not installed during the installation. Therefore, if you want to use WPS-PLUS with ALL-IN-1, you must perform an update installation (see Chapter 11) to install these �les, and answer YES to the prompt:

Do you want to incorporate WPS-PLUS [YES]?

D.3 Change to Using VAX ACMS

If you want to incorporate VAX ACMS with ALL-IN-1 , do the following:

1 Install VAX ACMS Version 3.1 (see the VAX ACMS Installation Guide)

2 Relink ALL-IN-1 (see the ALL-IN-1 Management Guide) and answer YES to

the question "Do you want to incorporate ACMS?"

D.4 Change the Location of an ALL-IN-1 Version 2.4 Area

If you want to move an ALL-IN-1 area to another disk, do the following:

1 Shut down ALL-IN-1 (see the ALL-IN-1 Management Guide).

2 Copy the directories in that area to the appropriate disk. A list of

ALL-IN-1 areas is given in the ALL-IN-1 Installation Guide Part 3 Market Installation. For a list of the directories in each area see Appendix C, Section C.3.

3 Enter the ALL-IN-1 manager’s ALL-IN-1 account:

$ ALL-IN-1 /USERNAME=MANAGER /OVERRIDE=SHUTDOWN

4 Change the ALL-IN-1 con�guration �le as follows:

a Enter A1CONFIG. The ALL-IN-1 System Con�guration Information form

is displayed.

b Enter the key of the component required:

Enter A1BASE for the base component. The base component description record is displayed.

Enter language name for the appropriate language component. The language component description record is displayed.

c Enter C to change the record.

d Move the cursor to the �eld relating to the �les that are to be moved.

For the base system the �elds are:

"File Location" for the ALL-IN-1 library �les

D�2 Changing the Con�guration of ALL-IN-1 V2.4

"Data Location" for the ALL-IN-1 data �les

"Site File Loc" for the ALL-IN-1 site library �les

"Site Data Loc" for the ALL-IN-1 site data �les

"ALL-IN-1 Mgr’s Dir" for the ALL-IN-1 manager’s directory Enter the new location of the �les. For the language system the �elds are:

"File Location" for the ALL-IN-1 language �les

"Site File Loc" for the ALL-IN-1 site language �les Enter the new location of the �les.

e Press RETURN.

f Press EXIT.

g Ensure that Message Router is started (see the Message Router books).

h Run the ALL-IN-1 Version 2.4 startup command procedure (see Section 14.6). If you are running ALL-IN-1 on a VAXcluster system you must run the startup command procedure on all nodes in the cluster.

D.5 Moving ALL-IN-1

If you want to move part or all of your ALL-IN-1 system to other disks, do the following:

1 Shut down ALL-IN-1.

2 Move each area of ALL-IN-1 (as described in Section D.4).

3 If you want to move mail areas, you must edit the information that is held

in the mail area master �les. Do this as follows:

a Use form SM_SDAF_MASTER to update the location of any SDAFs that you move.

b Use form SM_SHARED_DIR_MASTER to update the location of any shared directories that you move.

4 If you use Message Router, ensure that Message Router is started.

5 Run the ALL-IN-1 startup command procedure, A1V24START.COM,

to allow the changes to take effect. If you are running ALL-IN-1 on a VAXcluster system, you must run the startup command procedure on all nodes in the cluster. Changing the Con�guration of ALL-IN-1 V2.4 D�3

Post-installation (Cont.)

terminal characteristics for LQP02,

14�13 terminal characteristics for LQP03,

14�13 Preparing for

installation, 1�1 Prerequisite

software, 1�6 Printer Types Master �le

modi�cations to, 14�13 Product Authorization Key, 1�5

registering and loading, 13�10 Product identi�er, 13�2 Purge

�les during installation, 13�12

RRelease Notes, 2�1

accessing, 2�2 printing, 2�2 Remote

Message Router, 1�13, 1�19 system, 1�13 VMSmail Gateway con�guration,

14�11 Reporting problems, 14�19 Required operating system components, 1�6 Satellite node, 1�19, 13�17

Shared directories, 13�29

number of, 13�29 Software Product Description, 1�4, 1�5, A�4 Software Warranty Addendum, 1�5, A�4 SPD, 1�4, 1�5, A�4 SSA, 1�5, A�4 Startup command procedure

executing, 14�4 Structure Structure (Cont.) of this guide, xv SWA, 1�5, A�4 SYSGEN, 1�30 System backup, 13�3 System parameters, 1�30, 13�17 System Support Addendum, 1�5, A�4

TTerminal characteristics

LN03 printer, 14�13 LQP02 printer, 14�13 LQP03 printer, 14�13 Text library

compiling, 14�7 installing, 14�7 Transfer user accounts

password, 13�33 Translate WPS-PLUS and DX messages

to ASCII, 13�21 TXL compiling, 14�7 installing, 14�7

UUIC_{for ALL-IN-1 manager’s VMS account,}

13�34 for the transfer user accounts, 13�35 Upgrade installation

modi�cations for VTX, 14�13 Users

number of simultaneous, 13�16

VAXcluster

Local Area, 1�19 running ALL-IN-1, 1�16, 1�17 VAX DATATRIEVE, 1�8

integrating with, 1�11 VAX DECpage, 1�9 VAX FMS, A�3 VAX RALLY, 1�9

Index�4

VAX TEAMDATA, 1�9 VAX VTX, 1�9 VMS required version, 1�6 VMSINSTAL, 1�1, 3�1, 4�2, 5�2, 6�2,

7�2, 8�2, 9�2, 10�2, 11�2, 12�2 invoking, 13�1 VMSmail Gateway

con�guring, 14�11 VMS user name

for ALL-IN-1 manager’s account,

13�31, 13�32 VTX modi�cations for, 14�13

Warning messages, 3�2, 4�3, 5�3, 6�3,

7�3, 8�3, 9�3, 10�3, 11�2, 12�2 WPS-PLUS

incorporating, 13�13 integrating, 1�14 WPS-PLUS/VMS converting documents to ALL-IN-1,

14�18 Index�5