dt AV-U721J-TEBefore You Install VAX ACMS Version 3.2This package contains the VAX ACMS Version 3.2 software, installation instructions,

and user documentation.Follow these steps to install VAX ACMS Version 3.2 on your VMS operating system: 1. Read the Bill of Materials enclosed in the transparent plastic envelope. Check to determine that all listed items are in your kit. If any items are missing, contact your Digital representative.

2. Make sure that you have VMS Version 5.4-1 or higher installed on your system. 3. If you are planning to install the ACMS development kit, make sure that CDD/Plus Version 4.2A or higher is installed on your system.

4. If you plan to use DECforms with VAX ACMS, make sure that DECforms Version 1.3 or higher is installed on your system.

5. If you plan to use LSE with VAX ACMS, make sure that LSE Version 2.3 or higher is installed on your system.

6. If you plan to use TEAMDATA with VAX ACMS, make sure that TEAMDATA Version 1.3 or higher is installed on your system.The ACMS documentation set has been signi�cantly improved and reorganized in Version 3.2. Use the following guidelines to organize your documentation into the correct binder sizes (if you are updating an existing documentation set, use two of your existing 2 inch binders and two of your existing

2 12 inch binders): Volume 1

2 12 inch binder Volume 2A 2 inch binder Volume 2B 2 inch binder Volume 2C 2 inch binder Volume 3 2^{12} inch binder TP Case Study 2^{12} inch binderThe System Support Addendum (SSA) contains a complete list of the products that

are compatible with this version of VAX ACMS. The SSA is part of the Software Product Description (SPD).' Digital Equipment Corporation. 1991. All rights reserved.