F F

System

Support

Addendum

FPRODUCT NAME:

FVAX

BASIC,

Version

3.4SSA25.36.20-A

FHARDWARE REQUIREMENTS

FThese counts refer to the disk space required on the

system disk. The sizes are approximate; actual sizes may

FProcessors Supported

Fvary depending on the user’s system environment, con-

figuration, and software options.

VAX:

VAX 6000 Model 200 Series, VAX 6000 Model

300 Series, VAX 6000 Model 400 Series

FMemory Requirements for DECwindows Support:

FThe minimum supported memory for this application run-

VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX ning in a standalone DECwindows environment with both

8500, VAX 8530, VAX 8550, VAX 8600, VAX the client and server executing on that same system is

8650, VAX 8700, VAX 8800, VAX 8810, VAX

8 MB.

8820, VAX 8830, VAX 8840, VAX 8842, VAX

8974, VAX 8978

FOPTIONAL HARDWARE

FVAX-11/730, VAX-11/750, VAX-11/780, VAX-11/

Floating point intensive applications should be run on

785configurations with the appropriate hardware support for the floating point data types being used. Consult the base

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX operating system SPD for the Floating Point Accelerator

3100, MicroVAX 3300, MicroVAX 3400, or other floating point hardware appropriate for your

MicroVAX 3500, MicroVAX 3600, configuration.

MicroVAX 3800, MicroVAX 3900

FCLUSTER ENVIRONMENT

FVAXstation:

VAXstation II, VAXstation 2000,

VAXstation 3100 Series, VAXstation 3200,

This layered product is fully supported when installed on

VAXstation 3500, VAXstation 3520, any valid and licensed VAXcluster* configuration without

VAXstation 3540 restrictions. The

Fsections

of this product’s Software Product Description and

VAXserver:

VAXserver 3100 VAXserver 3300,

System Support Addendum detail any special hardware

VAXserver 3400, VAXserver 3500, required by this product.

VAXserver 3600, VAXserver 3602,

VAXserver 3800, VAXserver 3900,

*V5.x VAXcluster configurations are fully described in

VAXserver 6000-210, VAXserver 6000- the VAXcluster Software Product Description

310, VAXserver 6000-410, VAXserver

(29.78.xx) and include CI, Ethernet and Mixed

6000-420

Interconnect configurations.

FSOFTWARE REQUIREMENTS

FProcessors Not Supported

For Systems Using Terminals: (No DECwindows

FVAX-11/725, VAX-11/782, MicroVAX I,

FInterface):

FVAXstation I, VAXstation 8000

VMS Operating System V5.0 - V5.3

FProcessors Restrictions

For Workstations Running VWS:

FA TK50 Tape Drive is required for standalone MicroVAX

F�VMS Operating System V5.0 - V5.3

2000 and VAXstation 2000 systems.

F�VMS Workstation Software V4.2

FBlock Space Requirements (Block Cluster Size = 1):

For Workstations Running DECwindows:

FDisk space required during installation:

6,800 blocks

F�VMS Operating System V5.1 - V5.3 (and necessary

(3.5M bytes) components of VMS DECwindows)

Disk space required for use (permanent):

VAX BASIC supports a DECwindows compiler interface

6,600 blocks for compile qualifier selection on workstations. This inter-

(3.4M bytes) face is accessible from FileView.

FMarch

1990

AE-LT32D-TE dt FVAX BASIC,

Version

3.4SSA25.36.20-A

FThis product may run in either of the following ways:

F�VAX CDD/Plus V4.1 on VMS Operating System V5.0 -

V5.1

F�Stand-alone execution

F� running the X11 display

F�VAX CDD/Plus V4.1A on VMS Operating System V5.2

server and the client application on the same

- V5.3 machine.

To use VAX BASIC graphics statements:

F�Remote execution

F�- running the X11 display server

and the client application on different machines.

F�DEC GKS for VMS V4.0 Development or Run-time

License

VMS DECwindows is part of the VMS Operating System

Required to use the VAX Language-Sensitive Editor:

but must be installed separately. Installation of VMS

DECwindows gives you the option to install any or all of

F�VMS Operating System V5.1 - V5.3

the following three components:

F�VAX Language-Sensitive Editor V3.0

F�VMS DECwindows Compute Server (Base kit; in-

Required to fully use the /ANALYSIS__DATA qualifier:

cludes runtime support)

F�VMS Operating System V5.2 - V5.3

F�VMS DECwindows Device Support

F�VAX Source Code Analyzer V2.0

F�VMS DECwindows Programming Support

Required to fully use the /DESIGN qualifier:

For stand-alone execution, the following DECwindows components must be installed on the machine:

F�VMS DECwindows Compute Server (runtime support)

Please note the following restriction concerning the use of the /ANALYSIS__DATA and /DESIGN qualifiers with

VAX BASIC V3.4:

For remote execution, the following DECwindows components must be installed on the machines:

F�To load the analysis data files created by the /

ANALYSIS__DATA qualifier into a VAX Source Code

FServer Machine

FAnalyzer (SCA) library, you must use VAX Source

Code Analyzer V2.0.

F�VMS DECwindows Compute Server

F�To use the /DESIGN qualifier, you must have VAX

Language-Sensitive Editor (LSE) V3.0 installed on your system.

FClient Machine

FVAX Source Code Analyzer (SCA) V2.0 and VAX

Language-Sensitive Editor (LSE) V3.0 are available individually or in the VAXset Package R9.

FGROWTH CONSIDERATIONS

FVMS Tailoring

FThe minimum hardware/software requirements for any

future version of this product may be different than the

For VMS V5.x, the following VMS classes are required minimum requirements for the current version.

for full functionality of this layered product:

FDISTRIBUTION MEDIA

F�VMS Required Saveset

Tape:

9-track 1600 BPI Magtape (PE), TK50 Streaming

F�Programming Support

Tape

For more information on VMS classes and tailoring, refer

This product is also available as part of the VMS to the VMS Operating System Software Product

Consolidated Software Distribution on CDROM.

Description (SPD 25.01.xx).

FORDERING INFORMATION

OPTIONAL SOFTWARE

FSoftware Licenses: QL-095A*-**

To use %INCLUDE %FROM %CDD or the %REPORT

Software Media: QA-095A*-**

%DEPENDENCY directives and the

/Software Documentation: QA-095AA-GZ

DEPENDENCY__DATA qualifier:

Software Product Services: QT-095A*-** F2 FVAX BASIC,

Version

3.4SSA25.36.20-A

F*Denotes variant fields. For additional information on

The above information is valid at time of release. Please available licenses, services and media, refer to the contact your local Digital office for the most up-to-date appropriate price book.

information.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� DECwindows, Ethernet, MicroVAX, VAX, VAXcluster, VAXserver, VAXset, VAXstation, and VMS are trademarks of Digital Equipment Corporation. F3