F F

System

Support

Addendum

FPRODUCT NAME:

FDECdx/VMS,

Version

1.2SSA26.36.05-A

FHARDWARE REQUIREMENTS OPTIONAL HARDWARE

FProcessors Supported

FNone

VAX:

VAX 6210, VAX 6220, VAX 6230, VAX 6240,

FCLUSTER ENVIRONMENT

FVAX 6310, VAX 6312, VAX 6320, VAX 6330,

VAX 6333, VAX 6340, VAX 6350, VAX 6360

This layered product is fully supported when installed on

VAX 8200, VAX 8250, VAX 8300, VAX 8350, any valid and licensed VAXcluster* configuration without re-

VAX 8500, VAX 8530, VAX 8550, VAX 8600, strictions. The HARDWARE REQUIREMENTS sections of

VAX 8650, VAX 8700, VAX 8800, VAX 8810, this product’s Software Product Description and System

VAX 8820, VAX 8830, VAX 8840, VAX 8842,

Support Addendum detail any special hardware required by

VAX 8974, VAX 8978 this product.

VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/

*V5.x VAXcluster configurations are fully described in the

780VAXcluster Software Product Description (29.78.xx) and

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX include CI, Ethernet and Mixed Interconnect

3300/3400, MicroVAX 3500, MicroVAX 3600 configurations.

VAXstation:

VAXstation II, VAXstation 2000, VAXstation

FSOFTWARE REQUIREMENTS

F3100, VAXstation 3200, VAXstation 3500,

VAXstation 8000

VMS Operating System V4.7 - V5.0

VAXserver:

VAXserver 3300, VAXserver 3400,

MicroVMS Operating System V4.7

VAXserver 3500, VAXserver 3600,

VAXserver 3602, VAXserver 6210/6220,

DECmate II/III WPS, Version 2.0 at a minimum of V2.0 (with

VAXserver 6310/6320 communications software activated)

FProcessors Not Supported

VMS Tailoring

FVAXstation I, VAX-11/782, MicroVAX I

For VMS 5.x systems, the following VMS classes are re-

VMS system must also have an available local or remote quired for full functionality of this layered product:

serial full duplex asynchronous terminal line supported by the operating system.

F�VMS Required Saveset

Any valid DECmate II, III, with WPS-8 communication option

F�Secure User’s Environment

enabled. Each additional DECmate system simultaneously connected to the host requires its own line.

F�Utilities

FBlock Space Requirements (Block Cluster Size = 1):

FFor more information on VMS classes and tailoring, refer to

the VMS Operating System Software Product Description

Disk space required for installation:

(SPD 25.01.xx).

3,650 blocks

(1868.8K bytes)

FMicroVMS Tailoring

FDisk space required for use (permanent):

For MicroVMS 4.x systems, the following components of

500 blocks

MicroVMS are required for full functionality of this layered

(256K bytes) product:

These counts refer to disk space required on the system disk. The sizes are approximate; actual sizes may vary de-

F�Base System

pending on the user’s system environment, configuration and software options selected.

FMay

1989

AE-MM39B-TE

FDECdx/VMS, Version

1.2SSA26.36.05-A

OPTIONAL SOFTWARE

FORDERING INFORMATION

FSoftware License: QL-708A*-**

None

Software Media: QA-708A*-**

Software Documentation: QA-708AA-GZ

FGROWTH CONSIDERATIONS

FSoftware Product Services: QT-708A*-**

The minimum hardware/software requirements for any

*Denotes variant fields. For additional information on future version of this product may be different from minimum available licenses, services and media refer to the approrequirements for the current version.

priate price book.

FDISTRIBUTION MEDIA

FThe above information is valid at time of release. Please

contact your local DIGITAL office for the most up-to-date

Disk:

RX01 Floppy Diskette information.

Tape:

TK50 Streaming Tape, TU58 DECtape II Cartridge,

May 1989

9-track 1600 BPI Magtape (PE)

AE-MM39B-TE F2