F F

System

Support

Addendum

FPRODUCT NAME:

FDEC GKS forVMS,

Version

4.1SSA26.20.09-A

FHARDWARE REQUIREMENTS

FVT330 with black and white monitor

FProcessors Supported

FVT340 with color monitor

VAX:

VAX 6000 Model 200 Series, VAX 6000 Model

Tektronix

F� 4014 with enhanced graphics module (Option

300 Series, VAX 6000 Model 400 Series

34) or equivalent

VAX 8200, VAX 8250, VAX 8300, VAX 8350,

FNote:

FThe emulation of a Tektronix 4014 is not sup-

VAX 8500, VAX 8530, VAX 8550, VAX 8600, ported on any hardware.

VAX 8650, VAX 8700, VAX 8800, VAX 8810,

Tektronix 4107 terminal

VAX 8820, VAX 8830, VAX 8840, VAX 8842,

VAX 8974, VAX 8978

Tektronix 4207 terminal

VAX-11/730, VAX-11/750, VAX-11/780, VAX-

Tektronix 4128 terminal

11/785

Tektronix 4129 terminal

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

3100, MicroVAX 3300, MicroVAX 3400,

VAXstation II, VAXstation II/GPX

MicroVAX 3500, MicroVAX 3600, MicroVAX

3800, MicroVAX 3900

VAXstation 2000, VAXstation 3000 series

VAXstation:

VAXstation II, VAXstation 2000, VAXstation

FBlock Space Requirements (Block Cluster Size = 1):

F3100 Series, VAXstation 3200, VAXstation

FFull DEC GKS Kit

F3500, VAXstation 3520, VAXstation 3540,

Disk space required forinstallation:

10,300 blocks

VAXserver:

VAXserver 3100, VAXserver 3300,

(5.3M bytes)

VAXserver 3400, VAXserver 3500,

VAXserver 3600, VAXserver 3602,

Disk space required for use (permanent):

VAXserver 3800, VAXserver 3900, amaximum of9,600

VAXserver 6000-210, VAXserver 6000-310,

(4.9M

VAXserver 6000-410, VAXserver 6000-420 which may be less depending on the options selected

FProcessors Not Supported

Fduring installation.

MicroVAX I, VAXstation I, VAXstation 8000, VAX-11/725,

FDEC GKS Run-Time Kit

FVAX-11/782

5,600

FProcessor Restriction

F(2.9M

A TK50 Tape Drive is required for standalone MicroVAX

2000 and VAXstation 2000 systems.

of5,000

FTerminals

F(2.6M

One of the following devices is required:

during installation.

VT125 with black and white or optional color monitor

(ReGIS)

These block counts refer to the disk space required on the system disk. The sizes are approximate; actual sizes

VT240 with black and white monitor (ReGIS, Tek 4014) may vary depending on the user’s system environment,

VT241 with color monitor (ReGIS, Tek 4014) configuration, and software options selected.

F__________________

F� Tektronix is a registered trademark of Tektronix Incorporated.

F� PostScript is a registered trademark of Adobe Systems, Inc.

F� LaserWriter is a trademark of Apple Computer, Inc.

F� HPGL is a trademark of Hewlett-Packard Company.

F� MPS-2000 is a trademark of Lasergraphics.

FMarch

1990

AE-LT69C-TE dt FDEC GKS forVMS,

Version

4.1SSA26.20.09-A

FMemory Requirements for DECwindows Support

F*V5.x VAXcluster configurations are fully described in the VAXcluster Software Product Description

The minimum supported memory for this application run-

(29.78.xx) and include CI, Ethernet, and Mixed ning in a standalone DECwindows environment with both

Interconnect configurations.

the client and server executing on that same system is

5MB.

FSOFTWARE REQUIREMENTS*

OPTIONAL HARDWARE

FFor Systems Using Terminals (No DECwindows

Interface):

FDEC GKS also supports a variety of hardcopy output

devices and devices which are strictly compatible.

VMS Operating System V5.1 - V5.3

Hardcopy devices supported by DEC GKS are:

FFor Workstations Running VWS:

Compatible Sixel Devices

FVMS Operating System V5.1 - V5.3

F�Digital LN03 PLUS Laser Printer

VMS Workstation Software V4.0 - V4.1

F�LN03 with LN03S-UA upgrade kit

For Workstations Running DECwindows:

F�A34 with graphics option

VMS Operating System V5.1 - V5.3 (and the necessary

F�LA100

components of VMS DECwindows)

F�LA75

This product may run in either of the following ways:

F�LA50 (restricted to a 2:1 aspect ratio)

F�Standalone execution - Running the X11 display

server and the client application on the same

F�LA210

machines.

F�Tektronix 4611 hardcopy unit when connected to the

F�Remote Execution - Running the X11 display server

Tektronix 4014 computer display terminal.

and the client applicaton on different machines.

FCompatible Hewlett Packard Graphics Language

FVMS DECwindows is a part of the VMS Operating

F(HPGL

F�) Devices:

FSystem but must be installed separately. Installation of

the VMS DECwindows gives the user the option of in-

F�Digital LVP16 pen plotter

stalling any of the following three components:

F�HP7475 Hewlett Packard Pen Plotter

F�VMS DECwindows Base kit (Runtime Support)

F�HP7550 Hewlett Packard Pen Plotter

F�VMS DECwindows Device support

F�HP7580 Hewlett Packard Pen Plotter

F�VMS DECwindows Programming Language support

F�HP7585 Hewlett Packard Pen Plotter

For standalone execution, the following DECwindows

FFilm Recorders

Fcomponents must be installed on the machine.

F�Lasergraphic MPS-2000

F� Film Recorder

FInk Jet Plotters

F�Digital LJ250 Companion Color Printer

For remote execution, the following DECwindows components must be installed on the machines:

F�Digital LCG01 Color Ink Jet Plotter (ReGIS)

FServer Machine

FCompatible PostScript

F� Devices

FVMS DECwindows Base Kit

F�Apple LaserWriter

F�(Runtime support)

F�Apple LaserWriter +

VMS DECwindows Device support

F�LPS40 Laser Printer

Language support

F�LN03R ScriptPrinter Laser Printer

FClient Machine

CLUSTER ENVIRONMENT

(Runtime support)

This layered product is fully supported when installed on an valid and licensed VAXcluster* configuration without

Language Support restrictions. The

FHARDWARE

FREQUIREMENTS

F sections

of this product’s Software Product Description and

For the development of application programs that use

System Support Addendum detail any special hardware

DEC GKS under VMS, one of the DEC GKS supported required by this product.

languages is also required. F2 FDEC GKS forVMS,

Version

4.1SSA26.20.09-A

FVMS Tailoring

FDISTRIBUTION MEDIA

FFor VMS V5.x systems, the following VMS classes are

Tape:

9-track 1600 BPI Magtape (PE), TK50 required for full functionality of this layered product:

Streaming Tape

F�VMS Required Saveset

This product is also available as part of the VMS

Consolidated Software Distribution on CDROM.

F�Network Support

F�Programming Support

FORDERING INFORMATION

OPTIONAL SOFTWARE

FDevelopment System

FVAX FORTRAN V5.4

Software Licenses: QL-810A*-**

Software Media: QA-810A*-**

VAX Ada V2.1

Software Documentation: QA-810AA-GZ

VAX PASCAL V4.0

Software Product Services: QT-810A*-**

VAX C V3.1

FRun-Time Option

FVAX PL/I V3.3

Software Licenses: QL-811A*-**

Software Media: QA-811A*-**

VAX BASIC V3.3

Software Product Services: QT-811A*-**

VAX COBOL V4.3

*Denotes variant fields. For additional information on

VAX BLISS-32 Implementation Language V4.6 available licenses, services and media, refer to the appropriate price book.

FGROWTH CONSIDERATIONS

FThe above information is valid at time of release. Please

The minimum hardware/software requirements for any contact your local Digital office for the most up-to-date future version of this product may be different from the information.

minimum requirements of the current version.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� VAX, VMS, MicroVAX, VAXstation, VAXserver, VAXcluster, DECwindows, DEC GKS, ReGIS, VT, LN03, LA100, LA75, LA50, LA210, LVP16, LPS40

and LN03R are trademarks of Digital Equipment Corporation. F3