dtDEC GKS Version 4.1 Patch for ReGIS Devices

AV�NZ77A�TE

Dear Customer,

This patch �xes a problem that causes DEC GKS Version 4.1 input functions not to work on VT125, VT240, and VT340 (without a mouse) devices. Without this patch, programs that use input through these devices may hang.

Apply this patch to a DEC GKS Version 4.1 image only. The date on the DEC GKS Version 4.1 image should be 28-FEB-1990.

To apply this patch, copy VAXGFX$REGIS_DEV_HANDLER.EXE from SYS$LIBRARY: to a work directory. Execute the following commands:

$ PATCH VAXGFX$REGIS_DEV_HANDLER.EXE RETURN
PATCH > SET ECO 1 RETURN
PATCH > DELETE/INSTRUCTION 0000F1A6=’BEQL 0000F1EA’ RETURN
PATCH > REPLACE/INSTRUCTION 0F1F4 RETURN
OLD > ’BRW 0000F738’ RETURN
OLD > EXIT RETURN
NEW > ’BRW 0000F3DC’ RETURN
NEW > EXIT RETURN
PATCH > UPDATE RETURN
PATCH > EXIT RETURN
$

Test the result by de�ning the logical name VAXGFX$REGIS_DEV_HANDLER to point to your new copy, as follows:

$ DEFINE vaxgfx$regis_dev_handler $disk:[user]vaxgfx$regis_dev_handler.exe

You should attempt to run a GKS program that uses VT125, VT240, or VT340 (without a mouse) input. If the program runs properly, the patch was successful. If it does not run properly, contact your local support center.

If the patch was successful, copy the patched DEC GKS Version 4.1 image back to SYS$LIBRARY:. Use INSTALL to replace the existing copy, as follows:

$ INSTALL RETURN
INSTALL > REPLACE SYS$LIBRARY:vaxgfx$regis_dev_handler.exe RETURN
INSTALL > EXIT RETURN

'Digital Equipment Corporation. 1990. All Rights Reserved. 1