F F

System

Support

Addendum

FPRODUCT NAME:

FDECdecision,

Version

1.1SSA25.G2.01-A

FHARDWARE REQUIREMENTS

FBlock Space Requirements (Block Cluster Size = 1):

Processors Supported as Clients Only

With Rdb/VMS

FVAX:

VAX 6000 Model 200 Series, VAX 6000 Model

Disk space required for installation:

300 Series, VAX 6000 Model 400 Series

48,500 blocks

VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX

(25.0M bytes)

8500, VAX 8530, VAX 8550, VAX 8600, VAX

Disk space required for use (permanent):

8650, VAX 8700, VAX 8800, VAX 8810, VAX

42,500 blocks

8820, VAX 8830, VAX 8840, VAX 8842, VAX

(22.0M bytes)

8974, VAX 8978

FWithout Rdb/VMS

FVAX-11/730, VAX-11/750, VAX-11/780, VAX-11/

785Disk space required for installation:

25,500 blocks

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

(13.0M bytes)

3100, MicroVAX 3300, MicroVAX 3400,

MicroVAX 3500, MicroVAX 3600,

MicroVAX 3800, MicroVAX 3900

24,500 blocks

(12.5M bytes)

FProcessors Supported as Clients or Servers

FThese counts refer to the disk space required on the

VAXstation:

VAXstation II, VAXstation 2000, system disk. The sizes are approximate; actual sizes may

VAXstation 3100 Series, VAXstation 3200, vary depending on the user’s system environment, con-

VAXstation 3500, VAXstation 3520, figuration, and software options.

VAXstation 3540

FMemory Requirements

FVAXserver:

VAXserver 3100, VAXserver 3300,

VAXserver 3400, VAXserver 3500,

The minimum supported memory for this application run-

VAXserver 3600, VAXserver 3602, ning in a standalone DECwindows environment with both

VAXserver 3800, VAXserver 3900, the client and server executing on that same system is

VAXserver 6000-210, VAXserver 6000-

8 MB.

310, VAXserver 6000-410, VAXserver

6000-420

The performance and memory usage of DECwindows applications are particularly sensitive to system configura-

FProcessor Restriction

Ftion. Less memory may be required on the client system

(the system where the software is installed and executed)

A TK50 Tape Drive is required for standalone MicroVAX if the server (the component that displays the application)

2000 and VAXstation 2000 systems.

resides on another system. More memory may be re-

FProcessors Not Supported

Fquired on a system with several applications running or

where it may be desirable to improve the performance of

VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, an application.

VAXstation 8000

The minimum memory supported is 8 MB. However, the

FOther Hardware Requirements

Fuse of this software in conjunction with increased

Minimum disk required: One RD54 or two RZ23 disks memory capability improves performance. The memory size suggested for most typical hardware configurations

Terminals: VT100 is at least 12 MB.

F__________________

F� IBM is a registered trademark of International Business Machines Corporation.

F� PostScript is a registered trademark of Adobe systems, Inc.

F� HPGL is a trademark of Hewlett-Packard Corporation.

F� IDMS is a trademark of Cullinet Software, Inc.

F� Lotus 1-2-3 is a trademark of Lotus Development Corporation.

FApril

1990

AE-NE62B-TE dt FDECdecision, Version

1.1SSA25.G2.01-A

OPTIONAL HARDWARE

FFor remote execution, the following DECwindows compo-

nents must be installed on the machine:

DECdecision text files can be printed on any Digital text printer.

FServer Machine

FDECdecision PostScript

F� files can be printed using any

VMS DECwindows Compute Server

Digital PostScript printer (ScriptPrinter LN03R,

VMS DECwindows Device Support

PrintServer 20, PrintServer 40, or the PrintServer 40 Plus

FClient Machine

Flaser printer).

DECchart produces both monochrome and color

PostScript. Monochrome PostScript can be printed using

Rdb/VMS V3.1A Runtime Kit is included with any Digital PostScript printer (ScriptPrinter LN03R,

DECdecision. If you upgrade to a future version of VMS

PrintServer 20, PrintServer 40, and the PrintServer 40 that does not support Rdb/VMS V3.1A, it is necessary to

Plus Laser Printer). If the DECprint Utility for PostScript install the latest version of Rdb/VMS. (The Rdb/VMS to Sixel Printing for VMS is installed, then DECchart

Runtime license is packaged with VMS and therefore,

PostScript output (either color or monochrome) can be does not require a separate license.)

printed on the Digital LJ250 Companion Color Printer.

FVMS Tailoring

FCLUSTER ENVIRONMENT

FFor VMS V5.x systems, the following VMS class is re-

This layered product is fully supported when installed on quired for full functionality of this layered product:

any valid and licensed VAXcluster* configuration without

F�VMS Required Saveset

restrictions. The

FHARDWARE REQUIREMENTS

Fsections

of this product’s Software Product Description and

Optional:

Network Support (Required for Client/Server

System Support Addendum detail any special hardware split) required by this product.

For more information on VMS classes and tailoring, refer

*V5.x VAXcluster configurations are fully described in to the VMS Operating System Software Product the VAXcluster Software Product Description

Description (SPD 25.01.xx).

(29.78.xx) and include CI, Ethernet, and Mixed

FOPTIONAL SOFTWARE

FInterconnect configurations.

DECwrite for VMS V1.0

FSOFTWARE REQUIREMENTS

FCDA Converter Library for VMS V1.0 in conjunction with

FFor Workstations Running DECwindows

FDEC GKS for VMS V4.0 (For additional converters and

VMS Operating System V5.3-1 (and necessary compocolor hardcopy support) nents of VMS DECwindows)

VAX DATATRIEVE V5.0 (For access to DTR domains,

FFor PC DECwindows Interoperability

FDBMS, and RMS)

DECnet PCSA Client for DOS V3.0 - PC DECwindows

VIDA for DB2 V1.0 (For access to IBM

F� data)

Display Facility V2.0 (SPD 55.07.xx) and VMS Services

VIDA with IDMS/R V2.2 (For access to IBM data) for PCs V3.0 (SPD 30.50.xx). For more information, refer to the DECwindows Interoperability Compliance Matrix

FGROWTH CONSIDERATIONS

FSoftware Product Description (SPD 01.25.xx).

The minimum hardware/software requirements for any

This product may run in either of the following ways:

future version of this product may be different from the minimum requirements for the current version.

Stand-alone execution - Running the X11 display server and the client application on the same machine.

FDISTRIBUTION MEDIA

FRemote execution - Running the X11 display server and

Tape:

9-track 1600 BPI Magtape (PE), TK50 Streaming the client application on different machines.

Tape

VMS DECwindows is part of the VMS Operating System

This product is also available as part of the VMS but must be installed separately. Installation of VMS

Consolidated Software Distribution on CDROM.

DECwindows gives you the option to install any or all of

The software documentation for this product is also availthe following three components:

able as part of the VMS Online Documentation Library on

VMS DECwindows Compute Server (Base kit; includes

CDROM.

runtime support)

FORDERING INFORMATION

FVMS DECwindows Device Support

Software License: QL-VW3A*-**

VMS DECwindows Programming Support

Software Media: QA-VW3A*-**

Software Documentation: QA-VW3AA-GZ

For stand-alone execution, the following DECwindows

Software Product Services: QT-VW3A*-** components must be installed on the machine:

*Denotes variant fields. For additional information on available licenses, services and media, refer to the appropriate price book. F2 FDECdecision, Version

1.1SSA25.G2.01-A

FThe above information is valid at time of release. Please

contact your local Digital office for the most up-to-date information.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� DATATRIEVE, DBMS, DEC GKS, DECchart, DECdecision, DECprint, DECwindows, DDIF, LN03R, LVP16, PrintServer 20, PrintServer 40,

PrintServer 40 Plus, RMS, Rdb/VMS, VAX, VAXserver, VAXstation, VIDA and VMS are trademarks of Digital Equipment Corporation. F3