F F

Software

Product

Description

FPRODUCT NAME:

FVAX

Distributed

FileService,

SPD28.78.02

Version

1.2FDESCRIPTION

FThe features of VAX Distributed File Service software

are:The VAX Distributed File Service (DFS) is a DECnet-VAX

F�High performance access to remote disks

layered product that provides VMS users with the ability to use remote VAX disks as if they were directly attached

F�Applications require no modifications to use remote

to the local VAX system.

disks, since the disks appear to be local

DFS provides users and applications with transparent,

F�Uses less CPU resources than standard DECnet-VAX

high performance file access while using less CPU refile access sources than standard DECnet-VAX file access.

F�Supports all VMS file types

DFS systems can act as "servers" or "clients" or both.

F�Supports the following VMS file operations:

Servers make file resources available to clients. The re-

-Shared access (read) sources can vary in scope from a master file directory with all of the subordinate directories and files on a disk

-Exclusive access (read & write) volume to an individual file. The DFS server gives the

-All VMS Directory operations, including the creation resource a unique name and registers it with the VAX and deletion of directories

Distributed Name Service (DNS).

-Virtual I/O

The DFS client can then use the resource by means of the DFS MOUNT command. This command specifies the

-Mapped I/O

DNS name by which the resource was registered,

F�DFS access is transparent to most of the standard VMS

enables communication between the client and the

DCL commands (those commands which neither maserver, and creates a pseudodevice on the client system.

nipulate identifiers nor use logical, physical or write-

This pseudodevice makes the remote resouce appear to shared I/O).

the local system like a local disk. Users can then perform

F�Uses the VAX Distributed Name Service to provide lo-

operations on the pseudodevice, and DFS handles all of cation independence of data.

the network access and translation.

F�DFS can be used in any DECnet environment. Both

VAX Distributed Name Service is a prerequisite product.

Local Area Networks and Wide Area Networks are sup-

In order to use DFS, there must be at least one DNS ported. DFS is optimized for line speeds of 56,000 bits server in the network. DNS allows the name of the reper second and above.

source to be independent of its physical location on the network. DFS systems throughout the network can con-

F�File security provided through standard VMS proxy

tinue accessing a resource even if the resource location mechanism. The system manager on the server conis changed.

trols all file access.

A DFS license is required on each VAX server node that

F�Optional end-to-end checksum provided to guard

registers available directories or files and on each client against network faults.

node that uses the directories or files.

F�Management utility allows the user to control DFS com-

FFeatures

Fponents and to display statistical and error information.

FJuly1989

AE-KS64C-TE

FVAX Distributed

FileService,

SPD28.78.02

Version

1.2FRestrictions

FSOFTWARE LICENSING

F�Files opened for write are opened exclusively

This software is furnished under the licensing provisions of DIGITAL’s Standard Terms and Conditions. For more

F�Logical I/O is not supported

information about DIGITAL’s licensing terms and policies,

F�Installed files are not supported

contact your local DIGITAL office.

FHARDWARE REQUIREMENTS

LICENSE MANAGEMENT FACILITY SUPPORT

FVAX, MicroVAX, or VAXstation configuration as specified

This layered product supports the VMS License in the System Support Addendum (SSA 28.78.02-x)

Management Facility.

FSOFTWARE REQUIREMENTS*

FLicense units for this product are allocated on a CPU-

At least one DNS server must be installed and accessible capacity basis.

in the DECnet network. Refer to VAX Distributed Name

Service (SPD 28.79.xx) for further recommendations on

For more information on the License Management

DNS.

Facility, refer to the VMS Operating System Software

Product Description (SPD 25.01.xx) or the VMS

VMS or MicroVMS Operating System

Operating System documentation set.

DECnet-VAX

For more information on DIGITAL’s licensing policies,

*Refer to the System Support Addendum for availability and required versions of prerequisite/optional software

(SSA 28.78.01-x).

FSOFTWARE PRODUCT SERVICES

ORDERING INFORMATION

FA variety of service options are available. For more infor-

mation on these or other services, please contact your

Software Licenses: QL-VEQA*-** local DIGITAL office.

Software Media: QA-VEQA*-**

Software Documentation: QA-VEQAA-GZ

FSOFTWARE WARRANTY

FSoftware Product Services: QT-VEQA*-**

*Denotes variant fields. For additional information on

Warranty for this software product is provided by available licenses, services and media, refer to the ap-

DIGITAL with the purchase of a license for the product as propriate price book.

defined in the Software Warranty Addendum of this SPD. F2