F F

System

Support

Addendum

FPRODUCT NAME:

FMIRA

High

Availability

Management

SSA31.86.00-A

Software forVMS,

Version

1.0FHARDWARE REQUIREMENTS

OPTIONAL HARDWARE

FProcessors Supported

FThe device error detection process is limited to devices

where the driver uses the ON/OFF bit or the ERRCNT

MicroVAX:

MicroVAX 3400, MicroVAX 3800 error counter to signal/log that an error happened for this device.

VAXserver:

VAXserver 3400, VAXserver 3800

FCLUSTER ENVIRONMENT

FProcessors Not Supported

FMicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

This layered product is fully supported when installed on

3100, MicroVAX 3300, MicroVAX 3500, any valid and licensed VAXcluster* configuration without

MicroVAX 3600, MicroVAX 3900 restrictions. The

FHARDWARE REQUIREMENTS

Fsections

of this product’s Software Product Description and

VAXserver 3100, VAXserver 3300,

System Support Addendum detail any special hardware

VAXserver 3500, VAXserver 3600, required by this product.

VAXserver 3602, VAXserver 3900,

VAXserver 6000-210, VAXserver 6000-

*V5.x VAXcluster configurations are fully described in the

310, VAXserver 6000-410, VAXserver

VAXcluster Software Product Description (29.78.xx) and

6000-420 include CI, Ethernet, and Mixed Interconnect configurations.

VAX or VAXstation family of processors

FSOFTWARE REQUIREMENTS

FProcessor Restrictions

FVMS Operating System V5.3

The processor must be part of any valid DV-3xMx3-xx

MIRA Applications Switch Dual-Host configuration.

VAX Ada V1.4 - V1.5 (if this product is to be accessed from applications in an ADA environment)

MIRA Applications Switch systems based on the

MicroVAX 3400 require a minimum revision of D04 for

FVMS Tailoring

Fthe M7624 CPU module.

For VMS V5.x systems, the following VMS classes are

FOther Hardware Required

Frequired for full functionality of this layered product:

The MIRA Applications Switch watchdog board (KW32) is

F�VMS Required Saveset

based on the M3108-PA module. The minumum revision level for this module is E1.

F�Programming Support

FBlock Space Requirements (Block Cluster Size = 1):

F�System Programming Support

Disk space requirements forinstallation:

4200 blocks

F�Utilities

(2151K bytes)

For more information on VMS classes and tailoring, refer

Disk space requirements for use (permanent):

to the VMS Operating System Software Product

4000 blocks, excluding event logDescription (SPD 25.01.xx).

(2048K

FGROWTH CONSIDERATIONS

FThese counts refer to the disk space required on each

system disk. The sizes are approximate; actual sizes may

The minimum hardware/software requirements for any vary depending on the user’s system environment, confuture version of this product may be different from the figuration and software options selected.

minimum requirements of the current version.

FJune

1990

AE-PBFZA-TE dt FMIRA High

Availability

Management

SSA31.86.00-A

Software forVMS,

Version

1.0DISTRIBUTION MEDIA

FSoftware Documentation: QA-YHMAA-GZ

Software Product Services: QT-YHMA*-**

Tape: TK50 Streaming Tape

*Denotes variant fields. For additional information on

This product is also available as part of the VMS available licenses, services and media refer to the ap-

Consolidated Software Distribution on CDROM.

propriate price book.

FORDERING INFORMATION

FThe above information is valid at the time of release.

Software Licenses: QL-YHMA*-**

Please contact your local Digital office for the most up-to-

Software Media: QA-YHMAA-** date information.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� VAX, VMS and MicroVAX are trademarks of Digital Equipment Corporation. F2