F F

Software

Product

Description

FPRODUCT NAME:

FDEC

IEZ11

Class

Driver forVMS,

SPD31.41.00

Version 1.0

FDESCRIPTION SOFTWARE REQUIREMENTS

FThe DEC IEZ11 Class Driver is a VMS layered product

FVMS Operating System

Fwhich is part of the IEZ11 option. The IEZ11 option in-

Refer to the System Support Addendum

F(FSSAcludes the SCSI488/D bus converter and the IEZ11

31.41.00-x) for availability and required versions of software.

prerequisite/optional software.

The DEC IEZ11 Class Driver allows an application written

FORDERING INFORMATION

Fin a higher level language or in Macro 32 to monitor,

control and interface with IEEE488 devices using VMS

Software Licenses: QL-YEHA*-**

QIO system calls. The driver adheres to the VMS SCSI

Software Media: QA-YEHAA-** device architecture.

Software Documentation: QA-YEHAA-GZ

The IEZ11 driver supports most functions of the IEx11

Software Product Services: QT-YEHA*-** driver. The majority of IEx11 applications can be con-

*Denotes variant fields. For additional information on verted to run on the IEZ11 with only minor modifications.

available licenses, services and media, refer to the

Installation Test and Demo Software (ITADS) is included appropriate price book or contact your local Digital in the software kit. It provides a means of verifying that office.

the IEZ11 hardware and software are functioning properly

FNote:

FThe software can only be ordered in conjunction

and can be used as an application development and with the SCSI488/D bus converter. Refer to the debug tool.

systems and options catalog for IEZ11-** ordering

The SCSI488/D bus converter is an external box which information.

provides the capability of connecting an IEEE488 bus to the SCSI bus of a VAXstation or a MicroVAX. The

FSOFTWARE LICENSING

FSCSI488/D bus converter, software and license are or-

This Software is furnished under the licensing provisions dered under a single part number.

of Digital Equipment Corporation’s Standard Terms and

The maximum number of SCSI488/D bus converters that

Conditions. For more information about Digital’s licensing can be supported on a single SCSI bus is 6. This number terms and policies, contact your local Digital office.

is reduced by 1 for every I/O unit that resides on the

FLICENSE MANAGEMENT FACILITY SUPPORT

FSCSI bus. For example, on a VAXstation 3100 with dual

RZ23’s, one TK50 and one RD40, two IEZ11’s could be

This layered product supports the VMS License supported. As with all SCSI buses, other factors including

Management Facility.

cable length and quality can affect the actual number of

SCSI devices that can be supported.

License units for this Product are allocated on a User/

Activity basis.

The IEZ11 is supported under the VAXlab Software

Library (VSL) V1.4 (SPD 28-30-xx). VSL is a set of sub-

For more information on the License Management routine libraries for real-time data acquisition, scientific

Facility, refer to the VMS Operating System Software plotting, and data analysis.

Product Description (SPD 25.01.xx) or the License

Management Facility manual of the VMS Operating

FHARDWARE REQUIREMENTS

FSystem documentation set.

MicroVAX, VAXstation or VAXserver configuration as specified in the System Support Addendum (SSA

For more information about Digital’s licensing terms and

31.41.00-x).

policies, contact your local Digital office.

FApril

1990

AE-NU46A-TE dt FDEC IEZ11

Class

Driver forVMS,

SPD31.41.00

Version 1.0

SOFTWARE PRODUCT SERVICES

SOFTWARE WARRANTY

FA variety of service options are available from Digital. For

Warranty for this software product is provided by Digital more information, contact your local Digital office.

with the purchase of a license for the product as defined in the Software Warranty Addendum of this SPD.

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� DEC, DECstation, MicroVAX, VAX, VAXserver, VAXstation and VMS are trademarks of Digital Equipment Corporation. F2