F F

System

Support

Addendum

FPRODUCT NAME:

FVAX

DECscan VMS Software

Toolkit,

Version

2.1SSA26.98.02-B

FHARDWARE

FREQUIREMENTS

CLUSTER

FENVIRONMENT

FProcessor

FSupport

FThis layered product is fully supported when installed on

any valid and licensed VAXcluster* configuration without

VAX:

VAX 6000 Model 200 Series, VAX 6000 Model restrictions. The HARDWARE REQUIREMENTS sections

300 Series, VAX 6000 Model 400 Series, VAX of this product’s Software Product Description and

8200, VAX 8250, VAX 8300, VAX 8350, VAX

System Support Addendum detail any special hardware

8500, VAX 8530, VAX 8550, VAX 8600, VAX required by this product.

8650, VAX 8700, VAX 8800, VAX 8810, VAX

8820, VAX 8830, VAX 8840, VAX 8842, VAX

*V5.x VAXcluster configurations are fully described in the

8974, VAX 8978

VAXcluster Software Product Description (29.78.xx) and include CI, Ethernet, and Mixed Interconnect

VAX-11/750, VAX-11/780, VAX-11/785 configurations.

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

FSOFTWARE

F3300, MicroVAX 3400, MicroVAX 3500,

MicroVAX 3600, MicroVAX 3800, MicroVAX

VMS Operating System V5.0 - V5.2

3900

FVMS

FTailoring

FVAXstation:

VAXstation II, VAXstation 2000, VAXstation

3100, VAXstation 3200, VAXstation 3500,

For VMS V5.x systems, the following VMS classes are

VAXstation 8000 required for full functionality of this layered product:

FProcessors

FNotFSupported

F�VMS Required Saveset

MicroVAX I, VAXstation I, VAX-11/725, VAX-11/730,

F�Network Support

VAX-11/782, VAXserver 3500, VAXserver 3600,

F�Programming Support

VAXserver 3602

F�Secure User’s Environment

F�Utilities

FBlock

FSpace

FRequirements

F(Block

FCluster

FSize

F=F1):F�System Programming

Disk space required forinstallation:

6,600 blocks

For more information on VMS classes and tailoring, refer

(3,300K bytes) to the VMS Operating System Software Product

Description (SPD 25.01.xx).

foruse(permanent):

3,300

(1,650K

FOPTIONAL

FThese counts refer to the disk space required on the

VAX Ada V1.5 system disk. The sizes are approximate; actual sizes may

VAX BASIC V3.2 - V3.3 vary depending on the user’s system environment, con-

VAX BLISS-32 Implementation Language V4.4 - V4.5 figuration, and software options.

VAX C V2.4

FVAX FORTRAN V4.8 - V5.1

VAX PASCAL V3.7 - V3.8

The following Q-bus controller for communications to the

VAX PL/1 V3.1 - V3.2

I/O Vendor hardware is required:

VAX DECscan VMS and ELN BITBUS Drivers (VMS

F�IBQ01 DECscan (BITBUS) controller board - Supports

Driver only) V1.0 - V2.0 communications to the BITBUS compatible Honeywell

The BITBUS Starting Point RTP IOV Package V1.0 is

MicroSwitch and Phoenix INTERBUS-C

F� I/O devices.

sold by Computer Products Incorporated:

F__________________

F�INTERBUS-C is a trademark of Phoenix Limited.

FSeptember

1989

AE-LY03C-TE

FVAX DECscan VMS Software

Toolkit,

Version

2.1SSA26.98.02-B

FComputer Products Incorporated

future version of this product may be different from the

Measurement and Control Division minimum requirements for the current version.

2900 Gateway Drive

FDISTRIBUTION

FMEDIA

FPompano Beach, Florida 33069-4378

Telephone: (305) 974-5500

Disk:

RX33 Floppy Diskette

FAX: (305) 979-7371

Tape:

9-track 1600 BPI Magtape (PE), TK50 Streaming

DIGITAL does not sell nor technically support the

Tape

BITBUS Starting Point RTP IOV Package.

FORDERING

FINFORMATION

FThe Dataviews (DV-Tools and DV-Draw) package V5.0

Software Licenses: QL-VCSA*-** and V6.0 is sold by:

Software Media: QA-VCSA*-**

Software Documentation: QA-VCSAA-GZ

V.I. Corporation

Software Product Services: QT-VCSA*-**

160 Old Farm Road

Amherst, MA 01002

*Denotes variant fields. For additional information on

Telephone: (413) 253-3482 available licenses, services and media, refer to the appropriate price book.

DIGITAL does not sell nor technically support Dataviews.

The above information is valid at time of release. Please

FGROWTH

FCONSIDERATIONS

Fcontact your local DIGITAL office for the most up-to-date

The minimum hardware/software requirements for any information. F2