F F

Software

Product

Description

FPRODUCT NAME:

FVAX

PrintServer

Client

Software,

SPD27.67.04

Version

3.0FDESCRIPTION

FThe /PARAMETERS qualifier in the PRINT command is

used to pass PrintServer specific parameters to the print

The PrintServer

F� Client Software is a layered product

symbiont for processing. These parameters are as folthat enables suitably configured VMS or MicroVMS lows:

systems within a DECnet Ethernet network to access the

PrintServer 20

F�, PrintServer 40

F�, and PrintServer 40

F�Data__Type - Specifies the type of data in the print job

PlusF�.being sent to the printer. If the Data__Type is other than PostScript, the print symbiont will call one of the

The Client software consists of the following components:

supplied translators (ANSI text and Sixel Graphics,

F�A print symbiont to process print requests from one or

ReGIS, or Tektronix) to convert the data to PostScript more PrintServer printer queues.

prior to sending it to the PrintServer.

F�Distribution software to transmit the request and asso-

F�Input__Tray - Selects the printer input tray that will

ciated data over the Ethernet to a remote PrintServer supply the paper or media for this job.

via DECnet.

F�Output__Tray - Selects the printer output tray where the

F�Translators to convert ANSI Text and Sixel Graphics,

printed output will be deposited.

ReGIS, and Tektronix

F� 4010/4014 files into the

PostScript

F� language.

F�Messages - Specifies the disposition of messages gen-

erated by the print job.

F�A series of PostScript tools for creator software support.

These include a PostScript error handler, Font Metric

F�Page__Limit - Specifies the first and last logical pages

Files and Font Encoding Vectors for the ISO Latin to be printed for the job.

Alphabet Number 1 (ISO 8859/1) and DIGITAL Multinational Character Set for all of the built-in PostScript

F�Page__Orientation - Specifies the orientation of printed

fonts.

output on the page (portrait or landscape). This parameter is ignored when Data__Type is PostScript

The PrintServer Client software must be installed on each unless Number__Up is specified.

system that will be providing distributed printing services to its users via a PrintServer 20, PrintServer 40, or

F�Page__Size - Specifies the size of the logical pages

PrintServer 40 Plus.

being printed. This parameter is ignored if Data__Type is PostScript.

A system running the PrintServer Client software can transmit print requests to any PrintServer 20, PrintServer

F�Sheet__Size - Specifies the physical size of the sheets

40, or PrintServer 40 Plus on the network that is defined to be printed. This parameter will cause the appropriate in its network database. A maximum of 16 clients can input tray to be selected.

simultaneously access a PrintServer with only one client active at one time.

F�Sheet__Count - Specifies the number of times each

sheet is to be printed at the PrintServer.

VAX PrintServer Supporting Host Software (SPD

27.68.xx) is a companion product to this software.

F�Layup__Definition - Specifies the name of a file that

contains all of the page layup features (Borders,

FFeatures

FMargins, Margin Alternation, Pages per Sheet, First

Page, Page Order and Page Grid) except Number__Up.

FPrint Symbiont

F__________________ Tektronix is a registered trademark of Tektronix, Inc.

PostScript is a registered trademark of Adobe, Inc. FSeptember

1989

AE-HL88E-TE

FVAX PrintServer

Client

Software,

SPD27.67.04

Version

3.0F�Number__Up - Specifies the maximum number of

Font Encoding vectors for the ISO Latin Alphabet pages that can be printed on one side of a sheet.

Number 1 (ISO 8859/1) and DIGITAL Multinational

Character Set are provided for all of the built-in fonts.

F�Sides - Controls the number of sides printed per sheet

on the PrintServer 20. It also controls print-time condi-

FINSTALLATION

Ftional layout related to 2-sided printing when the creator

supports this feature; that is, it selects whether the

Only experienced customers should attempt installation layout of a page is simplex, duplex, or tumble.

of this software product. DIGITAL recommends that all other customers purchase DIGITAL’s Installation

The /SETUP qualifier may be used to send specified mo-

Services. These services provide for the installation of dules from a device control library to the printer. These the software product and the PrintServer 20, 40 and 40 modules may be encoded in the native data syntax of the

Plus hardware by an experienced DIGITAL Specialist.

printer (PostScript), or they may be encoded in the data syntax of the file(s), being printed (PostScript or ANSI

FCustomer Responsibilities

Fonly); the symbiont will pass the modules through the

ANSI translator if necessary.

Before installation of the software, the customer must:

The print symbiont also supplies the following accounting

F�Previously have installed all prerequisite software and

information for each print job: sheets of paper printed, hardware

Number of RMS Gets to all the user’s files in the print job and Number of QIO Writes over the network to the

F�Obtain, install and demonstrate as operational any

PrintServer.

equipment and facilities necessary to interface to

FTranslators

FDIGITAL’s communication equipment

Translator software allows users to print documents on

F�Make available for a reasonable period of time, as

the PrintServer with graphic protocols other than mutually agreed upon by DIGITAL and the customer, all

PostScript, the native language of the PrintServer 20, hardware, communication facilities and terminals that

PrintServer 40, and PrintServer 40 Plus by translating the are to be used during installation designated protocol into PostScript.

F�Supply to DIGITAL all of the information necessary for

The translators are invoked by the print symbiont at print installation of the software (e.g. as described in the time through the /PARAMETERS switch of the PRINT

PrintServer 40 Series Site Preparation Guide) command or by submission to a translator specific queue.

The translators provided convert the following data types

Installation of PrintServer Client Software will consist of into PostScript:

the following:

F�ANSI text and Sixel graphics compatible with the LN03

F�Verification that the installation information in the

excluding support for font cartridges

PrintServer Site Preparation Guide is complete for the

F�ReGIS compatible with the VT240

PrintServer 40 series of printers

F�Tektronix 4010/4014 compatible with VT240

F�Verification that a complete set of PrintServer Client

PostScript is a device-independent, page description lan-

Software media and documentation has been received guage that has the ability to describe the appearance of text, images, and graphic material on the printed page.

F�Verification that all hardware and software prerequisites

have been met and the equipment is operational

FPostScript Tools

FThe tools consist of the following:

F�Installation of the PrintServer Client Software on one

system (the PrintServer Supporting Host and

A PostScript error handler which prints the last partial

PrintServer Client Software may be installed on the page of output as well as information to help identify the same or separate system) error. This information includes the error name, the

PostScript operator that encountered the error, the oper-

F�The optional establishment of print queues for the three

and stack, and the graphics state of the machine at the supplied translators and PostScript on the PrintServer time of the error.

Client system

A series of ASCII-encoded Font Metric Files that contain

F�Modification of the VMS start-up files to automate the

information necessary for application programs to format start-up of print queues text. The Font Metric Files consist of four sections that describe different general properties of a font. These sec-

F�Modification of the DECnet databases to add the

tions include a global section that pertains to the font as

PrintServer node name and address a whole; a character metrics section that consists of information such as character widths; a kerning data section

F�Verification that the PrintServer Client Software has

that consists of information regarding different types of been correctly installed by running the Installation kerning; and a composite character section containing

Verification Program information for forming character composites such as accented letters. The kerning section and composite char-

Should a DIGITAL Specialist be required to modify the acter sections are optional and may not be present for a previously installed software parameters, a time and magiven font.

terials charge will apply. F2 FVAX PrintServer

Client

Software,

SPD27.67.04

Version

3.0HARDWARE REQUIREMENTS

SOFTWARE LICENSING

FThis software is furnished under the licensing provisions

VAX, MicroVAX or VAXstation configuration as specified of DIGITAL’s Standard Terms and Conditions. For more in the System Support Addendum (SSA 27.67.04-x).

information about DIGITAL’s licensing terms and policies,

FSOFTWARE REQUIREMENTS*

Fcontact your local DIGITAL office.

VMS Operating System or MicroVMS Operating System

The license to use this software is included with a

PrintServer. The license gives you the right to use the

DECnet-VAX software on a single CPU or equipment configuration and

VAX PrintServer Supporting Host Software the right to copy this software for use on any CPU or equipment configuration on a local area network that re-

*Refer to the System Support Addendum for availability quires access to a PrintServer 20, PrintServer 40 or and required versions of prerequisite/optional software

PrintServer 40 Plus. This includes a VAXcluster system.

(SSA 27.67.04-x).

FSOFTWARE PRODUCT SERVICES

ORDERING INFORMATION

FA variety of service options are available. For more infor-

Software Licenses: QL-797A*-** mation on these or other services, please contact your

Software Media: QA-797A*-** local DIGITAL office.

Software Documentation: QA-797AA-GZ

Software Product Services: QT-797A*-**

FSOFTWARE WARRANTY

F*Denotes variant fields. For additional information on

Warranty for this software product is provided by available licenses, services and media, refer to the ap-

DIGITAL with the purchase of a license for the product as propriate price book.

defined in the Software Warranty Addendum of this SPD.

F__________________ The DIGITAL Logo is a registered trademark of Digital Equipement Corporation.

PrintServer, PrintServer 20, PrintServer 40 and PrintServer 40 Plus are registered trademarks of Digital Equipment Corporation.

VAX, VMS, MicroVMS, MicroVAX, VAXstation, VAXserver, and DECnet-VAX are trademarks of Digital Equipment Corporation. F3