F F

System

Support

Addendum

FPRODUCT NAME:

FPBXserver,

Version

2.1SSA29.23.02-A

FHARDWARE REQUIREMENTS Other Hardware Required

FDELIX-AB

FPBX Supported

Terminals

FTelic-Alcatel OPUS 4000, Thomson 2600

Supported asynchronous terminal characteristics are as

FProcessors Supported (Load System)

Ffollows:

VAX:

VAX 6210, VAX 6220, VAX 6230, VAX 6240,

F�7 or 8 data bits

VAX 6310, VAX 6312, VAX 6320, VAX 6330,

F�1 or 2 stop bits

VAX 6333, VAX 6340, VAX 6350, VAX 6360,

VAX 8200, VAX 8250, VAX 8300, VAX 8350,

F�Parity: Even, odd, or none

VAX 8500, VAX 8530, VAX 8550, VAX 8600,

F�Speeds: 75, 300, 600, 1200, 2400, 4800, 9600, 19200

VAX 8650, VAX 8700, VAX 8800, VAX 8810, bpsVAX 8820, VAX 8830, VAX 8840, VAX 8842,

VAX 8974, VAX 8978

FDIGITAL Terminals Supported

FVAX-11/750, VAX-11/780, VAX-11/785

FVideo Terminals

FMicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

F�VT100, VT101, VT102, VT125, VT131

3300, MicroVAX 3400, MicroVAX 3500,

F�VT220, VT240, VT241

MicroVAX 3600, MicroVAX 3800,

F�VT320, VT330, VT340

MicroVAX 3900

FHardcopy Terminals (KSR Printers)

FVAXstation:

VAXstation II, VAXstation 2000,

VAXstation 3100, VAXstation 3200,

F�LA100, LA120 as KSR "...writers"

VAXstation 3500, VAXstation 3520,

FPCs

FVAXstation 3540, VAXstation 8000

F�DECmate II, III and III+

VAXserver:

VAXserver 3300, VAXserver 3400,

VAXserver 3500, VAXserver 3600,

F�Rainbow 100B, Rainbow 100+

VAXserver 3602, VAXserver 3800,

F�Professional 325/350/380

VAXserver 3900, VAXserver 6210,

VAXserver 6220, VAXserver 6310,

F�VAXmate

VAXserver 6320

FNote:

FThese PCs are supported both in VT100 emula-

tion mode and in block mode file transfer mode at

FNot Supported

Fa maximum speed of 9600 bps. Working in file

VAX-11/730, VAXstation I transfer mode must be permanently set to 8 bit characters without parity.

FProcessor Restrictions

3/Printers

FThe Load System must be connected on the same

Ethernet network using Digital Equipment Corporation

The PBXserver software support all the DIGITAL asyn-

Ethernet interface.

chronous serial (RS-232c) printers when accessed from

VMS and MicroVMS systems using XON/XOFF protocol.

A TK50 Tape Drive is required for standalone MicroVAX

FThis product is not warranted to support non-

2000 and VAXstation 2000 systems.

DIGITAL terminal devices and Personal

FProcessors Supported (Target System)

FComputers. However, those supporting VT100-like

characteristics may operate with this product. This

The Target System is the PBXserver (DELIX-AB) product does not support simultaneously 8 data bits and parity check.

FSeptember

1989

AE-LN52C-TE

FPBXserver, Version

2.1SSA29.23.02-A

Other Equipment

FService System

FTo connect to the Ethernet physical channel, the

The PBXserver software operates with all nodes which

PBXserver hardware requires both a transceiver drop support:

cable and an H4000 Transceiver, a DELNI, or DESTA.

MicroVMS Operating System V4.6 - V4.7 or

To connect to the PBX a shielded twisted-pair cable of

VMS Operating System V4.6 - V5.2 type L904 or equivalent must be furnished by the PBX

DECnet-VAX V4.6 - V5.2 manufacturer.

FVMS Tailoring

FPrinters and Terminals must be connected to the PBX

wiring by usual RS-232C plugs.

For VMS V5.x systems, the following VMS classes are required for full functionality of this layered product:

FBlock Space Requirements (Block Cluster Size = 1):

FDisk space requirements for installation:

F�VMS Required Saveset

F�Utilities

1,200 blocks

F�Networking Support

(600K bytes)

For more information on VMS classes and tailoring, refer

Disk space requirements for use (permanent):

to the VMS Operating System Software Product

1,100 blocks

Description (SPD 25.01.xx).

(550K bytes)

FMicroVMS Tailoring

FThese counts refer to the disk space required on each

system disk. The sizes are approximate; actual sizes may

For MicroVMS V4.x systems, the following VMS classes vary depending on the user’s system environment, conare required for full functionality of this layered product:

figuration and software options selected.

FCLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and licensed VAXcluster* configuration without

FGROWTH CONSIDERATIONS

Frestrictions. The HARDWARE REQUIREMENTS sections

of this product’s Software Product Description and

The minimum hardware/software requirements for any

System Support Addendum detail any special hardware future version of this product may be different from the required by this product.

minimum requirements of the current version.

*V5.x VAXcluster configurations are fully described in

FDISTRIBUTION MEDIA

Fthe VAXcluster Software Product Description

Tape:

TK50 Streaming Tape, 9-track 1600 BPI Magtape

(29.78.xx) and include CI, Ethernet and Mixed

Disk:

RX33 Floppy Diskette

Interconnect configurations.

FSOFTWARE REQUIREMENTS

FThis product is also available as part of the VMS

Consolidated Software Distribution on CDROM.

FLoad System

FORDERING INFORMATION

FThe Load System must support the Down-Line System

Loading facility of DECnet-VAX Phase IV (SPD 25.03.xx).

Software Licenses: QL-VCCE*-**

Software Media: QA-VCCE*-**

Software Documentation: QA-VCCEA-GZ

VMS Operating System V4.6 - V5.1-1

Software Product Services: QT-VCCE*-**

DECnet-VAX V4.6 - V5.1

*Denotes media variant. For additional information on

FTarget System (PBXserver)

Favailable licenses, services and media, refer to the

appropriate price book.

None

The above information is valid at the time of release.

Please contact your local DIGITAL office for the most up-to-date information. F2