F F

System

Support

Addendum

FPRODUCT NAME:

FDECwindows

DECnet/SNA

3270

SSA31.58.00-A

Terminal Emulator for VMS,

Version 1.0

FHARDWARE

FREQUIREMENTS

FDECnet/SNA Gateway (DECSA-FA) (SPD 30.15.xx)

DEC MicroServer (DEMSA-Ax) (SPD 25.C6.xx)

FProcessors

FSupported

FDEC MicroServer-SP (DEMSB-Ax) (SPD 25.C6.xx)

DEC ChannelServer (DESNA-Ax) (SPD 29.76.xx)

VAX:

VAX 6000 Model 200 Series

VAX 6000 Model 300 Series

VMS/SNA (SPD 27.01)

VAX 6000 Model 400 Series

FBlock

FSpace

FRequirements

F(Block

FCluster

FSize

F=F1):FVAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX

8500, VAX 8530, VAX 8550, VAX 8600, VAX

Disk space required for installation:

8650, VAX 8700, VAX 8800, VAX 8810, VAX

2,600 blocks

8820, VAX 8830, VAX 8840, VAX 8842, VAX

(1300K bytes)

8974, VAX 8978

VAX-11/750, VAX-11/780, VAX-11/785

Disk space required for use (permanent):

1,500 blocks

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

(750K bytes)

3300, MicroVAX 3400, MicroVAX 3500,

MicroVAX 3600, MicroVAX 3800,

These counts refer to the disk space required on the

MicroVAX 3900 system disk. The sizes are approximate; actual sizes may vary depending on the user’s system environment, con-

VAXstation:

VAXstation II, VAXstation 2000, figuration, and software options.

VAXstation 3100, VAXstation 3200,

VAXstation 3500, VAXstation 3520,

FMemory

FforFDECwindows

FSupportFVAXstation 3540, VAXstation 8000

The minimum supported memory for this application run-

VAXserver:

VAXserver 3300, VAXserver 3400, ning in a stand-alone DECwindows environment with

VAXserver 3500, VAXserver 3600, both the client and server executing on that same system

VAXserver 3602, VAXserver 3800, is 4 MB.

VAXserver 3900, VAXserver 6210,

The performance and memory usage of DECwindows ap-

VAXserver 6220, VAXserver 6310, plications are particularly sensitive to system configura-

VAXserver 6320 tion. Less memory may be required on the client system

FNotFSupported

F(the system where the software is installed and executed)

if the server (the component that displays the application)

VAX-11/730 resides on another system. More memory may be re-

FProcessor

FRestrictions

Fquired on a system with several applications running or

may be desirable to improve the performance of an

Remote Execution with a PC as a server machine is application.

unsupported.

The minimum memory supported is 4 MB. However, the

FOther

FHardware

FRequired

Fuse of this software in conjunction with increased

A properly configured DECnet/SNA Gateway or VMS/ memory capability improves performance. The memory

SNA system for access to the IBM mainframe environsize suggested for most typical hardware configurations ment is required:

is at least 6 MB.

FSeptember

1989

AE-NL56A-TE

FDECwindows DECnet/SNA

3270

SSA31.58.00-A

Terminal Emulator for VMS,

Version 1.0

CLUSTER

FENVIRONMENT

F�VMS DECwindows Compute Server (Base kit; in-

cludes runtime support)

This layered product is fully supported when installed on

F�VMS DECwindows Device Support

any valid and licensed VAXcluster* configuration without restrictions. The HARDWARE REQUIREMENTS sections

F�VMS DECwindows Programming Support

of this product’s Software Product Description and

System Support Addendum detail any special hardware

For stand-alone execution, the following DECwindows required by this product.

components must be installed on the machine:

*V5.x VAXcluster configurations are fully described in

F�VMS DECwindows Compute Server

the VAXcluster Software Product Description

(29.78.xx) and include CI, Ethernet and Mixed

Interconnect configurations.

For remote execution, the following DECwindows components must be installed on the machine:

FSOFTWARE

FREQUIREMENTS

FServer

FMachine

FThe DECwindows DECnet/SNA 3270 Terminal Emulator

for VMS requires one of the following products. Refer to

VMS DECwindows Device Support the respective SPD for prerequisite hardware and

FClient

Fsoftware.

VMS DECwindows Compute Server

F�VMS/SNA V2.0 (SPD 27.01.xx)

F�DECnet/SNA Gateway-CT V1.0 (SPD 29.76.xx)

FVMS

FTailoring

F�DECnet/SNA Gateway-ST V1.1 (SPD 25.C6.xx)

F�DECnet/SNA Gateway V1.5 (SPD 30.15.xx)

For VMS V5.x systems, the following VMS classes are required for full functionality of this layered product:

FFor

FaFDECnet/SNA

FGateway

Fenvironment:F�VMS Required Saveset

F�VMS Operating System V5.1 - V5.2 (and necessary

F�Network Support

components of VMS DECwindows)

F�Utilities

F�DECnet-VAX V5.1 - V5.2

For more information on VMS classes and tailoring, refer to the VMS Operating System Software Product

F�DECnet/SNA VMS Gateway Management V2.0 (for

Description (SPD 25.01.xx).

use with DEMSA, DEMSB, and DESNA hardware) is required on the gateway load host node.

FOPTIONAL

F�DECnet/SNA Gateway Management V1.5 (for use

None with DECSA hardware) is required on all VMS

FGROWTH

FCONSIDERATIONS

Fsystems from which the DECwindows DECnet/SNA

3270 Terminal Emulator for VMS provides access.

The minimum hardware/software requirements for any future version of this product may be different from the

FFor a VMS/SNA environment:

Fminimum requirements for the current version.

FDISTRIBUTION

FMEDIA

Fcomponents of VMS DECwindows)

Tape:

9-track 1600 BPI Magtape, TK50 Streaming Tape

F�VMS/SNA Software V2.0

This product is also available as part of the VMS

FWorkstations

FRunning

FDECwindows:

FConsolidated Software Distribution on CDROM.

This product may run in either of the following ways:

FORDERING

FINFORMATION

F�Stand-alone execution - Running the X11 display

Software Licenses: QL-VXBA*-** server and the client application on the same

Software Media: QA-VXBA*-** machine.

Software Documentation: QA-VXBAA-GZ

F�Remote execution - Running the X11 display server

Software Product Services: QT-VXBA*-** and the client application on different machines.

*Denotes variant fields. For additional information on

VMS DECwindows is part of the VMS Operating System available licenses, services and media, refer to the but must be installed separately. Installation of VMS appropriate price book.

DECwindows gives you the option to install any or all of

The above information is valid at time of release. Please the following three components:

contact your local DIGITAL office for the most up-to-date information.

F__________________ The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

DECwindows, DECnet, MicroVAX, VAX, and VAXstation are trademarks of Digital Equipment Corporation. F2