F F

Software

Product

Description

FPRODUCT NAME:

FDECnet/SNA VMS Remote

SPD26.85.04

Job Entry, Version 1.4

FDESCRIPTION

FThis queuing technique makes it possible for many RJE

users to submit jobs at the same time and to do so even

DECnet/SNA VMS Remote Job Entry (RJE) is a layered if the workstation is inactive. When the operator sets the software product that allows suitably configured VMS workstation on, the workstation transmits all the jobs in its systems within a DECnet network to function as an SNA/ queues. For each submitted job, the user specifies one or

RJE workstation or group of workstations that can more files containing JCL (Job Control Language) statetransmit batch jobs to an IBM

F� host and receive job

ments, data, or programs.

output. The VMS system user can prepare batch jobs in

FReceiving Job Output

Ffiles, submit the jobs, and obtain the job output. Access

to the IBM SNA host environment is via the DECnet/SNA

The IBM host returns job output to a workstation over

Gateway or VMS/SNA software.

various output streams. Each IBM output stream will have a VMS directory assigned to it. As output from jobs is

By using batch interaction with the IBM host system, RJE received on an output stream, it is assigned a file name can be used to submit data that can be used for periodic identical to the name given to the job as it is executed in update of databases and other applications. Easily modithe IBM system (normally names are specified by user fied translation tables resident in either the DECnet/SNA supplied JCL). This mechanism allows easy identification

Gateway or VMS/SNA convert ASCII code to a subset of of a particular job when several users share the same job

IBM multi-national EBCDIC for transmission to the IBM stream. In the DECnet/SNA Gateway environment, job host, and from EBCDIC to ASCII on reception of job output may be directed to a system on the DECnet netoutput.

work other than the initiating system.

FFeatures

FManaging the Workstation

FThe following are some of the features of RJE:

VMS users with the required privilege can issue a set of

F�Each workstation includes a console interface that an

restricted commands to manage the workstation. These operator can use to communicate with the Job Entry commands allow the user to initialize and control the

System in the IBM host.

workstation, and to communicate interactively with the

IBM batch subsystem. The following functions are

F�RJE can support record sizes of up to 245 characters.

available:

F�RJE supports data compression on reader streams

F�Set the workstation ON and OFF

and data decompression on printer and punch

F�Stop the transmission of a job

streams.

F�Collect logging information in a disk file

F�The RJE Server can be run on the VMS system to

increase throughput of the DECnet/SNA Gateway.

F�Display status

F�ASCII to EBCDIC translation is transparent to the user

F�Obtain on-line help information

but can be inhibited with /NOTRANSLATE qualifier on

FSpecifying a Server

Fthe ASSIGN command.

When using a DECnet/SNA Gateway, there is an option

FSending Jobs to the IBM Host

Fof using the RJEServer in the DECnet/SNA Gateway

Workstation users submit jobs to VMS queues. The

(default) or running the RJEServer on a VMS node. By workstation transmits the queued jobs to the IBM host running the RJEServer on a VMS node, you can utilize over the input streams associated with a queue.

idle VMS resources and increase throughput of your

DECnet/SNA Gateway.

F__________________

F� IBM is a registered trademark of the International Business Corporation.

FJuly1989

AE-EX17E-TE

FDECnet/SNA VMS Remote

SPD26.85.04

Job Entry, Version 1.4

INSTALLATION

SOFTWARE REQUIREMENTS*

FFor RJE to be DIGITAL supported, the customer must

FIn a DECnet/SNA Gateway Environment:

Fhave a DIGITAL supported DECnet/SNA Gateway or

F�VMS Operating System

VMS/SNA configuration. To have a DIGITAL supported

DECnet/SNA Gateway configuration, purchase of the

F�DECnet-VAX

Gateway Orientation/Installation Service is REQUIRED in conjunction with the customer’s first purchase of the

FIn a VMS/SNA Environment:

FDECnet/SNA Gateway. Refer to the DECnet/SNA

Gateway SPDs (SPD 30.15.xx, SPD 29.C6.xx, SPD

29.76.xx) for further details.

F�VMS/SNA

To have a DIGITAL supported VMS/SNA configuration,

FThe DECnet/SNA VMS Remote Job Entry software re-

Fpurchase of the VMS/SNA Orientation/Installation Service

Fquires one of the following:

Fis REQUIRED in conjunction with the customer’s first pur-

chase of VMS/SNA. Refer to the VMS/SNA Software

F�DECnet/SNA Gateway-CT

Product Description (SPD 27.01.xx) for further details.

F�DECnet/SNA Gateway-ST

Only experienced customers should attempt installation

F�DECnet/SNA Gateway

of this product. DIGITAL recommends that all other customers purchase DIGITAL’s Installation Services. These services provide for installation of the software product by an experienced DIGITAL Software Specialist.

*Refer to the System Support Addendum (SSA

26.85.04-x) for availability and required versions of

FCustomer Responsibilities

Fprerequisite/optional software.

Before DIGITAL installation of the software the customer

FORDERING INFORMATION

Fmust:

Software Licenses: QL-453A*-**

F�Have previously installed all requisite hardware includ-

Software Media: QA-453A*-** ing terminals.

Software Documentation QA-453AA-GZ

F�Obtain, install, and demonstrate as operational any

Software Product Services: QT-453A*-** modems and other equipment and facilities necessary

*Denotes variant fields. For additional information on to interface to DIGITAL’s communications equipment.

available licenses, services and media, refer to the

F�Demonstrate equivalence of operation for modems

appropriate price book.

other than Bell System 201C, 208A or 209A, AT&T

FSOFTWARE LICENSING

F2596 or 2556, Dataphone II (2096A, DIGITAL 2500, or

equivalent) type modems or, in Europe, PTT approved

This software is furnished under the licensing provisions modems.

of DIGITAL’s Standard Terms and Conditions. For more information about DIGITAL’s licensing terms and policies,

F�Have generated, to DIGITAL’s satisfaction, any neces-

contact your local DIGITAL office.

sary IBM host software that will be communicating with RJE and the DECnet/SNA Gateway or VMS/SNA.

FLICENSE MANAGEMENT FACILITY SUPPORT

F�Make available for a reasonable period of time, as

This layered product supports the VMS License mutually agreed by DIGITAL and the customer, all

Management Facility.

hardware, communications facilities, and terminals that are to be used during installation.

License units for this product are allocated on a CPUcapacity basis.

Delays caused by any failure to meet these responsibilities will be charged at the prevailing rate for time and

For more information on the License Management materials.

Facility, refer to the VMS Operating System Software

Product Description (SPD 25.01.xx) or the License

Successful use of this product requires that:

Management Facility manual of the VMS Operating

F�The customer must be prepared to work with both

System documentation set.

DIGITAL and IBM systems personnel to coordinate

For more information about DIGITAL’s licensing terms the pre-installation activities.

and policies, contact your local DIGITAL office.

F�The customer should be capable of modifying IBM

FSOFTWARE PRODUCT SERVICES

Fcomponent generation parameters to support the RJE

software and either the DECnet/SNA Gateway or

A variety of service options are available from DIGITAL.

VMS/SNA.

For more information contact your local DIGITAL office.

FHARDWARE REQUIREMENTS

SOFTWARE WARRANTY

FVAX, MicroVAX or VAXstation configuration as specified

Warranty for this software product is provided by in the System Support Addendum (SSA 26.85.04-x).

DIGITAL with the purchase of a license for the product as defined in the Software Warranty Addendum of this SPD. F2 FDECnet/SNA VMS Remote

SPD26.85.04

Job Entry, Version 1.4

WARRANTY LIMITATIONS

SOFTWARE

VERSION

RELEASE

PRODUCT

FIBM Supported Configurations

FJES2 MVS/SP-JES2

13.3FThis software has been tested and is warranted against

F13.4FIBM System/370 (includes 30xx and 43xx series) class

F13.5Fprocessor systems configured with the following IBM software. While this software may function correctly with

F13.6Fother IBM software and equipment, and with software

F22.0Fother than that supported by IBM, DIGITAL cannot offer

FJES3 MVS/SP-JES3

13.3Fits standard warranty for this software unless it has been

F13.4Ftested with such equipment and software configurations.

F13.513.6FThe following list shows the configurations with which the

F22.0Fsoftware has been tested and is warranted.

FVSE/SP:

21.6VSE/Power

2.0FPlease refer to the DECnet/SNA Gateway Software

Product Description (SPD 30.15.xx, SPD 29.76.xx, or

SPD 29.C6.xx) or the VMS/SNA Software Product

Description (SPD 27.01.xx) for additional information on supported IBM operating systems, access methods and communications front end software. F3