F F

Software

Product

Description

FPRODUCT NAME:

FDECnet/SNA VMS 3270

Terminal

Emulator,

SPD26.84.06

Version 1.5

FDESCRIPTION F-Category A terminal adapter (for 32 terminals)

The DECnet/SNA VMS 3270 Terminal Emulator (3270

-Configuration support D

TE) is a layered software product that allows users of a

-Common communications adapter

VTxxx terminal (or other DIGITAL terminal or personal computer in VT100, VT200 or VT300 mode) on suitably

-External modem interface configured VMS systems within a DECnet network to in-

F�IBM 3178 Display station with the following features:

teractively access IBM

F� host-based applications. These

applications have been originally developed for IBM 3270

-87-key keyboard with 24 program function (PF) keys display stations in a Systems Network Architecture (SNA) and 3 program assist (PA) keys networking environment. Access to the IBM host-based applications system from VMS systems is via the

-Audible alarm

DECnet/SNA Gateway or via VMS/SNA software.

-Up to 1920 characters

In normal operation, an IBM system transfers a formatted

-Protected and unprotected fields screen, much like a ‘‘form’’, to the 3270 block mode terminal and the user fills in any data required by the

-Local and host copy and printer order FF (formfeed)

‘‘form’’. When complete, the form is transmitted to the

-Alphanumeric and numeric data

IBM host as a single unit. This mechanism is emulated with a Digital character mode terminal by buffering the

-Intensified display, display, and non-display characters

‘‘form’’ in the DECnet host’s memory and displaying it on the terminal. When the screen ‘‘form’’ is complete, it is

-Auto-repeat keys (as available as a VT100 keyboard sent to the IBM host system via the DECnet/SNA

SET-UP feature)

Gateway or VMS/SNA.

-Click and ALT CURSR (as available through the VT100

Translation tables on the respective systems convert

ASCII terminal input (either DIGITAL Multinational

-SYS REQ (Allows user to switch between SSCP-LU

Character Set or National Replacement Character Set) to and LU-LU sessions) a subset of IBM multinational EBCDIC code for transfer through either the DECnet/SNA Gateway or VMS/SNA

F�Unsupported features of the IBM 3178 display station

software. These translation tables may be modified to fit are:non-standard character sets.

-Selector pen, Security lock, magnetic strip card and

Users invoke the 3270 utility using the local VMS operator identification card reader system’s command language, including qualifiers to specify the IBM system and system resources with which

-<-! (new line) as auto-repeat keys the user wishes to connect. While the emulation utility is

-<!<! (fast left) and !>!> (fast right) keys operating, the terminal screen will be formatted in a fashion similar to a 3270 display. When the user has finished

-TEST REQ or TEST, IDENT, DEV CNCL and CURSR work on the IBM system, the 3270 emulator is dismissed

BLINK functions and the terminal is ‘‘restored’’ as a VMS command ter-

-Structured fields minal.

The 3270 Terminal Emulator supports emulation of the

-Local function keys (keys that when operated, do not following features of an IBM 3270 Display Station when transmit any interface codes to the host applications) attached to an IBM 3274 1C controller with the following other than those supported as VT100/VT200/VT300 features:

SET-UP features

F__________________

F�IBM is a registered trademark of International Business Machines, Inc.

FJune

1989

AE-EX18F-TE

FDECnet/SNA VMS 3270

Terminal

Emulator,

SPD26.84.06

Version 1.5

F�IBM 3180 display station with the following features:

F�Screen sizes supported by the various models of 3278

are:-87-key keyboard with 24 program function (PF) keys and 3 program assist (PA) keys

Model 1 - Up to 960 characters

Model 2 - Up to 1920 characters

-Audible alarm

Model 3 - Up to 2560 characters

-Up to 3564 characters

Model 4 - Up to 3440 characters

Model 5 - Up to 3564 characters

-Protected and unprotected fields

F�Unsupported features of the IBM 3278 display station

-Local and host copy and printer order FF (formfeed) models 1, 2, 3, 4, 5 are:

-Alphanumeric and numeric data

-Selector pen, security lock, magnetic strip card and

-Intensified display, display and non-display characters operator identification card reader

-Auto-repeat keys (as available, as a VT keyboard SET-

-<! (new line) as an auto-repeat key

UP feature)

-<!<! (fast left) and !>!> (fast right) keys

-Click and ALT CURSR (as available, as a VT keyboard

SET-UP feature)

-TEST REQ or TEST, IDENT, DEV CNCL and CURSR

BLINK functions

-SYS REQ (Allows user to switch between SSCP-LU and LU-LU sessions)

-Structured fields

F�Unsupported features of the IBM 3180 display:

-Local function keys (keys that when operated, do not transmit any interface codes to the host applications) operator other than those supported as VT100/VT200/VT300

SET-UP features

-<-! (new line) as an auto-repeat key

-Field inherit keys

-Programmed symbol selection keys

This product has been designed such that it can be used with most IBM applications, however, those applications written using features not supported by the emulator (e.g.

-3270 Extended Data Stream

3270 Extended Data Stream) must be modified.

A readily available on-line HELP facility provides information on keys with altered 3270-oriented functions. The status line as implemented on an actual 3270 display is not supported, however much of the same information is

F�IBM 3278 display station Models 1, 2, 3, 4, and 5 with

reported on a special status line which may be overlaid the following features:

on the VT200’s 24th line. In addition, the VMS system manager has the ability to re-map certain IBM key func-

-87-key keyboard with 24 program function (PF) keys tions onto different locations on the DIGITAL keyboard.

FFeatures

FofFVersion

F1.5F- Audible alarm

- Protected and unprotected fields

F�VMS 3270 TE v1.5 will allow, on supported DECnet/

SNA gateways and VMS/SNA systems, secured LUs

- Local and host copy and printer order FF (formfeed)

(Logical Units) to be accessed via a password.

- Alphanumeric and numeric data

F�VMS 3270 TE v1.5 will allow up to 16 alphanumeric

- Intensified display, display and non-display characters characters to be coded in the ACCESSNAME parameter.

- Auto-repeat keys (as available as a VT keyboard SET-

F�VMS 3270 TE v1.5 will provide the ability to display

status information on the hardware status line when

- Click and ALT CURSR (as available, as a VT keyboard using a VT device (or VT emulator) that supports the hardware status line.

- SYS REQ (Allows user to switch between SSCP-LU

F�VMS 3270 TE v1.5 will support Digital’s License

Management Facility.

FSOURCE

FCODE

FSources of message files are available only for transla-

tion to languages other than English. Source code will not be distributed for general purposes. F2 FDECnet/SNA VMS 3270

Terminal

Emulator,

SPD26.84.06

Version 1.5

INSTALLATION

Customer

FResponsibilities

FBefore DIGITAL installation of the software the customer

FSoftware

FProduct

Version

Release

Fmust:

FTSO/E/XA

3.0F�Have previously installed all requisite hardware includ-

4.0ing terminals and DECnet/SNA gateway products.

Fqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq

F�Obtain, install, and demonstrate as operational any

ISPF/MVS

2.0modems and other equipment and facilities necessary

3.0to interface to DIGITAL’s communications equipment.

FISPF/PDF

2.0F�Have generated, to DIGITAL’s satisfaction, any neces-

3.0sary IBM host software that will be communicating with

Fthe DECnet/SNA gateway or with VMS/SNA and VMS

IMS21.03270 TE.

3.0F�Make available for a reasonable period of time, as

Fmutually agreed by DIGITAL and the customer, all hard-

CICS/OS/MVS

16.1ware, communications facilities, and terminals that are

7.0to be used during installation.

FNCCF

2.0Delays caused by any failure to meet these responsibili-

Fties will be charged at the prevailing rate for time and

NETVIEW

1.0materials.

2.0Successful use of this product requires that:

F�The customer must be prepared to work with both

FIBM

VMEnvironment

FDIGITAL and IBM systems personnel to coordinate the

Fpre-installation activities.

VM/SP

14.1F�The customer should be capable of modifying IBM com-

5.0ponent generation parameters to support either the

FDECnet/SNA gateway or VMS/SNA software and the CMS 4.13270 TE software.

5.0Only experienced customers should attempt installation

Fof this product. DIGITAL recommends that all other cus-

ISPF/VM

2.0tomers purchase DIGITAL’s Installation Services. These

Fservices provide for installation of the software product by

ISPF/PDF

2.0an experienced DIGITAL Software Specialist.

21.0FWARRANTY

FLIMITATIONS

FSupported

FConfigurations

FNETVIEW

1.02.0This software has been tested and is warranted against

FIBM System/370 (includes 30xx and 43xx series) class

processor systems configured with the following IBM soft-

DOS/VSE

Environment

Fware. While this software may function correctly with

Fother IBM software and equipment, and with software

other than that supported by IBM, DIGITAL cannot offer

VSE/SP

21.6its standard warranty for this software unless it has been

Ftested with such equipment and software configurations.

VSE/ICCF

21.0Fqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq

FThe following list shows the configurations with which the

ISPF/VSE

1.0software has been tested and is warranted:

1.0Fqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq

FIBM MVS Environment

FCICS/DOS/VS

16.0Fqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq qqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq

FMVS/SP

13.6NCCF

2.03.7Fqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqqq

F21.31.5Since the introduction of this software, other configura-

1.7tions may have been tested. Please contact your local

2.0DIGITAL office for up-to-date information regarding listed configurations. F3 FDECnet/SNA VMS 3270

Terminal

Emulator,

SPD26.84.06

Version 1.5

PREREQUISITE

FSUPPORT

ORDERING

FINFORMATION

FA Network Profile and a DECnet Customer Support Plan

Software Licenses: QL-454A*-**

(where appropriate) covering all VMS nodes that wish to

Software Media: QA-454A*-** access the IBM host based applications environment

Software Documentation: QA-454AA-GZ must be prepared jointly by DIGITAL and the customer.

Software Product Services: QT-454A*-**

For DECnet/SNA 3270 Terminal Emulator to be DIGITAL

*Denotes variant fields. For additional information on supported, the customer must have a DIGITAL supported available licenses, services and media refer to the ap-

DECnet/SNA gateway or VMS/SNA configuration.

propriate price book.

To have a DIGITAL supported DECnet/SNA gateway or

FSOFTWARE

FLICENSING

FVMS/SNA configuration, purchase of the Gateway

This software is furnished under the licensing provisions

Orientation/Installation Service (QSF0x-SZ) is of DIGITAL’s Terms and Conditions. For more informa-

REQUIRED in conjunction with the customer’s first purtion about DIGITAL’s licensing terms and policies, conchase of the DECnet/SNA gateway.

tact your local DIGITAL office.

FHARDWARE

FREQUIREMENTS

LICENSE

FMANAGEMENT

FFACILITY

F�VAX, MicroVAX, or VAXstation configuration as speci-

fied in the System Support Addendum (SSA 26.84.06-

This layered product supports the VMS License x).Management Facility.

F�Any properly configured DECnet/SNA gateway or VMS/

License units for this product are allocated on a CPU-

SNA system as specified in the System Support capacity basis.

Addendum (SSA 26.84.06-x).

For more information on the License Management

FREQUIREMENTS*

FFacility, refer to the VMS Operating System Software

In a DECnet/SNA Gateway Environment:

Product Description (SPD 25.01.xx) or the License

Management Facility manual of the VMS Operating

F�VMS Operating System

System documentation set.

F�DECnet-VAX

For more information about DIGITAL’s licensing terms

In a VMS/SNA environment:

and policies, contact your local DIGITAL office.

FPRODUCT

FSERVICES

F�VMS/SNA Software

A variety of service options are available from DIGITAL.

The DECnet/SNA VMS 3270 Terminal Emulator software

For more information contact your local DIGITAL office.

requires one of the following products:

FWARRANTY

FRefer to the respective SPDs for prerequisite hardware

and software.

Warranty for this software product is provided by

F�VMS/SNA (SPD 27.01.xx)

DIGITAL with the purchase of a license for the product as

F�DECnet/SNA Gateway-CT (SPD 29.76.xx)

defined in the Software Warranty Addendum of this SPD.

F�DECnet/SNA Gateway-ST (SPD 25.C6.xx)

F�DECnet/SNA Gateway (SPD 30.15.xx)

*Refer to the System Support Addendum for availability and required versions of prerequisite/optional software

(SSA 26.84.06-x). F4