F F

System

Support

Addendum

FPRODUCT NAME:

FVAX

3271

Protocol

Emulator,

SSA25.21.13-A

Version 2.5

FHARDWARE REQUIREMENTS VAX Communications

Max. No. of

Max. Line

System

Interface

Interfaces

Speed

FProcessors supported

F:VAX 6210

DMB32

49600 baud

The following table shows which combinations of VAX

VAX 6220 system, communications interface and communications

VAX 6230 line speed are supported configurations:

VAX 6240

VAX 6310

419200 baud#

FVAX 6312

FSystem

FVAX 6320

FMicroVAX:

FVAX 6330

VAX 6333

MicroVAX I

DPV11

14800 baud

VAX 6340

MicroVAX II

DSV11

2 (4 lines)

9600 baud

VAX 6350

29600 baud

VAX 6360

MicroVAX 3300

DSV11-S

19200 baud#

VAX 8200

MicroVAX 3400

DPV11-S

VAX 8250

DMF32*

MicroVAX 3500

DUP11*

19600 baud

MicroVAX 3600

VAX 8300

MicroVAX 3800

VAX 8350

MicroVAX 3900

FVAX:

FVAX 8500

VAX-11/725

DMF32

VAX 8530

VAX 8550

VAX-11/730

DUP11

VAX 8700

VAX 8800

VAX-11/750

VAX 8810

VAX 8820

VAX-11/780

VAX 8830

VAX-11/785

VAX 8840

VAX 8842

VAX 8600

VAX 8974

VAX 8650

VAX 8978

VAX 6000-410

FVAXstation:

FVAX 6000-420

VAX 6000-430

VAXstation II

1 (2 lines)

VAX 6000-440

VAXstation 3200

VAX 6000-450

VAXstation 3500

VAX 6000-460

F__________________

F� IBM is a registered trademark of IBM Corporation.

FNovember

1989

AE-LY56B-TE

FVAX 3271

Protocol

Emulator,

SSA25.21.13-A

Version 2.5 VAX Communications

Max. No. of

Max. Line

CLUSTER ENVIRONMENT*

System

Interface

Interfaces

Speed

FThis layered product is fully supported when installed on

FVAXserver:

Fany valid and licensed VAXcluster* configuration. It must

be installed once on each VAX, MicroVAX or VAXstation

VAXserver 3300

DPV11-S

49600 baud processor from which usage is planned. The

VAXserver 3400

DSV11-S

2 (4 lines)

19200 baud#

FHARDWARE REQUIREMENTS

F sections of this product’s

VAXserver 3500

Software Product Description and System Support

VAXserver 3600

Addendum detail any special hardware required by this

VAXserver 3602 product.

VAXserver 3800

VAXserver 3900

In order to configure some product specific attributes that must remain unique to each system, certain components

VAXserver 6210

DMB32

419200 baud# of the product are stored in the system specific environ-

VAXserver 6220 ment, SYS__$SPECIFIC:[SYSxxx] of the VAX, MicroVAX

VAXserver 6310 or VAXstation processor on which the installation is per-

VAXserver 6320 formed. The remaining components of the product, in-

*Requires use of a DWBUA UNIBUS to BI-bus Adapter cluding some or all of the executable images, will be installed common to all accessing systems.

#9600 baud is the maximum supported line speed for multiple interface configurations. Operation of multiple

*V5.x VAXcluster configurations are fully described in interface configurations at line speeds higher than the VAXcluster Software Product Description

9600 baud may result in unreliable operation.

(29.78.xx) and include CI, Ethernet and Mixed

Interconnect configurations.

Note that a DSV11 synchronous communications interface supports two separate communications lines.

FOPTIONAL HARDWARE

FProcessors Not Supported

F:F�VT2XX or VT3XX terminals

VAX-11/782

F�VT100 terminals with Advanced Video Option

VAXstation I, VAXstation 2000, VAXstation 3100 Series,

F�Any of the following terminals or personal computer

VAXstation 3520, VAXstation 3540, VAXstation 8000

(with the appropriate hardware and software) operat-

MicroVAX 2000, MicroVAX 3100 ing in VT100 emulation mode:

FProcessor Restrictions

F-Rainbow 100

FNote

F:An R80/RL02 configuration is required for VAX-11/

-DECmate/WPS

730 systems.

-PRO-325 or PRO-350 (with P/OS Operating System,

FBlock Space Requirements (Block Cluster Size = 1)

F:Version 1.7 and PRO/Communications)

Disk

Space required forinstallation:

1,150 blocks

The number of VT terminals (or Digital Personal

(589K bytes)

Computers running in VT100 emulation mode) supported space foruse(permanent):

750blocks by the 3270 Terminal Emulator utility will depend on ap-

(384K plication and system loading.

These block counts refer to the disk space required on

FSOFTWARE REQUIREMENTS

Fthe system disk. The sizes are approximate, actual sizes

may vary depending on the user’s system environment,

FOperating System

Fconfiguration, and software options selected.

VMS Operating System V5.0 - V5.2

The VAX 3271 PE requires approximately 10K bytes of non-paged memory for the first DMF32, DMB32 or

FLayered Products

FDSV11 device; 9K bytes are required for the first DUP11

VAX Wide Area Network Device Drivers V1.1 (SPD or DPV11 device. Each subsequent DMF32, DMB32 or

29.64.xx)

DSV11 device requires an additional 300 bytes, while an additional DUP11 or DPV11 device requires an additional

FVMS Tailoring

F350 bytes. Each terminal requires an additional 300 bytes

for a DMF32, DMB32 or DSV11 or 350 bytes for either a

For VMS V5.x systems, the following classes are re-

DUP11 or DPV11.

quired for full functionality of this layered product.

When the emulator is running, further non-paged memory

F�VMS Required Saveset

is allocated which is sufficient to accommodate the number and size of the buffers requested by the user. In

F�Programming Support

addition, each DMF32, DMB32 or DSV11 device uses approximately 4600 bytes of non-paged memory for data

F�System Programming Support

transfer. For all five device types, the VAX 3271 PE adds

24 bytes to the buffer size specified by the user.

F�Utilities F2 FVAX 3271

Protocol

Emulator,

SSA25.21.13-A

Version 2.5

GROWTH CONSIDERATIONS

ORDERING INFORMATION

FThe minimum hardware/software requirements for any

Software Licenses: QL-112A*-** future version of this product may be different from the

Software Media: QA-112A*-** minimum requirements for the current version.

Software Documentation: QA-112AA-GZ

Software Product Services: QT-112A*-**

The 3270 Terminal Emulator’s performance depends on system and line load, the IBM

F� application, and the rate

*Denotes variant fields. For additional information on of data entry. Refer to product release notes or your local available licenses, services and media, refer to the

Digital office for further information.

appropriate price book.

FDISTRIBUTION MEDIA

FThe above information is valid at the time of release.

Please contact your local Digital office for the most up-to-

Tape: 9-Track 1600 BPI Magtape (PE), TK50 Tape date information.

Cartridge

F__________________

F� The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

F� MicroVAX, VAX, VAXstation, VAXserver and VT are trademarks of Digital Equipment Corporation. F3