F F

System

Support

Addendum

FPRODUCT NAME:

FVIDA

forDB2

F�,Version

1.0SSA25.E7.00-A

FHARDWARE REQUIREMENTS

F�ECO REV 4 or later (VAX-11/780)

FVIDA Client for DB2

F�A minimum of four megabytes of memory

FProcessor Support

F�One 9-track 1600 BPI magnetic tape unit for installation

of the software

VAX:

VAX 6210, VAX 6220, VAX 6230, VAX 6240,

VAX 6310, VAX 6312, VAX 6320, VAX 6330,

F�Mass storage units to perform operational activities for

VAX 6333, VAX 6340, VAX 6350, VAX 6360, established databases

VAX 8200, VAX 8250, VAX 8300, VAX 8350,

F�WCS microcode version 123 or later

VAX 8500, VAX 8530, VAX 8550, VAX 8600,

VAX 8650, VAX 8700, VAX 8800, VAX 8820,

FFor VAX 82xx or VAX 83xx Systems

F:VAX 8830, VAX 8840, VAX 8842, VAX 8974,

VAX 8978

VAX-11/780, VAX-11/785

F�One 9-track 1600 BPI magnetic tape for installation of

the software

MicroVAX:

MicroVAX II, MicroVAX 2000, MicroVAX

3300, MicroVAX 3400, MicroVAX 3500,

MicroVAX 3600, MicroVAX 3800, MicroVAX

3900

FFor VAX 8974 and VAX 8978 Systems:

FVAXstation:

VAXstation II, VAXstation 2000, VAXstation

3100, VAXstation 3200, VAXstation 3500,

F�A minimum of four megabytes of memory (per

VAXstation 8000 processor)

VAXserver:

VAXserver 3300, VAXserver 3400,

VAXserver 3500, VAXserver 3600,

VAXserver 3602, VAXserver 6210,

F�Mass storage units to backup and restore established

VAXserver 6220, VAXserver 6310, databases

VAXserver 6320

FFor all other supported VAX Systems:

Not Supported

VAX 11/725, VAX-11/730, VAX-11/750, VAX

11/782, MicroVAX I, and VAXstation I

F�One 9-track 1600 BPI magnetic tape or TK50 tape drive

Systems for installation of the software

FProcessor Restrictions

FFor VAX-11/780 or VAX-11/785 Systems:

Fdatabases

F__________________

F� DB2 is a trademark of the International Business Machines Corporation.

FJune

1989

AE-MH80A-TE

FVIDA forDB2

F�,Version

1.0SSA25.E7.00-A

FBlock Space Requirements (Block Cluster Size = 1)

Operating System

F�VMS Operating System V5.0 or V5.1

Disk space required for installation:

3,000 blocks

(1.54M bytes)

FCommunications Software

FDisk space required for use (permanent):

F�DECnet/SNA VMS APPC/LU6.2 Programming Interface

V2.1 (SPD 26.88.xx)

1,900 blocks

(.97M bytes)

F�VIDA for DB2 requires any valid DIGITAL SNA connec-

tion as described by DECnet/SNA VMS APPC/LU6.2

These counts refer to the disk space required on the system

Programming Interface (SPD 26.88.xx) for connections disk. The sizes are approximate; actual sizes may vary deto IBM MVS/XA systems.

pending on the user’s system environment, configuration and software options selected.

FIBM Software

FYou must allow additional space for programs, logs, and

F�MVS/XA Operating System, any version that supports

temporary database cache files, and user interface software the required versions of CICS/OS/VS and DB2 such as VAX Data Distributor and VAX DATATRIEVE.

F�CICS/OS/VS Version 1, Release 7

FVIDA Server for DB2

F�DB2 Version 1, Release 3

FProcessor Support

F�DB2 Attachment Facility for CICS/OS/VS

F�Any IBM

F� S/370 processor or equivalent that supports

MVS/XA

F� .F�Assembler H

F�One 9-track 6250 BPI magnetic tape unit for installation

F�SMP/E Version 1, Release 4

of the software.

VIDA Server has been designed to operate with the IBM

FSpace Requirements

Fsoftware listed above. While other releases of the above

software may function correctly, DIGITAL cannot offer its

Disk space required (in 3380 tracks): 120 tracks standard warranty for such software unless it has been tested with the software and found acceptable to DIGITAL.

FOPTIONAL HARDWARE

FOther Software

Communications Support

FVIDA for DB2 does not include a user interface. Refer to the

Any Gateway configuration that supports any valid DIGITAL section on optional software for choices.

SNA connection as described by DECnet/SNA VMS APPC

LU6.2 Programming Interface (SPD 26.88.xx) for connec-

FVMS Tailoring

Ftions between VAX and IBM MVS/XA systems.

For VMS V5.x the following VMS classes are required for

FCLUSTER ENVIRONMENT

Ffull functionality of this layered product:

The VIDA Client for DB2 product is fully supported when

F�VMS Required Saveset

installed on any valid and licensed VAXcluster* configura-

F�Programming Support

tion without restrictions. The HARDWARE

F�Network Support

REQUIREMENTS sections of this product’s Software

F�Secure User’s Environment

Product Description and System Support Addendum detail

F�Utilities

any special hardware required by this product.

For more information on VMS classes and tailoring, refer to

*V5.x VAXcluster configurations are fully described in the the VMS Operating System Software Product Description

VAXcluster Software Product Description (SPD 29.78.xx)

(SPD 25.01.xx) and include CI, Ethernet and Mixed Interconnect

FOPTIONAL SOFTWARE

Fconfigurations.

One of the following must be used to provide a VIDA for

FSOFTWARE REQUIREMENTS

FDB2 user interface:

FVAX Software

FFor interactive query access use one or more of the

following:

F�VAX DATATRIEVE V4.2

F�VAX TEAMDATA V1.3

F�Interactive VAX SQL and RDO (Rdb/VMS V3.0)

F1F__________________

F� IBM is a registered trademark of the International Business Machines Corporation.

F� MVS/XA is a trademark of the International Business Machines Corporation. F2 FVIDA forDB2

F�,Version

1.0SSA25.E7.00-A

FFor application development using high level languages use

FGROWTH CONSIDERATIONS

Fone or more of the following precompilers supplied with the

The minimum hardware/software requirements for any

VAX Rdb/VMS V3.0 Full Development Option or VAX Rdb/ future version of this product may be different from the mini-

VMS V3.0 Development Upgrade. For more information mum requirements for the current version.

about VAX Rdb/VMS application development options and supported version of high level language compilers, please

FDISTRIBUTION MEDIA

Frefer to the VAX Rdb/VMS Software Product Description

(SPD 25.59.xx)

FVIDA Client for DB2

F�VAX Rdb/VMS precompilers for VAX BASIC, VAX C,

Tape:

9-track 1600 BPI Magtape (PE), TK50 Streaming

VAX COBOL, VAX FORTRAN, or VAX PASCAL

Tape

F�VAX SQL precompilers for VAX Ada, VAX C, VAX

COBOL, VAX FORTRAN, and VAX PL/I

FVIDA Server for DB2

F�VAX SQL Module Language for any language that sup-

Tape: 9-track 6250 BPI Magtape (PE) ports the VMS calling standard

F�Callable RDO for any language that supports the VMS

FORDERING INFORMATION

Fcalling standard

The VIDA for DB2 components are ordered separately. An

FOther Optional Software

Finstallation advisory service package and onsite user orien-

tation program is included in the VIDA for DB2 license.

F�VAX Rdb/VMS V3.0 Full Development Option

F1,2F�VAX Rdb/VMS V3.0 Interactive Option

F1,2FSoftware Licenses:

F�VAX Rdb/VMS V3.0 Run-time Option

F2FVIDA Client: QL-VTWA*-**

F�VAX TEAMDATA V1.3

F1FVIDA Server: QB-VTXA9-BA

F�VAX DATATRIEVE V4.2

F1FSoftware Media:

F�VAX CDD/Plus V4.0

VIDA Client: QA-VTWA*-**

F�VAX Data Distributor V2.0

VIDA Server: QA-VTXAA-*A

FNotes

F:FSoftware Documentation:

F1FVAX Rdb/VMS is not a prerequisite to VIDA for DB2.

VIDA for DB2 may be used with VAX DATATRIEVE or

VIDA Client: QA-VTWAA-GZ other DSRI compliant interfaces without any VAX Rdb/

VIDA Server: QA-VTXAA-GZ

VMS license. However, development of applications in

FSoftware Product Services:

Fhigh level languages is dependent upon tools (query utili-

ties and language precompilers) supplied in the VAX

VIDA Client: QT-VTWA*-**

Rdb/VMS Full Development Option. Support for applica-

VIDA Server: QT-VTXA*-** tion development using these products is obtained through the VAX Rdb/VMS license.

*Denotes variant fields. For additional information on

F2FTo access data from nodes in a network other than a

available licenses, services and media refer to the appronode on which VIDA Client is installed, either VAX Rdb/ priate price book.

VMS Full Development, VAX Rdb/VMS Interactive

Option, or VAX Rdb/VMS Run-Time Only Option soft-

The above information is valid at time of release. Please ware must be installed on the node from which the user contact your local DIGITAL office for the most up-to-date initiates the access.

information. F3