F F

System

Support

Addendum

FPRODUCT NAME:

FDECvoice

Software,

Version

1.1SSA29.97.01-A

FHARDWARE REQUIREMENTS

FProcessors Not Supported

Processor Support

F�For systems containing a DTC04-AA module, any

system containing a processor other than a KA630,

VAX:

VAX 6000 Model 200 Series,

KA650 or KA655 Q-bus processor is not supported.

VAX 6000 Model 300 Series,

VAX 6000 Model 400 Series,

F�VAX-11/725, MicroVAX I, VAXstation I and VAX-11/782

processors are not supported.

VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX

8500, VAX 8530, VAX 8550, VAX 8600, VAX

FProcessor Restrictions

F8650, VAX 8700, VAX 8800, VAX 8810, VAX

8820, VAX 8830, VAX 8840, VAX 8842, VAX

F�64K bytes of available Q-bus I/O memory space for

8974, VAX 8978 each DTC04-AA module installed in the system.

VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/

F�A maximum of sixteen DTC04-AA modules can be sup-

785ported on a single MicroVAX or VAXstation subject to the following restrictions:

MicroVAX:

MicroVAX II, Microvax 2000, MicroVAX

3100, MicroVAX 3300, MicroVAX 3400,

-The module can be mounted only in a BA23 or

MicroVAX 3500, MicroVAX 3600, MicroVAX

BA123 enclosure, or in a multiple BA23 enclosure

3800, MicroVAX 3900 such as the DTCAA-CA or the H9642 based dual-

VAXstation:

VAXstation II, VAXstation 2000, VAXstation

BA23 MicroVAX systems.

3100 Series, VAXstation 3200, VAXstation

-The number of available Q-bus quad-width slots and

3500, VAXstation 3520, VAXstation 33540, subject to available power and loading on the Q-bus.

VAXstation 8000

-The number of adjacent "B" size mounting slots on

VAXserver:

VAXserver 3100, VAXserver 3300, the I/O bulkhead. The I/O bulkhead space available

VAXserver 3400, VAXserver 3500, on various enclosures limits the number of Telephone

VAXserver 3600, VAXserver 3602,

Line Interfaces that can be installed on the system.

VAXserver 3800, VAXserver 3900,

VAXserver 6000-210, VAXserver 6000-310,

The following table contains the maximum limits of TLIs

VAXserver 6000-410, VAXserver 6000-420 and DTC04-AA modules. The actual number of TLIs and

DTC04-AA modules that can be installed in a system

All VAX, MicroVAX and VAXstation processors lised may be further reduced by available Q-bus slots and above are supported subject to the following restrictions:

power, or by other hardware or software installed on the

F�All functions requiring communications with or proc-

system:

essing by, a DTC04-AA module must be executed on a valid MicroVAX or VAXstation configuration, that is, a

FSystem

Maximum

Fconfiguration containing one or more DTC04-AA mo-

FEnclosure

TLIs

DTC04-AA

Fdules. The DTC04-aa hardware is supported only in the

DTCAA-CA

816BA23 and the BA123 series of enclosures and only when used with the KA630, KA650 or KA655 series of

H3490

36Q-bus processors.

H9642-S

36F�The synthesis name pronunciation routines require communications with, and processing by, a DECtalk

BA123

24DTC01 peripheral, DTC03 peripheral or a DECvoice

DTC04-AA module.

BA23

12FDecember

1989

AE-LZ26B-TE

FDECvoice Software,

Version

1.1SSA29.97.01-A

FThe DTCAA-CA series enclosures, built from the H3490-

FOPTIONAL HARDWARE

FE bulkhead and three BA23 enclosures, support a maxi-

None mum of eight TLIs; eight TLIs provide support for up to sixteen DTC04-AA modules.

FCLUSTER ENVIRONMENT

FThe H3490 bulkheads are used in the 630QE dual-BA23

This layered product is fully supported when installed on

MicroVAX systems, the H9642-S expansion enclosure any valid and licensed VAXcluster* configuration without and various other dual-BA23-based cabinetry. The H3490 restrictions. The

FHARDWARE REQUIREMENTS

Fbulkheads support a maximum of three TLIs; three TLIs

Sections of this product’s Software Product Description provide support for up to six DTC04-AA modules.

and System Support Addendum detail any special hard-

The BA123 enclosures support a maximum of two TLIs;

ware required by this product.

two TLIs provide support for up to four DTC04-AA modules.

*V5.x VAXcluster configurations are fully described in the

VAXcluster Software Product Description (29.78.xx) and

The single-BA23 enclosures support a maximum of one include CI, Ethernet, and Mixed Interconnect

TLI; one TLI provides support for up to two DTC04-AA configurations.

FSOFTWARE REQUIREMENTS

FThe performance of the real-time portions of the DTC04-

AA system is sensitive to processor, VAXcluster and

VMS Operating System V5.2 device interrupt latency. Degradations will be noticed if

DTC04 interrupts are blocked by any other software and/

FVMS Tailoring

For hardware in the MicroVAX or VAXstation system. A

dedicated MicroVAX system is recommended for optimal

For VMS V5.x systems, a minimum of the VMS Required

DECvoice performance.

Saveset is required if the DECvoice software is to be used in a run-time only environment, that is, no program

The DTC04-AA module is not distributed, nor shareable, debugging or development is to be conducted.

across nodes in the VAXcluster. The module must reside locally, that is, on the MicroVAX or VAXstation processor

To conduct program development with the DECvoice that performs the calls to the DECvoice libraries.

software, a minimum of both the VMS Required Saveset and Programming Support kits is required.

FOther Hardware Required

FFor more information on VMS classes and tailoring, refer

If a DTC04-AA Q-bus hardware module is installed in the to the VMS Operating System Software Product system, the following hardware is required:

Description (SPD 25.01.xx)

F�The base DTC04-AA DECvoice quad-width Q-bus

module.

FOPTIONAL SOFTWARE

F�An approved country-specific Telephone Line Interface

The microcode binaries for the DECvoice Software V1.1

(TLI), the CK-DTC04. (The TLI is currently only avail-

Continuous Word Speech Recognition Software are inable for the United States and Canada.) Each TLI supcluded in the DECvoice Software kit. The Continuous ports up to two DTC04-AA modules.

Word Recognition Software is a separately licensed product.

F�A minimum of 150 megabytes of local disk storage.

Digital recommends a KFQSA disk controller and one

The Continuous Word Recognition Software is licensed or more externally mounted RF71 disks for ease of storon a user/activity basis. When this product is licensed, a age expansion, separate disk power supply and the inpool of license units are made available. The specific herent dual-path and dual-host capabilities of the DSSI number of units in the pool varies based on the specific bus. A minimum of an RQDX3 disk controller and an license purchased. The DECvoice Software deducts a

RD54 disk is required.

fixed number of units (100) from the pool whenever the

F�A minimum of 8 megabytes of physical memory on any

Continuous Word Recognizer is made active, that is, system containing any DTC04-AA modules.

when loaded into a DECvoice DTC04-AA module. These units are returned to the pool when the Continuous Word

F�A minimum of 16 megabytes of physical memory on

Recognizer microcode is rendered inactive, that is, when any system containing nine or more DTC04-AA it is unloaded or otherwise made unavailable. The license unit allocation for the continuous word recognizer is not processor tiered; it is not based on CPU capacity.

FBlock Space Requirements (Block Cluster Size = 1):

FContinuous word recognizer licenses are tied only to rec-

Disk space required forinstallation:

14,431 blocks ognizer activity, not to specific DTC04-AA modules.

(7.4MB)

The isolated word recognizer and the optional foruse(permanent):

Continuous Word Recognizer are mutually exclusive;

they both cannot be used on the same DECvoice module

These counts refer to the disk space required on the at the same time. The recognizer in use on a specific system disk. The sizes are approximations; actual sizes

DECvoice module, when both are licensed, can be may vary depending on the user’s system environment, switched dynamically under the control of a user proconfiguration, and software options selected.

gram. F2 FDECvoice Software,

Version

1.1SSA29.97.01-A

FCertain versions of these products depend upon a spe-

FORDERING INFORMATION

Fcific version of the operating system. Refer to the System

Software Licenses: QL-VFUA*-**

Support Addendum of the product in question to deter-

Software Media: QA-VFUA*-** mine which version is necessary.

Software Documentation: QA-VFUAA-GZ

Software Product Services: QT-VFUA*-**

FGROWTH CONSIDERATIONS

FContinuous Word Recognizer Licenses: QL-YFCA*-**

The minimum hardware/software requirements for any

Continuous Word Recognizer Services: QT-YFCA*-** future version of this product may be different from the minimum requirements for the current version.

*Denotes variant fields. For additional information on available licenses, services and media, refer to the ap-

FDISTRIBUTION MEDIA

Fpropriate price book.

Tape:

9-track 1600 BPI Magtape, TK50 Tape Cartridge

The above information is valid at time of release. Please

This product is also available as part of the VMS contact your local Digital office for the most up-to-date

Consolidated Software Distribution on CDROM.

information.

F__________________ The DIGITAL Logo is a registered trademark of Digital Equipment Corporation.

VAX, VMS, MicroVAX, VAXstation, VAXserver and DECvoice are trademarks of Digital Equipment Corporation. F3