SystemSupportAddendum_{PRODUCT NAME: VMS Workstation Software, Version 4.3}

SSA 28.06.11-AHARDWARE REQUIREMENTS

Processors SupportedVAX:

VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 6000 Model 400 SeriesVAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978VAX-11/730, VAX-11/750, VAX-11/780, VAX- 11/785MicroVAX: MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX 3300, MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, MicroVAX 3800, MicroVAX 3900VAXstation: VAXstation II, VAXstation 2000, VAXstation 3100 Series, VAXstation 3200, VAXstation 3500, VAXstation 3520, VAXstation 3540VAXserver: VAXserver 3100, VAXserver 3300, VAXserver 3400, VAXserver 3500, VAXserver 3600, VAXserver 3602, VAXserver 3800, VAXserver 3900VAXserver 6000-210, VAXserver 6000-310, VAXserver 6000-410, VAXserver 6000-420Processors Not Supported

MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation 8000

Processor Restrictions

The VAXstation 3100 Series supported is with GPX Graphics.

The VAXstation 3540 is excluding VWS and DECwindows X11 Server.

VWS installs on the above non-workstation machines for clustered environments thus allowing VWS to boot into the cluster and take advantage of the windowing ayatem. VWS cannot run without a workstation.

Block Space Requirements (Block Cluster Size = 1):

Installation

The following table refers to the block size requirements necessary for the installation to �nish successfully and for permanent residence of the VWS software on the system disk. Decide what you want installed onto the disk then add up the block sized given in the tables. This will aid the small disk users who would like to install as much as possible but cannot do it all at one time.August 1990 AE-LT76E-TE dt

Table 1 INSTALLATION and PERMANENT Installation VWS

Saveset Option Blocks for Installation Permanent Blocks Required

A Initial Saveset 324 280 B VWS Images 4770 4770 C VWS Language Files 6174 „ D VWS Programming Guide Examples

540 540

E VWS 77 DPI Monochrome Fonts 1566 1566 F VWS 77 DPI Color/Grey Scale Fonts

2646 2646

G VWS 100 DPI Monochrome Fonts

846 846

H VWS 100 DPI Color/Grey Scale Fonts

1548 1548

A HCUIS Initial Saveset 108 0 B HCUIS Images 2412 2412

A SIGHT Initial Saveset 108 0 B SIGHT Images 558 558 C SIGHT Monochrome Fonts 1440 1440 D SIGHT Color/Grey Scale Fonts 2232 2232

A VWSDEMO Initial Saveset 162 0 B VWSDEMO DEMO Sources 1530 1530 C VWSDEMO DEMO Images 3636 3636

„ Plus amount required for each language chosen. See INSTALLATION and PERMANENT VWS LANGUAGE chart below.

Table 2 INSTALLATION and PERMANENT VWS LANGUAGE Chart

Language Support Desired Installation/Permanent Blocks Required

Ada 1806 BLISS 243 C 645 FORTRAN 264 MACRO 189 PASCAL 720 PL/I 717

Table 3 INSTALLATION and PERMANENT Installation VWS Migration Tools

Saveset Option Blocks for Installation Permanent Blocks Required

A VAXuisx Initial Saveset 180 80 B VAXuisx Images 810 810 C VAXuisx 77 DPI fonts in DECwindows format

990 990

D VAXuisx 100 DPI fonts in DECwindows format

612 612

E VAXuisx SIGHT fonts in DECwindows format

846 846

A UIS to DDIF Converter Initial Saveset

108 0

B UIS to DDIF Converter Images 234 234

A UIS Source Code Annotator Initial Saveset

108 0

B UIS Source Code Annotator Images

684 684

A VWS/DECwindows Server Initial Saveset

162 0

B VWS/DECwindows Server VMS V5.1 Files

450† 450†

C VWS/DECwindows Server VMS V5.2 Files

468† 468†

D VWS/DECwindows Server VMS V5.3 Files

5112 5112

A A Guide to Migrating VWS Applicationsto DECwindows

5112 5112

† One or the other is installed, depending on VMS Version.

NOTES:

The VWS043.A saveset is 800 blocks, all of which are initially put onto the system. This value must be included in storage calculations.

The block sizes given refer to approximate values; the actual sizes can vary depending on user’s system environment, con�guration, and software options selected. In general, the values given here are slightly higher than the actual values.

Sites that install VWS on a system running the DECwindows software will follow the path of a cluster installation.

Clustered systems must add in both the Monochrome and Color/Grey scale font values when adding up the number of blocks necessary.

With the exception of the VWS/DECwindows Server which requires VWS, the VWS Migration Tools Kit does not require VWS be installed and will run on any VMS system.

To run HCUIS and/or SIGHT on VAXuisx, the VWS and SIGHT fonts must be installed.

Native VWS/UIS does NOT support the VS3100 SPX Color Graphics Accelerator. This support is provided through DECwindows and VAXuisx.

VWS/UIS does NOT support the VAXstation 3520 and VAXstation 3540. These workstations are supported through DECwindows and VAXuisx.

SIGHT, HCUIS, VAXuisx, UISANN and UISCNV are all part of the common VWS043 Installation Guide. To install these products, (VWS043.A) is required.

HCUIS no longer requires a workstation to run.

No Software License is required to install and run the VWS Migration Tools Kit.

OPTIONAL HARDWARE

The following workstation-speci�c hardware is supported:

LA50, LA100, LA75, LA210, LA324, LN03, LN03R, LN03-PLUS, LVP16, LCP01, LCG01, LJ250, Print- Server 40, HP7475�, HP7550�, HP7580�, HP7585�, the Apple LaserWriter�, and the LASERGRAPHICS MPS-2000�.

Note: The LN03 does not support the printing of complex, multi-tone graphical images.

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and licensed VAXcluster* con�guration without restrictions. The HARDWARE REQUIREMENTS sections of this product’s Software Product Description and System Support Addendum detail any special hardware required by this product.

* V5.x VAXcluster con�gurations are fully described in the VAXcluster Software Product Description (29.78.xx) and include CI, Ethernet and Mixed Interconnect con�gurations.

SOFTWARE REQUIREMENTS

� VMS Operating System V5.0 - V5.3

For Workstations Running VWS:

� VMS Operating System V5.0 - V5.3

For the VAXuisx Run-Time Library, VMS V5.3 is required.

For the DECwindows X11/Server, UIS to DDIF Converter, UIS Source Code Annotator V5.1 - V5.3 is required.

VMS TAILORING

For VMS V5.x the following VMS classes are required for full functionality of this layered product:

VMS Required Saveset Programming Support VAX Workstation Support

For more information on VMS classes and tailoring, refer to the VMS Operating System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

DEC GKS for VMS V4.1 DEC PHIGS for VMS V2.1

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this product may be different from the requirements for the current version.

DISTRIBUTION MEDIA

Tape: 9-track 1600 BPI Magtape, TK50 Streaming Tape Cartridge.

Disk: RX33 Floppy Diskette

Note: After this release, RX33 distribution kits will no longer be available as distribution media.

This product is also available as part of the VMS Consolidated Software Distribution on CDROM.

ORDERING INFORMATION

Software Licenses: QL-A96A*-** Software Media: QA-A96A*-** Software Documentation: QA-A96AA-GZ Software Product Services: QT-A96A*-**

* Denotes variant �elds. For additional information on available licenses, services and media, refer to the appropriate price book.

The above information is valid at time of release. Please contact your local Digital of�ce for the most up-to-date information.

� HP7475, HP7550, HP7580, HP7585, HP7510 are registered trademarks of the Hewlett-Packard Company.

� Apple LaserWriter is a trademark of Apple Corporation, Inc.

� LASERGRAPHICS MPS-2000 is a trademark of LaserGraphics, Inc.

� The DIGITAL logo, VMS, VWS, VAX, MicroVAX, VAXstation, VAXserver, DECwindows, ReGIS, DEC GKS, DEC PHIGS and VAXset are trademarks of Digital Equipment Corporation.