4 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  ALL-IN-1, Version 2.4              SSA 27.30.04-A

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978

                    VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900

          VAXstation: VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540





                                       DIGITAL                   July 1990

                                                               AE-LT58C-TE

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          Processors Not Supported

          VAX:      VAX-11/725, VAX-11/730, VAX-11/782

          VAXserver: VAXserver 3100, VAXserver 3300,
                     VAXserver 3400, VAXserver 3500,
                     VAXserver 3600, VAXserver 3602,
                     VAXserver 3800, VAXserver 3900

                     VAXserver 6000-210, VAXserver 6000-310,
                     VAXserver 6000-410, VAXserver 6000-420

                    (VAXservers do not support interactive ALL-IN-1 opera-
                    tions.)

          MicroVAX: MicroVAX I

          VAXstation: VAXstation I, VAXstation 8000

          Processor Restriction

          A TK50 Tape Drive is required for standalone MicroVAX 2000 and
          VAXstation 2000 systems.

          ALL-IN-1 does not support diskless satellite systems in Ethernet
          and mixed interconnect clusters.

          The following processors are recommended for base memory config-
          urations. The actual amount of memory required is dependent on
          the number of simultaneous users. This information is being up-
          dated on a continuing basis. If any of the supported processors
          are not on this list, consult with your local Digital office.







                                          2

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A


          ________________________________________________________________
              
                             No of    Minimum
                             Proces-  Memory   Disk
          Processor          sors     MB       Drives

          MicroVAX 2000*     1        14       2

          MicroVAX II        1        16       2

          MicroVAX 3100      1        8        3

          VAX 8250           1        16       2

          VAX 8350           2        24       2

          MicroVAX           1        28       3
          3300/3400

          MicroVAX           1        32       4
          3500/3600

          VAX 6210           1        32       4

          MicroVAX 3800      1        48       4

          MicroVAX 3900      1        48       2

          VAX 6310           1        64       4

          VAX 8530           1        48       4

          VAX 6220           2        64       4

          VAX 8810           1        48       4




                                          3

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A

          ________________________________________________________________
              
                             No of    Minimum
                             Proces-  Memory   Disk
          Processor          sors     MB       Drives


          VAX 6230           3        128      5

          VAX 6320           2        128      5

          VAX 8820           2        96       6

          VAX 6240           1        128      6

          VAX 6330           3        128      7

          VAX 8830           3        128      8

          VAX 6340           4        128      8

          VAX 6350           5        192      9

          VAX 8840           4        128      9

          VAX 6360           6        192      10

          VAX 6000-410       1        64       4

          VAX 6000-420       2        128      6

          VAX 6000-430       3        192      8

          VAX 6000-440       4        192      10

          VAX_6000-450_______5________192______12_________________________



                                          4

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          *  VAXstation 2000 - The minimum configuration to run ALL-IN-1,
             Version 2.4 in stand-alone mode is 14MB of memory with a TK50
             expansion box and RD 54s. A 6MB system is suitable if running
             in a cluster.

          Other Hardware

          The following terminals are supported for text:

          o  VT100 series (VT100, VT100W, VT101, VT102, VT125) or ter-
             minals in VT100 emulation mode* (DECmate, Rainbow, Profes-
             sional)

          o  VT200 series (VT220, VT240, VT241)

          o  VT300 series (VT320, VT330, VT340)

          o  VT420 Text Video Terminal

          o  VT1000 in VT300 emulation mode or via DECwindows DECterm mode

          o  VAXmate in VT200 emulation mode

          o  VAXstation Series

          o  The following IBM[R] terminal keyboards on CUT mode terminals
             are supported using the CMX04 option card:

                122 Key Typewriter (native mode)
                122/104 Key Typewriter (emulation mode)
                102 Key Typewriter
                87 Key Typewriter

          o  The following processors are supported in VT220 emulation
             mode:

                DECstation 200
                DECstation 210
                DECstation 300
                DECstation 316
                DECstation 320

                                          5

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



                DECstation 350

          *  WPS-PLUS supports only those terminals with Advanced Video
             Option (AVO). It does not support the VT100 without AVO,
             VT131, DECmate I, or WS78.

          Technical Character Set Support:

          o  VT220, VT300 series terminals

          o  VAXstation II - supported in VT220 emulator mode

          o  DECmate II or DECmate III, with DECmate/WPS (minimum V2.1)
             software (in CX mode)

          o  VAXmate

          Printers:

          Personal:     LA50

                        LA70

                        LA75

                        LQP03 (with Optional Sheet Feeder)

          Shared:       LA100-PC

                        LA210

                        LN03 (with Optional Sheet Feeder)

                        LN03 PLUS (with Optional Sheet Feeder)





                                          6

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A




                        LN03R (Supported via the ANSI
                        translator; no Sheetfeeder Support)

                        LQP02 (with Optional Sheet Feeder)

                        LQP45 (with Optional Sheet Feeder)

                        QUME Wide Track Printer

                        LJ250



          Departmental: LP11

                        PrintServer 40 (LPS40) - Supported via the ANSI
                        translator

                        PrintServer 20 (LPS20) - Supported via the ANSI
                        Translator

          Note:    The LG31 can be operated in fallback mode only using
                   the LQP45 printer tables.

                   The LA324 can be operated using the LJ250 printer
                   tables.

                   The LA70 can be operated using the LA75 printer tables.










                                          7

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          Block Space Requirements (Block Cluster Size = 1):

          Entire installation placed on the system disk:

          With WPS-PLUS:

          Transient space 74,000 + number of shared directories x 1000
          (75,000 minimum) Permanent space 65,200 + space required for
          shared directories.

          Without WPS-PLUS:

          Transient space 63,000 + number of shared directories x 1000
          (64,000 minimum) Permanent space 54,500 + space required for
          shared directories.

          Installation divided on separate disks:

          With WPS-PLUS:

          ________________________________________________________________
                             Transient     Permanent
          ___________________Space_________Space__________________________

          Library files      39,000        31,200

          Data files         5,000         3,000

          Language files     28,000        25,000

          SDAF               1,000         1,000

          Accounts           1,000         1,000

          Shared directo-    1,000 each    *
          ries____________________________________________________________

          Without WPS-PLUS:

                                          8

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A


          ________________________________________________________________
                             Transient     Permanent
          ___________________Space_________Space__________________________

          Library files      33,000        26,500

          Data files:        4,000         3,000

          Language files     24,000        22,000

          SDAF               1,000         1,000

          Accounts           1,000         1,000

          Shared directo-    1,000 each    *
          ries____________________________________________________________

          NON-SAFETY MODE installation (Permanent space is the same for
          safety installation):

          With WPS-PLUS:

          ________________________________________________________________
                             Transient     Permanent
          ___________________Space_________Space__________________________

          System Disk        15,000        4,000 *

          ________________________________________________________________

          Without WPS-PLUS:

          ________________________________________________________________
                             Transient     Permanent
          ___________________Space_________Space__________________________

          System Disk        15,000        3,500 *



                                          9

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A


          ________________________________________________________________
                             Transient     Permanent
          ___________________Space_________Space__________________________


          ________________________________________________________________

          *  Space depends on the number and content of the directories.

          Additional space of approximately 1,000 blocks will be required
          on multi-lingual systems.

          The installation will run in SAFETY-MODE if there are approxi-
          mately 75,000 blocks free on the system disk.

          All sizes are approximations; actual sizes may vary depending on
          the users system environment, configuration and software options
          selected.

          OPTIONAL HARDWARE - Country Specific

          ALL-IN-1 supports any mass storage, unit record, terminal, or
          printer device supported by the prerequisite software.

          The autodial feature of the Communications application supports
          the following modems:

             Digital Equipment DF02-AC
             Digital Equipment DF03-AC
             Digital Equipment DF100 series modems
               Case 440/12
             Racal-Milgo MPS1222-AD
             Racal-Milgo MPS1222 with Racal-Vadic VA811

          CLUSTER ENVIRONMENT

          ALL-IN-1 is fully supported when installed on any valid and
          licensed VAXcluster* configuration without restrictions. The
          HARDWARE REQUIREMENTS sections of this product's Software Prod-
          uct Description and System Support Addendum detail any special
          hardware required by this product.

                                         10

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (SPD 29.78.xx) and
             include CI, Ethernet, and Mixed Interconnect configurations.




































                                         11

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          SOFTWARE REQUIREMENTS

          o  VMS Operating System V5.1 - V5.3 (DECwindows must be in-
             stalled for CDA usage)

          o  DECnet-VAX V5.1 - V5.3 is required for multinode support.

          o  VAX FMS V2.4 (included with the ALL-IN-1 Kit)

          o  VAX Notes V2.0/V2.1 (included with the ALL-IN-1 Kit - re-
             quired for Group Conferencing)

          o  CDA Converter Library for VMS V1.0 (included with the ALL-IN-
             1 Kit -required for CDA support)

          The following chart shows the necessary version levels of soft-
          ware required with the underlying VMS Operating System.

          ________________________________________________________________
                                VMS    VMS    VMS
          Software______________V5.1___V5.2___V5.3________________________

          ALL-IN-1 V2.4         Yes    Yes    Yes

          VAX Notes V2.0*       Yes    Yes    No

          VAX Notes V2.1*       No     No     Yes

          DECwindows/CDA        V1.0   V1.0   V2.0
          base

          ALL-IN-1 DESKtop      No     No     Yes
          for VMS DECwin-
          dows V1.0

          CDA Converter         Yes    Yes    Yes
          Library V1.0


                                         12

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A


          ________________________________________________________________
                                VMS    VMS    VMS
          Software______________V5.1___V5.2___V5.3________________________


          CDA Converter         No     No     Yes
          Library V1.1

          CDA PATCH             No     No     Yes

          VAX Message Router    V3.1   V3.1   V3.1

          Message Router VMS    V3.1   V3.1   V3.1
            Gateway

          ALL-IN-1 MAIL - VT    No     Yes    Yes
          V1.0

          ALL-IN-1 MAIL -       No     No     Yes
            DECwindows V1.0

          ALL-IN-1 MAIL -       No     Yes    Yes
          DOS V1.0

          ALL-IN-1 DESKTOP      Yes    Yes    Yes
           Server for VMS V1.0
          ____________________________________________________________

          *  To use VAX Notes with the DECwindows interface, the user must
             install VMS V5.3 and DECwindows V5.3. Any other version may
             result in incorrect operation of the DECwindows interface of
             VAX Notes.

          ALL-IN-1 provides an interface to the CDA support on a VMS sys-
          tem. The level of CDA support via ALL-IN-1 is entirely dependent
          on the level of CDA support on the VMS system.

          Note: ALL-IN-1 and ALL-IN-1 STARTER cannot coexist on the same
          system.

                                         13

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          VMS V5.1

          VMS has no built-in CDA support.

          DECwindows (separate kit) must be installed to get basic CDA
          support.

          DECwrite is required to have DECwrite style files.

          DECchart is required to have DECchart style files.

          CDA Converter Library for VMS V1.0 can be installed to provide
          additional CDA front-ends and back-ends (required for conver-
          sions to/from DX/WPS-PLUS).

          VMS V5.2

          VMS has basic CDA support for DDIF, TEXT and PS.

          DECwindows must be installed to use CDA.

          DECwrite is required to have DECwrite style files.

          DECchart is required to have DECchart style files.

          CDA Converter Library for VMS V1.0 can be installed to provide
          additional CDA front-ends and back-ends (required for conver-
          sions to/from DX/WPS-PLUS).

          VMS V5.3

          VMS has basic CDA support for DDIF, TEXT and PS.

          DECwindows must be installed to use CDA.

          DECwrite is required to have DECwrite style files.

          DECchart is required to have DECchart style files.

          CDA Converter Library for VMS V1.0 can be installed to provide
          additional CDA front-ends and back-ends (required for conver-
          sions to/from DX/WPS-PLUS).

          CDA Library V1.1 IFT1 can be installed on V5.3.

          VMS Tailoring

                                         14

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          For VMS V5.x systems, the following classes of VMS are required
          for full functionality of this layered product:

             o  Network Support

             o  Programming Support

             o  System Programming Support

             o  Secure User's Environment

             o  Utilities

             o  BLISS Required Files

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).





















                                         15

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          Country Specific Software

          At this time, only U.S. English is available. Please contact
          your Digital office for the latest information on other language
          versions and for details of supported multi-lingual configura-
          tions.

             o  Within the U.S. product, an auto-dial/re-dial facility is
                provided.

             o  Within the U.S. product, the following WPS-PLUS function-
                ality is available:

                -  A spelling verifier and corrector with a spelling
                   database of over 80,000 words which can be used in
                   conjunction with up to 12,000 additional user-specific
                   words.

                -  Usage alert which provides brief definitions of easily
                   confused words, such as ``effect'' and ``affect'' or
                   ``guarantee''and ``guaranty''.

                -  Electronic thesaurus, based on the Houghton Mifflin
                   Roget's II: The New Thesaurus which allows users to
                   obtain synonyms, including inflections (ie., -ed, -ing,
                   -ly) and short definitions based on parts of speech for
                   a selected word.

          OPTIONAL SOFTWARE

          VAX Message Router V3.1 (included with the ALL-IN-1 Kit)

          Message Router VMS Gateway V3.1 (included with the ALL-IN-1 Kit)

          DECdx/VMS V1.2

          Note: DECdx/VMS is only required to allow users to transfer
          DX documents between Digital's mainframes (in conjunction with
          DECdx/RSTS, DECdx/RSX and DECdx/TOPS-20).)

          DECtalk Mail Access V1.1

          DECpage V3.1

          VAX ACMS V3.1

                                         16

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



          VAX DATATRIEVE V5.0

          VAX RALLY V2.1

          VAX TEAMDATA V1.3

          VAX VTX V4.0

          VAX Language and Specialized Lexicons V2.0:

                British Lexicon V2.0
                Deutsch Lexicon V2.0
                Francais Lexicon V2.0
                American Medical Lexicon V2.0
                American Business Lexicon V2.0

          VAX Grammar Checker V1.0

          INSTALLATION

          This software product will be installed by Digital at no addi-
          tional charge if purchased concurrently with a Startup Service
          Package that includes installation service. Both the operating
          system and this product must be installed concurrently.

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          Tape: 9-Track 1600 BPI Magtape, TK50 CompacTape Cartridge

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

             Software Licenses: QL-AAAA*-**
             Software Media: QA-AAAA*-**
             Complete Documentation Kit: QA-AAA**-GZ

                ALL-IN-1/US Management Documentation:
                    QA-AAAAB-GZ

                                         17

 


          ALL-IN-1, Version 2.4                             SSA 27.30.04-A



                ALL-IN-1/ US AP&I Documentation Kit:
                   QA-AAAAC-GZ
                Customization Kit: QA-AAAAD-GZ

             Software Product Services: QT-AAAA*-**

             *  Denotes variant fields. For additional information on
                available licenses, services and media, refer to the
                appropriate price book.

          The above information is valid at the time of release. Please
          contact your local Digital office for the most up-to-date infor-
          mation.

          [R]  PostScript is a registered trademark of Adobe Systems Inc.

          [R]  IBM is a registered trademark of International Business
               Machines Corporation.

          [R]  The DIGITAL Logo is a trademark of Digital Equipment Corpo-
               ration.

          [TM] ALL-IN-1, DEC, DECmate, DECnet, DECnet-VAX, DECtalk,
               DECwrite, DECserver, DECstation, DDIF, DX, EDT, LA50, LA75,
               LJ250, LN03, LN03 PLUS, LN03R, LQP02, LQP03, MicroVAX,
               Professional, Rainbow, VAX, VAXstation, VAXserver, VMS,
               VT, WPS and WPS-PLUS are trademarks of Digital Equipment
               Corporation.












                                         18
