 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  ALL-IN-1 MAIL, Version 1.0         SSA 31.51.00-A

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978, VAX 9000

                    VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900

          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,






                                       DIGITAL                   June 1990

                                                               AE-NL25A-TK

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A




                    VAXstation 3540

          VAXserver:VAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,
                    VAXserver 3800, VAXserver 3900,

                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420

          Processors Not Supported:

          VAX:      VAX-11/725, VAX-11/730, VAX-11/782

          MicroVAX: MicroVAX I

          VAXstationVAXstation I, VAXstation 8000






          Other Hardware Requirements

          ALL-IN-1 MAIL for Video Terminals

          The software for ALL-IN-1 MAIL for Video Terminals is packaged
          with the ALL-IN-1 MAIL Server and runs on all the same supported
          processors as the Server.

          Its command-line interface is supported on any VT1xx, VT2xx, or
          VT3xx terminal, or any output device running a Digital supplied
          and supported emulator for the above.




                                          2

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          ALL-IN-1 MAIL for VMS DECwindows

          The software for ALL-IN-1 MAIL for VMS DECwindows is packaged
          with the ALL-IN-1 MAIL Server and runs on all the same supported
          processors as the Server. Use of the interface requires one
          of the following workstations, or a valid X11 display device
          supported by Digital.

          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540

          The client software must run within the same VAXcluster as the
          server software.

          When the product is used remotely by an X11 display device, the
          interface quality depends on the screen size, resolution and
          aspect of the X11 display server device.




















                                          3

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          Block Space Requirements for VMS Components

          (Block Cluster Size = 1)

          ________________________________________________________________
                        During    After,
                        In-       on        After,
                        stal-     system    on work
          Component_____lation____disk______disk__________________________

          All compo-    30,000[1] 8,550     18,200
          nents

          Server        22,200    3,500     17,500
          components

          DECwindows    3,000     3,000     700[2]
          Client

          VT Inter-     1,700     1,700     700[2]
          face

          DOS Client    350       350       700[2]
          Support
          ________________________________________________________________
          [1]Includes installation overhead.
          [2]Library_common_to_all_interfaces,_installed_once_____________

          The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options.

          The user space required on the server is determined by the
          amount of mail the user wishes to file.





                                          4

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          Memory Requirements for DECwindows Support

          The minimum supported memory for this application running in
          a standalone DECwindows environment with both the client and
          server executing on that same system is 8MB.

          The performance and memory usage of DECwindows applications are
          particularly sensitive to system configuration. Less memory may
          be required on the client system (the system where the software
          is installed and executed) if the display server (the component
          that displays the application) resides on another system. More
          memory may be required on a system with several applications
          running or to improve the performance of an application.

          ALL-IN-1 MAIL for DOS

          Support for 8-bit characters is provided only on EGA and VGA
          machines.

          Unless otherwise noted here, the ALL-IN-1 MAIL for DOS component
          runs on any valid configuration having a minimum of 640 KB of
          memory which is supported by DECnet PCSA Client for DOS. Refer
          to the DECnet PCSA Client for DOS Software Product Description
          (SPD 55.07.xx).

          420 KB of free memory is required after loading DECnet PCSA
          Client for DOS.

          Two versions of the image are provided; one which uses overlays
          and can be used on a PC with no expanded or extended memory,
          and another which uses the DOS-Extender and takes advantage of
          extended memory. The DOS-Extender version may only be used on
          PCs that use the Intel 286/386 CPU with 640 KB of conventional
          memory and 1 MB of extended (not expanded) memory. The DOS-
          Extender version is not supported on VAXmate. Both versions have
          the same functionality; the DOS-Extender version will provide
          better performance.


                                          5

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          ALL-IN-1 MAIL for DOS software can be stored either on the per-
          sonal computer's local storage device or on the server sys-
          tem. The maximum disk space required during the installation
          of all ALL-IN-1 MAIL for DOS software is 2.2 MB on a PC. Once
          installed, one version of the software occupies 1.15 MB of disk
          space.

          Installed as a disk service on the VAX, the software requires
          22,528 blocks on a VMS disk. The additional space required
          on the server is to house both the standard and DOS extender
          versions.

          CLUSTER ENVIRONMENT

          The VMS layered product components of this product are fully
          supported when installed on any valid and licensed VAXcluster *
          configuration without restrictions. The HARDWARE REQUIREMENTS
          sections of this product's Software Product Description and
          System Support Addendum detail any special hardware required by
          this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (SPD 29.78.xx) and
             include CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          For the ALL-IN-1 MAIL Server and ALL-IN-1 MAIL for Video Termi-
          nals:

          o  VMS Operating System V5.2 or V5.3

          o  DECnet-VAX V5.2 or V5.3

          For ALL-IN-1 MAIL for VMS DECwindows:

          o  VMS Operating System V5.3 (with necessary components of VMS
             DECwindows) on any CPU running DECwindows components.

          o  DECnet-VAX V5.3

                                          6

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          This product can run in any of the following ways:

          o  On a workstation which is in the same Local Area VAXcluster
             as the mail server software (stand-alone execution)

          o  On a separate workstation device which is not a member of
             the VAXcluster where the client and mail server software are
             running, but is connected to it via DECnet (remote execution)

          o  On the server CPU or VAXcluster using an attached X11 display
             device supported by Digital

          VMS DECwindows is part of the VMS Operating System but must be
          installed separately. Installation of VMS DECwindows gives the
          user the option to install any or all of the following three
          components:

          o  VMS DECwindows Compute Server (Base kit; includes runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          For stand-alone execution, the following DECwindows components
          must be installed on the workstation machine:

          o  VMS DECwindows Base

          o  VMS DECwindows Device Support

          For remote execution, the following DECwindows components must
          be installed on the machines:

          On the X11 Display Device:

          o  VMS DECwindows Compute Server

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

                                          7

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          On the X11 Client System:

          o  VMS DECwindows Compute Server

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          For ALL-IN-1 MAIL for DOS:

          On the PC:

          o  MS-DOS or PC-DOS versions supported by DECnet/PCSA version
             2.2 or 3.0

          o  DECnet PCSA Client for DOS: PC V2.2 or 3.0
             or

          o  DECnet/PCSA Client: VAXmate V2.2

          On its corresponding ALL-IN-1 MAIL Server:

          o  VMS Operating System V5.2 or V5.3

          o  DECnet-VAX V5.2 or V5.3

          o  VMS Services for PCs V3.0

          Internationalization

          Language options are under development. Please see future ver-
          sions of this document for availability of ALL-IN-1 MAIL in
          local languages.

          OPTIONAL SOFTWARE:

          o  CDA Converter Library for VMS V1.0 (SPD 31.31.xx)

          o  VAX Message Router V3.1 (SPD 26.33.xx)

          o  VAX Message Router VMSmail Gateway V3.1 (SPD 26.33.xx)

          o  ULTRIX Mail Connection V1.1 (SPD 29.05.xx)

          o  VAX Message Router/P Gateway V1.1 (SPD 28.94.xx)

                                          8

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          o  VAX Message Router/S Gateway V1.1 (SPD 29.24.xx)

          o  VAX Message Router Telex Gateway V1.0A (SPD 29.96.xx)

          o  VAX MAILGATE for MCI Mail V2.0 (SPD 27.34.xx)

          o  VAX Message Router X.400 Gateway V2.1 (SPD 27.50.xx)

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          For all components:

          Tape:    9-track 1600 BPI Magtape (PE)
                   TK50 Streaming Tape

          In addition, for the DOS interface only:

          RX24 (3 1/2 inch) hard-shelled
          diskettes
          RX31 (5 1/4 inch) floppy
          diskettes
          RX33 (5 1/4 inch) high-density
          floppy diskettes

          ORDERING INFORMATION

          Operation of this product requires an ALL-IN-1 MAIL Server, and
          at least one ALL-IN-1 MAIL client.

          Server Options:

          Choose one of the following server options:

                                          9

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          ALL-IN-1 MAIL Server for VMS:

             Software Licenses: QL-YCZ99-**
             Software Media: QA-YCZA*-**
             Software Documentation: QA-YCZAA-GZ
             Software Product Services: QT-YCZA*-**

          The media kit includes media and documentation for the server,
          and media only (no documentation or license) for the DECwindows
          and Video Terminals clients. See client listings for licensing
          information for these clients.

          ALL-IN-1 MAIL Local Area Network Server Package:

          This package is used in implementations where there is no re-
          quirement to exchange mail beyond a single server, or where the
          Message Router is already owned:

             Software License and Media (TK50 only):
               QB-YFTA9-AA
             Software Product Services: QT-YCZA*-**

          Includes license, media and documentation for ALL-IN-1 MAIL
          Server, implemented on any single CPU.

          ALL-IN-1 MAIL Wide Area Network Server Package:

          This package is used in multi-server configurations, or where
          there is a requirement to interwork with another messaging
          product:

             Software Licenses: QL-YFUA9-J*
             Software Product Services: QT-YCZA*-**

          Includes licenses for ALL-IN-1 MAIL Server, Message Router, VMS-
          mail Gateway, and Message Router X.400 Gateway. Media and docu-
          mentation update service for these components must be purchased
          separately depending upon which components will be implemented:
          See service offerings for ALL-IN-1 MAIL Server for VMS, plus
          one of the two gateway packages: Message Router VMSmail Gateway
          (SPD 26.33.xx) or Message Router X.400 Gateway (SPD 27.50.xx).

                                         10

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          Service on either gateway covers service for the Message Router
          itself.

             Software Media: QA-YFUAA-**

          Includes media and documentation for ALL-IN-1 MAIL Server,
          Message Router, and VMSmail Gateway. Media and documentation for
          the Message Router X.400 Gateway must be purchased separately.

          Client Options:

          ALL-IN-1 MAIL for VMS DECwindows:

             Software Licenses: QL-VZ7A*-**
             Software Media: included with server media
             Software Documentation: QA-VZ7AA-GZ
             Software Product Services: QT-VZ7A*-**

          ALL-IN-1 MAIL for DOS:

             Software Licenses: QL-VZ8AW-** or included
               with DECnet PCSA Client for DOS
             Software Media: QA-VZ8A*-**
             Software Documentation: QA-VZ8AA-GZ
             Software Product Services: QT-VZ8A*-**

          ALL-IN-1 MAIL for Video Terminals:

             Software Licenses: QL-YHSA9-**
             Software Media: included with server media
             Software Documentation: QA-YHSAA-GZ
             Software Product Services: QT-YHSA*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media, refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

                                         11

 


          ALL-IN-1 MAIL, Version 1.0                        SSA 31.51.00-A



          Note: For the purposes of this Software Product Description,
          IBM's Personal Computer Disk Operating System, Microsoft Corpo-
          ration's MS-DOS, and COMPAQ Computer Corporation's COMPAQ MS-DOS
          are referred to simply as DOS.

          [R]  IBM is a registered trademark of IBM Corporation.

          [R]  MS-DOS is a registered trademark of Microsoft Corporation.

          [TM] PROFS and SNADS are trademarks of IBM Corporation.

          [R]  The DIGITAL Logo is a registered trademark of Digital
               Equipment Corporation.

          [TM] ALL-IN-1, DECwindows, MicroVAX, MicroVMS, ULTRIX, ULTRIX
               Mail Connection, VAXserver, VAXstation, VMS and VT are
               trademarks of Digital Equipment Corporation.






















                                         12
