PRODUCT NAME: AAF01/VMS Subroutine Library, Version 2.0         SSA 27.49.01-A
              (for VMS Operating Systems)


HARDWARE REQUIREMENTS

Processors supported

VAX:  VAX 8600, VAX 8650

      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

MicroVAX: MicroVAX II

VAXstation: VAXstation 3200

Processors not supported

VAX: VAX 6210, VAX 6220, VAX 6230, VAX 6240, VAX 8200, VAX 8250, VAX 8300,
     VAX 8350, VAX 8500, VAX 8530, VAX 8550, VAX 8700, VAX 8800, VAX 8810, 
     VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978

     VAX-11/725, VAX-11/782

MicroVAX: MicroVAX I, MicroVAX 2000, MicroVAX 3500/3600

VAXstation: VAXstation I, VAXstation II, VAXstation 2000, VAXstation 3500
            VAXstation 8000

VAXserver:  VAXserver 3500/3600/3602

Other hardware required

^  One DRE11-C or DRQ11-C interface
^  One AAF01-A Interface
^  Hardware capable of reading one of the distribution media upon which this 
   product is offered.

Block space requirements (Block Cluster Size = 1):

Disk space required for installation:           850 blocks  
                                              (425K bytes) 

Disk space required for use (permanent):        550 blocks  
                                              (275K bytes) 

These counts refer to the disk space required on the system disk. The sizes
are approximate; actual sizes may vary depending on the user's system
environment, configuration, and software options selected. 
  
OPTIONAL HARDWARE

^  Up to eight AAF01-A Interfaces
^  ASF01-A 16-Channel Simultaneous Sample and Hold

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and
licensed VAXcluster* configuration without restrictions. The HARDWARE
REQUIREMENTS sections of this product's Software Product Description and
System Support Addendum detail any special hardware required by this product.

* V5.x VAXcluster configurations are fully described in the VAXcluster 
  Software Product Description (29.78.xx) and include CI, Ethernet and Mixed 
  Interconnect configurations.

SOFTWARE REQUIREMENTS

VMS Operating System, V5.0
DRX11-C/VMS Driver, V6.0

VMS Tailoring

The following VMS classes are required for full functionality of this layered
product: 

^  VMS Required Saveset
^  Programming Support
^  System Programming Support

OPTIONAL SOFTWARE

VAX-11 FORTRAN, V5.0

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this
product may be different from the minimum requirements for the current
version. 

DISTRIBUTION MEDIA

Disk: RX50 Floppy Diskette, RX33 Floppy Diskette

Tape: 9-track 1600 BPI Magtape (PE), TK50 Tape Cartridge

ORDERING INFORMATION

Software Licenses:  QL-EFRA*-**
Software Media:  QA-EFRA*-**
Software Documentation:  QA-EFRAA-GZ

* Denotes variant fields. For additional information on available licenses,
  services and media refer to the appropriate price book.

The above information is valid at time of release. Please contact your local
DIGITAL office for the most up-to-date information. 




October 1988
AE-MR88A-TE

