 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  VAX ACMS, Version 3.2       SSA 25.50.10-A
                          (Application Control and Man-
                          agement System)

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:     VAXft 3000-310,
                    VAX 4000 Model 200,
                    VAX 4000 Model 300,
                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 6000 Model 500 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840

                    VAX 9000-210, VAX 9000 Model 400 Series

                    VAX-11/730, VAX-11/750, VAX-11/780,
                    VAX-11/785

           MicroVAX:MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900


                                    DIGITAL                 May 1991

                                                         AE-LT05C-TE

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)


           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

           VAXserver: VAXserver 3100, VAXserver 3300,
                      VAXserver 3400, VAXserver 3500,
                      VAXserver 3600, VAXserver 3602,
                      VAXserver 3800, VAXserver 3900,
                      VAXserver 4000 Model 200
                      VAXserver 4000 Model 300

                      VAXserver 6000-210, VAXserver 6000-210,
                      VAXserver 6000-310, VAXserver 6000-320,
                      VAXserver 6000-410, VAXserver 6000-420,
                      VAXserver 6000-510, VAXserver 6000-520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAX-11/725, VAX 11/782, VAXsta-
           tion 8000

           Processor Restrictions

           A TK50 Tape Drive is required for standalone Microvax 2000
           and VAXstation 2000 systems.

           For MicroVAX II and VAXstation II systems:

           o  Minimum - an RD53 disk drive for system disk

           For VAX ACMS and VAX ACMS Run-time Option:

           o  At lease 4MB of memory (A typical configurations may re-
              quire more memory.)





                                       2

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           For VAX ACMS Remote Access Option:

           o  At least 2MB of memory (typical configurations may re-
              quire more memory).

           Other Hardware Required

           Disk Space Requirements (Block Cluster Size = 1):

           Development System

           Disk space required for     18,800 blocks
           installation:
                                       (9.6M bytes)

           Disk space required for     15,800 blocks
           use (permanent):
                                       (8.1M bytes)

           Run-time Option

           Disk space required for     17,400 blocks
           installation:
                                       (9M bytes)

           Disk space required for     15,200 blocks
           use (permanent):
                                       (7.8M bytes)

           Remote Access Option

           Disk space required for     10,500 blocks
           installation:
                                       (5.4M bytes)

           Disk space required for     8,800 blocks
           use (permanent):
                                       (4.5M bytes)



                                       3

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.


           OPTIONAL HARDWARE

           Any device supported by the prerequisite software.

           Any DECnet hardware as required by the distributed VAX ACMS
           environment.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.

           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (29.78.xx) and
              include CI, Ethernet and Mixed Interconnect configura-
              tions.

           SOFTWARE REQUIREMENTS

           For VAX ACMS

           o  VMS Operating System V5.4-1

           Layered Products

           o  VAX CDD/Plus V4.2A - V4.3

           For VAX ACMS Run-time Option

           o  VMS Operating System V5.4-1

                                       4

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           For VAX ACMS Remote Access Option

           o  VMS Operating System V5.4-1

           o  DECnet-VAX V5.0 - V5.4-1

           VMS Tailoring

           For VMS V5.x systems, the following VMS classes are required
           for full functionality of this layered product:

           Full Development Kit

           o  VMS Required Saveset

           o  Programming Support

           o  System Programming Support

           o  Utilities

           Run-time Only Kit

           o  VMS Required Saveset

           o  Programming Support

           o  System Programming Support

           o  Utilities

           Remote Kit

           o  VMS Required Saveset

           o  Network Support

           o  System Programming Support

           o  Utilities

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

                                       5

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           OPTIONAL SOFTWARE

           Certain versions of these products depend on a specific ver-
           sion of the Operating System. Please refer to the System Sup-
           port Addendum of the product in question to determine which
           version is required.

           o  ALL-IN-1 V2.2 - V2.4

           o  DECforms V1.3

           o  DECtp Desktop for ACMS V1.0

           o  DECtrace for VMS V1.0A - V1.1

           o  VAX Ada V1.0 - V2.2

           o  VAX BASIC V3.0 - V3.4

           o  VAX BLISS-32 Implementation Language V4.0 - V4.6

           o  VAX C V2.0 - V3.2

           o  VAX COBOL V4.0 - V4.4

           o  VAX COBOL GENERATOR V1.0 - V1.3

           o  VAX DATATRIEVE V4.0 - V5.1

           o  VAX DBMS V4.2

           o  VAX DEC/CMS V2.0 - V3.4

           o  VAX DEC/MMS V2.2 - V2.6

           o  VAX DEC/Test Manager V2.0 - V3.2

           o  VAX DIBOL V2.0 - V4.1A

           o  VAX FMS V2.2 - V2.4

           o  VAX FORTRAN V4.0 - V5.6

           o  VAX Language-Sensitive Editor/Source Code
              Analyzer V2.3 - 3.1

           o  VAX PASCAL V3.0 - V4.2

                                       6

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           o  VAX PL/I V2.0 - V3.4

           o  VAX RALLY V1.1 - V2.2

           o  VAX Rdb/VMS V4.0

           o  VAX TEAMDATA V1.3 - V1.4

           o  VAX TDMS V1.7 - V1.9A

           o  VAXset Package - Release 10.0

           o  VMS Volume Shadowing V1.2 - V5.4-1

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           The software documentation for this product is also avail-
           able as part of the VMS Online Documentation Library on CDROM.

           ORDERING INFORMATION

           Software Licenses:
              Development System: QL-079A*-**
              Run-Time: QL-076A*-**
              Remote Access: QL-Y30A*-**

           Software Media:
              Development System: QA-079A*-**
              Run-time: QA-076A*-**
              Remote Access: QA-Y30A*-**

                                       7

 



           VAX ACMS, Version 3.2                     SSA 25.50.10-A
           (Application Control and Management System)

           Software Documentation:
              Development System: QA-079AA-GZ
              Run-time: QA-076AA-GZ
              Remote Access: QA-Y30AA-GZ

           Software Product Services:
              Development System: QT-079A*-**
              Run-time: QT-076A*-**
              Remote Access: QT-Y30A*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           [TM]The DIGITAL Logo, ALL-IN-1, ACMS, CDD/Plus, CI, DEC,
               DECdtm, DECforms, DECnet, DECtp, DECtrace, MicroVAX,
               MicroVMS, VAX, VAX ACMS, VAX Ada, VAX BASIC, VAX C,
               VAX COBOl, VAX DATATRIEVE, VAX DBMS, VAX DIBOL,
               VAX FMS, VAX FORTRAN, VAX PASCAL, VAX RALLY, VAX
               Rdb/VMS, VAX TEAMDATA, VAXset, VAXcluster, VMS,
               VAXstation, and VAXserver are trademarks of Digital
               Equipment Corporation.















                                       8
