






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  ALL-IN-1 STARTER, Version 2.4      SSA 25.D9.01-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840,
               VAX 9000-210, VAX 9000-410

               VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900






                                  DIGITAL               November 1990

                                                          AE-MT89B-TE

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX 11/730, VAX-11/782,
     VAXstation 8000

     VAXserver processors

     Processor Restriction

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     ALL-IN-1 STARTER does not support diskless satellite systems in
     Ethernet and mixed interconnect clusters.

     The following processors are recommended for base memory config-
     urations. The actual amount of memory required is dependent on
     the number of simultaneous users. This information is being up-
     dated on a continuing basis. If any of the supported processors
     are not on this list, consult with your local Digital office.

     ________________________________________________________________
                               Minimum
                   No. of      Memory      Disk
     Processor_____Processors__MB__________Drives____________________

     MicroVAX      1           14          2
     2000*

     MicroVAX      1           16          2
     II


                                     2

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                               Minimum
                   No. of      Memory      Disk
     Processor_____Processors__MB__________Drives____________________


     MicroVAX      1           8           3
     3100

     VAX 8250      1           16          2

     VAX 8350      2           24          2

     MicroVAX      1           28          3
     3300/3400

     MicroVAX      1           32          4
     3500/3600

     VAX 6210      1           32          4

     MicroVAX      1           48          4
     3800

     MicroVAX      1           48          2
     3900

     VAX 6310      1           64          4

     VAX 8530      1           48          4

     VAX 6220      2           64          4

     VAX 8810      1           48          4

     VAX 6230      3           128         5




                                     3

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                               Minimum
                   No. of      Memory      Disk
     Processor_____Processors__MB__________Drives____________________


     VAX 6320      2           128         5

     VAX 8820      2           96          6

     VAX 6240      4           128         6

     VAX 6330      3           128         7

     VAX 8830      3           128         8

     VAX 6340      4           128         8

     VAX 6350      5           192         9

     VAX 8840      4           128         9

     VAX 6360      6           192         10

     VAX 6000-     1           64          4
     410

     VAX 6000-     2           128         6
     420

     VAX 6000-     3           192         8
     430

     VAX 6000-     4           192         10
     440





                                     4

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                               Minimum
                   No. of      Memory      Disk
     Processor_____Processors__MB__________Drives____________________


     VAX 6000-     5           192         12
     450_____________________________________________________________

     *  VAXstation 2000 - The minimum configuration to run ALL-IN-1
        STARTER Version 2.4 in stand-alone mode is 14MB of memory
        with a TK50 expansion box and RD54s. A 6MB system is suitable
        if running in a cluster.

     Other Hardware

     The following terminals are supported for text:

     o  VT100 series (VT100, VT100W, VT101, VT102, VT125) or ter-
        minals in VT100 emulation mode* (DECmate, Rainbow, Profes-
        sional)

     o  VT200 series (VT220, VT240, VT241)

     o  VT300 series (VT320, VT330, VT340)

     o  VT420 Text Video Terminal

     o  VT1000 in VT300 emulation mode or via DECwindows DECterm mode

     o  VAXmate in VT200 emulation mode

     o  VAXstation Series

     o  The following IBM[R] terminal keyboards on CUT mode terminals
        are supported using the CMX04 option card:

           122 Key Typewriter (native mode)
           122/104 Key Typewriter (emulation mode)
           102 Key Typewriter
           87 Key Typewriter

                                     5

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     o  The following processors are supported in VT220 emulation
        mode:

           DECstation 200
           DECstation 210
           DECstation 300
           DECstation 316
           DECstation 320
           DECstation 350

     *  WPS-PLUS supports only those terminals with Advanced Video
        Option (AVO). It does not support the VT100 without AVO,
        VT131, DECmate I, or WS78.

     Technical Character Set Support:

     o  VT220, VT300 series terminals

     o  VAXstation II - supported in VT220 emulator mode

     o  DECmate II or DECmate III, with DECmate/WPS (minimum V2.1)
        software (in CX mode)

     o  VAXmate

     Printers:

     Personal:   LA50

                 LA70

                 LA75

                 LQP03 (Optional Sheet Feeder also
                 supported)

     Shared:     LA100-PC

                 LA210

                                     6

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A




                 LN03 (Optional Sheet Feeder also
                 supported)

                 LN03 PLUS (Optional Sheet Feeder also
                 supported)

                 LN03R (Supported via the ANSI translator;
                 no Sheetfeeder Support)

                 LQP02 (Optional Sheet Feeder also
                 supported)

                 LQP45 (Optional Sheet Feeder also
                 supported)

                 QUME Wide Track Printer

                 LJ250

     Departmental:
                 LP11

                 DEClaser 2000 series

                 PrintServer 40 (LPS40) - Supported via the ANSI
                 translator

                 PrintServer 20 (LPS20) - Supported via the ANSI
                 Translator

     Notes:

        The LG31 can be operated in fallback mode only using the
        LQP45 printer tables.

        The LA324 can be operated using the LJ250 printer tables.



                                     7

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



        The LA70 can be operated using the LA75 printer tables.

     Block Space Requirements (Block Cluster Size = 1):

     Entire installation placed on the system disk:


































                                     8

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     With WPS-PLUS:

     Transient space 74,000 + number of shared directories x 1000
     (75,000 minimum). Permanent space 65,200 + space required for
     shared directories.

     Without WPS-PLUS:

     Transient space 63,000 + number of shared directories x 1000
     (64,000 minimum). Permanent space 54,500 + space required for
     shared directories.

     Installation divided on separate disks:

     With WPS-PLUS:

     ________________________________________________________________
                   Transient     Permanent
     ______________Space_________Space_______________________________

     Library       39,000        31,200
     files

     Data files    5,000         3,000

     Language      28,000        25,000
     files

     SDAF          1,000         1,000

     Accounts      1,000         1,000

     Shared        1,000 each    *
     directories_____________________________________________________

     Without WPS-PLUS



                                     9

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                   Transient     Permanent
     ______________Space_________Space_______________________________

     Library       33,000        26,500
     files

     Data          4,000         3,000
     files:

     Language      24,000        22,000
     files

     SDAF          1,000         1,000

     Accounts      1,000         1,000

     Shared di-    1,000 each    *
     rectories_______________________________________________________

     NON-SAFETY MODE installation (Permanent space is the same for
     safety installation):

     With WPS-PLUS:

     ________________________________________________________________
                   Transient     Permanent
     ______________Space_________Space_______________________________

     System        15,000        4,000 *
     Disk____________________________________________________________

     Without WPS-PLUS:







                                    10

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                   Transient
                               Permanent
     ______________Space_______Space_________________________________

     System        15,000      3,500 *
     Disk____________________________________________________________

     *  Space depends on the number and content of the directories.

     Additional space of approximately 1,000 blocks will be required
     on multi-lingual systems.

     The installation will run in SAFETY-MODE if there are approxi-
     mately 75,000 blocks free on the system disk.

     All sizes are approximations; actual sizes may vary depending on
     the users system environment, configuration and software options
     selected.

     OPTIONAL HARDWARE

     ALL-IN-1 supports any mass storage, unit record, terminal, or
     printer device supported by the prerequisite software.

     The autodial feature of the Communications application supports
     the following modems:

        Digital Equipment DF02-AC
        Digital Equipment DF03-AC
        Digital Equipment DF100 series modems
        Case 440/12
        Racal-Milgo MPS1222-AD
        Racal-Milgo MPS1222 with Racal-Vadic VA811

     Note: The availability of these product options may vary by
     country. Customers should contact their local Digital office for
     information or availability.

     CLUSTER ENVIRONMENT

                                    11

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     ALL-IN-1 STARTER is fully supported when installed on any valid
     and licensed VAXcluster* configuration without restrictions.
     The HARDWARE REQUIREMENTS sections of this product's Software
     Product Description and System Support Addendum detail any
     special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (SPD 29.78.xx) and
        include CI, Ethernet, and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     o  VMS Operating System V5.1 - V5.4 (DECwindows must be in-
        stalled for CDA usage.)

     o  DECnet-VAX V5.1 - V5.4 is required for multinode support.

     o  VAX FMS V2.4 (included with the ALL-IN-1 Kit)

     o  CDA Converter Library for VMS V1.1 (included with the ALL-IN-
        1 STARTER Kit - required for CDA support)

     The following chart shows the necessary version levels of soft-
     ware required with the underlying VMS Operating System.

     ________________________________________________________________
                   VMS      VMS      VMS      VMS
     Software______V5.1_____V5.2_____V5.3_____V5.4___________________

     ALL-IN-1      Yes      Yes      Yes      Yes
     STARTER
     V2.4

     DECwindows/CDAYes      Yes      No       No
     base V1.0

         V2.0      No       No       Yes      Yes


                                    12

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                   VMS      VMS      VMS      VMS
     Software______V5.1_____V5.2_____V5.3_____V5.4___________________


     CDA Con-      Yes      Yes      Yes      Yes
     verter
     Library
     V1.0

     CDA Con-      No       No       Yes      Yes
     verter
     Library
     V1.1

     CDA PATCH     No       No       Yes      No

     VAX Mes-      Yes      Yes      Yes      Yes
     sage
     Router
     V3.1

     Message       Yes      Yes      Yes      Yes
     Router VMS
     Gateway
     V3.1

     ALL-IN-1      No       Yes      Yes
     MAIL - VT
     V1.0

     ALL-IN-1      No       No       Yes
     MAIL -
     DECwindows
     V1.0





                                    13

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A


     ________________________________________________________________
                   VMS      VMS      VMS      VMS
     Software______V5.1_____V5.2_____V5.3_____V5.4___________________


     ALL-IN-1      No       Yes      Yes
     MAIL -
     DOS V1.0

     ALL-IN-1      Yes      Yes      Yes
     DESKTOP
     Server
     for VMS
     V1.0____________________________________________________________

     ALL-IN-1 STARTER provides an interface to the CDA support on
     a VMS system. The level of CDA support via ALL-IN-1 STARTER
     is entirely dependent on the level of CDA support on the VMS
     system.

     Note: ALL-IN-1 and ALL-IN-1 STARTER cannot coexist on the same
     system.

     VMS V5.1

     VMS has no built-in CDA support.

     DECwindows (separate kit) must be installed to get basic CDA
     support.

     DECwrite is required to have DECwrite style files.

     DECchart is required to have DECchart style files.

     CDA Converter Library for VMS V1.0 can be installed to provide
     additional CDA front-ends and back-ends (required for conver-
     sions to/from DX/WPS-PLUS).

     VMS V5.2

     VMS has basic CDA support for DDIF, TEXT and PS.

                                    14

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     DECwindows must be installed to use CDA.

     DECwrite is required to have DECwrite style files.

     DECchart is required to have DECchart style files.

     CDA Converter Library for VMS V1.0 can be installed to provide
     additional CDA front-ends and back-ends (required for conver-
     sions to/from DX/WPS-PLUS).

     VMS V5.3

     VMS has basic CDA support for DDIF, TEXT and PS.

     DECwindows must be installed to use CDA.

     DECwrite is required to have DECwrite style files.

     DECchart is required to have DECchart style files.

     CDA Converter Library for VMS V1.0 can be installed to provide
     additional CDA front-ends and back-ends (required for conver-
     sions to/from DX/WPS-PLUS).

     VMS V5.4

     VMS has basic CDA support for DDIF, TEXT and PS.

     DECwindows must be installed to use CDA.

     DECwrite is required to have DECwrite style files.

     DECchart is required to have DECchart style files.

     CDA Converter Library for VMS V1.0 can be installed to provide
     additional CDA front-ends and back-ends (required for conver-
     sions to/from DX/WPS-PLUS).

     VMS Tailoring

     For VMS V5.x systems, the following classes of VMS are required
     for full functionality of this layered product:

     o  Network Support

                                    15

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     o  Programming Support

     o  System Programming Support

     o  Secure User's Environment

     o  Utilities

     o  BLISS Required Files

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     Country Specific Software

     At this time, only U.S. English is available. Please contact
     your Digital office for the latest information on other language
     versions and for details of supported multi-lingual configura-
     tions.

     o  Within the U.S. product, an auto-dial/re-dial facility is
        provided.

     o  Within the U.S. product, the following WPS-PLUS functionality
        is available:

        -  A spelling verifier and corrector with a spelling database
           of over 80,000 words which can be used in conjunction with
           up to 12,000 additional user-specific words.

        -  Usage alert which provides brief definitions of easily
           confused words, such as ``effect'' and ``affect'' or
           ``guarantee''and ``guaranty''.

        -  Electronic thesaurus, based on the Houghton Mifflin Ro-
           get's II: The New Thesaurus which allows users to obtain
           synonyms, including inflections (ie., -ed, -ing, -ly) and
           short definitions based on parts of speech for a selected
           word.

     OPTIONAL SOFTWARE

                                    16

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     o  VAX Message Router V3.1 (included with the ALL-IN-1 STARTER
        Kit)

        Message Router VMS Gateway V3.1 (included with the ALL-IN-1
        STARTER Kit)

     o  DECdx/VMS V1.2

        Note: DECdx/VMS is only required to allow users to transfer
        DX documents between Digital's mainframes (in conjunction
        with DECdx/RSTS, DECdx/RSX and DECdx/TOPS-20).

     o  DECpage V3.1

     o  VAX Language and Specialized Lexicons V2.0:

           British Lexicon V2.0
           Deutsch Lexicon V2.0
           Francais Lexicon V2.0
           American Medical Lexicon V2.0
           American Business Lexicon V2.0

     o  VAX Grammar Checker V1.0

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Tape: 9-Track 1600 BPI Magtape, TK50 Tape Cartridge

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

                                    17

 


     ALL-IN-1 STARTER, Version 2.4                     SSA 25.D9.01-A



     Software Licenses: QL-VNNA*-**
     Software Media: QA-VNNA*-**
     Complete Documentation Kit: QA-VNNAA-GZ
     Software Product Services: QT-VNNA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at the time of release. Please
     contact your local Digital office for the most up-to-date infor-
     mation.

     [R]  PostScript is a registered trademark of Adobe Systems Inc.

     [R]  IBM is a registered trademark of International Business
          Machines Corporation.

     [TM] The DIGITAL Logo, ALL-IN-1, DEC, DECmate, DECnet, DECnet-
          VAX, DECtalk, DECwrite, DECserver, DECstation, DDIF, DX,
          EDT, LA50, LA75, LJ250, LN03, LN03 PLUS, LN03R, LQP02,
          LQP03, MicroVAX, Professional, Rainbow, VAX, VAX FMS, VAXs-
          tation, VAXserver, VMS, VT, WPS and WPS-PLUS are trademarks
          of Digital Equipment Corporation.















                                    18
