 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  BASEstar for VMS, Version 3.0      SSA 33.17.01-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX 9000-210, VAX 9000 Model 400 Series

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900





                                  DIGITAL                  March 1991

                                                          AE-PD08B-TE

 


     BASEstar for VMS, Version 3.0                     SSA 33.17.01-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,

                 VAXserver 4000 Model 300
                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     A minimum of 8 megabytes of memory and an RD54 or equivalent
     disk drive for a base level installation with no options in-
     stalled.

     A minimum of 13 megabytes of memory and an RD54 and RD53 or
     equivalent disk drive are required for an installation with the
     Library option installed.

     Disk Space Requirements (Block Cluster Size = 1):



                                     2

 


     BASEstar for VMS, Version 3.0                     SSA 33.17.01-A



     Disk space required for installation:

          BCC               31,500 blocks
                            (16,128K bytes)

          BCCUTL            2,800 blocks
                            (1,433K bytes)

          BCCLIB            16,190 blocks
                            (8,289K bytes)

          DCM               13,000 blocks
                            (6,656K bytes)

          BRI               1,150 blocks
                            (588K bytes)

     Disk space required for use (permanent):

          BCC               24,300 blocks
                            (12,441K bytes)

          BCCUTL            200 blocks
                            (102K bytes)

          BCCLIB            15,920 blocks
                            (8,151K bytes)

          DCM               12,700 blocks
                            (6,502K bytes)

          BRI               800 blocks
                            (409K bytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

                                     3

 


     BASEstar for VMS, Version 3.0                     SSA 33.17.01-A



     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     VMS Operating System V5.3 - V5.4

     VAX FMS, at a minimum of V2.3 (Runtime system) is required only
     if the Menu System will be used. It is not required for basic
     BASEstar operation.

     VMS Tailoring

     For VMS V5.x, the following VMS classes are required for full
     functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  System Programming Support

     o  Secure User's Environment

     o  Utilities

     o  RMS Journaling Files

     o  Miscellaneous Files

                                     4

 


     BASEstar for VMS, Version 3.0                     SSA 33.17.01-A



     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated

     ORDERING INFORMATION

     Software Licenses:

     BASEstar for VMS: QL-YU9A*-**
     BASEstar Runtime for VMS: QL-YUAA*-**

     Software Media:

     BASEstar for VMS: QA-YU9AA-**
     BASEStar Runtime for VMS: QA-YUAAA-**

     Software Documentation:

     BASEstar for VMS: QA-YU9AA-GZ
     BASEstar for VMS Runtime: QA-YUAAA-GZ
     System Management: QA-YU9AB-GZ
     General User: QA-YU9AC-GZ
     Programming: QA-YU9AD-GZ

     Software Product Services:

     BASEstar for VMS: QT-YU9A*-**
     BASEstar Runtime for VMS: QT-YUAA*-**

                                     5

 


     BASEstar for VMS, Version 3.0                     SSA 33.17.01-A



     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   MS-DOS is a registered trademark of Digital Equipment
           Corporation.

     [R]   UNIX is a registered trademark of UNIX System Laborato-
           ries, Incorporated.

     [TM]  The DIGITAL Logo, VAX, VAXstation, VAXserver, MicroVAX,
           VMS and BASEstar are trademarks of Digital Equipment
           Corporation.






















                                     6
