 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECprint Printing Services for VMS,SSA 32.41.00-A
                    Version 4.0

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX 9000-210, VAX 9000-410

               VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900




                                  DIGITAL               December 1990

                                                          AE-PC26A-TE

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0



     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,

                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, VAX-11/730, MicroVAX I, VAXstation I, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Other Hardware Required

     At least one Digital PostScript printer, as follows:

     o  ScriptPrinter (LN03R)

     o  LN03 Image Printer (LN03Q)

     o  DEClaser 2150 (LN05R)

     o  DEClaser 2250 (LN06R)

     o  PrintServer 20

                                     2

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0


     o  PrintServer 40

     o  PrintServer 40 Plus

     o  Colormate PS[R]

     For DEClaser/ScriptPrinter Printer Configurations:

     o  At least one DEClaser 2150 or 2250 printer or ScriptPrinter
        (LN03R)

     o  Serial Interface via RS232 or MMJ with Adapter

     o  One of the following serial interfaces is required:

           DHV11 (9600 baud)
           DZQ11 (9600 baud)
           DHU11 (9600 baud)
           DMZ32 (4800 baud)
           DMF32 (9600 baud)
           DMB32 (9600 baud)
           DECserver 100 (9600 baud)
           DECserver 200/MC (19.2K baud)
           DECserver 250 (19.2K baud)
           DECserver 300 (19.2K baud)
           DECserver 500 (9600 baud)
           DECserver 550 (9600 baud)
           MUXserver 100 (19.2K baud)
           MUXserver 300 (19.2K baud)

     o  The ScriptPrinter (LN03R), DEClaser 2150 (LN05R) and DEClaser
        2250 (LN06R) dip switches and corresponding serial interface
        must be set for 8-bit, no parity communications, XON/XOFF
        flow control.

     o  For DEClaser Printers, a PostScript cartridge, and a minimum
        of two megabytes of memory for the DEClaser 2150 and three
        megabytes of memory for the DEClaser 2250.

     For LN03 Image Printer Configurations:

     o  At least one LN03 Image Printer (LN03Q)

                                     3

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0


     o  A minimum of 9 megabytes of memory; 13 megabytes of memory is
        recommended for enhanced performance.

     For PrintServer Configurations Only:

     o  A valid PrintServer printer configuration and Supporting Host
        software

     o  An Ethernet Controller Interface for the client system:

           DELUA
           DEUNA
           DEBNT
           DEQNA
           DELQA

     o  An Ethernet physical channel for the printer, and one of the
        following:

           Ethernet transceiver (H400)
           Local Network Interconnect (DELNI)
           ThinWire Ethernet Station Adapter (DESTA)

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      4,500 blocks
     installation:
                                  (2.3M bytes)

     Disk space required for
     use (permanent:)

     With ALL-IN-1 compatibil-    4,500 blocks
     ity kit:
                                  (2.3M bytes)

     Without ALL-IN-1 compati-    2,500 blocks
     bility kit:
                                  (1.3M bytes)

                                     4

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0


     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V5.3 - V5.4

     Desktop-VMS V1.0 - V1.1

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support (for PrintServer support)*

     o  Secure User's Environment

     o  Utilities (for support of DECserver connected printers)*

     o  DECwindows Application Files (for printing DDIF encoded
        bitonal images)*

     *  These are optional features; installations that do not use
        these features do not need to install the tailoring classes
        indicated.

                                     5

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0


     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     For PrintServer Configurations Only:

     o  DECnet-VAX V5.3 - V5.4

     o  VAX PrintServer Supporting Host Software V3.2 installed on
        one system on the same Ethernet.

     For LN03 Image Devices:

     o  Image Printer Support Software

     o  VMS Tailoring Class: DECwindows applications programming























                                     6

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0


     OPTIONAL SOFTWARE

     o  VAX Distributed Queuing Service V1.1

     o  VAXimage Application Services V1.0

     o  VAXimage Scanning Application V1.0

     o  LN03 Soft Font Kits

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     ORDERING INFORMATION

     Software Licenses: QL-YNCA*-**
     Software Media: QA-YNCA*-**
     Software Documentation: QA-YNCAA-GZ
     Software Product Services: QT-YNCA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   PostScript is a registered trademark of Adobe Systems,
           Inc.

     [R]   HP PCL Level IV is a registered trademark of Hewlett-
           Packard Corporation.

                                     7

 


     DECprint Printing Services for VMS,               SSA 32.41.00-A
     Version 4.0



     [R]   Tektronix is a registered trademark of Tektronix, Inc.

     [R]   LaserJet is a registered trademark of Hewlett-Packard
           Corporation.

     [R]   Colormate PS is a registered trademark of NEC.

     [TM]  The DIGITAL Logo, VAX, VMS MicroVAX, VAXstation,
           VAXserver, VAXcluster, ALL-IN-1, WPS-PLUS, ReGIS, DEC-
           net, DECwindows, and DECprint are trademarks of Digital
           Equipment Corporation.



























                                     8
