DECdx/VMS, Version 1.2                                   SSA 26.36.05-A

HARDWARE REQUIREMENTS

Processors Supported

VAX:	      VAX 6210, VAX 6220, VAX 6230, VAX 6240, VAX 6310, VAX 6312, 
              VAX 6320, VAX 6330, VAX 6333, VAX 6340, VAX 6350, VAX 6360  
              VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, 
              VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, 
              VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978

	      VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/780

MicroVAX:	   MicroVAX II, MicroVAX 2000, MicroVAX 3300/3400, MicroVAX 
                   3500, MicroVAX 3600

VAXstation:	   VAXstation II, VAXstation 2000, VAXstation 3100, 
                   VAXstation 3200, VAXstation 3500, VAXstation 8000

VAXserver:	   VAXserver 3300, VAXserver 3400, VAXserver 3500, 
                   VAXserver 3600, VAXserver 3602, VAXserver 6210/6220, 
                   VAXserver 6310/6320

Processors Not Supported

VAXstation I, VAX-11/782, MicroVAX I

VMS system must also have an available local or remote serial full duplex 
asynchronous terminal line supported by the operating system. 
   
Any valid DECmate II, III, with WPS-8 communication option enabled. Each 
additional DECmate system simultaneously connected to the host requires its 
own line. 

Block Space Requirements (Block Cluster Size = 1):

Disk space required for installation:
					       3,650 blocks
					       (1868.8K bytes)

Disk space required for use (permanent):
					       500 blocks
					       (256K bytes)

These counts refer to disk space required on the system disk. The sizes are 
approximate; actual sizes may vary depending on the user's system 
environment, configuration and software options selected.

OPTIONAL HARDWARE

None

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions. The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product. 

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet and 
    Mixed Interconnect configurations.

SOFTWARE REQUIREMENTS

VMS Operating System V4.7 - V5.0

MicroVMS Operating System V4.7

DECmate II/III WPS, Version 2.0 at a minimum of V2.0 (with communications 
software activated) 

VMS Tailoring

For VMS 5.x systems, the following VMS classes are required for full 
functionality of this layered product:

oo   VMS Required Saveset

oo   Secure User's Environment

oo   Utilities

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (SPD 25.01.xx).

MicroVMS Tailoring

For MicroVMS 4.x systems, the following components of MicroVMS are required 
for full functionality of this layered product: 

oo   Base System

oo   Secure User's Environment

OPTIONAL SOFTWARE

None

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from minimum requirements for the current version.

DISTRIBUTION MEDIA

Disk:	RX01 Floppy Diskette 

Tape:	TK50 Streaming Tape, TU58 DECtape II Cartridge, 9-track 1600 BPI 
        Magtape (PE)


 
 

ORDERING INFORMATION

Software License: QL-708A*-**
Software Media: QA-708A*-**
Software Documentation: QA-708AA-GZ
Software Product Services: QT-708A*-**
    
*   Denotes variant fields. For additional information on available 
    licenses, services and media refer to the appropriate price book.

The above information is valid at time of release. Please contact your 
local DIGITAL office for the most up-to-date information.

May 1989
AE-MM39B-TE

