 













             Installing DEC GKS-3D for VMS

             Order Number: AA-LM44B-TE



             October 1990



             This document contains instructions for installing DEC GKS-3D
             on the VMS operating system. It also explains how to read the
             online release notes before or after installing this product.




             Revision/Update Information:  This revised manual supersedes
                                           the information in the DEC GKS-
                                           3D Installation Guide (Order
                                           No. AA-LM44A-TE).

             Operating System and Version: VMS Version 5.3 or higher
                                           VAXstation Requirement:
                                           VAXstation Windowing Software
                                           Version 4.0 or higher
                                           DECwindows Version 5.3 or
                                           higher

             Software Version:             DEC GKS-3D Version 1.1
             digital equipment corporation
             maynard, massachusetts

 


             Theiinformationrin9this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.

             ©  Digital Equipment Corporation 1989, 1990.

             All Rights Reserved.
             Printed in U.S.A.

             The postpaid Reader's Comments forms at the end of this docu-
             ment request your critical evaluation to assist in preparing
             future documentation.

             The following are trademarks of Digital Equipment Corporation:

             CDA         LN03                VAXcluster
             DDIF        MASSBUS             VAX RMS
             DDIS        MicroVAX            VAXstation
             DEC         PrintServer 40      VMS
             DECnet      Q-bus               VMS/ULTRIX Connection
             DECUS       ULTRIX              VT
             DECstation  ULTRIX Mail         XUI
                         Connection
             DECsystem   ULTRIX Worksystem
                         Software
             DECwindows  UNIBUS
             DTIF        VAX                 DIGITAL

             X Window System, Version 11, is a registered trademark of
             Massachusetts Institute of Technology.

                                                                    ZK5465

 






             This document was prepared using VAX DOCUMENT, Version 1.2






































                                                                        -3

 















                                                                  Contents
          ________________________________________________________________

          Preface .........................................................    vii


          ________________________________________________________________
          Chapter 1  Preparing to Install DEC GKS-3D

               1.1   Required Operating System Components............  1-1

               1.2   Prerequisite Software............................. 1-2

               1.3   VMS License Management Facility ................. 1-2

               1.4   Installation Procedure Requirements.............  1-3
                     1.4.1 Privileges.................................. 1-3
                     1.4.2 Disk Space.................................. 1-3
                     1.4.3 System Parameters.......................... 1-4
                           1.4.3.1Calculating the Values for
                                  GBLPAGES and GBLSECTIONS..........   1-5
                           1.4.3.2Changing System Parameter Values
                                  with AUTOGEN........................ 1-6
                     1.4.4 Process Account Quotas....................  1-6
                     1.4.5 VMSINSTAL Requirements....................  1-8
                     1.4.6 Backing Up Your System Disk..............   1-8
                     1.4.7 DEC GKS-3D Requirements...................  1-8
                     1.4.8 License Management Utility
                           Requirements................................ 1-9


                                                                       iii

 






          ________________________________________________________________
          Chapter 2  Installing DEC GKS-3D

               2.1   General Information ............................... 2-1
                     2.1.1 Accessing the Online Release Notes......    2-1
                     2.1.2 Running the Installation Verification
                           Procedure (IVP)............................ 2-2
                     2.1.3 Aborting the Installation ................  2-2

               2.2   The Installation Procedure ....................... 2-3
                     2.2.1 Invoking VMSINSTAL......................... 2-3
                     2.2.2 Installation Questions....................  2-4
                     2.2.3 Informational Messages....................  2-9
                     2.2.4 Running the Installation Verification
                           Procedure (IVP)............................ 2-10
                     2.2.5 Completing the Installation Procedure ..   2-10

               2.3   Error Recovery .....................................   2-11


          ________________________________________________________________
          Chapter 3  After Installing DEC GKS-3D

               3.1   Editing the System Files.......................... 3-1

               3.2   Cluster Considerations............................ 3-2

               3.3   User Account Requirements ........................ 3-3
                     3.3.1 Privileges.................................. 3-3
                     3.3.2 Running the Installation Verification
                           Procedure After Installation.............   3-3

               3.4   Determining and Reporting Problems..............  3-4






          iv

 






          ________________________________________________________________
          Appendix A Sample Installation

               A.1   Full Development Kit Installation...............  A-1

               A.2   Run-Time Kit Installation ........................ A-4


          ________________________________________________________________
          Appendix B Files and Logical Names Installed on Your
                     System

               B.1   DEC GKS-3D Development Kit Files for VMS.......   B-1

               B.2   DEC GKS-3D Run-Time Kit Files for VMS ..........  B-5

               B.3   Logical Names ......................................  B-7

          ________________________________________________________________
          Tables

               1-1   Disk Space Requirements........................... 1-4

               1-2   Required System Parameter Values ................ 1-4

               1-3   Process Account Quotas for the Installing
                     Account .............................................   1-7












                                                                         v

 














                                                                   Preface
          ________________________________________________________________



             This document describes how to install DEC GKS-3D on the VMS
             operating system. It is intended for system managers. This
             document applies to Version 1.1 of DEC GKS-3D.

             Keep this document with your distribution kit. You will need
             it to install maintenance updates or to reinstall DEC GKS-3D
             for any other reason.

             At the back of this document are two Reader's Comments forms.
             If you have any comments about this document, please fill out
             one form and mail it. Your comments will be considered for
             the next revision of the installation guide.

             The installation procedure is described step-by-step and is,
             for the most part, self-explanatory. The system prompts you
             to answer questions and to change volumes, and waits for you
             to tell it to continue.

          ____________________________________________________________

          Associated Documents

             For more information about installing DEC GKS-3D on a VMS
             system, see your processor-specific installation/operations
             guide.

             For specific questions on your operating system, refer to the
             documentation set for that operating system.

                                                                       vii

 





          ____________________________________________________________

          Conventions Used in This Document

             Defaults appear in brackets ([])  throughout the installation
             procedure. Red ink indicates user input. The RETURN key is
             symbolized as <RET>. <CTRL/x> indicates that you must press
             the key labeled CTRL while you simultaneously press another
             key, for example CTRL/C.































          viii

 

















                                                                      Chapter 1


                                                Preparing to Install DEC GKS-3D
               ________________________________________________________________


                  This chapter describes the preparations and requirements
                  necessary for installing DEC GKS-3D.

                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Be sure to
                  verify the contents of your kit with this information. If
                  your kit is damaged or if you find that parts of it are
                  missing, contact your Digital representative.

                  DEC GKS-3D provides online release notes. Digital strongly
                  recommends that you read the release notes before proceeding
                  with the installation.

               ____________________________________________________________

               1.1  Required Operating System Components

                  DEC GKS-3D runs on the VMS operating system, Version 5.3 or
                  higher. DEC GKS-3D requires the following VMS classes for
                  full functionality of the product:

                   o VMS required saveset

                   o Utilities, if the DEC GKS-3D for VMS online HELP is to be
                     installed

                   o Network support, where full DECwindows network functional-
                     ity is required




                                           Preparing to Install DEC GKS-3D  1-1

 











                   o Programming support, with the DEC GKS-3D development kit
                     for GKS-3D application development

               ____________________________________________________________

               1.2  Prerequisite Software

                  To install DEC GKS-3D on a VAXstation, you must have one of
                  the following products installed:

                   o VAXstation Windowing Software Version 4.0 or higher

                   o VMS Version 5.3 or higher with its related DECwindows
                     version

               ____________________________________________________________

               1.3  VMS License Management Facility

                  The VMS License Management Facility (LMF) is available with
                  Version 5.3 of the VMS operating system. If you are in-
                  stalling DEC GKS-3D on a VMS Version 5.3 or higher system,
                  you must register your software license.

                  The license registration information you need is contained
                  in the Product Authorization Key (PAK) that is shipped with
                  DEC GKS-3D. The PAK is a paper certificate that contains
                  information about the license you have to run a particular
                  piece of software.

                  It is best to register your DEC GKS-3D license before you
                  perform the installation. During the installation, you are
                  asked if you have registered the DEC GKS-3D license and
                  loaded the appropriate authorization key. If you have not
                  already done so, you can complete the installation; however,
                  you will not be able to run either the DEC GKS-3D software
                  or its Installation Verification Procedure (IVP). Once you
                  perform the license registration and have loaded an autho-
                  rization key, you will be able to run the IVP and use DEC
                  GKS-3D.

                  To register a license under a VMS Version 5.3 system, first
                  log in to the system manager's account, SYSTEM. You then have
                  a choice of two ways to perform the registration:

                   o Invoke the SYS$UPDATE:VMSLICENSE.COM procedure. When it
                     prompts you for information, respond with data from your
                     Product Authorization Key (PAK).

               1-2  Preparing to Install DEC GKS-3D

 











                   o Issue the LICENSE REGISTER DCL command with the appro-
                     priate qualifiers that correspond to information on the
                     PAK.

                  For complete information on using LMF, see the manual on the
                  License Management Utility in the VMS documentation set.

               ____________________________________________________________

               1.4  Installation Procedure Requirements

                  This section describes various requirements for installing
                  DEC GKS-3D. Before you begin, you should perform a system
                  disk (or disks) backup. The installation procedure takes
                  approximately 5 to 30 minutes, depending on your type of
                  media and your system configuration.

                  The following sections describe the privileges and resources
                  you must have to install DEC GKS-3D.

               ____________________________________________________________

               1.4.1  Privileges

                  To install DEC GKS-3D, you must be logged in to an account
                  that has SETPRV or at least the following privileges:

                   o CMKRNL

                   o WORLD

                   o SYSPRV

                  Note that VMSINSTAL turns off BYPASS privilege at the start
                  of the installation.

               ____________________________________________________________

               1.4.2  Disk Space

                  Installing DEC GKS-3D requires a certain amount of free
                  storage disk space during the installation. Once DEC GKS-
                  3D is installed, less storage space is required. Table 1-1
                  summarizes the storage requirements for DEC GKS-3D.

                                           Preparing to Install DEC GKS-3D  1-3

 











                  Table 1-1:  Disk Space Requirements
                  _____________________________________________________________
                                   Blocks
                                   During
                  Kit______________InstallationBlocks_After_Installation_______

                  DECGKS3D         12,000      11,000

                  DECGKS3DRT_______8,000_______7,000___________________________

                  To determine the number of free disk blocks on the current
                  system disk, enter the following command at the DCL prompt:

                    $ SHOW DEVICE SYS$SYSDEVICE <RET>

               ____________________________________________________________

               1.4.3  System Parameters

                  Table 1-2 lists the minimum required system parameter values
                  for the installation. Depending on the kinds of programs
                  and applications running at your site, you might need higher
                  values for some settings.

                  Table 1-2:  Required System Parameter Values
                  _____________________________________________________________
                  System_Parameter___________Value_____________________________

                  GBLSECTIONS[1]             n + 25
                  [1]The_n_variable_refers_to_the_system_parameter_values_that_

                  are currently in use. To install DEC GKS-3D, you must raise
                  those values by the number indicated. (See Section 1.4.3.1.)
                  _____________________________________________________________

                  The following sections show you how to check system parameter
                  values, calculate values for the GBLPAGES and GBLSECTIONS
                  system parameters, and change parameter values with the VMS
                  AUTOGEN command procedure.






               1-4  Preparing to Install DEC GKS-3D

 










               ____________________________________________________________

               1.4.3.1  Calculating the Values for GBLPAGES and GBLSECTIONS

                  To install and run DEC GKS-3D, you must set the correct
                  values for the GBLPAGES and GBLSECTIONS system parameters.

                  The values for GBLSECTIONS in Table 1-2 indicate that you
                  must have at least 25 sections available on your system for
                  the installation to process successfully. To calculate how
                  many global sections your system has, perform the following
                  steps:

                   1. Run the VMS Install Utility (INSTALL) using the following
                     DCL command:

                       $ INSTALL <RET>
                       INSTALL> LIST/GLOBAL/SUMMARY <RET>

                     The INSTALL utility displays a summary of global pages
                     and global sections used by your system, as well as the
                     current number of unused global pages. For example:

                                     Summary of Local Memory Global Sections

                          258 Global Sections Used,  22580/3420 Global Pages Used/Unused

                   2. Note the amount shown for "Global Sections Used" (258 in
                     the example), then exit.

                       INSTALL> EXIT <RET>

                   3. Run the SYSGEN utility and use the SHOW command to de-
                     termine the number of global sections that have been
                     allocated:

                       $ RUN SYS$SYSTEM:SYSGEN <RET>
                       SYSGEN> USE CURRENT <RET>
                       SYSGEN> SHOW GBLSECTIONS <RET>

                       Parameter Name    Current   Default   Minimum   Maximum Unit  Dynamic
                       --------------    -------   -------   -------   ------- ----  -------
                       GBLSECTIONS           512       250        20      4095 Sections



                                           Preparing to Install DEC GKS-3D  1-5

 











                   4. Subtract the amount shown in the summary (258 in the
                     example) from the amount allocated (512 in the exam-
                     ple). If the difference is less than the number re-
                     quired in Table 1-2, you need to increase the value of
                     the GBLSECTIONS parameter. Exit from SYSGEN.

                       SYSGEN> EXIT <RET>

                  Section 1.4.3.2 describes the procedures for increasing this
                  value as well as those of other system parameters. Refer to
                  the VMS documentation on system management and operations for
                  more information.

               ____________________________________________________________

               1.4.3.2  Changing System Parameter Values with AUTOGEN

                  You use the AUTOGEN command procedure to change system param-
                  eters. AUTOGEN automatically adjusts values for parameters
                  that are associated with the ones you reset manually. To
                  change system parameters with AUTOGEN, you must edit the
                  following file:

                    $ EDIT SYS$SYSTEM:MODPARAMS.DAT <RET>

                  After you change the values of the appropriate parameters,
                  run the AUTOGEN procedure to recalculate your system parame-
                  ters. Enter the following command at the DCL prompt:

                    $ @SYS$UPDATE:AUTOGEN GETDATA REBOOT <RET>

                  AUTOGEN performs an automatic system shutdown and reboots
                  when it has finished. Rebooting your system makes the new
                  parameter values active. Also on VMS systems Version 5.3,
                  you may wish to add the [NO]FEEDBACK parameter to the AUTOGEN
                  command line. For more information about using AUTOGEN, see
                  the instructions on modifying system parameters in the VMS
                  documentation on system management and operations.

               ____________________________________________________________

               1.4.4  Process Account Quotas

                  The account you use to install DEC GKS-3D must have suf-
                  ficient quotas to enable you to perform the installation.
                  Table 1-3 summarizes the process quotas required to perform
                  the installation.

               1-6  Preparing to Install DEC GKS-3D

 











                  Table 1-3:  Process Account Quotas for the Installing Account
                  _____________________________________________________________
                  Account_Quota____Value_______________________________________

                  ASTLM            24

                  BIOLM            18

                  BYTLM            18,000

                  DIOLM            18

                  ENQLM            30

                  FILLM____________20__________________________________________

                  User account quotas are stored in the file SYSUAF.DAT. You
                  use the VMS Authorize Utility to verify and change user
                  account quotas. First set your directory to SYS$SYSTEM and
                  then run AUTHORIZE:

                    $ SET DEFAULT SYS$SYSTEM <RET>
                    $ RUN AUTHORIZE <RET>
                    UAF>

                  At the AUTHORIZE prompt (UAF>), use the SHOW command with an
                  account name to check a particular account. For example:

                    UAF> SHOW SMITH <RET>

                  To change a quota, use the MODIFY command at the UAF> prompt.
                  MODIFY has the following format:

                        MODIFY account-name /quota-name=nnnn

                  The following example changes the FILLM quota for the SMITH
                  account and then exits from the Authorize Utility:

                    UAF> MODIFY SMITH /FILLM=50 <RET>
                    UAF> EXIT <RET>

                  After you exit from the utility, the VMS system displays
                  messages indicating whether or not changes were made. Once
                  the changes have been made, you must log out and log in again
                  for the new quotas to take effect.

                                           Preparing to Install DEC GKS-3D  1-7

 











                  For more information on modifying account quotas, see the
                  description of the AUTHORIZE utility in the VMS documentation
                  on system management and operations.

               ____________________________________________________________

               1.4.5  VMSINSTAL Requirements

                  When you invoke VMSINSTAL, it checks the following:

                   o Whether you have set your default device and directory to
                     SYS$UPDATE

                   o Whether you are logged in to a privileged account

                   o Whether you have adequate quotas for installation

                   o Whether DECnet is up and running

                   o Whether any users are logged in to the system

                  If VMSINSTAL detects any problems during the installation, it
                  notifies you of the problem and asks if you want to continue
                  the installation. In some instances, you can enter YES to
                  continue. To stop the installation process and correct the
                  situation, enter NO or press RETURN. Then correct the problem
                  and restart the installation.

               ____________________________________________________________

               1.4.6  Backing Up Your System Disk

                  At the beginning of the installation, VMSINSTAL asks if you
                  have backed up your system disk. Digital recommends that you
                  do a system disk backup before installing any software on top
                  of the operating system.

                  Use the backup procedures that have been established at your
                  site. For details on performing a system disk backup, see the
                  section on the Backup Utility in the VMS documentation set.

               ____________________________________________________________

               1.4.7  DEC GKS-3D Requirements

                  DEC GKS-3D makes the following checks during the installa-
                  tion:

                   o Disk check

                   o Global pages check

               1-8  Preparing to Install DEC GKS-3D

 











                   o Global sections check

                   o Help library check

               ____________________________________________________________

               1.4.8  License Management Utility Requirements

                  You will need to register and load your license for DEC GKS-
                  3D before you start the installation to run the Installation
                  Verification Procedure (IVP). Refer to the VMS documentation
                  on the License Management Utility for information about
                  registering your license.
































                                           Preparing to Install DEC GKS-3D  1-9

 

















                                                                      Chapter 2


                                                          Installing DEC GKS-3D
               ________________________________________________________________


                  This chapter describes how to install DEC GKS-3D. Section 2.2
                  contains a step-by-step description of the installation
                  procedure.

               ____________________________________________________________

               2.1  General Information

                  This section includes information about accessing release
                  notes, determining files and logical names added to your
                  system, running the Installation Verification Procedure
                  (IVP), and aborting the installation. Refer to Appendix B
                  for a list of files and logical names that are added to your
                  system during installation.

               ____________________________________________________________

               2.1.1  Accessing the Online Release Notes

                  DEC GKS-3D provides online release notes. If you specify
                  OPTIONS N when you invoke VMSINSTAL, the installation pro-
                  cedure asks you if you want to display or print the release
                  notes. The release notes question comes near the beginning
                  of the installation. You should review the release notes
                  in case they contain any information about changes in the
                  installation procedures.

                  After DEC GKS-3D has been installed, the release notes are
                  located in the following files for development and run-time
                  only kits respectively:


                                                     Installing DEC GKS-3D  2-1

 











                    SYS$HELP:DECGKS3D011.RELEASE_NOTES

                    SYS$HELP:DECGKS3DRT011.RELEASE_NOTES

                  Online help also directs you to the release notes file. After
                  the installation, you can enter the following command to
                  review the Help facility:

                    $ HELP GKS3D RELEASE_NOTES <RET>

               ____________________________________________________________

               2.1.2  Running the Installation Verification Procedure (IVP)

                  The Installation Verification Procedure (IVP) for DEC GKS-3D
                  verifies the installation. During the installation, you are
                  asked if you want to run the IVP as part of the installation.
                  If you respond YES, VMSINSTAL runs the IVP. It is recommended
                  that you run the IVP to be sure that DEC GKS-3D is installed
                  correctly.

                  After DEC GKS-3D is installed, you can run the IVP inde-
                  pendently to verify that the software is available on your
                  system. You might also want to run the IVP after a system
                  failure to be sure that users can access DEC GKS-3D.

                  If the IVP fails for any reason, the following messages are
                  displayed:

                    The DECGKS3D V1.1 Installation Verification Procedure failed.

                    %VMSINSTAL-E-IVPFAIL, The IVP for DEC GKS-3D V1.1 has failed.

                  Running the IVP is described further in Section 2.2.4.

               ____________________________________________________________

               2.1.3  Aborting the Installation

                  To abort the installation procedure at any time, press
                  CTRL/Y. When you press CTRL/Y, the installation procedure
                  deletes all files it has created up to that point and exits.
                  You can then start the installation again.


               2-2  Installing DEC GKS-3D

 










               ____________________________________________________________

               2.2  The Installation Procedure

                  The DEC GKS-3D installation process consists of a series of
                  questions and informational messages, as described in the
                  following sections.

                  Before you begin the DEC GKS-3D installation, define the
                  destination for the output of the Installation Verification
                  Procedure (IVP) with the following command, and replace node
                  with your node name:

                    $ DEFINE DECW$DISPLAY node::0.0 <RET>

               ____________________________________________________________

               2.2.1  Invoking VMSINSTAL

                  To start the installation, invoke the VMSINSTAL command
                  procedure from a privileged account, such as the SYSTEM
                  account. Next, invoke VMSINSTAL. You use the following syntax
                  to invoke VMSINSTAL:

                        @SYS$UPDATE:VMSINSTAL product-name device-name:
               [OPTIONS N] <RET>

                  product-name
                  The installation name for the component. For DEC GKS-3D, use
                  the following installation names:

                   o DECGKS3D (for development kit)

                   o DECGKS3DRT (for run-time only kit)

                  device-name
                  The name of the device on which you plan to mount the media.
                  For example, MUA0: is the device name for a tape drive. It is
                  not necessary to use the console drive for this installation.
                  However, if you do use the console drive, you should replace
                  any media you removed once the installation is completed.

                  OPTIONS N
                  An optional parameter that indicates you want to be prompted
                  to display or print the release notes. If you do not include
                  the OPTIONS N parameter, VMSINSTAL does not prompt you to
                  display or print the release notes. You are strongly recom-
                  mended to read the release notes before proceeding with this
                  installation.

                                                     Installing DEC GKS-3D  2-3

 











                  VMSINSTAL has several other options. For more information,
                  see the VMS documentation on software installation.

                  The following example displays the development kit and the
                  run-time only kit commands to invoke VMSINSTAL to install
                  DEC GKS-3D from tape drive MUA0:. It also shows the system
                  response. This example uses the OPTIONS N parameter for
                  printing or displaying release notes.

                    $ @SYS$UPDATE:VMSINSTAL DECGKS3D MUA0: OPTIONS N <RET>

                    $ @SYS$UPDATE:VMSINSTAL DECGKS3DRT MUA0: OPTIONS N <RET>

                          VAX/VMS Software Product Installation Procedure V5.3-2

                    It is 20-AUG-1990 at 14:53.
                    Enter a question mark (?) at any time for help.

                  If you do not supply either the product name or the device
                  name, VMSINSTAL prompts you for this information later during
                  the installation procedure. VMSINSTAL does not prompt you for
                  any options, so be sure to include OPTIONS N on the VMSINSTAL
                  command line to access the release notes before installation.

               ____________________________________________________________

               2.2.2  Installation Questions

                  This section describes the questions that appear during
                  the installation. See Appendix A for a sample installation
                  procedure.

                  Each question in the installation is marked with an asterisk
                  (*) at the beginning of the line. Some questions show the
                  default response in brackets, for example [YES]. If you want
                  to give the default response, press the RETURN key.

                   1. DECnet status

                     VMSINSTAL notifies you if DECnet is running and displays a
                     list of all active processes. It then asks if you want to
                     continue the installation. You should install DEC GKS-3D
                     on a standalone system or cluster with DECnet shut down.
                     NO is the default response to the question.

               2-4  Installing DEC GKS-3D

 











                       %VMSINSTAL-W-DECNET, Your DECnet network is up and running.
                          .
                          .
                          .
                       * Do you want to continue anyway [NO]?

                   2. System backup

                     VMSINSTAL asks if you are satisfied with your system
                     backup. You should always back up your system disk before
                     performing an installation. If you are satisfied with the
                     backup of your system disk, press RETURN. Otherwise, enter
                     NO to discontinue the installation. After you back up your
                     system disk, you can restart the installation.

                       * Are you satisfied with the backup of your system disk [YES]?

                   3. Mounting the media

                     You should now mount the first distribution volume on
                     the device you specified when you invoked VMSINSTAL. The
                     device name appears in the line preceding the question.
                     VMSINSTAL then asks you if you are ready to continue with
                     the installation.

                     If you respond YES to indicate that you are ready,
                     VMSINSTAL displays a message that the media containing
                     DEC GKS-3D has been mounted on the specified device and
                     that the installation has begun. For example:

                       Please mount the first volume of the set on MUA0.
                       * Are you ready? YES <RET>
                       %MOUNT-I-MOUNTED, DECGKS3D MOUNTED ON MUA0 (NODE 1)

                        The following products will be processed:
                        DECGKS3D V1.1

                           Beginning installation of DECGKS3D V1.1 at 14:58

                       %VMSINSTAL-I-RESTORE, Restoring product saveset A...

                     If you entered the wrong device name when you invoked
                     VMSINSTAL and need to restart the installation, enter NO
                     in response to the "Are you ready?" question. To abort the
                     installation for other reasons, press CTRL/Y.

                   4. Additional media volumes

                                                     Installing DEC GKS-3D  2-5

 











                     If your installation kit contains more than one volume,
                     VMSINSTAL prompts you to mount the additional volumes
                     and then asks you to indicate that you are ready for the
                     installation to proceed.

                       %BACKUP-I-READYREAD, mount volume 2 on MUA0 for reading

                       Enter "YES" when ready:YES <RET>

                   5. Release notes

                     If you specified OPTIONS N when you invoked VMSINSTAL,
                     you are now given four options for reviewing the release
                     notes.

                       Additional Release Notes Options:

                           1. Display release notes
                           2. Print release notes
                           3. Both 1 and 2
                           4. None of the above

                       * Select option [2]:

                     If you select option 1, VMSINSTAL displays the release
                     notes immediately on the console terminal. You can termi-
                     nate the display at any time by pressing CTRL/C.

                     If you select option 2, VMSINSTAL prompts you for the name
                     of the print queue that you want to use:

                       * Queue name [SYS$PRINT]:<RET>

                     You can enter a queue name or press RETURN to send the
                     file to the default output print device.

                     If you select option 3, VMSINSTAL displays the release
                     notes immediately on the console terminal and then prompts
                     you for a queue name for the printed version.

                   6. Continuing the installation

                     The installation procedure now asks if you want to con-
                     tinue the installation. To continue, enter YES. Otherwise,
                     press RETURN. In either case, the release notes are copied
                     to a file in the SYS$HELP directory. For example:

               2-6  Installing DEC GKS-3D

 











                       * Do you want to continue the installation [NO]?:YES <RET>
                       %VMSINSTAL-I-RELMOVED, The product's release notes have been
                           successfully moved to SYS$HELP.

                     The release notes for development and run-time kits are
                     located respectively in the following files:

                       SYS$HELP:DECGKS3D011.RELEASE_NOTES

                       SYS$HELP:DECGKS3DRT011.RELEASE_NOTES

                                                 NOTE

                         The name of the release notes file installed by
                         VMSINSTAL consists of the current product name and
                         version number. Do not delete release notes for
                         previous versions of DEC GKS-3D.

                   7. Choosing to purge files

                     You have the option of purging files from previous ver-
                     sions of DEC GKS-3D that are superseded by this installa-
                     tion. Purging is recommended; however, if you need to keep
                     files from the previous version, enter NO in response to
                     the question.

                       * Do you want to purge files replaced by this installation [YES]?

                   8. Choosing to run the Installation Verification Procedure
                     (IVP)

                     The installation procedure now asks if you want to run the
                     Installation Verification Procedure. The IVP for DEC GKS-
                     3D checks to be sure that the installation is successful.
                     It is recommended that you run the IVP.

                       * Do you wish to perform the Installation Verification Procedure [YES]?

                     The IVP displays the picture shown in Figure 2-1






                                                     Installing DEC GKS-3D  2-7

 











                  _____________________________________________________________












































               2-8  Installing DEC GKS-3D

 











                   9. License Registration

                     The installation procedure asks if you have registered and
                     loaded your authorization key for DEC GKS-3D, and prints
                     out information specific to the particular license, for
                     example:

                       Product: GKS3D
                       Producer: DEC
                       Version: 1.1
                       Release Date: 15-OCT-1990

                     For the run-time kit:

                       Product: GKS3D-RT
                       Producer: DEC
                       Version: 1.1
                       Release Date: 15-OCT-1990

                     The installation also inquires:

                       * Does this product have an authorization key registered and loaded?

                     If you have not registered and loaded your authorization
                     key, you must answer "NO" to this question. A successful
                     installation of DEC GKS-3D depends upon an authoriza-
                     tion key being registered and loaded. Please be certain
                     that this has been completed before proceeding with the
                     installation.

               ____________________________________________________________

               2.2.3  Informational Messages

                  At this point, the installation procedure displays a number
                  of informational messages that report on the progress of
                  the installation. There are no further questions. If the
                  installation procedure has been successful up to this point,
                  VMSINSTAL moves the new or modified files to their target
                  directories, updates help files, and updates DCL tables, if
                  necessary. If you asked for files to be purged, that work is
                  done now. The following messages are displayed:

                    %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
                    directories...

                                                     Installing DEC GKS-3D  2-9

 










               ____________________________________________________________

               2.2.4  Running the Installation Verification Procedure (IVP)

                  If you chose to run the IVP, VMSINSTAL runs it now. When the
                  IVP runs successfully, you see the following display:

                           Beginning the DEC GKS-3D Installation Verification Procedure (IVP).
                           The IVP will take 1 to 5 minutes depending on your CPU.

                           Since you are running on a VAXstation the Installation
                           Verification Procedure will be run with DEC GKS-3D device type 211
                           (DECW). Output will be done to the node indicated by the logical
                           name DECW$DISPLAY.

                           The DECGKS3D V1.1 Installation Verification Procedure (IVP) completed
                           successfully. If the results of the Installation Verification
                           Procedure (IVP) look like the illustration provided with the
                           DEC GKS-3D Installation Guide, then installation has been successful.

               ____________________________________________________________

               2.2.5  Completing the Installation Procedure

                  The following messages indicate that the entire installation
                  procedure is complete:

                       Installation of DECGKS3D V1.1 completed at 18:02

                       VMSINSTAL procedure done at 18:02

                  You can now log out of the privileged account:

                    $ LOGOUT <RET>
                    SYSTEM     logged out at 20-AUG-1990 18:05.

                  Note that VMSINSTAL deletes or changes entries in the process
                  symbol tables during the installation. Therefore, if you are
                  going to continue using the system manager's account and you
                  want to restore these symbols, you should log out and log in
                  again.





               2-10  Installing DEC GKS-3D

 










               ____________________________________________________________

               2.3  Error Recovery

                  If errors occur during the installation itself or when the
                  IVP is running, VMSINSTAL displays failure messages. If the
                  installation fails, the following message is displayed:

                    %VMSINSTAL-E-INSFAIL, The installation of DECGKS3D V1.1 has failed.

                  If the IVP fails, the following messages are displayed:

                    The DECGKS3D V1.1 Installation Verification Procedure failed.

                    %VMSINSTAL-E-IVPFAIL, The IVP for DEC GKS-3D V1.1 has failed.

                  Errors can occur during the installation if any of the fol-
                  lowing conditions exist:

                   o The operating system version is incorrect.

                   o A prerequisite software version is incorrect.

                   o Quotas necessary for successful installation are insuffi-
                     cient.

                   o System parameter values for successful installation are
                     insufficient.

                   o The VMS help library is currently in use.

                   o The product is not properly licensed.

                   o The metafile input handler is not installed.

                   o The default output handler, defined by the logicals
                     GKS3D$WSTYPE and GKS3D$CONID, is not installed.

                  The following errors may occur during execution of the IVP.

                   o IVP failure.

                       DECGKS3D-F-IVP, GKS-3D installation verification procedure failed

                   o Workstation handler not installed.

                       GKS3D-E-ERROR_23, specified workstation type does not exist in
                        routine OPEN WORKSTATION

                                                    Installing DEC GKS-3D  2-11

 











                     First, ensure that the metafile input handler is in-
                     stalled. Then ensure that the definition of GKS3D$WSTYPE
                     is a valid workstation type, including bit masks, and
                     that GKS3D$CONID corresponds to a physical device that is
                     supported and functional.

                   o The connection ID and workstation type are not compatible.

                       GKS3D-E-ERROR_26, specified workstation cannot be opened
                        in routine OPEN WORKSTATION

                     Ensure that the definitions of GKS3D$CONID and GKS3D$WSTYPE
                     make valid pairs, and that GKS3D$CONID corresponds to a
                     physical device that is supported and installed.

                   o There are not enough unused color entries available for
                     GKS-3D in DECwindows.

                       DECGKS3D-E-ERROR_NEG_2, requested color map could not be created
                        in routine OPEN WORKSTATION

                     Set the bit n in the workstation bit mask %x0nmm00Da. For
                     example, for workstation type 211, specify %x010000D3.

                  For descriptions of the error messages generated by these
                  conditions, see the VMS documentation on system messages,
                  recovery procedures, and VMS software installation. If you
                  are notified that any of these conditions exist, you should
                  take the appropriate action as described in the message.
                  (You might need to change a system parameter or increase
                  an authorized quota value.) For information on installation
                  requirements, see Chapter 1.













               2-12  Installing DEC GKS-3D

 

















                                                                      Chapter 3


                                                    After Installing DEC GKS-3D
               ________________________________________________________________


                  After installing DEC GKS-3D, you must perform the following
                  tasks:

                   o Edit the system startup files.

                   o Reboot the system.

                   o Set user account quotas.

                   o Modify system parameter settings.

                  This chapter also explains how to run the Installation
                  Verification Procedure (IVP) after the software has been
                  installed.

               ____________________________________________________________

               3.1  Editing the System Files

                  You must edit the system startup file to provide for auto-
                  matic startup of DEC GKS-3D when your system is rebooted.

                  Add the command line that starts DEC GKS-3D to the system
                  startup file, SYS$MANAGER:SYSTARTUP_V5.COM. You must position
                  this new command line after the line that invokes the network
                  startup command procedure. The following example shows the
                  network startup command line followed by the startup command
                  line for DEC GKS-3D:

                    $ @SYS$STARTUP:STARTNET
                         .
                         .
                         .
                    $ @SYS$STARTUP:GKS3D$STARTUP

                                               After Installing DEC GKS-3D  3-1

 










               ____________________________________________________________

               3.2  Cluster Considerations

                  If you want to run DEC GKS-3D on multiple nodes of a
                  VAXcluster, first check to see that you have the appropriate
                  software license. Then, follow these steps after installing
                  DEC GKS-3D:

                   1. Run the following command on each node of the cluster that
                     has the software license:

                       $ @SYS$STARTUP:GKS3D$STARTUP <RET>

                   2. Prepare the system-specific roots on other nodes by issu-
                     ing the following commands on each node:

                       $ CREATE/DIRECTORY SYS$SPECIFIC:[SYSHLP.EXAMPLES.GKS3D] <RET>
                       $ CREATE/DIRECTORY SYS$SPECIFIC:[SYSTEST.GKS3D] <RET>

                   3. Verify the installation by running the IVP on each
                     node. Information about running the IVP is given in
                     Section 3.3.2.

                       $ RUN GKS3D$TEST:GKS3D$IVP <RET>

                   4. Determine if the INSTALL utility was used to install
                     GKS3D$RTLIB.EXE.

                      a. Log in to a node on the cluster.

                      b. Run INSTALL and enter the following command at the
                        INSTALL> prompt:

                          INSTALL> LIST SYS$LIBRARY:GKS3D$RTLIB.EXE <RET>

                        The INSTALL utility displays how the GKS3D$RTLIB was
                        installed. For example:

                          DISK$SYSTEM01:<SYS0.SYSCOMMON.SYSLIB>.EXE
                              GKS3D$RTLIB;1    Open     Share         Lnkbl

                        If an error occurs with this command, GKS-3D was not
                        properly installed.

                      c. Repeat steps a and b for each node of the cluster.

               3-2  After Installing DEC GKS-3D

 










               ____________________________________________________________

               3.3  User Account Requirements

                  To use DEC GKS-3D, user accounts on your system must have
                  certain privileges and quotas. The next two sections contain
                  information on these requirements.

               ____________________________________________________________

               3.3.1  Privileges

                  To use DEC GKS-3D, each account must have at least the TMPMBX
                  and NETMBX privileges. Use the VMS Authorize Utility to
                  determine whether users have the privileges they require.

               ____________________________________________________________

               3.3.2  Running the Installation Verification Procedure After
                      Installation

                  The DEC GKS-3D IVP reads a three-dimensional image from a
                  metafile workstation (GKS3D$TEST:GKS3D$IVP.DAT). The metafile
                  is large and execution tests the DEC GKS-3D installation
                  thoroughly.

                  The image is output to the default OUTPUT or OUTIN work-
                  station, which is defined by the workstation identifier
                  and connection identifier (the logicals GKS3D$WSTYPE and
                  GKS3D$CONID respectively). The default workstation types are
                  as follows:

                   o VAX: Sixel

                   o Workstation running DECwindows: DECwindows

                   o Workstation running VAXstation Workstation Software (VWS):
                     VWS

                  To redirect the IVP output to another workstation, redefine
                  the logicals.

                  Run the IVP using the following command:

                    $ RUN GKS3D$TEST:GKS3D$IVP <RET>

                  For example, if you want to run the DECwindows IVP on a re-
                  mote node, ensure that you have the access rights on the
                  server for remote use and that the GKS-3D DECwindows han-
                  dler is installed. Then enter the following commands, and
                  substitute your node name for node REMOTE:

                                               After Installing DEC GKS-3D  3-3

 











                    $ DEFINE GKS3D$WSTYPE 211 <RET>
                    $ DEFINE GKS3D$CONID  REMOTE::0.0 <RET>
                    $ RUN GKS3D$TEST:GKS3D$IVP <RET>

                  Output is on a remote server.

               ____________________________________________________________

               3.4  Determining and Reporting Problems

                  If an error occurs while DEC GKS-3D is being used and you
                  believe that the error is caused by a problem with DEC GKS-
                  3D, take one of the following actions:

                   o If you have a basic or DECsupport Software Agreement,
                     you should call your Customer Support Center. (With these
                     services, you receive telephone support that provides
                     high-level advisory and remedial assistance.)

                   o If you have a Self-Maintenance Software Agreement, you can
                     submit a Software Performance Report (SPR).

                   o If you purchased DEC GKS-3D within the past 90 days and
                     you think the problem is caused by a software error, you
                     can submit a Software Performance Report (SPR).

                  If you find an error in the DEC GKS-3D documentation, you
                  should fill out and submit the Reader's Comments form at the
                  back of the document in which the error was found. Include
                  the section and page number where the error was found.















               3-4  After Installing DEC GKS-3D

 

















                                                                     Appendix A


                                                            Sample Installation
               ________________________________________________________________


                  This appendix contains two sample installations of DEC GKS-
                  3D. These samples were run on a system that had no previous
                  version of DEC GKS-3D installed.

                  The sample installations assume that DECnet has been shut
                  down, that no users are logged on to your system, and that
                  OPTIONS N is specified to print the release notes. The
                  Installation Verification Procedure (IVP) runs at the end
                  of the installation.

               ____________________________________________________________

               A.1  Full Development Kit Installation

                  This section contains a sample installation for the DEC GKS-
                  3D full development kit.

                  Before you begin the DEC GKS-3D installation, define the
                  destination for the output of the Installation Verification
                  Procedure (IVP) with the following command, and replace node
                  with your node name:

                    $ DEFINE DECW$DISPLAY node::0.0 <RET>

                  The sample installation follows:

               $ @SYS$UPDATE:VMSINSTAL DECGKS3D MUA0: OPTIONS N <RET>

                      VAX/VMS Software Product Installation Procedure V5.3-2

               It is 20-AUG-1990 at 14:53.

               Enter a question mark (?) at any time for help.

               * Are you satisfied with the backup of your system disk [YES]? yes <RET>

                                                       Sample Installation  A-1

 











               The following products will be processed:

                 DECGKS3D V1.1

                      Beginning installation of DECGKS3D V1.1 at 14:58

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...

                   Release notes included with this kit are always copied to SYS$HELP.

                   Additional Release Notes Options:

                1.  Display release notes
                2.  Print release notes
                3.  Both 1 and 2
                4.  None of the above

               * Select option [2]: 1 <RET>

               * Do you want to continue the installation [NO]? YES <RET>

               %VMSINSTAL-I-RELMOVED, The product's release notes have been successfully moved
                to SYS$HELP.
               %VMSINSTAL-I-RESTORE, Restoring product save set B ...
               * Do you want to purge files replaced by this installation [YES]? yes <RET>

                      PostScript is a registered trademark of Adobe Systems, Inc.
                      LaserWriter is a registered trademark of Apple Computer, Inc.
                      Tektronix is a registered trademark of Tektronix, Inc.

                      This kit contains an Installation Verification Procedure (IVP)
                      to verify the correct installation of the DEC GKS-3D product.
                      It can be run prior to the conclusion of this procedure by answering
                      "YES" to the IVP prompt or invoked after the installation as
                      follows :

                       RUN SYS$SYSROOT:[SYSTEST.GKS3D]GKS3D$IVP
                      or
                       RUN GKS3D$TEST:GKS3D$IVP

               * Do you wish to perform the Installation Verification Procedure [YES]? yes <RET>

                       Product:      GKS3D
                       Producer:     DEC
                       Version:      1.1
                       Release Date: 15-OCT-1990

               * Does this product have an authorization key registered and loaded? YES <RET>

               A-2  Sample Installation

 











                      STARTING to perform all the installation work. No additional
                      user actions are necessary from this point. The remaining part
                      of the installation will take ( 5 - 30 minutes ) depending on
                      your CPU.

                      The DEC GKS-3D run-time library has been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D VAXstation marker fonts have been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D language bindings have been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D Fonts have been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D Language files have been processed successfully.

                      The installation procedure is continuing...

                  %VMSINSTAL-I-SYSDIR, This product creates system directory
                  [SYSHLP.EXAMPLES.GKS3D].

                  If you intend to execute this layered product on other nodes in your
                  VAXcluster, and you have the appropriate software license, you must
                  prepare the system-specific roots on the other nodes by issuing the
                  following command on each node (using a suitably privileged account):

                      $ CREATE/DIRECTORY SYS$SPECIFIC:[SYSHLP.EXAMPLES.GKS3D]

                      This kit contains example programs to demonstrate how to interface
                      with the DEC GKS-3D product. The example programs are located in:

                       SYS$SYSROOT:[SYSHLP.EXAMPLES.GKS3D]
                      or
                       GKS3D$EXAMPLES:

                   %VMSINSTAL-I-SYSDIR, This product creates system directory [SYSTEST.GKS3D].

                   If you intend to execute this layered product on other nodes in your
                   VAXcluster, and you have the appropriate software license, you must
                   prepare the system-specific roots on the other nodes by issuing the
                   following command on each node (using a suitably privileged account):

                      $ CREATE/DIRECTORY SYS$SPECIFIC:[SYSTEST.GKS3D]

                                                       Sample Installation  A-3

 











                      DEC GKS-3D has built successfully.
                      Continuing installation...

                 System Manager:

                      Upon completion of this installation, please be sure to
                      edit the system startup files as described in the DEC GKS-3D
                      Installation Guide.

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

                      Beginning the DEC GKS-3D Installation Verification Procedure (IVP).
                      The IVP will take 1 to 5 minutes depending on your CPU.

                      Since you are running on a VAXstation the Installation
                      Verification Procedure will be run with DEC GKS-3D device type 211
                      (DECW). Output will be done to the node indicated by the logical
                      name DECW$DISPLAY.

                      The DECGKS3D V1.1 Installation Verification Procedure (IVP) completed
                      successfully. If the results of the Installation Verification
                      Procedure (IVP) look like the illustration provided with the
                      DEC GKS-3D Installation Guide, then installation has been successful.

                      Installation of DECGKS3D V1.1 completed at 18:02

                      VMSINSTAL procedure done at 18:02

               ____________________________________________________________

               A.2  Run-Time Kit Installation

                  This section contains a sample installation for the DEC GKS-
                  3D run-time only kit.

                  Before you begin the DEC GKS-3D installation, define the
                  destination for the output of the Installation Verification
                  Procedure (IVP) with the following command, and replace node
                  with your node name:

                    $ DEFINE DECW$DISPLAY node::0.0 <RET>

                  The sample installation follows:

               $ @SYS$UPDATE:VMSINSTAL DECGKS3DRT MUA0: OPTIONS N <RET>

                      VAX/VMS Software Product Installation Procedure V5.3-2

               It is 20-AUG-1990 at 14:53.

               Enter a question mark (?) at any time for help.

               A-4  Sample Installation

 











               * Are you satisfied with the backup of your system disk [YES]? yes <RET>

               The following products will be processed:

                 DECGKS3DRT V1.1

                      Beginning installation of DECGKS3DRT V1.1 at 14:58

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...

                   Release notes included with this kit are always copied to SYS$HELP.

                   Additional Release Notes Options:

                1.  Display release notes
                2.  Print release notes
                3.  Both 1 and 2
                4.  None of the above

               * Select option [2]: 1 <RET>

               * Do you want to continue the installation [NO]? YES <RET>

               %VMSINSTAL-I-RELMOVED, The product's release notes have been successfully moved
                to SYS$HELP.
               %VMSINSTAL-I-RESTORE, Restoring product save set B ...
               * Do you want to purge files replaced by this installation [YES]? yes <RET>

                      PostScript is a registered trademark of Adobe Systems, Inc.
                      LaserWriter is a registered trademark of Apple Computer, Inc.
                      Tektronix is a registered trademark of Tektronix, Inc.

                      This kit contains an Installation Verification Procedure (IVP)
                      to verify the correct installation of the DEC GKS-3D product.
                      It can be run prior to the conclusion of this procedure by answering
                      "YES" to the IVP prompt or invoked after the installation as
                      follows :

                       RUN SYS$SYSROOT:[SYSTEST.GKS3D]GKS3D$IVP
                      or
                       RUN GKS3D$TEST:GKS3D$IVP

               * Do you wish to perform the Installation Verification Procedure [YES]? yes <RET>

                       Product:      GKS3D-RT
                       Producer:     DEC
                       Version:      1.1
                       Release Date: 15-OCT-1990

               * Does this product have an authorization key registered and loaded? YES <RET>

                                                       Sample Installation  A-5

 











                      STARTING to perform all the installation work. No additional
                      user actions are necessary from this point. The remaining part
                      of the installation will take ( 5 - 30 minutes ) depending on
                      your CPU.

                      The DEC GKS-3D run-time library has been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D VAXstation marker fonts have been processed successfully.

                      The installation procedure is continuing...

                      The DEC GKS-3D Fonts have been processed successfully.

                      The installation procedure is continuing...

               %VMSINSTAL-I-SYSDIR, This product creates system directory [SYSTEST.GKS3D].

                   If you intend to execute this layered product on other nodes in your
                   VAXcluster, and you have the appropriate software license, you must
                   prepare the system-specific roots on the other nodes by issuing the
                   following command on each node (using a suitably privileged account):

                      $ CREATE/DIRECTORY SYS$SPECIFIC:[SYSTEST.GKS3D]

                      DEC GKS-3D has built successfully.
                      Continuing installation...

                 System Manager:

                      Upon completion of this installation, please be sure to
                      edit the system startup files as described in the DEC GKS-3D
                      Installation Guide.

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...

                      Beginning the DEC GKS-3D Installation Verification Procedure (IVP).
                      The IVP will take 1 to 5 minutes depending on your CPU.

                      Since you are running on a VAXstation the Installation
                      Verification Procedure will be run with DEC GKS-3D device type 211
                      (DECW). Output will be done to the node indicated by the logical
                      name DECW$DISPLAY.

                      The DECGKS3DRT V1.1 Installation Verification Procedure (IVP) completed
                      successfully. If the results of the Installation Verification
                      Procedure (IVP) look like the illustration provided with the
                      DEC GKS-3D Installation Guide, then installation has been successful.

                      Installation of DECGKS3DRT V1.1 completed at 18:02

               A-6  Sample Installation

 











                      VMSINSTAL procedure done at 18:02












































                                                       Sample Installation  A-7

 

















                                                                     Appendix B


                               Files and Logical Names Installed on Your System
               ________________________________________________________________


                  The DEC GKS-3D installation procedure installs a number of
                  files on your system and defines some logical names. Sections
                  B.1 and B.2 list the installed files. Section B.3 lists
                  the logical names that are added to the system logical name
                  table.

               ____________________________________________________________

               B.1  DEC GKS-3D Development Kit Files for VMS

                  The following list contains the directories and file names of
                  all files installed for the development kit:

                    Directory SYS$COMMON:[SYS$STARTUP]

                    GKS3D$STARTUP.COM

                    Directory SYS$COMMON:[SYSFONT]

                    GKS3D$MARKERS.VWS$FONT
                    GKS3D$MARKERS.VWS$VAFONT

                    Directory SYS$COMMON:[SYSHLP]

                    DECGKS3D011.RELEASE_NOTES

                    Directory SYS$COMMON:[SYSHLP.EXAMPLES.GKS3D]





                          Files and Logical Names Installed on Your System  B-1

 











                    GKS3D$EXAMPLES_BUILD.COM
                    GKS3D$IMM_MODE_XFORM.C
                    GKS3D$IMM_MODE_XFORM.EXE
                    GKS3D$SEGMENT_XFORM.C
                    GKS3D$SEGMENT_XFORM.EXE
                    GKS3D$SIMPLE_CUBE.DAT
                    GKS3D$SIMPLE_GARAGE.DAT
                    GKS3D$SIMPLE_PYRAMID.DAT





































               B-2  Files and Logical Names Installed on Your System

 











                    Directory SYS$COMMON:[SYSLIB]

                    GKS3D$CBND.H
                    GKS3D$CBND.OLB
                    GKS3D$DEFS.ADA
                    GKS3D$DEFS.BAS
                    GKS3D$DEFS.FOR
                    GKS3D$DEFS.H
                    GKS3D$DEFS.PAS
                    GKS3D$DEFS.PLI
                    GKS3D$DEFS.R32
                    GKS3D$ERRORS.ADA
                    GKS3D$ERRORS.BAS
                    GKS3D$ERRORS.FOR
                    GKS3D$ERRORS.H
                    GKS3D$ERRORS.PAS
                    GKS3D$ERRORS.PLI
                    GKS3D$ERRORS.R32
                    GKS3D$FORBND.FOR
                    GKS3D$FORBND.OLB
                    GKS3D$GKSBND.OLB
                    GKS3D$GKSRTLIB.EXE
                    GKS3D$MI_WS_HANDLER.EXE
                    GKS3D$MO_WS_HANDLER.EXE
                    GKS3D$RTLIB.EXE
                    GKS3D$WISS_WS_HANDLER.EXE
                    GKS3D$WSM_WS_HANDLER.EXE

                    Directory SYS$COMMON:[SYSLIB]
















                          Files and Logical Names Installed on Your System  B-3

 











                    VAXGFX$CGMO_DEV_HANDLER.EXE
                    VAXGFX$COLSIX_DEV_HANDLER.EXE
                    VAXGFX$DDIF_COLOR_TABLE.DAT
                    VAXGFX$DDIF_DEV_HANDLER.EXE
                    VAXGFX$DECW_DEV_HANDLER.EXE
                    VAXGFX$FONT_NEG01.FNT
                    VAXGFX$FONT_NEG02.FNT
                    VAXGFX$FONT_NEG03.FNT
                    VAXGFX$FONT_NEG04.FNT
                    VAXGFX$FONT_NEG05.FNT
                    VAXGFX$FONT_NEG06.FNT
                    VAXGFX$FONT_NEG07.FNT
                    VAXGFX$FONT_NEG08.FNT
                    VAXGFX$FONT_NEG09.FNT
                    VAXGFX$FONT_NEG10.FNT
                    VAXGFX$FONT_NEG11.FNT
                    VAXGFX$FONT_NEG12.FNT
                    VAXGFX$FONT_NEG13.FNT
                    VAXGFX$FONT_NEG14.FNT
                    VAXGFX$FONT_NEG15.FNT
                    VAXGFX$FONT_NEG16.FNT
                    VAXGFX$FONT_NEG17.FNT
                    VAXGFX$FONT_NEG18.FNT
                    VAXGFX$FONT_NEG19.FNT
                    VAXGFX$FONT_NEG20.FNT
                    VAXGFX$FONT_NEG21.FNT
                    VAXGFX$FONT_NEG22.FNT
                    VAXGFX$FONT_NEG23.FNT
                    VAXGFX$FONT_NEG24.FNT
                    VAXGFX$HPGL_DEV_HANDLER.EXE
                    VAXGFX$PS_DEV_HANDLER.EXE
                    VAXGFX$REGIS_DEV_HANDLER.EXE
                    VAXGFX$RTL.EXE
                    VAXGFX$SIXEL_DEV_HANDLER.EXE
                    VAXGFX$TEK41_DEV_HANDLER.EXE
                    VAXGFX$TEK_DEV_HANDLER.EXE
                    VAXGFX$UIS_DEV_HANDLER.EXE

                    Directory SYS$COMMON:[SYSMSG]

                    GKS3D$MSGS.EXE

                    Directory SYS$COMMON:[SYSTEST.GKS3D]


               B-4  Files and Logical Names Installed on Your System

 











                    GKS3D$IVP.DAT
                    GKS3D$IVP.EXE

               ____________________________________________________________

               B.2  DEC GKS-3D Run-Time Kit Files for VMS

                  The following list contains the directories and file names of
                  all files installed for the run-time kit:

                    Directory SYS$COMMON:[SYS$STARTUP]

                    GKS3D$STARTUP.COM

                    Directory SYS$COMMON:[SYSFONT]

                    GKS3D$MARKERS.VWS$FONT
                    GKS3D$MARKERS.VWS$VAFONT

                    Directory SYS$COMMON:[SYSHLP]

                    DECGKS3DRT011.RELEASE_NOTES

                    Directory SYS$COMMON:[SYSHLP.EXAMPLES.GKS3D]

                    GKS3D$IMM_MODE_XFORM.EXE
                    GKS3D$SEGMENT_XFORM.EXE
                    GKS3D$SIMPLE_CUBE.DAT
                    GKS3D$SIMPLE_GARAGE.DAT
                    GKS3D$SIMPLE_PYRAMID.DAT

                    Directory SYS$COMMON:[SYSLIB]

                    GKS3D$GKSRTLIB.EXE
                    GKS3D$MI_WS_HANDLER.EXE
                    GKS3D$MO_WS_HANDLER.EXE
                    GKS3D$RTLIB.EXE
                    GKS3D$WISS_WS_HANDLER.EXE
                    GKS3D$WSM_WS_HANDLER.EXE






                          Files and Logical Names Installed on Your System  B-5

 











                    Directory SYS$COMMON:[SYSLIB]

                    VAXGFX$CGMO_DEV_HANDLER.EXE
                    VAXGFX$COLSIX_DEV_HANDLER.EXE
                    VAXGFX$DDIF_COLOR_TABLE.DAT
                    VAXGFX$DDIF_DEV_HANDLER.EXE
                    VAXGFX$DECW_DEV_HANDLER.EXE
                    VAXGFX$FONT_NEG01.FNT
                    VAXGFX$FONT_NEG02.FNT
                    VAXGFX$FONT_NEG03.FNT
                    VAXGFX$FONT_NEG04.FNT
                    VAXGFX$FONT_NEG05.FNT
                    VAXGFX$FONT_NEG06.FNT
                    VAXGFX$FONT_NEG07.FNT
                    VAXGFX$FONT_NEG08.FNT
                    VAXGFX$FONT_NEG09.FNT
                    VAXGFX$FONT_NEG10.FNT
                    VAXGFX$FONT_NEG11.FNT
                    VAXGFX$FONT_NEG12.FNT
                    VAXGFX$FONT_NEG13.FNT
                    VAXGFX$FONT_NEG14.FNT
                    VAXGFX$FONT_NEG15.FNT
                    VAXGFX$FONT_NEG16.FNT
                    VAXGFX$FONT_NEG17.FNT
                    VAXGFX$FONT_NEG18.FNT
                    VAXGFX$FONT_NEG19.FNT
                    VAXGFX$FONT_NEG20.FNT
                    VAXGFX$FONT_NEG21.FNT
                    VAXGFX$FONT_NEG22.FNT
                    VAXGFX$FONT_NEG23.FNT
                    VAXGFX$FONT_NEG24.FNT
                    VAXGFX$HPGL_DEV_HANDLER.EXE
                    VAXGFX$PS_DEV_HANDLER.EXE
                    VAXGFX$REGIS_DEV_HANDLER.EXE
                    VAXGFX$RTL.EXE
                    VAXGFX$SIXEL_DEV_HANDLER.EXE
                    VAXGFX$TEK41_DEV_HANDLER.EXE
                    VAXGFX$TEK_DEV_HANDLER.EXE
                    VAXGFX$UIS_DEV_HANDLER.EXE

                    Directory SYS$COMMON:[SYSMSG]

                    GKS3D$MSGS.EXE

                    Directory SYS$COMMON:[SYSTEST.GKS3D]

               B-6  Files and Logical Names Installed on Your System

 











                    GKS3D$IVP.DAT
                    GKS3D$IVP.EXE

               ____________________________________________________________

               B.3  Logical Names

                  The following logical names are entered into the system
                  logical name tables when DEC GKS-3D is installed. These
                  names are stored in the product's startup file. They are
                  automatically entered into the system logical name table
                  whenever the system reboots or whenever the software is
                  invoked.

                    (LNM$PROCESS_TABLE)

                    (LNM$JOB_80326230)

                    (LNM$GROUP_000200)

                    (LNM$SYSTEM_TABLE)

                      "GKS3D$ASF" = "INDIVIDUAL"
                      "GKS3D$CONID" = "0::0"
                      "GKS3D$ERROR" = "ON"
                      "GKS3D$EXAMPLES" = "SYS$COMMON:[SYSHLP.EXAMPLES.GKS3D]"
                      "GKS3D$LIST_TYPES" = "2"
                            = "3"
                            = "5"
                            = "210"
                            = "211"
                            = "212"
                            = "213"
                            = "41"
                            = "10"
                            = "11"
                            = "12"
                            = "13"
                            = "14"
                            = "15"
                            = "16"
                            = "17"
                            = "70"
                            = "72"
                            = "80"
                            = "82"

                          Files and Logical Names Installed on Your System  B-7

 











                            = "83"
                            = "84"
                            = "85"
                            = "86"
                            = "87"
                            = "88"
                            = "31"
                            = "32"
                            = "33"
                            = "34"
                            = "35"
                            = "38"
                            = "39"
                            = "91"
                            = "92"
                            = "93"
                            = "51"
                            = "52"
                            = "53"
                            = "54"
                            = "55"
                            = "56"
                            = "61"
                            = "62"
                            = "65"
                            = "66"
                            = "250"
                            = "7"
                      "GKS3D$NDC_CLIP" = "ON"
                      "GKS3D$STROKE_FONT1" = "SYS$COMMON:VAXGFX$FONT_NEG01.FNT"
                      "GKS3D$STROKE_FONT_LIST" = "1"
                            = "NEG_1"
                            = "NEG_2"
                            = "NEG_3"
                            = "NEG_4"
                            = "NEG_5"
                            = "NEG_6"
                            = "NEG_7"
                            = "NEG_8"
                            = "NEG_9"
                            = "NEG_10"
                            = "NEG_11"
                            = "NEG_12"
                            = "NEG_13"

               B-8  Files and Logical Names Installed on Your System

 











                            = "NEG_14"
                            = "NEG_15"
                            = "NEG_16"
                            = "NEG_17"
                            = "NEG_18"
                            = "NEG_19"
                            = "NEG_20"
                            = "NEG_21"
                            = "NEG_22"
                            = "NEG_23"
                            = "NEG_24"
                      "GKS3D$TEST" = "SYS$COMMON:[SYSTEST.GKS3D]"
                      "GKS3D$WSTYPE" = "211"

                    (DECW$LOGICAL_NAMES)

                    (GKS3D$TABLE)
                      "GKS3D$DEVICE_10" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_11" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_12" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_13" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_14" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_15" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_16" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_17" = "VAXGFX$REGIS_DEV_HANDLER"
                      "GKS3D$DEVICE_210" = "VAXGFX$DECW_DEV_HANDLER"
                      "GKS3D$DEVICE_211" = "VAXGFX$DECW_DEV_HANDLER"
                      "GKS3D$DEVICE_212" = "VAXGFX$DECW_DEV_HANDLER"
                      "GKS3D$DEVICE_213" = "VAXGFX$DECW_DEV_HANDLER"
                      "GKS3D$DEVICE_250" = "VAXGFX$DDIF_DEV_HANDLER"
                      "GKS3D$DEVICE_31" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_32" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_33" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_34" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_35" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_38" = "VAXGFX$SIXEL_DEV_HANDLER"
                      "GKS3D$DEVICE_39" = "VAXGFX$LASER_DEV_HANDLER"
                      "GKS3D$DEVICE_41" = "VAXGFX$UIS_DEV_HANDLER"
                      "GKS3D$DEVICE_51" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_52" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_53" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_54" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_55" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_56" = "VAXGFX$HPGL_DEV_HANDLER"
                      "GKS3D$DEVICE_61" = "VAXGFX$PS_DEV_HANDLER"

                          Files and Logical Names Installed on Your System  B-9

 











                      "GKS3D$DEVICE_62" = "VAXGFX$PS_DEV_HANDLER"
                      "GKS3D$DEVICE_65" = "VAXGFX$PS_DEV_HANDLER"
                      "GKS3D$DEVICE_66" = "VAXGFX$PS_DEV_HANDLER"
                      "GKS3D$DEVICE_7"  = "VAXGFX$CGMO_DEV_HANDLER"
                      "GKS3D$DEVICE_70" = "VAXGFX$TEK_DEV_HANDLER"
                      "GKS3D$DEVICE_72" = "VAXGFX$TEK_DEV_HANDLER"
                      "GKS3D$DEVICE_80" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_82" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_83" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_84" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_85" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_86" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_87" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_88" = "VAXGFX$TEK41_DEV_HANDLER"
                      "GKS3D$DEVICE_91" = "VAXGFX$COLSIX_DEV_HANDLER"
                      "GKS3D$DEVICE_92" = "VAXGFX$COLSIX_DEV_HANDLER"
                      "GKS3D$DEVICE_93" = "VAXGFX$COLSIX_DEV_HANDLER"
                      "GKS3D$DEVICE_TAB_10" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_11" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_12" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_13" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_14" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_15" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_16" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_17" = "VAXGFX$$REGIS_DFT"
                      "GKS3D$DEVICE_TAB_210" = "VAXGFX$$DECW_DFT"
                      "GKS3D$DEVICE_TAB_211" = "VAXGFX$$DECW_DFT"
                      "GKS3D$DEVICE_TAB_212" = "VAXGFX$$DECW_DFT"
                      "GKS3D$DEVICE_TAB_213" = "VAXGFX$$DECW_DFT"
                      "GKS3D$DEVICE_TAB_250" = "VAXGFX$$DDIF_DFT"
                      "GKS3D$DEVICE_TAB_31" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_32" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_33" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_34" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_35" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_38" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_39" = "VAXGFX$$SIXEL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_41" = "VAXGFX$$UIS_DFT"
                      "GKS3D$DEVICE_TAB_51" = "VAXGFX$$HPGL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_52" = "VAXGFX$$HPGL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_53" = "VAXGFX$$HPGL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_54" = "VAXGFX$$HPGL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_55" = "VAXGFX$$HPGL_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_56" = "VAXGFX$$HPGL_OUTPUT_DFT"

               B-10  Files and Logical Names Installed on Your System

 











                      "GKS3D$DEVICE_TAB_61" = "VAXGFX$$PS_DFT"
                      "GKS3D$DEVICE_TAB_62" = "VAXGFX$$PS_DFT"
                      "GKS3D$DEVICE_TAB_65" = "VAXGFX$$PS_DFT"
                      "GKS3D$DEVICE_TAB_66" = "VAXGFX$$PS_DFT"
                      "GKS3D$DEVICE_TAB_7"  = "VAXGFX$$CGMO_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_70" = "VAXGFX$$TEK_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_72" = "VAXGFX$$TEK_DFT"
                      "GKS3D$DEVICE_TAB_80" = "VAXGFX$$TEK4107_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_82" = "VAXGFX$$TEK4107_DFT"
                      "GKS3D$DEVICE_TAB_83" = "VAXGFX$$TEK4207_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_84" = "VAXGFX$$TEK4207_DFT"
                      "GKS3D$DEVICE_TAB_85" = "VAXGFX$$TEK4128_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_86" = "VAXGFX$$TEK4128_DFT"
                      "GKS3D$DEVICE_TAB_87" = "VAXGFX$$TEK4129_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_88" = "VAXGFX$$TEK4129_DFT"
                      "GKS3D$DEVICE_TAB_91" = "VAXGFX$$COLSIX_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_92" = "VAXGFX$$COLSIX_OUTPUT_DFT"
                      "GKS3D$DEVICE_TAB_93" = "VAXGFX$$COLSIX_OUTPUT_DFT"
                      "GKS3D$FUNCTION_TAB_10" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_11" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_12" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_13" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_14" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_15" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_16" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_17" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_2" = "GKS3D$$MO_WFT"
                      "GKS3D$FUNCTION_TAB_210" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_211" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_212" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_213" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_250" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_3" = "GKS3D$$MI_WFT"
                      "GKS3D$FUNCTION_TAB_31" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_32" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_33" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_34" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_35" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_38" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_39" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_41" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_5" = "GKS3D$$WISS_WFT"
                      "GKS3D$FUNCTION_TAB_51" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_52" = "GKS3D$$WSM_WFT"

                         Files and Logical Names Installed on Your System  B-11

 











                      "GKS3D$FUNCTION_TAB_53" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_54" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_55" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_56" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_61" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_62" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_65" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_66" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_7"  = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_70" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_72" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_80" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_82" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_83" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_84" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_85" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_86" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_87" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_88" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_91" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_92" = "GKS3D$$WSM_WFT"
                      "GKS3D$FUNCTION_TAB_93" = "GKS3D$$WSM_WFT"
                      "GKS3D$STROKE_FONT_NEG1" = "SYS$COMMON:VAXGFX$FONT_NEG01.FNT"
                      "GKS3D$STROKE_FONT_NEG10" = "SYS$COMMON:VAXGFX$FONT_NEG10.FNT"
                      "GKS3D$STROKE_FONT_NEG11" = "SYS$COMMON:VAXGFX$FONT_NEG11.FNT"
                      "GKS3D$STROKE_FONT_NEG12" = "SYS$COMMON:VAXGFX$FONT_NEG12.FNT"
                      "GKS3D$STROKE_FONT_NEG13" = "SYS$COMMON:VAXGFX$FONT_NEG13.FNT"
                      "GKS3D$STROKE_FONT_NEG14" = "SYS$COMMON:VAXGFX$FONT_NEG14.FNT"
                      "GKS3D$STROKE_FONT_NEG15" = "SYS$COMMON:VAXGFX$FONT_NEG15.FNT"
                      "GKS3D$STROKE_FONT_NEG16" = "SYS$COMMON:VAXGFX$FONT_NEG16.FNT"
                      "GKS3D$STROKE_FONT_NEG17" = "SYS$COMMON:VAXGFX$FONT_NEG17.FNT"
                      "GKS3D$STROKE_FONT_NEG18" = "SYS$COMMON:VAXGFX$FONT_NEG18.FNT"
                      "GKS3D$STROKE_FONT_NEG19" = "SYS$COMMON:VAXGFX$FONT_NEG19.FNT"
                      "GKS3D$STROKE_FONT_NEG2" = "SYS$COMMON:VAXGFX$FONT_NEG02.FNT"
                      "GKS3D$STROKE_FONT_NEG20" = "SYS$COMMON:VAXGFX$FONT_NEG20.FNT"
                      "GKS3D$STROKE_FONT_NEG21" = "SYS$COMMON:VAXGFX$FONT_NEG21.FNT"
                      "GKS3D$STROKE_FONT_NEG22" = "SYS$COMMON:VAXGFX$FONT_NEG22.FNT"
                      "GKS3D$STROKE_FONT_NEG23" = "SYS$COMMON:VAXGFX$FONT_NEG23.FNT"
                      "GKS3D$STROKE_FONT_NEG24" = "SYS$COMMON:VAXGFX$FONT_NEG24.FNT"
                      "GKS3D$STROKE_FONT_NEG3" = "SYS$COMMON:VAXGFX$FONT_NEG03.FNT"
                      "GKS3D$STROKE_FONT_NEG4" = "SYS$COMMON:VAXGFX$FONT_NEG04.FNT"
                      "GKS3D$STROKE_FONT_NEG5" = "SYS$COMMON:VAXGFX$FONT_NEG05.FNT"
                      "GKS3D$STROKE_FONT_NEG6" = "SYS$COMMON:VAXGFX$FONT_NEG06.FNT"
                      "GKS3D$STROKE_FONT_NEG7" = "SYS$COMMON:VAXGFX$FONT_NEG07.FNT"

               B-12  Files and Logical Names Installed on Your System

 











                      "GKS3D$STROKE_FONT_NEG8" = "SYS$COMMON:VAXGFX$FONT_NEG08.FNT"
                      "GKS3D$STROKE_FONT_NEG9" = "SYS$COMMON:VAXGFX$FONT_NEG09.FNT"
                      "GKS3D$WORKSTATION_10" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_11" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_12" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_13" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_14" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_15" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_16" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_17" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_2" = "GKS3D$MO_WS_HANDLER"
                      "GKS3D$WORKSTATION_210" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_211" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_212" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_213" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_250" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_3" = "GKS3D$MI_WS_HANDLER"
                      "GKS3D$WORKSTATION_31" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_32" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_33" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_34" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_35" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_38" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_39" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_41" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_5" = "GKS3D$WISS_WS_HANDLER"
                      "GKS3D$WORKSTATION_51" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_52" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_53" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_54" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_55" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_56" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_61" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_62" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_65" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_66" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_7"  = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_70" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_72" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_80" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_82" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_83" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_84" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_85" = "GKS3D$WSM_WS_HANDLER"

                         Files and Logical Names Installed on Your System  B-13

 











                      "GKS3D$WORKSTATION_86" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_87" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_88" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_91" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_92" = "GKS3D$WSM_WS_HANDLER"
                      "GKS3D$WORKSTATION_93" = "GKS3D$WSM_WS_HANDLER"







































               B-14  Files and Logical Names Installed on Your System
