 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  DECintact, Version 2.0      SSA 29.58.04-A

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:       VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000 Model 210,
                      VAX 9000 Model 400 Series

                      VAXft 3000 Model 310

                      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,



                                    DIGITAL                July 1991

                                                         AE-LT11E-TE

 



           DECintact, Version 2.0                    SSA 29.58.04-A



                      MicroVAX 3900

           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 4000 Model 200,
                      VAXserver 4000 Model 300

                      VAXserver 6000 Model 210,
                      VAXserver 6000 Model 220,
                      VAXserver 6000 Model 310,
                      VAXserver 6000 Model 320,
                      VAXserver 6000 Model 410,
                      VAXserver 6000 Model 420,
                      VAXserver 6000 Model 510,
                      VAXserver 6000 Model 520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXsta-
           tion 8000

           Processor Restrictions:

           A TK50 Tape Drive is required for standalone MicroVAX 2000
           and VAXstation 2000 systems.







                                       2

 



           DECintact, Version 2.0                    SSA 29.58.04-A


           Disk Space Requirements (Block Cluster Size = 1):

           Disk space required for     52,000 blocks
           installation:
                                       (26,624 Kbytes)

           Disk space required for     46,000 blocks
           use (permanent):
                                       (23,552 Kbytes)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.

           OPTIONAL HARDWARE

           o  VT100, VT200, VT300, VT400 (in VT200 emulation mode) ter-
              minals.

           o  Any device supported by the prerequisite software.

           o  Any DECNET hardware as required by the distributed DECin-
              tact environment, including VAX front-end processors in
              conjunction with the DECintact product's operation in a
              host VAX orVAXcluster system.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.






                                       3

 



           DECintact, Version 2.0                    SSA 29.58.04-A


           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (SPD 29.78.xx)
              and include CI, Ethernet, and Mixed Interconnect config-
              urations.


           SOFTWARE REQUIREMENTS

           For Systems Using Terminals (No DECwindows Interface):

           VMS Operating System V5.4

           For Workstations Running VWS:

           VMS Operating System V5.4 

           VMS Workstation Software V4.3

           In addition to these requirements, DECnet-VAX V5.4 is re-
           quired for Remote-Access Option.

           VMS Tailoring

           For VMS V5.x the following VMS classes are required for full
           functionality of this layered product:

           o  VMS Required Saveset

           o  Network Support

           o  Programming Support

           o  System Programming Support

           o  Secure User's Environment

           o  Utilities

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).


                                       4

 



           DECintact, Version 2.0                    SSA 29.58.04-A


           OPTIONAL SOFTWARE

           o  DECforms V1.3

           o  DECnet-VAX V5.4

           o  DEctrace for VMS V1.1

           o  VAX BASIC V3.4

           o  VAX C V3.2

           o  VAX COBOL V4.4

           o  VAX CDD/Plus V4.3

           o  VAX DBMS V4.2

           o  VAX DEC/MMS V2.3-V2.5

           o  VAX DEC/Test Manager V2.3-V3.0

           o  VAX FORTRAN V5.5

           o  VAX Language-Sensitive Editor V3.1

           o  VAX Pascal V4.1

           o  VAX PL/I V3.4

           o  VAX Rdb/VMS V4.0

           o  VMS Volume Shadowing V5.4

           Certain versions of these products depend upon a specific
           version of the operating system. Please see the System Sup-
           port Addendum of the product in question to determine which
           version is required.

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

                                       5

 



           DECintact, Version 2.0                    SSA 29.58.04-A


           DISTRIBUTION MEDIA

           9 track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           The software documentation for this product is also avail-
           able as part of the VMS Online Documentation Library on CDROM.

           ORDERING INFORMATION

           Development Option

           Software Licenses: QL-VF1A*-**
           Software Media: QA-VF1A*-**
           Software Documentation: QA-VF1AA-GZ
           Software Product Services: QT-VF1A*-**

           Run-Time Option

           Software Licenses: QL-VF2A*-**
           Software Media: QA-VF2A*-**
           Software Documentation: QA-VF2AA-GZ
           Software Product Services: QT-VF2A*-**
















                                       6

 



           DECintact, Version 2.0                    SSA 29.58.04-A


           Remote-Access Option

           Software Licenses: QL-VF3A*-**
           Software Media: QA-VF3A*-**
           Software Documentation: QA-VF3AA-GZ
           Software Product Services: QT-VF3A*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           [TM]The DIGITAL Logo, CI, DEC, DECdtm, DECforms, DEC-
               trace, DECnet, DECnet-VAX, DECintact, MicroVAX, VAX,
               VAX BASIC, VAX C, VAX CDD/Plus, VAX COBOL, VAX DBMS,
               VAX FORTRAN, VAX Pascal, VAX RMS, VAXcluster, VAXft,
               VAXserver, VAXstation, VMS, VT100, VT200, and VT300
               are trademarks of Digital Equipment Corporation.




















                                       7
