 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  DECram for VMS, Version 1.0            SSA
           34.26.00-A

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:       VAXft 3000-310

                      VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000-210, VAX 9000 Model 400 Series

                      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,
                      MicroVAX 3900


                                    DIGITAL                July 1991

                                                         AE-PFM2A-TE

 



           DECram for VMS, Version 1.0               SSA 34.26.00-A



           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 4000 Model 200,
                      VAXserver 4000 Model 300

                      VAXserver 6000-210, VAXserver 6000-220,
                      VAXserver 6000-310, VAXserver 6000-320,
                      VAXserver 6000-410, VAXserver 6000-420,
                      VAXserver 6000-510, VAXserver 6000-520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXsta-
           tion 8000

           Processor Restrictions

           A TK50 Tape Drive is required for standalone MicroVAX 2000
           and VAXstation 2000 systems.

           Disk Space Requirements (Block Cluster Size = 1):

           Disk space required for     1,600 blocks
           installation:
                                       (819.2 Kbytes)

           Disk space required for     655 blocks
           use (permanent):
                                       (335.4 Kbytes)



                                       2

 



           DECram for VMS, Version 1.0               SSA 34.26.00-A


           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.

           Memory Requirements

           The amount of required memory depends on the number and size
           of the DECram device(s) created.

           CLUSTER ENVIRONMENT

           This layered product is supported in a VAXcluster environ-
           ment, however, it cannot be served in a VAXcluster.

           SOFTWARE REQUIREMENTS

           VMS Operating System V5.2 - V5.4

           VMS Tailoring

           For VMS V5.x systems, the following VMS class is required
           for full functionality of this layered product:

           o  VMS Required Saveset

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.






                                       3

 



           DECram for VMS, Version 1.0               SSA 34.26.00-A


           DISTRIBUTION MEDIA

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           ORDERING INFORMATION

           Software Licenses: QL-GJ9A*-**
           Software Media: QA-GJ9A*-**
           Software Product Services: QT-GJ9A*-**

           DECram for VMS documentation is available on the media kit
           only in text and PostScript® formats.

           o  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           ®   PostScript is a registered trademark of Adobe Sys-
               tems, Incoporated.

           [TM]The DIGITAL Logo, DEC, MicroVAX, TK, VAX, VAXcluster,
               VAXft, VAXserver, VAXstation, and VMS are trademarks
               of Digital Equipment Corporation.











                                       4
