 















             DECview3D____________________________________
             Installation Guide


                                                              AA-FC85D-TE




             May 1991

             This guide explains how to install and start the DECview3D
             software.




             Revision/Update Information:  This revised manual supersedes
                                           the DECview3D Installation
                                           Guide, Version 2.0 (Part Number
                                           AA-FC85C-TE).

             Operating System:             VMS Version 5.3 or higher

             Software Version:             Version 2.1


             digital equipment corporation
             maynard, massachusetts

 
             _____________________________________________
             First Printing, July 1985
             Revised, April, 1987
             Revised, April 1990
             Revised, May 1991

             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.

             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.

             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.

             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.

             © Digital Equipment Corporation 1991

             All Rights Reserved.
             Printed in U.S.A.

             The postpaid Reader's Comments form on the last page of this
             document requests the user's critical evaluation to assist in
             preparing future documentation.

             The following are trademarks of Digital Equipment Corporation:
             BASEVIEW, DEC, DECpresent, DECview3D, DECwindows, DECwrite,
             ReGIS, VAX, VAXcluster, VAX DOCUMENT, VAXstation, VMS, VT,
             and the DIGITAL logo.

             The following are third-party trademarks: Calcomp is a
             trademark of California Computer Products Corporation; HP-GL
             is a trademark of Hewlett-Packard Company; Interleaf is a
             trademark of Interleaf, Inc.; PostScript is a trademark of
             Adobe Systems, Inc.; TEKTRONIX is a trademark of Tektronix,
             Inc.

             This document was prepared using VAX DOCUMENT, Version 1.2














          ________________________________________________________________


                                                                  Contents




          About This Guide.........................................      v


          1  Preparing to Install DECview3D

                   Required Operating System Components............    1-1
                   Prerequisite Hardware...........................    1-2
                   Prerequisite and Optional Software..............    1-2
                   License Registration............................    1-3
                   Installation Procedure Requirements.............    1-3
                     Privileges and Disk Space ....................    1-4
                     System Parameter Values ......................    1-4
                           Calculating the Values for GBLPAGES and
                           GBLSECTIONS.............................    1-5
                           Changing System Parameter Values........    1-5
                     Process Quotas for the Installing Account ....    1-7
                     VMSINSTAL Requirements .......................    1-8
                     Backing Up Your System Disk ..................    1-8
                     DECview3D Requirements .......................    1-8





                                                                       iii

 

          2  Installing DECview3D

                   Installation Procedure..........................    2-1
                   Error Recovery..................................    2-7


          3  After Installing DECview3D

                   Displaying the Release Notes....................    3-1
                   Running the Installation Verification
                   Procedure.......................................    3-1
                   Editing the System Files........................    3-2
                   VAXcluster Considerations.......................    3-2
                   User Account Requirements.......................    3-3
                     Privileges ...................................    3-3
                     User Account Quotas ..........................    3-3
                     Setting Up User Accounts .....................    3-3
                   Determining and Reporting Problems..............    3-4


          A  Sample Installation


          B  New Files and Logical Name Definitions


          Tables

             1-1  Prerequisite and Optional Software...............    1-2

             1-2  Disk Space Requirements..........................    1-4

             1-3  Minimum Required System Parameters...............    1-4

             1-4  Process Account Quotas that Exceed Required
                  Default Values...................................    1-7

             3-1  User Account Quotas for Using DECview3D..........    3-3

             B-1  DECVIEW3D021.A...................................    B-1

             B-2  DECVIEW3D021.B...................................    B-2

             B-3  DECVIEW3D021.C...................................    B-3

             B-4  DECVIEW3D021.D...................................    B-6

             B-5  DECVIEW3D021.E...................................    B-7

             B-6  DECVIEW3D021.F...................................    B-8

             B-7  DECVIEW3D021.G...................................    B-9


          iv
                                                                         

 














          ________________________________________________________________


                                                          About This Guide




             The DECview3D software is an application used to view and
             distribute graphics data from various types of systems.
             The DECview3D software reads several different graphics
             format files and translates them into an internal format. The
             graphics data can then be displayed, manipulated, searched
             for information, and annotated.

             The software can create output files in several different
             graphics formats which can be used for hard copy, electronic
             distribution, technical documentation, and storage. The
             DECview3D software can be integrated with other software
             applications such as document-processing applications, online
             information distribution systems, and computer-aided process
             planning (CAPP) applications.

             Although DECview3D is designed as an application for the
             DECwindows workstation and graphics terminal environments,
             it is also designed as one of the cooperating applications
             with the DECwrite document-processing application and
             the DECpresent presentation application. The DECview3D
             software can incorporate graphics data into the revisable
             technical documents created with the DECwrite software or


                                                                         v

 






             the presentation information created with the DECpresent
             software.

          Purpose of This Guide

             The DECview3D Installation Guide gives requirements
             and provides instructions for installing the DECview3D
             application.

          Who Should Use This Guide

             This guide is for system managers or users who install the
             DECview3D software.

             You should be familiar with system management procedures.

          Structure of This Guide

             This book contains the following sections:

              _ Chapter 1, Preparing to Install DECview3D, describes the

                prerequisites for using the DECview3D software.

              _ Chapter 2, Installing DECview3D, gives a step-by-step

                description of the process of installing the software.

              _ Chapter 3, After Installing DECview3D, gives instructions

                for including the DECview3D software in system management
                procedures and for preparing users' accounts.

              _ Appendix A, Sample Installation, is a log of an installa-

                tion.

              _ Appendix B, New Files and Logical Name Definitions, is a

                list of files that are created during an installation and
                a list of all logical names that are defined.

          vi

 






          Associated Documents

             For more information about the DECview3D software, see the
             following:

              _ DECview3D Reference Manual describes all DECview3D

                operations.

              _ DECview3D Integration Guide instructs you on how to use

                the DECview3D software with other applications.

              _ DECview3D User's Guide instructs you on how to use the

                software.

              _ DECview3D Quick Reference Guide shows how to perform basic

                DECview3D operations.

          Conventions

             This manual uses the following documentation conventions and
             symbols:















                                                                       vii

 





             _____________________________________________________________
             Convention_______Meaning_____________________________________

             mouse            This term refers to any pointing device,
                              such as a mouse, a puck, or a stylus.

             MB1, MB2, MB3    MB1 indicates the left mouse button, MB2
                              indicates the middle mouse button, and
                              MB3 indicates the right mouse button.
                              The buttons can be redefined by using the
                              Pointer function of the DECwindows Session
                              Manager's Customize menu.

             Ctrl/x           Ctrl/x indicates that you hold down the Ctrl
                              key while you press another key or mouse
                              button (indicated here by x).

             Enter            The word enter means to type information at
                              your keyboard, and then press Return.

                              Command examples are in monospaced type,
                              and show all user-entered commands in
             $ SHOW TIME      bold letters. Displays or output lines of
             06-NOV-90 07:53:22rompting characters that the system prints

                              are shown in regular type.

             filespec         Lowercase words in examples indicate that
                              you supply an input value for the word. For
                              example, filespec tells you to specify a
                              file name.

             Italics__________Titles_of_manuals_are_in_italics.___________








          viii

 

















                                                                              1
               ________________________________________________________________

                                                 Preparing to Install DECview3D




                  This chapter discusses the preparations and requirements for
                  installing the DECview3D software.

                  Your bill of materials (BOM) and indented bills report (BIL)
                  specify the number and contents of your media. Be sure to
                  verify the contents of your kit with this information. If
                  your kit is damaged or if you find that parts of it are
                  missing, contact your Digital representative.

                  The DECview3D software provides online release notes. Digital
                  strongly recommends that you read the release notes before
                  proceeding with the installation. For information about
                  how to access the online release notes, see the section in
                  Chapter 2 entitled "Installation Procedure."

               Required Operating System Components

                  The VMS operating system comes with a variety of support
                  options, or classes. Classes include such features as
                  networking and RMS journaling. The DECview3D software
                  requires only the VMS-required saveset. See the Software
                  Support Addendum (SSA), which comes with the Software Product
                  Description (SPD), for any additional requirements.











                                            Preparing to Install DECview3D  1-1

 











               Prerequisite Hardware

                  The Installation Verification Procedure (IVP) at the
                  conclusion of the installation requires either a terminal
                  with ReGIS graphics capability or a DECwindows display
                  device.

               Prerequisite and Optional Software

                  Table 1-1 provides information about the software you must
                  have installed on your system before installing the DECview3D
                  software. The table also includes information about optional
                  software that you can use together with the DECview3D
                  software. The System Software Addendum (SSA) contains a
                  complete list of prerequisite and optional software and their
                  required version numbers.

                  Table 1-1    Prerequisite and Optional Software

                  _____________________________________________________________
                  Prerequisite
                  Products______________Purpose________________________________

                  VMS Version 5.3 or    Operating system
                  higher

                  _____________________________________________________________
                  Optional_Products_____Purpose________________________________

                  DECwindows Version    Workstation window software for VMS
                  2.0                   Version 5.3

                  DECwindows Version    Workstation window software for VMS
                  2.1                   Version 5.4

                  DECwrite Version 1.0  Document processing software that
                  or 1.1                can be integrated with the DECview3D
                                        software

                  DECpresent Version    Document formatting software for
                  1.0                   preparing presentations that can be
                  ____________________  integrated with the DECview3D software






               1-2  Preparing to Install DECview3D

 





               License Registration

                  You must register the DECview3D license through the VMS
                  License Management Facility (LMF) in accordance with
                  the license agreement signed by your site. The license
                  registration information you need is contained in the Product
                  Authorization Key (PAK) that is shipped with the DECview3D
                  software. The PAK is a paper certificate that contains
                  information about the license to run a particular piece of
                  software.

                  During the installation, the system asks whether you have
                  registered the DECview3D license and loaded the appropriate
                  PAK. You must register and load your license for the
                  DECview3D software before you start the installation in order
                  to run the IVP at the end of the installation.

                  To register a license under VMS, first log in to the system
                  manager's account, SYSTEM. You then have a choice of two ways
                  to perform the registration:

                   _ Invoke the SYS$UPDATE:VMSLICENSE.COM procedure. When it

                     prompts you for information, respond with data from your
                     PAK.

                   _ At the DCL prompt, enter the LICENSE REGISTER command

                     with the appropriate qualifiers that correspond to PAK
                     information.

                  If you plan to use the DECview3D software on more than
                  one node in a VAXcluster, you will need to perform a
                  license load on the other nodes after you complete this
                  installation. See the section in Chapter 3 entitled
                  "VAXcluster Considerations."

                  For complete information about using LMF, see the manual on
                  the License Management Utility in the VMS documentation set.

               Installation Procedure Requirements

                  This section and those that follow discuss various
                  requirements for installing the DECview3D software.

                  The installation takes approximately 15 to 30 minutes,
                  depending on your type of media and your system
                  configuration.

                  Installing the DECview3D software and running the
                  Installation Verification Procedure (IVP) on a standalone
                  VAX 2000 system takes 22 minutes.




                                            Preparing to Install DECview3D  1-3

 









                  Privileges and Disk Space

                  To install the DECview3D software, you must be logged in
                  to an account that has SETPRV or at least the following
                  privileges:

                   _ CMKRNL

                   _ WORLD

                   _ SYSPRV

                  Note that the VMSINSTAL procedure turns off BYPASS privilege
                  at the start of the installation.

                  The requirements for free disk storage space are different
                  during installation and after installation. Table 1-2
                  summarizes the storage requirements.

                  Table 1-2    Disk Space Requirements

                  _____________________________________________________________
                            Blocks During
                  Kit_______Installation________Blocks_After_Installation______

                  DECview3D 17,500              17,000

                  Version
                  2.1__________________________________________________________

                  To determine the number of free disk blocks on the current
                  system disk, enter the following command at the DCL prompt:

                    $ SHOW DEVICE SYS$SYSDEVICE

                  System Parameter Values

                  Installation of the DECview3D software requires the following
                  minimum system parameter settings, as listed in Table 1-3.

                  Table 1-3    Minimum Required System Parameters

                  _____________________________________________________________
                  System_Parameter______Minimum_Value__________________________

                  GBLPAGES              6,200

                                                       (continued on next page)



               1-4  Preparing to Install DECview3D

 











                  Table 1-3 (Cont.)    Minimum Required System Parameters

                  _____________________________________________________________
                  System_Parameter______Minimum_Value__________________________

                  GBLSECTIONS___________70_____________________________________

                  The following sections show you how to:

                   _ Check system parameter values

                   _ Change parameter values with the VMS AUTOGEN command

                     procedure

                  Calculating the Values for GBLPAGES and GBLSECTIONS   The
                  values for GBLPAGES and GBLSECTIONS in Table 1-3 indicate
                  that you must have at least 6,800 unused global pages and 75
                  unused global sections available for the installation.

                  To ensure that you have an adequate number of free global
                  pages and free global sections in your system, use the
                  following procedure:

                   1 Use the DCL F$GETSYI lexical function to determine the
                     number of free global pages and free global sections:

                       $ WRITE SYS$OUTPUT F$GETSYI("FREE_GBLPAGES")
                       $ WRITE SYS$OUTPUT F$GETSYI("FREE_GBLSECTS")

                   2 If the number of free global pages or free global sections
                     is less than the number specified in Table 1-3, you must
                     increase the value using the AUTOGEN command procedure.

                  The next section describes the procedures for changing
                  these values. For more information, refer to the VMS system
                  management documentation.

                  Changing System Parameter Values   Use the AUTOGEN command
                  procedure to change system parameters. The AUTOGEN procedure
                  automatically adjusts values for parameters that are
                  associated with the values you reset manually. To change
                  system parameters, edit the following file:

                    SYS$SYSTEM:MODPARAMS.DAT



                                            Preparing to Install DECview3D  1-5

 











                  To modify incremental parameters such as GBLPAGES and
                  GBLSECTS, use ADD_. The following example increases the
                  global page setting by 2000:

                    ADD_GBLPAGES = 2000

                  Note that when you set the page file quota, do not use a
                  value that exceeds the amount of page file space available on
                  the system.

                  After you make all your changes, exit from the editor and
                  execute the AUTOGEN procedure to recalculate your system
                  parameters. Enter the following command at the DCL prompt:

                    $ @SYS$UPDATE:AUTOGEN GETDATA REBOOT

                  When you specify REBOOT, the AUTOGEN procedure performs an
                  automatic system shutdown and then reboots the system. Any
                  users logged on to the system are immediately disconnected
                  during the shutdown. The automatic reboot puts the new
                  parameter values into effect.

                  The AUTOGEN procedure automatically adjusts some of the
                  SYSGEN parameters based on the consumption of resources since
                  the last reboot. If you do not want to take advantage of this
                  automatic adjustment, include the NOFEEDBACK qualifier on the
                  AUTOGEN command line.

                  For more information about using the AUTOGEN procedure, see
                  the VMS System Management Subkit.


















               1-6  Preparing to Install DECview3D

 









                  Process Quotas for the Installing Account

                  The account you use to install the DECview3D software
                  must have sufficient quotas to enable you to perform the
                  installation. You can install the DECview3D software using
                  the required default quotas for running VMSINSTAL.COM, with
                  the exception of the quotas listed in Table 1-4.

                  Table 1-4    Process Account Quotas that Exceed Required
                               Default Values

                  _____________________________________________________________
                  Account_Quota____Value_______________________________________

                  FILLM            100
                  WSQUO            1024[1]
                  _____________________________________________________________
                  [1]The value for WSEXT must be equal to or greater than the
                  WSQUO value.
                  _____________________________________________________________

                  Account quotas are stored in the file SYSUAF.DAT. Use the VMS
                  Authorize Utility (AUTHORIZE) to verify and change account
                  quotas. First set your directory to SYS$SYSTEM and then run
                  AUTHORIZE:

                    $ SET DEFAULT SYS$SYSTEM
                    $ RUN AUTHORIZE
                    UAF>

                  At the UAF> prompt, enter the SHOW command with an account
                  name to check a particular account. For example:

                    UAF> SHOW SMITH

                  To change a quota, enter the MODIFY command. The following
                  example changes the FILLM quota for the SMITH account and
                  then exits from the utility:

                    UAF> MODIFY SMITH /FILLM=100
                    UAF> EXIT

                  After you exit from the utility, the system displays messages
                  indicating whether or not changes were made. Once the changes
                  have been made, you must log out and log in again for the new
                  quotas to take effect.

                  For more information about modifying account quotas, see
                  the description of the Authorize Utility in the VMS System
                  Management Subkit.



                                            Preparing to Install DECview3D  1-7

 









                  VMSINSTAL Requirements

                  When you invoke the VMSINSTAL utility, it checks the
                  following:

                   _ Whether you have set your default device and directory to

                     SYS$UPDATE

                   _ Whether you are logged in to a privileged account

                   _ Whether you have adequate quotas for installation

                   _ Whether any users are logged in to the system

                  If the VMSINSTAL utility detects any problems during the
                  installation, it notifies you and asks if you want to
                  continue the installation. In some instances, you can enter
                  YES to continue. To stop the installation process and correct
                  the situation, enter NO or press Return. Then correct the
                  problem and restart the installation.

                  Backing Up Your System Disk

                  At the beginning of the installation, the VMSINSTAL procedure
                  asks if you have backed up your system disk. Digital
                  recommends that you do a system disk backup before installing
                  any software.

                  Use the backup procedures that are established at your site.
                  For details about performing a system disk backup, see the
                  section on the Backup Utility in the VMS System Management
                  Subkit.

                  DECview3D Requirements

                  The VMSINSTAL procedure has been modified to confirm that
                  your system meets the following requirements:

                   _ VMS Version 5.3 or higher has been installed.

                   _ Adequate disk space is available.

                   _ Proper installation account parameters are set.

                   _ Proper system parameters are set.




               1-8  Preparing to Install DECview3D

 

















                                                                              2
               ________________________________________________________________

                                                           Installing DECview3D




                  This chapter explains how to install the DECview3D software.
                  The section entitled "Installation Procedure" contains a
                  step-by-step description of the installation procedure.

               Installation Procedure

                  The DECview3D installation procedure consists of a series of
                  questions and informational messages. See Appendix A for a
                  sample installation.

                  To abort the installation procedure at any time, press
                  Ctrl/Y. When you press Ctrl/Y, the installation procedure
                  deletes all files it has created up to that point and exits.
                  You can then start the installation again.

                   1 Invoke VMSINSTAL.

                       @SYS$UPDATE:VMSINSTAL saveset-name device-name OPTIONS N

                     To start the installation, invoke the VMSINSTAL command
                     procedure from a privileged account, such as the SYSTEM
                     account. The VMSINSTAL procedure is in the SYS$UPDATE
                     directory. The following list defines the elements of the
                     VMSINSTAL command procedure:

                     saveset-name
                     The installation name for the component. For the DECview3D
                     software, use the following installation name:

                       DECVIEW3D021




                                                      Installing DECview3D  2-1

 








                     device-name
                     The name of the device on which you plan to mount the
                     media. For example, MTA0: is the device name for a tape
                     drive. It is not necessary to use the console drive for
                     this installation. However, if you do use the console
                     drive, you should replace any media you removed once the
                     installation is complete.

                     OPTIONS N
                     An optional parameter that indicates you want to see the
                     question on release notes. If you do not include the
                     OPTIONS N parameter, the VMSINSTAL procedure does not
                     inquire about the release notes. You should review the
                     release notes before proceeding with the installation
                     in case they contain additional information about the
                     installation. If you are restarting the installation and
                     have already reviewed the release notes, you do not need
                     to specify OPTIONS N.

                     Note that there are several other options you can select
                     when you invoke the VMSINSTAL procedure.

                      _ AUTO_ANSWER option (A): Initially creates a file

                        that contains your answers to VMSINSTAL questions and
                        prompts. You can then use the option (and the answer
                        file) to save time during a reinstallation (typically
                        after upgrading your system).

                      _ GET SAVE SET option (G): Lets you store product save

                        sets temporarily on a magnetic tape or in a disk
                        directory.

                      _ FILE LOG option (L): Logs all activity to the terminal

                        during installation.

                      _ ALTERNATE ROOT option (R): Lets you install the

                        product to a system root other than that of the running
                        system.

                     For detailed information about these options, see the VMS
                     documentation on software installation in the VMS System
                     Management Subkit. If you specify more than one option,
                     separate the options with commas (OPTIONS A,N).

                     The following example installs DECview3D from tape drive
                     MTA0: and shows the system response. This example uses the
                     OPTIONS N release note parameter.



               2-2  Installing DECview3D

 








                       $ @SYS$UPDATE:VMSINSTAL DECVIEW3D021 MTA0: OPTIONS N

                           VMS Software Product Installation Procedure V5.4


                       It is 10-JAN-1991 at 17:00.
                       Enter a question mark (?) at any time for help.

                     If you do not supply either the product name or the
                     device name, the VMSINSTAL procedure prompts you for
                     this information later in the installation procedure. The
                     VMSINSTAL procedure does not prompt you for any options,
                     so be sure to include OPTIONS N on the VMSINSTAL command
                     line to access the release notes during the installation.

                   2 Confirm system backup.

                       * Are you satisfied with the backup of your system disk
                                                                        [YES]?

                     Always back up your system disk before performing an
                     installation. If you are satisfied with the backup of
                     your system disk, press Return. Otherwise, enter NO to
                     discontinue the installation. After you back up your
                     system disk, you can restart the installation.

                   3 Mount the media.

                       Please mount the volume of the set on MTA0:.
                       * Are you ready? [YES]

                     Mount the distribution volume on the device you specified
                     when you invoked the VMSINSTAL utility. The device name
                     appears in the line preceding the prompt. The VMSINSTAL
                     procedure then asks you if you are ready to continue
                     with the installation. Press Return to continue the
                     installation. If you entered the wrong device name and
                     need to restart the installation, enter NO in response to
                     the prompt.

                       %MOUNT-I-MOUNTED, DECview3D MOUNTED ON _$$MTA0: (NODE 1)
                       The following products will be processed:
                         DECview3D V2.1

                           Beginning installation of DECview3D
                       V2.1 at 17:02

                       %VMSINSTAL-I-RESTORE, Restoring product saveset A...



                                                      Installing DECview3D  2-3

 








                     If you respond YES to indicate that you are ready, the
                     VMSINSTAL procedure displays a message that the media
                     containing DECview3D has been mounted on the specified
                     device and that the installation has begun.

                   4 Select a release notes option.

                     If you specified OPTIONS N when you started the
                     installation, the VMSINSTAL procedure asks a question
                     on release notes.

                     For VMS Version 5.2 or higher, you see the following
                     display:

                       Release notes included with this kit are always copied
                                                                 to SYS$HELP.

                       Additional Release Notes Options:

                        1.  Display release notes
                        2.  Print release notes
                        3.  Both 1 and 2
                        4.  None of the above

                       * Select option [2]:

                     If you select option 1, the release notes are displayed
                     immediately on the console terminal. You can terminate the
                     display at any time by pressing Ctrl/C.

                     If you select option 2, the VMSINSTAL procedure prompts
                     you for the name of the print queue:

                       * Queue name [SYS$PRINT]:

                     You can press Return to send the file to the default
                     output print device, or you can enter another queue name.

                     If you select option 3, the VMSINSTAL procedure displays
                     the release notes immediately on the console terminal and
                     then prompts you for a queue name for the printed version.

                     Select option 4 if you reviewed the release notes and are
                     restarting the installation.

                       * Do you want to continue the installation [N]?:
                       %VMSINSTAL-I-RELMOVED, The product's release notes have
                                          been successfully moved to SYS$HELP.

                     To continue the installation, enter YES. Otherwise, press
                     Return. In either case, the release notes are copied to




               2-4  Installing DECview3D

 







                     the SYS$HELP directory. See Chapter 3, After Installing
                     DECview3D, for instructions on displaying the release
                     notes after installation.

                   5 Choose to copy example graphics files.

                       * Do you want the DECview3D example files [YES]?

                     The example files are graphics files that can be used to
                     learn and test the DECview3D software.

                   6 Purge files.

                       * Do you want to purge files replaced by this
                                                        installation [YES]?

                     If this is a reinstallation of the software, you have the
                     option to purge files from previous installations of the
                     DECview3D software.

                   7 Choose the Installation Verification Procedure (IVP)
                     option.

                       * Do you want to run the IVP after the
                                                            installation [YES]?

                     The IVP for the DECview3D software checks to be sure that
                     the installation is successful. It is recommended that you
                     run the IVP.

                     After DECview3D is installed, you can run the IVP
                     independently to verify that the software is available on
                     your system. You might need to run the IVP after a system
                     failure to make sure that users can access the DECview3D
                     software. See Chapter 3, After Installing DECview3D, for
                     instructions on running the IVP after installation.

                   8 Identify the type of device that will run the IVP.

                       Please enter the number corresponding to the device on
                       which to display the output of the IVP.

                       1. DECwindows Device
                       2. VT340
                       3. VT330
                       4. VT241
                       5. VT240
                       6. Do not run the IVP

                       Enter Number [1]:




                                                      Installing DECview3D  2-5









                     Select the appropriate option to identify the display
                     device.

                     If you are installing the software on a DECwindows device,
                     and you have used the SET HOST command to create a log
                     of the procedure, you must enable the logging process to
                     display the output of the IVP on the DECwindows device.
                     The installation procedure requests the name of the node
                     that will display the output of the IVP. The procedure
                     also inquires if the Session Manager Security on this node
                     has been set up to allow this access. If this has not been
                     done, the IVP cannot display on that node.

                   9 Respond to license registration queries.

                       Product:       DECVIEW3D
                       Producer:      DEC
                       Version:       2.1
                       Release Date:  01-JUL-1990

                       * Does this product have an authorization key
                                                   registered and loaded?

                     The installation procedure displays license information
                     about your product, and then asks if you have registered
                     and loaded your Product Authorization Key (PAK).

                     If you have not registered and loaded your PAK, you must
                     answer NO to this question. You must register and load
                     your PAK to successfully complete the installation. If
                     you have not done so, you should stop the installation,
                     register and load your PAK, and then restart the
                     installation.

                   10 Read informational messages.

                     At this point, the installation procedure displays a
                     number of informational messages that report on the
                     progress of the installation. There are no further
                     questions. If the installation procedure has been
                     successful up to this point, the VMSINSTAL procedure moves
                     the new or modified files to their target directories,
                     updates help files, and updates DCL tables, if necessary.
                     If you chose to have files purged, that work is done now.
                     The following message is displayed at the conclusion of
                     the installation.

                       %VMSINSTAL-I-MOVEFILES, files will now be moved to
                                                 their target directories...




               2-6  Installing DECview3D

 







                   11 Observe the Installation Verification Procedure (IVP).

                     If you chose to run the IVP, it begins now. When the IVP
                     runs successfully, you see the following display:

                     Select the Quit function and then the No button.

                   12 End the installation procedure.

                       Installation of DECview3D V2.1
                       completed at 17:21

                          VMSINSTAL procedure done at 17:21

                     The previous messages indicate that the entire
                     installation procedure is complete.

                     You can now log out of the privileged account:

                       $ LOGOUT
                       SYSTEM     logged out at 10-JAN-1991 17:22

                     Note that the VMSINSTAL procedure deletes or changes
                     entries in the process symbol tables during the
                     installation. Therefore, if you are going to continue
                     using the system manager's account and you want to restore
                     these symbols, you must log out and log in again.

               Error Recovery

                  If errors occur during the installation itself or when
                  the Installation Verification Procedure (IVP) is running,
                  the VMSINSTAL utility displays failure messages. If the
                  installation fails, you see the following message:

                    %VMSINSTAL-E-INSFAIL, The installation of DECview3DV2.1
                                                                has failed.

                  If the IVP fails, you see these messages:

                    The DECview3D V2.1 Installation Verification Procedure
                                                                    failed.

                    %VMSINSTAL-E-IVPFAIL, The IVP for DECview3D V2.1 has
                                                                    failed.

                  Errors can occur during the installation if any of the
                  following conditions exist:





                                                      Installing DECview3D  2-7

 










                   _ The VMS operating system version is incorrect.

                   _ Quotas necessary for successful installation are
                     insufficient.

                   _ System parameter values for successful installation are
                     insufficient.

                   _ The VMS help library is currently in use.

                   _ The product license has not been registered and loaded.

                  For descriptions of the error messages generated by these
                  conditions, see the VMS documentation on system messages,
                  recovery procedures, and VMS software installation. If
                  you are notified that any of these conditions exist, take
                  the appropriate action as described in the message. For
                  information about installation requirements, see Chapter 1.






























               2-8  Installing DECview3D

 















                                                                              3
               ________________________________________________________________

                                                     After Installing DECview3D




                  The following tasks take place after installing the DECview3D
                  software:

                   _ Viewing the release notes

                   _ Running the Installation Verification Procedure separately

                   _ Editing the system startup and shutdown files

                   _ Making the product usable on a VAXcluster

                   _ Setting user account quotas

                   _ Reporting problems

               Displaying the Release Notes

                  The release notes are in the following location:

                    SYS$HELP:DECVIEW3D021.RELEASE_NOTES

                  After the installation, you can enter the following command
                  to review the release notes through the Help facility:

                    $ HELP DECVIEW3D RELEASE_NOTES

               Running the Installation Verification Procedure

                  You usually run the Installation Verification Procedure (IVP)
                  during installation. If you want to run the IVP separately
                  to ensure the integrity of installed files should system
                  problems occur, execute the following command procedure:

                    $ @SYS$TEST:VIEW$IVP



                                                After Installing DECview3D  3-1

 









               Editing the System Files

                  You must edit the system startup file to provide for
                  automatic startup of DECview3D when your system is rebooted.

                  Add the command that starts the DECview3D software to the
                  system startup file, SYS$MANAGER:SYSTARTUP_V5.COM:

                    $ @SYS$STARTUP:CGI$STARTUP.COM
                    $ @SYS$STARTUP:CIMI$STARTUP.COM
                    $ @SYS$STARTUP:VIEW$STARTUP.COM

               VAXcluster Considerations

                  If you installed the DECview3D software in a VAXcluster
                  environment, you must perform the following operations on
                  each node of the cluster:

                   _ Replace the DCL tables.

                   _ Edit the startup files.

                   _ Load the license.

                  Replace DCL Tables

                  On each node in the cluster, replace the DCL tables using the
                  following command:

                    $ INSTALL REPLACE SYS$LIBRARY:DCLTABLES.EXE

                  Edit Startup Files

                  On each node, edit the startup file to include the following
                  commands.

                    $ @SYS$STARTUP:CGI$STARTUP.COM
                    $ @SYS$STARTUP:CIMI$STARTUP.COM
                    $ @SYS$STARTUP:VIEW$STARTUP.COM

                  Load License

                  On each node, load the license for the DECview3D software
                  using the following command:

                    $ LICENSE LOAD DECVIEW3D




               3-2  After Installing DECview3D

 






               User Account Requirements

                  To work with the DECview3D software, user accounts on your
                  system must have certain privileges and quotas. The next two
                  sections contain information about these requirements. The
                  third section discusses how to set up user accounts.

                  Privileges

                  Each account must have at least the TMPMBX and NETMBX
                  privileges. Use the VMS Authorize Utility to determine
                  whether users have the privileges they require.

                  User Account Quotas

                  You must make sure that user accounts have sufficient
                  quotas to be able to use DECview3D. Table 3-1 summarizes
                  the required minimum user account quotas.

                  Table 3-1    User Account Quotas for Using DECview3D

                  _____________________________________________________________
                  Account_Quota____Value_______________________________________

                  ASTLM            24
                  BIOLM            18
                  BYTLM            18,000
                  DIOLM            18
                  ENQLM            30
                  FILLM            100
                  PGFLQUO          40,000
                  WSQUO            1024[1]
                  _____________________________________________________________
                  [1]The values for WSEXT must be equal to or greater than the
                  WSQUO value.
                  _____________________________________________________________

                  See "Process Quotas for the Installing Account" in Chapter 1
                  for a description of how to verify and change account quotas.

                  Setting Up User Accounts

                  The default device for the DECview3D software is a DECwindows
                  workstation. If users will use the DECview3D software only
                  on a terminal device, you can add the following symbol
                  definition to their login command files where device is the
                  appropriate terminal device from among the following:

                     VT340
                     VT330
                     VT241
                     VT240

                    $ 3DVIEW:==3DVIEW/INTERFACE=device



                                                After Installing DECview3D  3-3

 









                  Users can then invoke the software without having to specify
                  a device.

               Determining and Reporting Problems

                  If you encounter a problem while using the DECview3D
                  software, report it to Digital. Depending on the nature of
                  the problem and the type of support you have, you can take
                  one of the following actions:

                   _ Call Digital if your software contract or warranty

                     agreement entitles you to telephone support.

                   _ Submit a Software Performance Report (SPR).

                   _ Fill out and submit a Reader's Comments form if the

                     problem has to do with the DECview3D documentation. There
                     is a Reader's Comments form at the back of each manual.
                     Use the form from the manual in which you found the error.
                     Include the section and page number.

                  Review the Software Product Description (SPD) and Warranty
                  Addendum for an explanation of warranty. If you encounter
                  a problem during the warranty period, report the problem as
                  indicated above or follow alternate instructions provided by
                  Digital for reporting SPD nonconformance problems.
















               3-4  After Installing DECview3D

 















                                                                              A
               ________________________________________________________________

                                                            Sample Installation




                  This appendix contains a sample installation of DECview3D
                  software. This sample was run on a system that had no
                  previous version of DECview3D installed.

                  The sample installation assumes that no users are logged on
                  to your system, and that OPTIONS N is specified to print the
                  release notes. The Installation Verification Procedure (IVP)
                  runs at the end of the installation.

               $ SET DEF SYS$UPDATE
               $ @VMSINSTAL.com DECVIEW3D021 DISK$1:[KITS] options N

                       VAX/VMS Software Product Installation Procedure V5.4

               It is 11-APR-1991 at 12:15.

               Enter a question mark (?) at any time for help.
               * Are you satisfied with the backup of your system disk
                                                          [YES]? yes

               The following products will be processed:
                 DECVIEW3D V2.1

                       Beginning installation of DECVIEW3D V2.1 at 12:16

               %VMSINSTAL-I-RESTORE, Restoring product save set A ...
               %VMSINSTAL-I-RELMOVED, Product's release notes have been
                  moved to SYS$HELP.
               * Do you want the DECview3D example files [YES]? yes
               * Do you want to purge files replaced by this installation
                                                                 [YES]? yes






                                                       Sample Installation  A-1

 
               * Do you want to run the IVP after installation [YES]? yes
                       Please enter the number coresponding to the device on
                       which to display the output of the IVP.

                       1. DECwindows Device
                       2. VT340
                       3. VT330
                       4. VT241
                       5. VT240
                       6. Do not run the IVP

                       Enter Number [1]: 1

                       Product:      DECVIEW3D-USER, DECVIEW3D or BASEVIEW
                       Producer:     DEC
                       Version:      2.1
                       Release Date: 01-JUL-1990

               * Does this product have an authorization key registered and
                                                                   loaded? yes

                       No more questions will be asked during this installation.
                       Installation will take approximately 15 to 30 minutes.

                       Installation of Saveset B is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set B ...

                       Installation of Saveset C is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set C ...

                       Upon completion of this installation, please add the
                       following line to the site specific startup file:

                               $ @SYS$STARTUP:CGI$STARTUP.COM

                       Installation of Saveset D is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set D ...

                       Installation of Saveset E is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set E ...

                       Installation of Saveset F is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set F ...

                       Upon completion of this installation, please add the
                       following line to the site specific startup file:

                               $ @SYS$STARTUP:CIMI$STARTUP.COM



               A-2  Sample Installation





                       Installation of Saveset G is in progress.

               %VMSINSTAL-I-RESTORE, Restoring product save set G ...

               *****************************************************************
               *   If the following message is displayed, it can be ignored:   *
               *    "The CLI table does not contain verb name DECVIEW3D"       *
               *****************************************************************

               %CDU-W-NOSUCHVERB, The CLI table does not contain verb name
                                                                  DECVIEW3D

               Upon completion of this installation, please add the following
               line to the site specific startup file:

                               $ @SYS$STARTUP:VIEW$STARTUP.COM

               %VMSINSTAL-I-MOVEFILES, Files will now be moved to their
                                                        target directories...

                       Beginning the DECVIEW3D Installation Verification

              ******************************************************************
              *                         NOTICE                                 *
              *  To run the IVP at a later time, type the following command:   *
              *     $ @SYS$COMMON:[SYSTEST]view$IVP.COM                        *

              ******************************************************************

          **********************************************************************

              Beginning the DECview3D V2.1 Installation Verification Procedure.

              ****************************************************************
              * +----------------------------------------------------------+ *
              * |                                                          | *
              * |    Please choose the Quit function from the File menu    | *
              * |             after DECview3D has been invoked.            | *
              * |                                                          | *
              * +----------------------------------------------------------+ *
              ****************************************************************

                 The Installation Verification Program for the DECview3D V2.1
                              has been completed successfully.

             *******************************************************************

                       Installation of DECVIEW3D V2.1 completed at 12:33

                       VMSINSTAL procedure done at 12:33


               $ logout
                 SYSTEM       logged out at 11-APR-1991 12:34:14.23


                                                        Sample Installation  A-3






                                                                              B
               ________________________________________________________________

                                         New Files and Logical Name Definitions




                  The DECview3D installation procedure installs a number of
                  files on your system and defines a logical name.

                  The following logical name is entered into the system logical
                  name table when the DECview3D software is installed:

               ________________________________________________________________
               Logical_Name________Definition__________________________________

               VIEW$EXAMPLES_______SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3D]______

                  This name is stored in the DECview3D software's startup file.
                  It is entered into the system logical name table whenever the
                  system reboots or whenever the software is invoked.

                  The following tables contain the names of all files created
                  on your system when the DECview3D software is installed. The
                  kit contains the following files.

                  Table B-1    DECVIEW3D021.A

                  _____________________________________________________________
                  Target
                  Directory___File_Name________________________________________

                  SYS$HELP____DECview3D021.RELEASE_NOTES_______________________








                                    New Files and Logical Name Definitions  B-1

 








               Table B-2    DECVIEW3D021.B

               ________________________________________________________________
               Target
               Directory_____File_Name___________________Description___________

               SYS$LIBRARY   VIEW$GKSRTLIB.EXE           Shareable image file

               SYS$LIBRARY   VIEW$GKS$INQ_LIB.EXE        Shareable image file

               SYS$LIBRARY   VIEW$GKSMSG.EXE             Shareable image file

               SYS$LIBRARY   VIEW$RTL.EXE                Shareable image file

               SYS$LIBRARY   VIEW$GKS$WS_MANAGER.EXE     Workstation manager
                                                         file

               SYS$LIBRARY   VIEW$GKS$WS_MANAGER_CGM.EXE Workstation manager
                                                         file

               SYS$LIBRARY   VIEW$GKS$MI_WS_HANDLER.EXE  Workstation handler
                                                         file

               SYS$LIBRARY   VIEW$GKS$MO_WS_HANDLER.EXE  Workstation handler
                                                         file

               SYS$LIBRARY   VIEW$CGMO_DEV_HANDLER.EXE   Output device handler

               SYS$LIBRARY   VIEW$COLSIX_DEV_HANDLER.EXE Output device handler

               SYS$LIBRARY   VIEW$HPGL_DEV_HANDLER.EXE   Output device handler

               SYS$LIBRARY   VIEW$PS_DEV_HANDLER.EXE     Output device handler

               SYS$LIBRARY   VIEW$SIXEL_DEV_HANDLER.EXE  Output device handler

               SYS$LIBRARY   VIEW$DDIF_DEV_HANDLER.EXE   Output device handler

               SYS$LIBRARY   VIEW$DDIF_COLOR_TABLE.DAT   Output device handler

               SYS$LIBRARY   VIEW$REGIS_DEV_HANDLER.EXE  Display device handler

               SYS$LIBRARY   VIEW$DECW_DEV_HANDLER.EXE   Display device handler

                                                       (continued on next page)





               B-2  New Files and Logical Name Definitions









               Table B-2 (Cont.)    DECVIEW3D021.B

               ________________________________________________________________
               Target
               Directory_____File_Name___________________Description___________

               DECW$SYSTEM   VIEW$GFX.UID                User interface
               _DEFAULTS                                 definition file

               DECW$SYSTEM   VIEW$GFX_EN.UID             User interface
               _DEFAULTS_________________________________definition_file_______

               Table B-3    DECVIEW3D021.C

               ________________________________________________________________
               Target
               Directory_____File_Name____________Description__________________

               SYS$SHARE     CGI$SHR.EXE          Common Graphics Interface
                                                  image file

               SYS$SHARE     CGI$DEFS.FOR         Definitions of constants

               SYS$SHARE     CGI$DEFS.H           Definitions of constants

               SYS$SHARE     CGI$DEFS.PEN         Definitions of constants

               SYS$SHARE     CGI$ENTS.FOR         Declaration of function calls

               SYS$SHARE     CGI$ENTS.H           Declaration of function calls

               SYS$SHARE     CGI$ENTS.PEN         Declaration of function calls

               SYS$SHARE     CGI$GKS.EXE          Graphical Kernel System image
                                                  file

               SYS$SHARE     CGI$HPGLDDO.EXE      HP Plotter snapshot format
                                                  file

               SYS$SHARE     CGI$NULLDDO.EXE      Snapshot format file

               SYS$SHARE     CGI$INTERLEAFDDO.EXE Interleaf format file

                                                       (continued on next page)






                                    New Files and Logical Name Definitions  B-3





               Table B-3 (Cont.)   DECVIEW3D021.C
 
               ---------------------------------------------------------------
               Target
               Directory_____File_Name____________Description__________________

               SYS$SHARE     CGI$REGISDDO.EXE     ReGIS snapshot format file

               SYS$SHARE     CGI$SIXELDDO.EXE     SIXEL snapshot format file

               SYS$SHARE     CGI$TEKDDO.EXE       Tektronix snapshot format
                                                  file

               SYS$SHARE     CGI$STROKE_FONT1.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT2.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT3.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT4.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT5.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT6.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT7.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT8.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT9.FNT Text markup font file

               SYS$SHARE     CGI$STROKE_FONT10.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT12.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT13.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT14.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT15.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT16.FNTText markup font file

                                                       (continued on next page)




               B-4  New Files and Logical Name Definitions

 



               Table B-3 (Cont.)    DECVIEW3D021.C

               ________________________________________________________________
               Target
               Directory_____File_Name____________Description__________________

               SYS$SHARE     CGI$STROKE_FONT17.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT18.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT19.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT20.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT21.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT22.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT24.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT25.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT26.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT27.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT28.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT29.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT30.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT31.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT32.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT33.FNTText markup font file

                                                       (continued on next page)









                                    New Files and Logical Name Definitions  B-5









               Table B-3 (Cont.)    DECVIEW3D021.C

               ________________________________________________________________
               Target
               Directory_____File_Name____________Description__________________

               SYS$SHARE     CGI$STROKE_FONT34.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT35.FNTText markup font file

               SYS$SHARE     CGI$STROKE_FONT36.FNTIGES text markup font file

               SYS$SHARE     CGI$STROKE_FONT37.FNTIGES text markup font file

               SYS$SHARE     CGI$STROKE_FONT38.FNTIGES text markup font file

               SYS$STARTUP   CGI$STARTUP.COM      Common Graphics Interface
               ___________________________________startup_file_________________

               Table B-4    DECVIEW3D021.D

               ________________________________________________________________
               Target
               Directory_____File_Name_________Description_____________________

               SYS$SHARE     RDSG$SHR.EXE      Run-time Data Structure Geometry
                                               image file

               SYS$SHARE     RDSG$MSG.FOR      Definitions of messages

               SYS$SHARE     RDSG$MSG.H        Definitions of messages

               SYS$SHARE     RDSG$MSG.PEN      Definitions of messages

               SYS$SHARE     RDSG$DEF.FOR      Definitions of constants

               SYS$SHARE     RDSG$DEF.H        Definitions of constants

               SYS$SHARE     RDSG$DEF.PEN      Definitions of constants

               SYS$SHARE     RDSG$ENT.FOR      Declaration of function calls

               SYS$SHARE     RDSG$ENT.H        Declaration of function calls

                                                       (continued on next page)



               B-6  New Files and Logical Name Definitions

 







               Table B-4 (Cont.)    DECVIEW3D021.D

               ________________________________________________________________
               Target
               Directory_____File_Name_________Description_____________________

               SYS$SHARE_____RDSG$ENT.PEN______Declaration_of_function_calls___

               Table B-5    DECVIEW3D021.E

               ________________________________________________________________
                                     Sample Graphics Files
               Target_Directory_____________________File_Name_____Description__

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DCAR.IGES      IGES

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DF18.IGES      IGES

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DTK50.TXT      ASCII

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DF15.CALCOMP960CalComp960

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DFAN.HPGL      HP-GL

               SYS$COMMON:[SYSHLP.EXAMPLES.DECVIEW3DTEST.LAYOUT___Layout_file__

               ________________________________________________________________
                                       Translator Files
               Target
               Directory_____File_Name_______________Description_______________

               SYS$SHARE     TRANS$ASCII_SHR.EXE     Shareable image file

               SYS$SHARE     TRANS$CALCOMP960_SHR.EXEShareable image file

               SYS$SHARE     TRANS$HPGL_SHR.EXE      Shareable image file

               SYS$SHARE     TRANS$IGES_SHR.EXE      Shareable image file

               SYS$SHARE_____TRANS$LINK_SHR.EXE______Shareable_image_file______








                                    New Files and Logical Name Definitions  B-7

 






               Table B-6    DECVIEW3D021.F

               ________________________________________________________________
               Target
               Directory_____File_Name_______________Description_______________

               SYS$SHARE     CIMI$CTSHR.EXE          Shareable image file

               SYS$SHARE     CIMI$GSRVSHR.EXE        Shareable image file

               SYS$SHARE     CIMI$SLIBSHRSHR.EXE     Shareable image file

               SYS$SHARE     CIMI$DEF.H              Definitions of constants

               SYS$STARTUP___CIMI$STARTUP.COM________Startup_procedure_________

































               B-8  New Files and Logical Name Definitions

 











               Table B-7    DECVIEW3D021.G

               ________________________________________________________________
               Target
               Directory_____File_Name___________________Description___________

               SYS$SHARE     VIEW$SHR.EXE                Shareable image file

               SYS$SHARE     VIEW$COMMAND_LINE_TEXT.EXE  Shareable image file

               DECW$SYSTEM   VIEW$TRANS_USER_DATA.UID    User interface
               _DEFAULTS                                 definition file

               DECW$SYSTEM   VIEW$WIDGETS.UID            User interface
               _DEFAULTS                                 definition file

               DECW$SYSTEM   VIEW$WIDGETS_VT.UID         User interface
               _DEFAULTS                                 definition file

               DECW$SYSTEM   VIEW$WIDGETS_VTNM.UID       User interface
               _DEFAULTS                                 definition file

               SYS$HELP      HELPLIB.HLB                 Online HELP library

               SYS$HELP      VIEW$HELP.HLB               Online HELP module

               SYS$LIBRARY   VIEW$SYMBOL.LIB             Symbols library

               SYS$LIBRARY   DCLTABLES.EXE               DCL table files

               SYS$SYSTEM    DECVIEW3D.EXE               Executable image file

               SYS$STARTUP   VIEW$STARTUP.COM            Defines the location
                                                         of the user interface
                                                         definition files

               SYS$LIBRARY   WRITE$AIL_SHR.EXE           Application
                                                         Integration Library
               __________________________________________file_for_AIL_V1.0_____

                  Save Set G also contains the following files for the IVP:







                                    New Files and Logical Name Definitions  B-9

 










               ________________________________________________________________
               Target_Directory________________File_Name_______________________

               SYS$COMMON:[SYSTEST.DECVIEW3D]  VIEW$IVP.COM

               SYS$COMMON:[SYSTEST.DECVIEW3D]__VIEW$TESTFILE.LAYOUT____________











































               B-10  New Files and Logical Name Definitions
