 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECview3D for VMS, Version 2.1     SSA 26.95.05-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840
               VAX 9000-210, VAX 9000 Model 400 Series

               VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900






                                  DIGITAL                    May 1991

                                                          AE-LT45D-TE

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,

                 VAXserver 4000-300,
                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Other Hardware Required

     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      17,500 blocks
     installation:
                                  (8.6M bytes)

     Disk space required for      17,000 blocks
     use (permanent):


                                     2

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A




                                  (8.3M bytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     Memory Requirements for DECwindows Support

     The minimum supported memory for this application running in
     a standalone DECwindows environment with both the client and
     server executing on that same system is 9 Mbytes.

     The performance and memory usage of DECwindows applications are
     particularly sensitive to system configuration. Less memory may
     be required on the client system (the system where the software
     is installed and executed) if the server (the component that
     displays the application) resides on another system. More memory
     may be required on a system with several applications running
     or where it may be desirable to improve the performance of an
     application.

     The minimum memory supported is 9 Mbytes. However, the use of
     this software in conjunction with increased memory capability
     improves performance. The memory size suggested for most typical
     hardware configurations is at least 12 Mbytes.












                                     3

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A



     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     VMS Operating System V5.4

     For Workstations Running VMS:

     VMS Operating System V5.4 (and the necessary components of VMS
     DECwindows)

     This product may run in either of the following ways:

     o  Stand-alone execution - running the X11 display server and
        the client application on the same machine.

     o  Remote execution - running the X11 display server and the
        client application on different machines.

     VMS DECwindows is part of the VMS Operating System but must
     be installed separately. Installation of VMS DECwindows gives
     users the option to install any or all of the following three
     components:

     o  VMS DECwindows Compute Server (Base kit; includes runtime
        support)

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

                                     4

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A



     For stand-alone execution, the following DECwindows components
     must be installed on the machine:

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

     For remote execution, the following DECwindows components must
     be installed on the machine:

     Server Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

     Client Machine

     o  VMS DECwindows Compute Server

     o  VMS DECwindows Device Support

     o  VMS DECwindows Programming Support

     VMS Tailoring

     For VMS V5.x, the following VMS classe is required for full
     functionality of this layered product:

     o  VMS Required Saveset

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

                                     5

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A



     DISTRIBUTION MEDIA

     9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     The software documentation for this product is also available as
     part of the VMS Online Documentation Library on CDROM.

     ORDERING INFORMATION

     Software Licenses: QL-796**-**
     Software Media: QA-796A*-**
     Software Documentation: QA-796AA-GZ
     Software Product Services: QT-796A*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   Tektronix is a registered trademark of Tektronix, Incorpo-
           rated.

     [R]   Interleaf is a registered trademark of Interleaf, Incorpo-
           rated.

     [R]   HP-GL is a trademark of Hewlett-Packard company.

     [R]   CalComp is a trademark of California Computer Products
           Corporation.

     [R]   PostScript is a registered trademark of Adobe Systems,
           Incorporated.




                                     6

 


     DECview3D for VMS, Version 2.1                    SSA 26.95.05-A




     [TM]  The DIGITAL Logo, VAX, VMS, MicroVAX, VAXstation,
           VAXserver, VAXcluster, ReGIS, DECview3D, DECpre-
           sent, DECwrite, LiveLink, DECwindows, PrintServer 20,
           PrintServer 40, LN03, LN013, LN03 PLUS, VT and TK50 are
           trademarks of Digital Equipment Corporation.

































                                     7
