

          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  VMS DECwindows/Deutsch V2.1        SSA 25.Z4.01-A

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840, VAX 8842,
                    VAX 8974, VAX 8978, VAX-11/730,
                    VAX-11/750, VAX-11/780, VAX-11/785.

          MICROVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900.

          VAXstationVAXstation II, VAXstation 2000,
                    VAXstation 3100 Series, VAXstation 3200,
                    VAXstation 3500, VAXstation 3520,
                    VAXstation 3540.

          VAXserver:VAXserver 3100, VAXserver 3300,
                    VAXserver 3400, VAXserver 3500,
                    VAXserver 3600, VAXserver 3602,



                                       DIGITAL                October 1990

                                                               AE-PBPMB-TE

 


          VMS DECwindows/Deutsch V2.1                       SSA 25.Z4.01-A




                    VAXserver 3800, VAXserver 3900,
                    VAXserver 6000-210, VAXserver 6000-310,
                    VAXserver 6000-410, VAXserver 6000-420.

          Processors Not Supported:

          VAX:      VAX-11/725, VAX-11/782.
          MicroVAX: MicroVAX I.
          VAXstationVAXstation I, VAXstation 8000.

          Processor Restriction:

          A TK50 Tape Drive is required for standalone MicroVAX 2000 and
          VAXstation 2000 systems.

          Block Space Requirements (Block Cluster Size = 1)

          Disk space required for installation:
          VMS DECwindows/Deutsch V2.1: 7.000 Blocks
          Lernprogramm: 2.400 Blocks
          FileView Lernprogramm: 14.500 Blocks

          Disk space required for use (permanent):
          VMS DECwindows/Deutsch V2.1: 7.000 Blocks
          Lernprogramm: 2.000 Blocks
          FileView Lernprogramm: 14.000 Blocks

          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration and software
          options.

          Memory Requirements For DECwindows Support

          The minimum supported memory for this application running in
          a standalone DECwindows environment with both the client and
          server executing on that same system is 6 mb. At least 8 mb is
          required for use in a VAXcluster.

          CLUSTER ENVIRONMENT

                                          2

 


          VMS DECwindows/Deutsch V2.1                       SSA 25.Z4.01-A



          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          * V5.x VAXcluster configurations are fully described in the
          VAXcluster Software Product Description (29.78.xx) and include
          CI, Ethernet and Mixed Interconnect configurations.






























                                          3

 


          VMS DECwindows/Deutsch V2.1                       SSA 25.Z4.01-A



          SOFTWARE REQUIREMENTS

          VMS Operating System V5.4 and (necessary components of VMS
          DECwindows)

          Note: All VMS DECwindows V2.1 Language Variants run on VMS V5.4
          releases only.

          Refer to the VMS Operating System Software Product Descrip-
          tion (SPD Number 25.01.XX) for availability and versions of
          required software and for information regarding components of
          VMS DECwindows.

          This product may run in either of the following ways:

          Stand-alone execution - Running the X11 display server and the
          client application on the same machine.

          Remote execution - Running the X11 display server and the client
          application on different machines.

          VMS TAILORING CLASSES

          All classes of VMS are required for full functionality of this
          layered product.

          For more information on VMS classes and tailoring refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          OPTIONAL SOFTWARE

          In addition to your own language variant of DECwindows V2.1, the
          following V2.1 language variants are or will be available:

          Dutch          VMS DECwindows/Nederlands
          French         VMS DECwindows/Français
          French         VMS DECwindows/Canadien-français
          Canadian

                                          4

 


          VMS DECwindows/Deutsch V2.1                       SSA 25.Z4.01-A




          German         VMS DECwindows/Deutsch
          Italian        VMS DECwindows/Italiano
          Norwegian      VMS DECwindows/Norsk
          Swedish        VMS DECwindows/Svenska
          Swiss-         VMS DECwindows/Français/CH
          French
          Swiss-         VMS DECwindows/Deutsch/CH
          German
          Swiss-         VMS DECwindows/Italiano/CH
          Italian

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          Tape - TK50 Streaming Tape, 9-track 1600 BPI Magtape 9 (PE)

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          ORDERING INFORMATION

          Software Media QA-YFSGA-**
          Software Documentation QA-YFSGA-**

          * Denotes variant fields. for additional information on avail-
          able licenses, services and media refer to the appropriate price
          book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [TM] X Window System, Version 11 and its derivations (X, X11, X
          Version 11, X Window System) are trademarks of the Massachusetts
          Institute of Technology.

                                          5
