 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  DECwrite/British for VMS, Version 1.1         
	  SSA 25.R7.01-A

          HARDWARE REQUIREMENTS

          Processors Supported:

          VAX:      VAXft 3000-310

                    VAX 4000 Model 300

                    VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series,
                    VAX 6000 Model 500 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8600,
                    VAX 8650, VAX 8700, VAX 8800, VAX 8810,
                    VAX 8820, VAX 8830, VAX 8840

                    VAX 9000-210, VAX 9000-410

                    VAX-11/730, VAX-11/750, VAX-11/780,
                    VAX-11/785

          MicroVAX: MicroVAX II, MicroVAX 2000,
                    MicroVAX 3100, MicroVAX 3300,
                    MicroVAX 3400, MicroVAX 3500,
                    MicroVAX 3600, MicroVAX 3800,
                    MicroVAX 3900



                                       DIGITAL               November 1990

                                                               AE-NW35B-TE

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A




          VAXstation: VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540

          VAXserver:  VAXserver 3100, VAXserver 3300,
                      VAXserver 3400, VAXserver 3500,
                      VAXserver 3600, VAXserver 3602,
                      VAXserver 3800, VAXserver 3900

                      VAXserver 4000 Model 300

                      VAXserver 6000-210, VAXserver 6000-220,
                      VAXserver 6000-310, VAXserver 6000-320,
                      VAXserver 6000-410, VAXserver 6000-420,
                      VAXserver 6000-510, VAXserver 6000-520

          Processors Not Supported

          VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
          8000

          Processor Restrictions

          DECwrite will run on any of the above processors, but requires
          either a workstation, a VT1200 V2.0, or an Intel [R] 80286 or
          80386 with PC DECwindows for display.

          Block Space Requirements (Block Cluster Size = 1):

          Disk space required for      30,100 blocks
          installation:
                                       (15.4 Mbytes)

          Disk space required for      28,000 blocks
          use (permanent):
                                       (14.3 Mbytes)


                                          2

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A



          These counts refer to the disk space required on the system
          disk. The sizes are approximate; actual sizes may vary depending
          on the user's system environment, configuration, and software
          options.

          Memory Requirements

          A minimum of 8 Mbytes of memory is required on a workstation
          to operate DECwrite and VMS whether DECwrite is running on the
          workstation or on another processor.

          A minimum of 3 Mbytes of memory is required on a VT1200 to
          display DECwrite.

          OPTIONAL HARDWARE

          DECwrite files can be printed using any Digital Post-
          Script [R] printer, ScriptPrinter, (LN03R), PrintServer 20,
          PrintServer 40 or PrintServer 40 Plus.

          The DECchart component of DECwrite produces both monochrome
          and color PostScript[R]. Monochrome PostScript can be printed
          using any Digital PostScript printer as listed above. If the
          DEC GKS product or runtime system, and the CDA Converter Library
          is installed, then the DDIF Graphics Hardcopy converter can be
          used to generate the color and monochrome sixel formats (printed
          on the Digital LJ250 Companion Color Printer) and the HPGL[TM]
          format (printed on the Digital LVP16). If the DECprint Utility
          for PostScript to Sixel Printing for VMS is installed, then
          DECchart PostScript output (either color or monochrome) can be
          printed on the LJ250 Companion Color Printer.

          DECwrite will accept images scanned with the MD-300 Scanner.


                                          3

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A



          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (29.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          VMS Operating System V5.3 - V5.4 (and necessary components of
          VMS DECwindows)

          Note: VMS V5.3 does not support Display PostScript[TM] exten-
          sions.

          This product may run in either of the following ways:

          o  Stand-alone execution - Running the X11 display server and
             the client application on the same machine.

          o  Remote execution - Running the X11 display server and the
             client application on different machines.

          VMS DECwindows is part of the VMS Operating System but must be
          installed separately. Installation of VMS DECwindows gives the
          user the option to install any or all of the following three
          components:

          o  VMS DECwindows Compute Server (Base kit; includes runtime
             support)

          o  VMS DECwindows Device Support

          o  VMS DECwindows Programming Support

          For stand-alone execution, the following DECwindows components
          must be installed on the machine:

                                          4

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A



          o  VMS DECwindows Compute Server (Base kit; includes runtime
             support)

          o  VMS DECwindows Device Support

          For remote execution, the following DECwindows components must
          be installed on the server machine and client machine:

          o  VMS DECwindows Compute Server (runtime support)

          o  VMS DECwindows Device Support

          VMS Tailoring

          For VMS 5.x systems, the following VMS classes are required for
          full functionality of this layered product:

          o  VMS Required Saveset

          Optional:

          o  Network Support - required for cluster or server systems

          o  Utilities - required for mail

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx).

          PC DECwindows Display Facility

          The PC DECwindows Display Facility is an MS-DOS[R] application
          that implements an X server that uses the industry-standard X
          Window System, Version 11 (X11) protocol. DECwrite executing
          on a remote VMS system with DECnet may be displayed on and
          receive input from the personal computer. The PC DECwindows
          Display Facility is supported only on Intel 80286 and 80386
          machines. Refer to the DECnet PCSA Client for DOS, Version 3.0
          Software Product Description (SPD 55.07.xx) for full hardware
          and software requirements.

                                          5

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A



          OPTIONAL SOFTWARE

             DECdecision V1.1
             DECview3D for VMS V2.0
             DECimage Scan Software for VMS V2.0
             CDA Converter Library for VMS V1.0
             DECnet PCSA Client for DOS V3.0
             International Lexicon/Français for VMS V1.0
             International Lexicon/Deutsch for VMS V1.0
             International Lexicon/British for VMS V1.0
             International Lexicon/Español for VMS V1.0
             International Lexicon/Nederlands for VMS V1.0
             International Lexicon/Svenska for VMS V1.0
             International Lexicon/American English for VMS   V1.0 (in-
             cluded with the U.S. Version)
             International Lexicon/American Business for VMS   V1.0
             International Lexicon/American Medical for VMS   V1.0

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the requirements for
          the current version.

          DISTRIBUTION MEDIA

          Tape : 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          This product is also available as part of the VMS Consolidated
          Software Distribution on CDROM.

          The software documentation for this product is also available as
          part of the VMS Online Documentation Library on CDROM.

          ORDERING INFORMATION

          Software Licenses: QL-VVFE9-PB
          Software Media: QA-VVFEA-H*
          Software Documentation: QA-VVFEA-GZ
          Software Product Services: QT-VVFE*-**

                                          6

 


          DECwrite/British for VMS, Version 1.1             SSA 25.R7.01-A



          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media, refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [R]  Intel is a registered trademark of Intel Corporation.

          [R]  Lotus 1-2-3 is a registered trademark of Lotus Development
               Corporation.

          [R]  PostScript is a registered trademark of Adobe Systems, Inc.

          [R]  Microsoft is a registered trademark of Microsoft Corpora-
               tion.

          [R]  MS-DOS is a registered trademark of Microsoft Corporation.

          [TM] Display PostScript is a trademark of Adobe Systems, Inc.

          [TM] WordPerfect is a trademark of WordPerfect Corporation.

          [TM] HPGL is a trademark of Hewlett-Packard Corporation.

          [TM] The DIGITAL Logo, CDA, DECimage, DECnet, DECwrite, DEC-
               chart, DECdecision, DECwindows, DDIF, DX, EVE, EDT,
               GOLD KEY, LiveLink, MicroVAX, VAX, VMS, VAXcluster, VMS,
               VAXstation, VAXserver, PrintServer 20, PrintServer 40,
               PrintServer 40 Plus, LN03 and WPS-PLUS are trademarks of
               Digital Equipment Corporation.







                                          7
