 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  VAX Distributed Queuing Service, Version 1.2
           SSA 28.80.02-A

           HARDWARE REQUIREMENTS

           Processors Supported

           VAX:       VAXft 3000-310

                      VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000-210, VAX 9000 Model 400 Series

                      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,



                                    DIGITAL                 May 1991

                                                         AE-MA43D-TE

 



           VAX Distributed Queuing Service, Version 1SSA 28.80.02-A



                      MicroVAX 3900

           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500

           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 4000 Model 200,
                      VAXserver 4000 Model 300

                      VAXserver 6000-210, VAXserver 6000-220,
                      VAXserver 6000-310, VAXserver 6000-320,
                      VAXserver 6000-410, VAXserver 6000-420,
                      VAXserver 6000-510, VAXserver 6000-520

           Processors Not Supported

           MicroVAX I, VAXstation I, VAX-11/725, VAX-11/782, VAXsta-
           tion 8000, VAXstation 3520, VAXstation 3540

           Processor Restrictions:

           A TK50 tape drive is required for standalone MicroVAX 2000
           and VAXstation 2000 systems.

           A network interface controller supported by DECnet-VAX is
           required.

           Disk Space Requirements (Block Cluster Size = 1):

           Disk space required for     1,400 blocks
           installation:




                                       2

 



           VAX Distributed Queuing Service, Version 1SSA 28.80.02-A



                                       (716.8 Kbytes)

           Disk space required for     700 blocks
           use (permanent):
                                       (358.4 Kbytes)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.

           In addition, disk space is required on a temporary basis to
           hold working directories and queued files.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any specific hardware required by this prod-
           uct.

           *  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (SPD 29.78.xx)
              and include CI, Ethernet, and Mixed Interconnect config-
              urations.

           SOFTWARE REQUIREMENTS

           VMS Operating System V5.3 - V5.4
           DECnet-VAX V5.0 - V5.4

           VMS Tailoring

           For VMS V5.x systems, the following VMS classes are required
           for full functionality of this layered product:



                                       3

 



           VAX Distributed Queuing Service, Version 1SSA 28.80.02-A


           o  VMS Required Saveset

           o  Network Support

           o  Secure User's Environment

           For more information on VMS classes and tailoring, refer to
           the VMS Operating System Software Product Description (SPD
           25.01.xx).

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

           ORDERING INFORMATION

           Software Licenses: QL-VENA*-**
           Software Media: QA-VENA*-**
           Software Documentation: QA-VENAA-GZ
           Software Product Services: QT-VENA*-**

           *  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Contact
           your local Digital office for the most up-to-date informa-
           tion.







                                       4

 



           VAX Distributed Queuing Service, Version 1SSA 28.80.02-A



           [TM]The DIGITAL Logo, CI, DEC, DECnet, MicroVAX, TK,
               VAXstation, VAXft, VAXserver, VAXcluster, VAX, and
               VMS are trademarks of Digital Equipment Corporation.





































                                       5
