 






          System
          Support
          Addendum

          ________________________________________________________________

          PRODUCT NAME:  DRB32 VMS DRIVERS, Version 3.0     SSA 27.69.02-A

          HARDWARE REQUIREMENTS

          Processors Supported

          VAX:      VAX 6000 Model 200 Series,
                    VAX 6000 Model 300 Series,
                    VAX 6000 Model 400 Series

                    VAX 8200, VAX 8250, VAX 8300, VAX 8350,
                    VAX 8500, VAX 8530, VAX 8550, VAX 8700
                    VAX 8800, VAX 8810, VAX 8820, VAX 8830,
                    VAX 8840, VAX 8842, VAX 8974, VAX 8878

                    VAX 9000 Model 200 Series

          Processors Not Supported

          VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/782, VAX-
          11/785, VAX 8600, VAX 8650, MicroVAX systems, VAXserver systems
          and VAXstation systems.

          A minimum system configuration includes:

          o  One VAXBI based VAX host system

          o  One DRB32-M (minimum requirement for UQDRIVER) or

          o  One DRB32-M and one DRB32-W (minimum requirement for UQW-
             DRIVER) or


                                       DIGITAL              September 1990

                                                               AE-LX37B-TE

 


          DRB32 VMS DRIVERS, Version 3.0                    SSA 27.69.02-A



          o  One DRB32-M and one DRB32-E ( minimum requirement for UQ-
             DRIVER with long length cables)

          Block Space Requirements (Block Cluster Sizes = 1):

          The installation procedure allows the user to install the
          drivers on a system, or to simply copy the sources off the kit,
          or both. The disk space requirements depend on the option the
          user selects:

                                               DRB32-M/-E

                              Peak        Final


          Install and copy    5600        2800
          sources:

          Copy sources        2500        2000
          only:

          Install only:       5600        1200



                                                 DRB32-W

                              Peak        Final



          Install and copy    5600        2000
          sources:

          Copy sources        1600        1300
          only:



                                          2

 


          DRB32 VMS DRIVERS, Version 3.0                    SSA 27.69.02-A




          Install only:       5600        1100

          These block counts refer to the disk space required on the
          system disk. The sizes are approximate; actual sizes may vary
          depending on the user's system environment, configuration,
          software options selected, and any modifications by the user.

          OPTIONAL HARDWARE

          The number of additional DRB32s will depend on system config-
          uration and user's application. DRB32s can be configured on
          multiple VAXBIs. Refer to the VAX Systems and Options Guide for
          specifics.

























                                          3

 


          DRB32 VMS DRIVERS, Version 3.0                    SSA 27.69.02-A



          CLUSTER ENVIRONMENT

          This layered product is fully supported when installed on any
          valid and licensed VAXcluster* configuration without restric-
          tions. The HARDWARE REQUIREMENTS sections of this product's
          Software Product Description and System Support Addendum detail
          any special hardware required by this product.

          *  V5.x VAXcluster configurations are fully described in the
             VAXcluster Software Product Description (29.78.xx) and in-
             clude CI, Ethernet and Mixed Interconnect configurations.

          SOFTWARE REQUIREMENTS

          VMS Operating System V5.0 or greater

          VMS Operating System V5.0 supports DRB32 VMS DRIVER V3.0. This
          can include, but is not limited to V5.0, V5.1, V5.2, V5.3 and
          V5.4.

          VMS Tailoring

          The following VMS classes are required for full functionality of
          this layered product:

          o  VMS Required Saveset

          o  Programming Support

          o  System Programming Support

          o  Utilities

          o  Miscellaneous Files

          For more information on VMS classes and tailoring, refer to
          the VMS Operating System Software Product Description (SPD
          25.01.xx). OPTIONAL SOFTWARE

          In order to modify the test programs provided with the DRB32 VMS
          DRIVERS layered product, VAX FORTRAN at a minimum of V4.4 and
          VAX C at a minimum of V3.0.

                                          4

 


          DRB32 VMS DRIVERS, Version 3.0                    SSA 27.69.02-A



          No optional software is necessary to modifiy the device drivers
          of the kit.

          GROWTH CONSIDERATIONS

          The minimum hardware/software requirements for any future ver-
          sion of this product may be different from the minimum require-
          ments for the current version.

          DISTRIBUTION MEDIA

          Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

          ORDERING INFORMATION

          Software Licenses: QL-VF5A*-**
          Software Media: QA-VF5A*-**
          Software Documentation: QA-VF5AA-GZ
          Software Product Services: QT-VF5A*-**

          *  Denotes variant fields. For additional information on avail-
             able licenses, services and media refer to the appropriate
             price book.

          The above information is valid at time of release. Please con-
          tact your local Digital office for the most up-to-date informa-
          tion.

          [TM]  The DIGITAL Logo, VAX, MicroVAX, VAXstation, VAXserver and
                VMS are trademarks of Digital Equipment Corporation.









                                          5
