 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECserver 200 for VMS, Version 3.1 SSA 27.53.05-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAXft 3000-310,
               VAX 4000 Model 300,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX 9000-210, VAX 9000 Model 400 Series

               VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900





                                  DIGITAL                  March 1991

                                                          AE-LT16D-TE

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A




     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540

     VAXserver:  VAXserver 3100, VAXserver 3300,
                 VAXserver 3400, VAXserver 3500,
                 VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900,

                 VAXserver 6000-210, VAXserver 6000-220,
                 VAXserver 6000-310, VAXserver 6000-320,
                 VAXserver 6000-410, VAXserver 6000-420,
                 VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
     8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     The DECserver 200 software runs on any of the following packaged
     hardware options:

     DSRVB-**

     ** Denotes product variant models. For additional information,
     refer to the appropriate price book.

     Use the following SHIELDED cables with each of the physical
     lines depending on the connection required beyond the cable
     concentrator:


                                     2

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A




     BC22D       Null modem cable for local terminal or printer
                 connections.

     BC22E       Full modem straight through cable for modem connec-
                 tions.

     BC22F       Full modem straight through cable for modem connec-
                 tions.

     BC22R       Recommended null modem cable for host systems and
                 other devices, including those that use CTS/RTS flow
                 control.

     BC17D       Null modem cable for host systems and other devices
                 that do not use CTS/RTS flow control.

     OPTIONAL HARDWARE

     Terminals Supported

     The DECserver 200 software supports the following Digital termi-
     nal devices that have keyboards:

     o  LA12, LA34, LA35, LA36, LA38

     o  All VTxxx terminals

     Supported terminal parameters are:

     o  Character size: 7 or 8 bits per character

     o  Parity: Even, Odd, or None

     The automatic line speed detection (Autobaud) feature is sup-
     ported for either seven-bit characters with even parity or
     eight-bit characters with no parity.


                                     3

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A



     The DECserver 200 software also supports Digital Asian terminal
     device variants when accessed from VMS/Hanzi systems. Please
     refer to the VMS/HANZI SPD for a complete listing of supported
     devices.

     The DECserver 200 software also supports Digital Asian termi-
     nal device variants when accessed from VMS/Japanese systems.
     Please refer to the VMS/Japanese SPD for a complete listing of
     supported devices.

     The DECserver 200 software also supports the following Digital
     Personal Computers (PCs) in both terminal emulation mode and
     file transfer mode:

     o  Professional 325, 350, 380

     o  Rainbow 100A, 100B, 100+, 190

     o  DECmate II

     o  DECmate III

     o  VAXmate

     o  DECstation

     Note: This product is NOT WARRANTED to support non-Digital ter-
     minal devices or personal computers. However, terminals support-
     ing VT100 or VT200-like characteristics and personal computers
     supporting IBM[R] PC, IBM PC/XT and IBM PC/AT characteristics
     may operate with this product.

     Printers Supported

     The DECserver 200 software supports the following Digital asyn-
     chronous printers when accessed from VMS systems:

     o  All LJ, LA, LQP, LXY, LN0, LG, and DTC printing devices.

     The DECserver 200 software also supports Digital Asian printer
     device variants when accessed from VMS/Hanzi systems. Please
     refer to the VMS/HANZI SPD for a complete listing of supported
     devices.

                                     4

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A



     The DECserver 200 software also supports Digital Asian printer
     device variants when accessed from VMS/Japanese systems. Please
     refer to the VMS/Japanese SPD for a complete listing of sup-
     ported devices.

     Modems Supported

     For DECserver 200/MC:

     o  DF03, DF112, DF124, DF224, DF242, DFM X.29 pad, and DECmodem
        V32 full-duplex asynchronous modems for either dial-in or
        dial-out use. Also supported are private or leased line modem
        applications, however, connections to data switches are NOT
        WARRANTED but may operate with this product.

     Disk Space Requirements (Block Cluster Size= 1):

     Disk space required for       900 blocks
     installation:

                                   (435.2K bytes)


     Disk space required for       764 blocks
     use (permanent):

                                   (391.7K bytes)

     These counts refer to the disk space required on the downline
     load host system disk. The sizes are approximate; actual sizes
     may vary depending on the user's system environment, configura-
     tion, and software options.

     CLUSTER ENVIRONMENT





                                     5

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A



     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet, and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V4.7 - V5.4
     DECnet-VAX V4.7 - V5.4

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).










                                     6

 


     DECserver 200 for VMS, Version 3.1                SSA 27.53.05-A



     OPTIONAL SOFTWARE

     Terminal Server Manager V1.3

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Disk: TK50 Streaming Tape, Tape: 9-track 1600 BPI Magtape (PE)

     ORDERING INFORMATION

     Software Licenses: QL-VCBA*-**
     Software Media: QA-VCBA*-H*
     Software Documentation: QA-VCBAA-GZ
     Software Product Services: QT-VCBA*-**
     LAT Networks Concept Guide: AA-LD84B-TK

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [R]   IBM is a registered trademark of International Business
           Machines Corporation.

     [TM]  The DIGITAL Logo, VAX, MicroVAX, VAXstation, VAXserver,
           VMS, LAT, ULTRIX, RSX-11M-PLUS, Rainbow, Professional,
           DECstation, VAXcluster, DECmate, DECnet and DECserver are
           trademarks of Digital Equipment Corporation.


                                     7
