PDP-11 DATATRIEVE/VAX  Version 3.3                        SSA 25.14.18-A

HARDWARE REQUIREMENTS

Processor Support

VAX:	      VAX 6210, VAX 6220, VAX 6230, VAX 6240, VAX 6310, VAX 6312, 
              VAX 6320, VAX 6330, VAX 6333, VAX 6340, VAX 6350, VAX 6360, 
              VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, 
              VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, 
              VAX 8820, VAX 8830, VAX 8840, VAX 8842 VAX 8974, VAX 8978

	      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

VAXserver:	 VAXserver 6210, VAXserver 6220, VAXserver 6310, VAXserver 
                 6320

Processors Not Supported

MicroVAX, VAXstation, VAXserver 3300, VAXserver 3400, VAXserver 3500, 
VAXserver 3600, VAXserver 3602

Block Space Requirements (Block Cluster Size = 1):

Disk space required for installation:

						3,300 blocks
						(1.69M bytes)

Disk space required for use (permanent):

						2,400 blocks
						(1.23M bytes)

These counts refer to the disk space required on the system disk. The sizes 
are approximate; actual sizes may vary depending on the user's system 
environment, configuration, and software options selected. Verify that 
within this disk space requirement that you have 275 contiguous blocks. 

OPTIONAL HARDWARE

None

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions. The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product.

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet and 
    Mixed Interconnect configurations.

SOFTWARE REQUIREMENTS

VMS Operating System V5.1

VAX-11 RSX V2.4

VMS Tailoring

This product runs under VAX-11 RSX. For VMS V5.x systems, the following VMS 
classes are required for full functionality of this layered product: 

oo   VMS Required Saveset

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

None

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from the minimum requirements for the current 
version.

DISTRIBUTION MEDIA

Disk:	 RX01 Floppy Diskette

Tape:	 9-track 1600 BPI Magtape (PE), TU58 DECtape II Cartridge

ORDERING INFORMATION

Software Licenses:  QL-105A*-**
Software Media:  QA-105A*-**
Software Documentation:  QA-105AA-GZ
Software Product Services:  QT-105A*-**

*   Denotes variant fields. For additional information on available 
    licenses, services and media, refer to the appropriate price book.

The above information is valid at time of release. Please contact your 
local DIGITAL office for the most up-to-date information.



