 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DECelms, Version 1.1               SSA 31.79.01-A
                    (DEC Extended LAN Management Software)

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAX 4000 Model 300, VAXft 3000-310,
               VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

               VAX 9000-210, VAX 9000-410

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900





                                  DIGITAL               December 1990

                                                          AE-PAKOB-TE

 


     DECelms, Version 1.1                              SSA 31.79.01-A
     (DEC Extended LAN Management Software)



     VAXstationVAXstation II, VAXstation 2000,
               VAXstation 3100 Series, VAXstation 3200,
               VAXstation 3500, VAXstation 3520,
               VAXstation 3540

     VAXserver:VAXserver 3100, VAXserver 3300,
               VAXserver 3400, VAXserver 3500,
               VAXserver 3600, VAXserver 3602,
               VAXserver 3800, VAXserver 3900

               VAXserver 6000-210, VAXserver 6000-220,
               VAXserver 6000-310, VAXserver 6000-320,
               VAXserver 6000-410, VAXserver 6000-420,
               VAXserver 6000-510, VAXserver 6000-520

     Processors Not Supported

     VAX-11/725, MicroVAX I, VAXstation I, VAXstation 8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Other Hardware Required

     RA60 system disk is required at minimum.

     Block Space Requirements (Block Cluster Size = 1):

     Disk space required for      2,700 blocks
     installation:
                                  (1.3M bytes)

     Disk space required for      2,500 blocks
     use (permanent):
                                  (1.2M bytes)

                                     2

 


     DECelms, Version 1.1                              SSA 31.79.01-A
     (DEC Extended LAN Management Software)


     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V5.2 - V5.4

     VMS Tailoring

     For VMS V5.x, the following VMS classes are required for full
     functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     LAN Traffic Monitor V1.2 (if LAN Bridge 100 or 150 is to be used
     as a monitor device)

     GROWTH CONSIDERATIONS

                                     3

 


     DECelms, Version 1.1                              SSA 31.79.01-A
     (DEC Extended LAN Management Software)


     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

     Software Licenses: QL-YFPA*-**
     Software Media: QA-YFPA*-**
     Software Documentation: QA-YFPAA-GZ
     Software Product Services: QT-YFPA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM]  Ethermodem is a trademark of Chipcom Corporation.

     [TM]  The DIGITAL Logo, VAX, VMS, MicroVAX, VAXstation and
           VAXserver are trademarks of Digital Equipment Corporation.









                                     4
