 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  DEC InfoServer Client for VMS, Version 1.0    SSA
     33.91.01-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:        VAX 4000 Model 300

                 VAX 6000 Model 200 Series,
                 VAX 6000 Model 300 Series,
                 VAX 6000 Model 400 Series

                 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500,
                 VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700,
                 VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840

                 VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900

     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540



                                  DIGITAL                January 1991

                                                          AE-PF8SB-TE

 


     DEC InfoServer Client for VMS, Version 1.0        SSA 33.91.01-A




     VAXserver:  VAXserver 3100, VAXserver 3300, VAXserver 3400,
                 VAXserver 3500, VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900

                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220, VAXserver
                 6000-310, VAXserver 6000-320, VAXserver 6000-410,
                 VAXserver 6000-420, VAXserver 6000-510, VAXserver
                 6000-520

     Processors Not Supported

     VAX:        VAXft 3000-310

                 VAX 6000 Model 500 Series

                 VAX 9000-210, VAX 9000-410

                 VAX-11/725, VAX-11/782

     MicroVAX:   MicroVAX I


     VAXstation: VAXstation I, VAXstation 8000

     Processor Restrictions

     A TK50 Tape Drive is required for standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Other Hardware Required

     An Ethernet adapter is required for all processors installing
     this product.



                                     2

 


     DEC InfoServer Client for VMS, Version 1.0        SSA 33.91.01-A



     Disk Space Requirements (Block Cluster Size = 1):

     Disk space required for      1,500 blocks
     installation:
                                  (768.0 Kbytes)

     Disk space required for      625 blocks
     use (permanent):
                                  (320.0 Kbytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     CLUSTER ENVIRONMENT

     This product is fully functional when installed on any valid
     and licensed VAXcluster* configuration without restrictions.
     The HARDWARE REQUIREMENTS sections of this product's Software
     Product Description and System Support Addendum detail any
     special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.04) and in-
        clude CI, Ethernet, and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     For Systems Using Terminals (No DECwindows Interface):

     VMS Operating System V5.0-V5.3

     For Workstations Running VWS:

     VMS Operating System V5.0-V5.3

     For Workstations Running DECwindows:

                                     3

 


     DEC InfoServer Client for VMS, Version 1.0        SSA 33.91.01-A



     VMS Operating System V5.1-V5.3 (and necessary components of VMS
     DECwindows)

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     The software documentation for this product is also available as
     part of the VMS Online Documentation Library on CDROM.






                                     4

 


     DEC InfoServer Client for VMS, Version 1.0        SSA 33.91.01-A



     ORDERING INFORMATION

     Software Media: QA-GGWA*-**
     Software Documentation: QA-GGWAA-GZ

     The InfoServer 100 includes 4 Access Licenses. Additional Access
     Licenses should be purchased for clients exceeding this number
     (4). The InfoServer Client Access License grants the right to
     access the InfoServer 100 by one client node.

     InfoServer Access Licenses: QL-YTC99-AA

     *  Denotes variant fields. For additional information on avail-
        able licenses, services, and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM] The DIGITAL Logo, CI, DEC, DECwindows, MicroVAX, VAX,
          VAXcluster, VAXft, VAXserver, VAXstation, and VMS are
          trademarks of Digital Equipment Corporation.
















                                     5
