 






           System
           Support
           Addendum

           _________________________________________________________
           _________________________________________________________

           PRODUCT NAME:  VAXft System Services, Version 1.2     SSA
           31.64.02-A

           HARDWARE REQUIREMENTS

           Processors Supported:

           VAX:       VAXft Model 110,
                      VAXft Model 310,
                      VAXft Model 410,
                      VAXft Model 610,
                      VAXft Model 612

           Processors Not Supported:

           VAX:       VAX 4000 Model 200,
                      VAX 4000 Model 300

                      VAX 6000 Model 200 Series,
                      VAX 6000 Model 300 Series,
                      VAX 6000 Model 400 Series,
                      VAX 6000 Model 500 Series

                      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX
                      8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650,
                      VAX 8700, VAX 8800, VAX 8810, VAX 8820, VAX
                      8830, VAX 8840

                      VAX 9000 Model 210,
                      VAX 9000 Model 400 Series



                                    DIGITAL                July 1991

                                                         AE-NL39C-TE

 



           VAXft System Services, Version 1.2        SSA 31.64.02-A



                      VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

           MicroVAX:  MicroVAX II, MicroVAX 2000,
                      MicroVAX 3100, MicroVAX 3300,
                      MicroVAX 3400, MicroVAX 3500,
                      MicroVAX 3600, MicroVAX 3800,
                      MicroVAX 3900

           VAXstation:VAXstation II, VAXstation 2000,
                      VAXstation 3100 Series, VAXstation 3200,
                      VAXstation 3500, VAXstation 3520,
                      VAXstation 3540


           VAXserver: VAXserver 3100, VAXserver 3300, VAXserver
                      3400, VAXserver 3500, VAXserver 3600,
                      VAXserver 3602, VAXserver 3800, VAXserver
                      3900

                      VAXserver 4000 Model 200,
                      VAXserver 4000 Model 300

                      VAXserver 6000 Model 210,
                      VAXserver 6000 Model 220,
                      VAXserver 6000 Model 310,
                      VAXserver 6000 Model 320,
                      VAXserver 6000 Model 410,
                      VAXserver 6000 Model 420,
                      VAXserver 6000 Model 510,
                      VAXserver 6000 Model 520

           Processor Restrictions

           A TF70 Tape Drive is recommended as a load device for soft-
           ware media on standalone VAXft Model 110, 310, and 410 sys-
           tems. Either a TF70 or TF85 Tape Drive or TF857 Tape Loader




                                       2

 



           VAXft System Services, Version 1.2        SSA 31.64.02-A


           are recommended as a load device for software media on stan-
           dalone VAXft Model 610 and 612 Systems. VAXft System Ser-
           vices software will be installed at the factory for the con-
           venience of the customer, but installation is not warranted
           by Digital. The purchase of a VAXft System Services Media
           kit is still recommended.

           Disk Space Requirements (Block Cluster Size = 1):

           Disk space required for     750 blocks
           installation:
                                       (0.3 Mbytes)

           Disk space required for     650 blocks
           use (permanent):
                                       (0.26 Mbytes)

           These counts refer to the disk space required on the sys-
           tem disk. The sizes are approximate; actual sizes may vary
           depending on the user's system environment, configuration,
           and software options.

           CLUSTER ENVIRONMENT

           This layered product is fully supported when installed on
           any valid and licensed VAXcluster* configuration without re-
           strictions. The HARDWARE REQUIREMENTS sections of this prod-
           uct's Software Product Description and System Support Ad-
           dendum detail any special hardware required by this prod-
           uct.

           o  V5.x VAXcluster configurations are fully described in the
              VAXcluster Software Product Description (SPD 29.78.xx)
              and include CI, DSSI, Ethernet, and Mixed Interconnect
              configurations.






                                       3

 



           VAXft System Services, Version 1.2        SSA 31.64.02-A


           SOFTWARE REQUIREMENTS

           For Systems Using Terminals (No DECwindows Interface):

           VMS Operating System V5.4

           GROWTH CONSIDERATIONS

           The minimum hardware/software requirements for any future
           version of this product may be different from the require-
           ments for the current version.

           DISTRIBUTION MEDIA

           TK50 Streaming Tape

           This product is also available as part of the VMS Consol-
           idated Software Distribution on CDROM.

           ORDERING INFORMATION

           Software Licenses: QL-YEAA*-**
           Software Media: QA-YEAA*-**
           Software Documentation: QA-YEAAA-GZ
           Software Product Services: QT-YEAA*-**

           o  Denotes variant fields. For additional information on avail-
              able licenses, services, and media, refer to the appro-
              priate price book.

           The above information is valid at time of release. Please
           contact your local Digital office for the most up-to-date
           information.

           [TM]The DIGITAL Logo, CI, DEC, DECwindows, MicroVAX, TK,
               VAX, VAXcluster, VAXft, VAXserver, VAXstation, and
               VMS are trademarks of Digital Equipment Corporation.




                                       4
