 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  VAX DECgraph, Version 1.6          SSA 26.07.11-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:      VAX 6000 Model 200 Series,
               VAX 6000 Model 300 Series,
               VAX 6000 Model 400 Series,
               VAX 6000 Model 500 Series,
               VAX 9000 Model 210

               VAX 8200, VAX 8250, VAX 8300, VAX 8350,
               VAX 8500, VAX 8530, VAX 8550, VAX 8600,
               VAX 8650, VAX 8700, VAX 8800, VAX 8810,
               VAX 8820, VAX 8830, VAX 8840, VAX 8842,
               VAX 8974, VAX 8978

               VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/785

     MicroVAX: MicroVAX II, MicroVAX 2000,
               MicroVAX 3100, MicroVAX 3300,
               MicroVAX 3400, MicroVAX 3500,
               MicroVAX 3600, MicroVAX 3800,
               MicroVAX 3900

     VAXstationVAXstation II, VAXstation 2000,
               VAXstation 3100, VAXstation 3200,
               VAXstation 3500, VAXstation 3520,



                                  DIGITAL              September 1990

                                                          AE-LT66D-TE

 


     VAX DECgraph, Version 1.6                         SSA 26.07.11-A




               VAXstation 3540

     VAXserver:VAXserver 3100, VAXserver 3300,
               VAXserver 3400, VAXserver 3500,
               VAXserver 3600, VAXserver 3602,
               VAXserver 3800, VAXserver 3900,

               VAXserver 6000-210, VAXserver 6000-310,
               VAXserver 6000-410, VAXserver 6000-420

     Processors Not Supported

     VAX-11/725, VAX-11/782, MicroVAX I, VAXstation I, VAXstation
     8000

     Other Hardware Required

     o  VT125 (at a minimum of Rev. 102), VT240, VT241, or VT300
        series terminal,

     o  DECmate II or III (DECmate/WPS, at a minimum of Version
        2.1)/DECmate III PLUS (DECmate/WPS, at a minimum of Ver-
        sion 2.2) with appropriate Graphics Option module; Graphics
        Terminal Emulator required if WPS not installed.

     o  Rainbow 100 computer with a terminal emulator and the ReGIS
        application diskette, or DECterm V2.0 terminal emulator or

     o  VAXmate with VT240 terminal emulator. If DMF32 is used, it
        must be at a minimum of Rev. F.

     Note: GIGI terminals and the Professional 350 terminal emulator
     are not supported.

     Block Space Requirements (Block Cluster Size = 1):



                                     2

 


     VAX DECgraph, Version 1.6                         SSA 26.07.11-A




     Disk space required for      3,500 blocks
     installation:
                                  (1.80M bytes)

     Disk space required for      1,600 blocks
     use (permanent):
                                  (0.82M bytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     OPTIONAL HARDWARE

     o  LCG01 color inkjet printer (formerly LCP01)

     o  VR241 RGB color monitor

     o  LN03 (at a minimum of Rev. 3.8), LN03 PLUS, and LPS40 laser
        printers. Complex graphics on the LN03 may require an addi-
        tional RAM cartridge

     o  LA12, LA50, or LA75 printers (for black and white single
        size)

     o  LA100, LA210, or LA34-VA printers (for black and white single
        or double size)










                                     3

 


     VAX DECgraph, Version 1.6                         SSA 26.07.11-A



     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet and Mixed Interconnect configurations.

     SOFTWARE REQUIREMENTS

     VMS Operating System V5.4

     VMS Tailoring

     The following VMS classes are required for full functionality of
     this layered product:

     o  VMS Required Saveset

     o  Programming Support

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     OPTIONAL SOFTWARE

     VMS Workstation Software V4.2
     VAX DATATRIEVE V4.2
     VAX DECalc V3.1

     VAX DECgraph can be used with VAX DECalc as described in SPD
     25.79.xx provided VAX DECgraph is installed on the system before
     the installation of VAX DECalc. GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the minimum require-
     ments for the current version.

                                     4

 


     VAX DECgraph, Version 1.6                         SSA 26.07.11-A



     DISTRIBUTION MEDIA

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

     ORDERING INFORMATION

     Software Licenses: QL-360A*-**
     Software Media: QA-360A*-**
     Software Documentation: QA-360AA-GZ
     Software Product Services: QT-360A*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM]  The DIGITAL Logo, DECgraph, VAX, MicroVAX, VAXstation,
           VAXserver and VMS are trademarks of Digital Equipment
           Corporation.














                                     5
