 
















          VAX DECgraph
          Installation Guide


          Order Number: AA-R430E-TE

          Software Version:             DECgraph Version 1.6

          Operating System:             VAX/VMS Version 5.0 or
                                        higher


          August 1990

          This manual describes the steps required for system
          managers to install the VAX DECgraph graphic plotting
          software.

 





          ________________________
          August 1990

          __________
          The information in this document is subject to change
          without notice and should not be construed as a
          commitment by Digital Equipment Corporation. Digital
          Equipment Corporation assumes no responsibility for
          any errors that may appear in this document.

          The software described in this document is furnished
          under a license and may be used or copied only in
          accordance with the terms of such license.

          No responsibility is assumed for the use or
          reliability of software on equipment that is not
          supplied by Digital Equipment Corporation or its
          affiliated companies.

          Restricted Rights: Use, duplication, or disclosure
          by the U.S. Government is subject to restrictions as
          set forth in subparagraph (c)(1)(ii)  of the Rights in
          Technical Data and Computer Software clause at DFARS
          252.227-7013.

          __________
          Copyright ©1990 by Digital Equipment Corporation

          All Rights Reserved.
          Printed in U.S.A.

          __________
          The postpaid READER'S COMMENTS form on the
          last page of this document requests the user's
          critical evaluation to assist in preparing future
          documentation.

          The following are trademarks of Digital Equipment
          Corporation:

          DEC             DECUS         RSX
          DEC/CMS         DECwriter     UNIBUS
          DEC/MMS         DIBOL         VAX
          DECalc          EduSystem     VAX Xway
          DECalc-Plus     FMS-11        VAXcluster
          DECgraph        IAS           VMS
          DECnet          MASSBUS       VT
          DECslide        PDP
          DECsystem-10    PDT
          DECsystem-20    RSTS          DIGITAL

          This document was prepared using VAX DOCUMENT, Version
          1.2

 






          _______________________________________________________

          Contents

                _________________________________________________
                PREFACE                                         v

          _______________________________________________________
          CHAPTER 1  PREINSTALLATION                          1-1

                _________________________________________________
                1.1   THE DISTRIBUTION KIT                    1-1

                _________________________________________________
                1.2   PREREQUISITE SOFTWARE                   1-1

                _________________________________________________
                1.3   INSTALLATION PROCEDURE REQUIREMENTS     1-2

                1.3.1     Checking the System
                          Parameters  ____________________    1-2

                1.3.2     Special Requirements  __________    1-4

          _______________________________________________________
          CHAPTER 2  INSTALLATION                             2-1

                _________________________________________________
                2.1   INSTALLING DECGRAPH                     2-1

                _________________________________________________
                2.2   INSTALLATION PROCEDURE                  2-2

                _________________________________________________
                2.3   INSTALLATION ERROR MESSAGES             2-9







                                                              iii

 


          Contents



          _______________________________________________________
          CHAPTER 3  POST-INSTALLATION PROCEDURES             3-1

                _________________________________________________
                3.1   MODIFYING THE SYSTEM STARTUP
                      COMMAND FILE                            3-1

                _________________________________________________
                3.2   MODIFYING GRAPHSIXEL.COM                3-2

                _________________________________________________
                3.3   INSTALLATION VERIFICATION PROCEDURE
                      (IVP)                                   3-3

                _________________________________________________
                3.4   DATATRIEVE VERIFICATION                 3-4


          _______________________________________________________
          APPENDIX A  SAMPLE INSTALLATION                     A-1


          _______________________________________________________
          TABLES

                1-1       Directories and Files for
                          DECgraph Installation  _________    1-5














          iv

 





          _______________________________________________________

          Preface


          This installation guide describes how to install
          VAX DECgraph on the VAX/VMS operating system. It is
          intended for system managers.

          Keep this document with your distribution kit. You
          will need to refer to it again if you receive any
          maintenance updates or need to reinstall DECgraph.

          The installation procedure is described step by step.
          The dialog is interactive. The installation procedure
          prompts you to answer questions.

          This installation guide does not contain release
          notes. Release notes are on-line. You can display and
          print the release notes from within the installation
          procedure.

          To read the release notes after installation, type or
          print the file SYS$HELP:GRAPH016.RELEASE_NOTES.

          __________________________________________________________________

          Conventions

          This manual uses the following conventions:

          _______________________________________________________
          Convention__Meaning____________________________________

          <RETURN>    Keys are shown with boxes around them.

          <CTRL/X>    Two keys separated by a forward slash
                      means you should hold down the first key
                      and press the second. In the example here,
          ____________you_should_hold_down_<CTRL>_and_press_<X>._


                                                                v

 






          _______________________________________________________

   1      Preinstallation




          This chapter describes how to prepare for installing
          VAX DECgraph V1.6 software on your VAX/VMS system.

          __________________________________________________________________

   1.1    The Distribution Kit

          You can receive DECgraph V1.6 on magnetic tape (16MT9)
          or tape cartridge (TK50) media.

          The installation procedure will prompt you to mount
          the volumes. To mount the distribution medium, see
          the Guide to VAX/VMS Software Installation for your
          system. The guide also details several options to the
          installation procedure. Be sure to read it.

          Each distribution kit includes all files needed to
          install and execute DECgraph V1.6. Release notes about
          installing and operating DECgraph are available on-
          line. You can display them and print them from within
          the installation procedure (See section 2.2, step 6).

          The DECgraph kit contains two savesets: GRAPH016.A and
          GRAPH016.B

          __________________________________________________________________

   1.2    Prerequisite Software

          To run DECgraph V1.6, you must have VMS V5.0 or later
          on your system.



                                                              1-1

 


          Preinstallation


          __________________________________________________________________

   1.3    Installation Procedure Requirements

          Before you can install DECgraph, you must have the
          following:

          o  A DECgraph distribution kit

          o  Access to a privileged system manager's account

          o  A minimum of 3500 free blocks on the system disk
             during installation (1600 blocks are allocated to
             DECgraph after installation.)

          o  A minimum of 100 unused global pages and a minimum
             of 5 global sections

          o  A DECgraph license installed and loaded

          ___________________________

   1.3.1  Checking the System Parameters

          Before you install DECgraph you must compare the
          required number of global pages and global sections
          with the values on your system. The installation
          procedure checks these system parameters. If a
          parameter does not meet the minimum value, the
          results are unpredictable. Refer to the Guide to
          Setting Up a VMS System in the VAX/VMS documentation
          for information about modifying GBLPAGES and/or
          GBLSECTIONS values.

          To determine the number of global pages and sections
          on your system, do the following:

          1  Invoke the INSTALL utility by entering:

                $ INSTALL

          2  Determine the number of available global pages by
             entering:

                INSTALL> LIST/GLOBAL/SUMMARY

          1-2

 


                                                  Preinstallation



             This command determines whether your system has
             enough available global pages to install DECgraph.
             It displays a summary of the number of global
             sections used, the number of global pages used,
             and the number of global pages unused.

             DECgraph requires 100 global pages. If there are
             fewer than 100 unused pages, you can delete an
             existing known image (with the INSTALL utility).
             You can also increase the GBLPAGES system parameter
             with the SYSTEM GENERATION utility by using
             AUTOGEN.COM. For more information about using
             AUTOGEN, refer to the Guide to Setting Up a VMS
             System in the VAX/VMS documentation.

             Note the number of global sections used because you
             will need the information when checking the global
             sections.

          3  Exit from the INSTALL utility by entering:

                INSTALL> EXIT

          4  Determine the number of available global sections
             by using the SYSGEN utility. Enter the following:

                $ RUN SYS$SYSTEM:SYSGEN
                SYSGEN> USE CURRENT
                SYSGEN> SHOW GBLSECTIONS

             These commands determine whether your system
             has enough available global sections to install
             DECgraph. The first number displayed is the maximum
             number of global sections. Compare this number to
             the number of global sections in use displayed by
             the INSTALL utility (in Step 2).

             DECgraph requires five global sections. Therefore,
             if the amount displayed plus five exceeds the
             system maximum, you must increase the number of
             available global sections before you can install
             DECgraph.

                                                              1-3

 


          Preinstallation



             To increase the amount, you must increase the
             GBLSECTIONS parameter with the SYSTEM GENERATION
             utility by using AUTOGEN.COM. For more information
             about AUTOGEN, refer to the Guide to Setting Up a
             VMS System in the VAX/VMS documentation.

             If the amount displayed plus five is less than the
             system maximum, you can install DECgraph.

          ___________________________

   1.3.2  Special Requirements

          DECgraph operation requires permanent disk space in
          the following directories:

          o  GRAPH$LIBRARY

          o  SYS$HELP

          o  SYS$STARTUP

          o  SYS$SHARE

          o  SYS$SYSTEM

          o  SYS$TEST

          o  SYS$SYSROOT:[SYSTEST.GRAPH016]

          Table 1-1 shows the files in the directories.










          1-4

 


                                                  Preinstallation



          Table 1-1  Directories and Files for DECgraph
          ___________Installation________________________________

          Directory________File__________________________________

          GRAPH$LIBRARY    GRAPHSIXEL.COM
                           PAL1.GRP
                           PAL2.GRP
                           PAL3.GRP
                           PAL4.GRP
                           PAL5.GRP
                           PAL6.GRP
                           PAL7.GRP
                           PAL8.GRP
                           PAL9.GRP
                           PAL10.GRP
                           PAL11.GRP
                           PAL12.GRP
                           SAMPLE.GRD
                           SAMPLE.GRG
                           SAMPLE.GRI
                           SAMPLE1.GRL
                           SAMPLE2.GRL

          SYS$HELP         GRAPH016.RELEASE_NOTES
                           GRAPHHELP.HLB

          SYS$STARTUP      GRAPH$START.COM

          SYS$SHARE        GRAPHSHR.EXE

          SYS$SYSTEM       DECGRAPH.EXE

          SYS$TEST         GRAPH$IVP.COM

          [SYSTEST.GRAPH016GRAPH$IVP.GRO_________________________

          Your system needs at least 3500 free blocks before you
          attempt this installation.


                                                              1-5

 


          Preinstallation



          Use the following command to determine if you have
          enough free disk blocks on your system disk (or target
          disk system) to install DECgraph:

             $ SHOW DEVICE SYS$SYSDEVICE




































          1-6

 






          _______________________________________________________

   2      Installation




          This chapter explains how to install DECgraph and
          describes error messages you might receive during the
          installation.

          __________________________________________________________________

   2.1    Installing DECgraph

          This section contains the steps you follow to install
          DECgraph. You will have to log on to the system
          manager's account and make a backup of the system
          disk, checking all parameters. You should install
          DECgraph in stand-alone mode. You will have to make
          sure all users have logged off the system and that
          all batch jobs are complete. Then you will shut down
          the DECnet network and invoke VMSINSTAL to install
          DECgraph.

          The installation procedure prompts you to enter
          information. Most queries require a simple YES or NO
          answer. Respond with Y or N, as appropriate, or press
          <Return> to choose the default.

          Enhancements to VMSINSTAL in future releases of VMS
          might result in additional prompts appearing during
          the course of the installation. Although such prompts
          might not be documented in this installation guide,
          the installation will proceed normally.

          The DECgraph installation procedure takes between
          2 and 30 minutes to complete depending on your
          particular VAX configuration.


                                                              2-1

 


          Installation


          __________________________________________________________________

   2.2    Installation Procedure

          1  Make a backup of the system disk and check the
             system parameters.

          2  Log on to the system manager's account. Set the
             default directory to SYS$UPDATE by entering:

                $ SET DEFAULT SYS$UPDATE

          3  Start the installation by entering:

                $ @VMSINSTAL GRAPH016 device OPTIONS N

             device is the name of the device on which you will
             mount the DECgraph distribution media. VMSINSTAL
             displays information similar to the following:

                       VAX/VMS Software Product Installation Procedure V5.0

                  It is 22-APR-1990 at 08:08.
                  Enter a question mark (?) at any time for help.

             VMSINSTAL displays a warning message if users are
             logged on to the system or DECnet is running. You
             can stop the installation procedure by pressing
             <Return> when prompted to continue the installation
             procedure. If you continue, VMSINSTAL then asks you
             if you are satisfied with the backup of your system
             disk:

                  Are you satisfied with the backup of your system disk [YES]?

             If you have not made a backup of your system disk,
             type N and press <Return>. You will exit from the
             installation procedure.

             If you have backed up your system disk, enter Y or
             just press <Return> to continue the installation
             procedure.

          2-2

 


                                                     Installation



          4  Mount the first installation kit volume when
             VMSINSTAL displays a message similar to the
             following:

                  Please mount the first volume of the set on [device].
                  Are you ready?

          5  After mounting the first volume, type Y and press
             <Return> to continue the installation procedure.
             VMSINSTAL displays the following messages:

                  %MOUNT-I-MOUNTED, GRAPH mounted on [device]:

                  The following products will be processed:

                          GRAPH V1.6

                               Beginning installation of GRAPH V1.6 at 08:10

                  %VMSINSTAL-I-RESTORE, Restoring product saveset A ...

                  Release Note Options:

                       1. Display release notes
                       2. Print release notes
                       3. Both 1 and 2
                       4. Copy release notes to SYS$HELP
                       5. Do not display, print or copy release notes

                  * Select option [2]:

          6  Select a release notes option. If you select Option
             1, VMSINSTAL displays the release notes immediately
             on your screen. If you select option 2 or 3,
             VMSINSTAL prompts you for a queue name:

                  * Queue name  [SYS$PRINT]:

             Enter a queue name or press <Return> to indicate
             the default output print device SYS$PRINT.

             If you select Option 4, VMSINSTAL copies the
             release notes to the SYS$HELP directory.

             If you select Option 5, VMSINSTAL does not display,
             print, or copy the release notes.

                                                              2-3

 


          Installation



             VMSINSTAL asks if you want to continue with the
             installation:

                  Do you want to continue the installation?

          7  Type N and press <Return> to stop the installation.
             Enter Y to continue.

             If you enter Y to continue the installation,
             VMSINSTAL displays the following message:

                  ********************************************************
                  *                                                      *
                  *                 VAX DECgraph V1.6                    *
                  *                                                      *
                  *               Installation Procedure                 *
                  *                                                      *
                  *    Copyright 1990, Digital Equipment Corporation     *
                  *                                                      *
                  ********************************************************

                          Product:       DECGRAPH
                          Producer:      DEC
                          Version:       1.6
                          Release Date:  24-SEP-1990

                  * Does this product have an authorization key registered and loaded?

             If your license is loaded, enter Y at the prompt.
             If you enter Y and you do not have a license
             loaded, your IVP will fail. The installation
             proceeds as normal, but you will not be able to
             use DECgraph until you load a valid license on the
             system. Refer to the VMS License Management Utility
             Manual for information on installing and loading
             licenses.

             If you enter N at the prompt, VMSINSTAL lets you
             exit the installation to load the license on to the
             system with the following prompt:

          2-4

 


                                                     Installation



                  You do not have the DECgraph license currently loaded on your system.
                  You may continue with this installation, or you may stop to load the
                  license at this time. If you do continue, you will not be able to use
                  the DECgraph product until the license is loaded.

                  *Do you wish to continue with the DECgraph installation? [N]?

             If you enter N, the installation stops. If you
             enter Y or you do have a license loaded, VMSINSTAL
             verifies that you have adequate disk space.

          8  Next you will be prompted for the directory
             into which to place the DECgraph library files.
             This directory is pointed to by the logical
             GRAPH$LIBRARY. If this logical is defined, it is
             translated, and this becomes the default directory.
             If that directory exists, then you will see the
             following prompt:

                  The directory SYS$COMMON:[DECGRAPH] currently exists on your system.
                  * Would you like to place the GRAPH V1.6 library files there [YES]?

             If the directory does not exist, or the
             logical GRAPH$LIBRARY is not defined then
             SYS$COMON:[DECGRAPH] becomes the default directory,
             and the following prompt is displayed:

                  * Where would you like to place the GRAPH V1.6 library files?
                  [SYS$COMMON:[DECGRAPH]]:

             If the directory that you specify does not exist,
             you will then receive the following message:

                  %GRAPH-I-NOEXIST, SYS$COMMON:[DECGRAPH] does not currently exist.
                  * Would you like to create SYS$COMMON:[DECGRAPH]:
                  %VMSINSTAL-I-SYSDIR, This product creates system directory [DECGRAPH].

                  If you intend to execute this layered product on other nodes in your
                  VAXcluster, and you have the appropriate software license, you must
                  prepare the system-specific roots on the other nodes by issuing the
                  following command on each node (using a suitably privileged account):

                           $ CREATE /DIRECTORY SYS$SPECIFIC:[DECGRAPH]

                                                              2-5

 


          Installation



             If the directory that you specified does exist, you
             receive this message:

                  %CREATE-I-EXISTS, SYS$COMMON:[DECGRAPH] already exists

                  If you intend to execute this layered product on other nodes in your
                  VAXcluster, and you have the appropriate software license, you must
                  prepare the system-specific roots on the other nodes by issuing the
                  following command on each node (using a suitably privileged account):

                          $ CREATE /DIRECTORY SYS$SPECIFIC:[DECGRAPH]

          9  Next you will be prompted for the DATATRIEVE data
             entry option. This provides the ability to access
             data from DATATRIEVE and display it in DECgraph.
             For more information on using DATATRIEVE with
             DECgraph, see the VAX DECgraph User's Manual. For
             more information on DATATRIEVE, see the DATATRIEVE
             Reference Manual. If you select the DATATRIEVE
             interface, the following will be displayed:

                  Enter ? to get help.
                  * Do you have DATATRIEVE V4.2 or later on the system,
                  and would you like to link DECgraph with it [NO]? yes

                  Searching for DATATRIEVE shareable images.
                  Please wait (less than 5 minutes) ....

                  The DATATRIEVE shareable image ([SYSLIB]DTRSHR.EXE)
                  is found on your system.

                  * Do you want to link DECgraph with it [YES]?

                  DECgraph will be linked with the DATATRIEVE shareable
                  image [SYSLIB]DTRSHR.EXE.

          10 VMSINSTAL asks if you want to purge the files the
             current installation replaces:

                  * Do you want to purge the files replaced by this installation [YES]?

             Press <Return> or enter Y to purge the old version
             of DECgraph from your system. Enter N to keep the
             old version of DECgraph.

          2-6

 


                                                     Installation



             VMSINSTAL then creates a test directory to put the
             test graph used for the Installation Verification
             Procedure (IVP):

                  %VMSINSTAL-I-SYSDIR, This product creates system directory
                  [SYSTEST.GRAPH016].

                  If you intend to execute this layered product on the other nodes
                  in your VAXcluster, and you have the appropriate software license,
                  you must prepare the system-specific roots on the other nodes by
                  issuing the following command on each node (using a suitable
                  privileged account):

                         $ CREATE /DIRECTORY SYS$SPECIFIC:[SYSTEST.GRAPH016]

          11 VMSINSTAL now gives you the choice of running the
             Installation Verification Procedure (IVP). The
             IVP tests to determine if the installation was
             successful. The IVP takes from 2 to 20 minutes to
             complete, depending on your configuration.

             However, you cannot run the IVP if your DECgraph
             license is not loaded. If it is not loaded,
             VMSINSTAL displays the following message:

                  You do not have a license installed on your system. Since the
                  Installation Verification Procedure requires the license to be loaded,
                  it will not be run. Once this installation has finished and the
                  license is loaded, it is highly recommended to run the IVP by hand. To
                  do this, type:

                   @SYS$TEST:GRAPH$IVP.COM

             If your license is loaded, VMSINSTAL displays the
             following prompt:

                  * Do you want to run the IVP after the installation [YES]?

          12 To run the Installation Verification Procedure,
             press <Return>. VMSINSTAL copies files from the
             distribution kit and performs the installation. It
             displays the following messages:

                                                              2-7

 


          Installation



                  All questions necessary for the installation of DECgraph have been
                  answered.

                  After all files have been copied from the distribution kit, the
                  DECgraph installation procedure will continue for about 10 minutes.

                  %VMSINSTAL-I-RESTORE, Restoring product save set B ...

                  DECgraph is installed with the DATATRIEVE data entry option.

                          ******* Modification to SYS$MANAGER:SYSTARTUP_V5.COM *******

                  To complete the DECgraph installation, you MUST add the following
                  line to your system startup file (SYS$MANAGER:SYSTARTUP_V5.COM):

                      @SYS$STARTUP:GRAPH$START.COM

                  %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
                  directories...

          13 If you elected to run the IVP, you will see the
             following messages:

                     ************************************************************
                     *                                                          *
                     *                     VAX DECgraph V1.6                    *
                     *                                                          *
                     *            Installation Verification Procedure           *
                     *                                                          *
                     *       Copyright 1990, Digital Equipment Corporation      *
                     *                                                          *
                     ************************************************************

                  Please wait for the Installation Verification Procedure to complete.
                  The IVP takes from 2 to 20 minutes to complete depending on your
                  configuration.

                  The VAX DECgraph Installation Verification completed successfully.

             If the installation did not pass the verification
             procedures, you will see a failure message.

          2-8

 


                                                     Installation



          14 When the installation procedure is complete,
             VMSINSTAL displays the following message:

                     Installation of GRAPH V1.6 completed at 08:20

                     VMSINSTAL procedure done at 08:20

             The DECgraph installation is complete.

          15 If you installed DECgraph from the console drive,
             you must dismount the DECgraph media and remount
             your console media.

          __________________________________________________________________

   2.3    Installation Error Messages

          This section describes error messages you might
          receive during installation.

             Operating System Failure

                If the power goes off during the installation
                procedure or the operating system fails for any
                other reason, you must restart the system and
                the installation procedure.

          The following errors can occur during the installation
          procedure:

             %GRAPH-E-BADPAGE, DECgraph V1.6 requires 100 free
             GBLPAGES to install

                Facility: VAX DECgraph
                Severity: Error
                Explanation: DECgraph requires 100 global pages.
                Make sure that at least 100 global pages are
                available on your system disk and repeat the VAX
                DECgraph V1.6 installation.

             %GRAPH-E-BADSECT, DECgraph V1.6 requires 5 free
             GBLSECTIONS to install

                Facility: VAX DECgraph

                                                              2-9

 


          Installation



                Severity: Error
                Explanation: DECgraph requires 5 global
                sections. Make sure that at least 5 global
                sections are available on your system disk and
                repeat the VAX DECgraph V1.6 installation.


             %GRAPH-E-BADVMS, GRAPH V1.6 requires VMS Version
             5.0 or later to install

                Facility: VAX DECgraph
                Severity: Error
                Explanation: Your VAX system must be running VMS
                V5.0 or later to install VAX DECgraph V1.6.
                VMSINSTAL detected that an earlier version
                of VMS is running on your system. Upgrade to
                VMS V5.0 and then repeat the VAX DECgraph V1.6
                installation.

             %GRAPH-E-NOSPACE, There is insufficient disk space
             to continue the installation. GRAPH V1.6 requires
             3500 free blocks to install.

                Facility: VAX DECgraph
                Severity: Error
                Explanation: The system disk on your system must
                have at least 3500 free blocks to install VAX
                DECgraph V1.6. VMSINSTAL found less than 3500
                blocks and terminated. Make sure that at least
                3500 blocks are available on your system disk
                and repeat the VAX DECgraph V1.6 installation.










          2-10

 






          _______________________________________________________

   3      Post-installation Procedures




          This chapter explains how to:

          o  Modify the system startup command file

          o  Modify GRAPHSIXEL.COM if your system has an LN03
             printer

          o  Run the Installation Verification Procedure (IVP)

          o  Verify the DATATRIEVE link

          __________________________________________________________________

   3.1    Modifying the System Startup Command File

          Refer to the VMS documentation on system management
          for further instructions on modifying your system
          startup command file (SYSTARTUP_V5.COM).

          You must add a line to the system startup command
          file (SYSTARTUP_V5.COM) that makes the DECgraph images
          known to the system and defines GRAPH$LIBRARY. To
          do this, you must execute the command procedure
          GRAPH$START.COM, which is in directory SYS$STARTUP.
          This file INSTALLs the two DECgraph images,
          DECGRAPH.EXE and GRAPHSHR.EXE, and defines
          GRAPH$LIBRARY to be the directory that you specified
          during installation.

          If this is the first time you are installing DECgraph
          on your system, then add the following line to your
          system startup command procedure, SYSTARTUP_V5.COM:

               $ @SYS$STARTUP:GRAPH$START.COM

                                                              3-1

 


          Post-installation Procedures



          If you are upgrading from a previous version of
          DECgraph, you must delete the following lines from
          your SYSTARTUP_V5.COM file:

               $ INSTALL="$INSTALL/COMMAND_MODE"
               $ INSTALL
               DELETE SYS$SYSTEM:DECGRAPH.EXE
               DELETE SYS$SHARE:GRAPHSHR.EXE
               ADD SYS$SYSTEM:DECGRAPH.EXE/OPEN/SHARED
               ADD SYS$SHARE:GRAPHSHR.EXE/OPEN/SHARED
               ^Z
               $DEFINE/SYSTEM GRAPH$LIBRARY ...

          Replace the lines above with the following command:

               $ @SYS$STARTUP:GRAPH$START.COM

          __________________________________________________________________

   3.2    Modifying GRAPHSIXEL.COM

          If your system has an LN03 printer, DECgraph provides
          a command procedure, GRAPHSIXEL.COM, to help you print
          sixel files. To use GRAPHSIXEL.COM, you must assign
          the symbol DEFQUEUE to the LN03 print queue on your
          system.

          Modify GRAPHSIXEL.COM as follows:

          1  Using an editor, open the file GRAPHSIXEL.COM, and
             locate the following line:

                  $ defqueue = ""

          2  Type your LN03 print queue symbol between the
             quotation marks. For example, if your LN03 print
             queue symbol is LN03_QUEUE, type the following:

                  $ defqueue = "LN03_QUEUE"


          3-2

 


                                     Post-installation Procedures


          __________________________________________________________________

   3.3    Installation Verification Procedure (IVP)

          When you have completed the installation procedure,
          you can verify that DECgraph has been installed
          correctly on your system. You will need about 30
          minutes to complete this procedure. The first part of
          the procedure should take 20 minutes, and the second
          part should take 10 minutes.

          Before you begin this procedure, you must have:

          o  VAX DECgraph V1.6 installed on your system, using
             the procedures outlined in this manual.

          o  A supported graphics terminal.

          o  Correct terminal characteristics to run DECgraph.

          o  A loaded DECgraph license.

          To run the Installation Verification Procedure (IVP),
          do the following:

          1  Verify that your terminal characteristics are
             correct.

          2  To execute the IVP, enter the following:

                  $ @SYS$TEST:GRAPH$IVP

             Below is a sample of the IVP dialog.

                     ************************************************************
                     *                                                          *
                     *                     VAX DECgraph V1.6                    *
                     *                                                          *
                     *            Installation Verification Procedure           *
                     *                                                          *
                     *       Copyright 1990, Digital Equipment Corporation      *
                     *                                                          *
                     ************************************************************

                                                              3-3

 


          Post-installation Procedures



                  Please wait for the Installation Verification Procedure to complete.
                  The IVP takes from 2 to 20 minutes to complete depending on your
                  configuration.

          3  If the IVP completes successfully, it displays the
             following message:

                  The VAX DECgraph V1.6 Installation Verification completed successfully.

             If the IVP fails, it displays the following
             message:

                  The VAX DECgraph V1.6 Installation Verification has failed.

          __________________________________________________________________

   3.4    DATATRIEVE Verification

          If you installed DECgraph with DATATRIEVE, you should
          verify that DATATRIEVE is accessible from DECgraph:

          1  Log on to a supported graphics terminal and
             invoke DECgraph by typing GRAPH and then pressing
             <RETURN>. The Main Menu screen with the VAX
             DECgraph logo appears. The highlight is on the HELP
             icon (question mark).

          2  Press the down arrow key and then the left arrow
             key to select the DATA icon. Next press <RETURN>.
             The Data Entry submenu appears below the Main Menu.

          3  Press the down arrow key to move the highlight to
             the DTR icon. Press the RETURN key. The Main Menu
             screen disappears and the DATATRIEVE prompt (DTR>)
             appears.

          4  Exit from DATATRIEVE by typing EXIT and then
             pressing the RETURN key. The Keyboard Data Entry
             Screen appears. This screen contains a number
             of fields, (for example, Main Title, Subtitle, X
             data type). Towards the left, a column of single
             character fields appears with the letters DTR at
             the top of the column. This verifies DATATRIEVE
             access.

          3-4

 


                                     Post-installation Procedures



          5  Press <CTRL/Z> to exit from the Keyboard Data Entry
             Screen and return to the Main Menu screen.

          6  Press the up arrow key. The highlight moves to the
             STOP icon (hand) in the upper left corner.

          7  Press <RETURN> to exit from DECgraph and return to
             DCL level.

































                                                              3-5

 






          _______________________________________________________

   A      Sample Installation





           VAX/VMS Software Product Installation Procedure V5.3

          It is 28-MAY-1990 at 11:39.

          Enter a question mark (?) at any time for help.

          * Are you satisfied with the backup of your system disk [YES]?

          The following products will be processed:
            GRAPH V1.6

           Beginning installation of GRAPH V1.6 at 11:40

          %VMSINSTAL-I-RESTORE, Restoring product save set A ...

              Release notes included with this kit are always copied to SYS$HELP.

              Additional Release Notes Options:

           1.  Display release notes
           2.  Print release notes
           3.  Both 1 and 2
           4.  None of the above

          * Select option [2]: 4
          * Do you want to continue the installation [NO]? YES

          %VMSINSTAL-I-RELMOVED , The product's release notes have been
          successfully moved to SYS$HELP.




                                                              A-1

 


          Sample Installation



          ***************************************************************
          *                                                             *
          *                   VAX DECgraph V1.6                         *
          *                                                             *
          *                 Installation Procedure                      *
          *                                                             *
          *       Copyright 1990, Digital Equipment Corporation         *
          *                                                             *
          ***************************************************************

                  Product:      DECGRAPH
                  Producer:     DEC
                  Version:      1.6
                  Release Date: 24-SEP-1990

          * Does this product have an authorization key registered and loaded? YES

          The directory SYS$SYSROOT:[DECGRAPH] currently exists on your system.
          * Would you like to place the GRAPH V1.6 library files there [YES]?
          %VMSINSTAL-I-SYSDIR, This product creates system specific directory
          [DECGRAPH].
          %CREATE-I-EXISTS, VMI$SPECIFIC:[DECGRAPH] already exists
          %GRAPH-I-LIBCRTD, The DECgraph library has been created.
          Enter ? to get help.
          * Do you have DATATRIEVE V4.2 or later on the system,
          and would you like to link DECgraph with it [NO]? YES

          Searching for DATATRIEVE shareable images.
          Please wait (less than 5 minutes) ....

          The DATATRIEVE shareable image ([SYSLIB]DTRSHR.EXE)
          is found on your system.
          * Do you want to link DECgraph with it [YES]?
          DECgraph will be linked with the DATATRIEVE shareable image
          [SYSLIB]DTRSHR.EXE.

          * Do you want to purge files replaced by this installation [YES]?

          %VMSINSTAL-I-SYSDIR, This product creates system directory
          [SYSTEST.GRAPH016].
          %CREATE-I-EXISTS, VMI$COMMON:[SYSTEST.GRAPH016] already exists
          %CREATE-I-EXISTS, VMI$SPECIFIC:[SYSTEST.GRAPH016] already exists

          A-2

 


                                              Sample Installation



              If you intend to execute this layered product on other nodes in your
              VAXcluster, and you have the appropriate software license, you must
              prepare the system-specific roots on the other nodes by issuing the
              following command on each node (using a suitably privileged account):

           $ CREATE /DIRECTORY SYS$SPECIFIC:[SYSTEST.GRAPH016]
          * Do you want to run the IVP after the installation [YES]?

          All questions necessary for the installation of DECgraph have been
          answered.

          The DECgraph files which are still on the distribution kit will now
          be copied to the system.

          After all files have been copied from the distribution kit, the DECgraph
          installation procedure will continue for about 10 minutes.

          %VMSINSTAL-I-RESTORE, Restoring product save set B ...
          DECgraph is installed with the DATATRIEVE data entry option.

          %DCL-I-SUPERSEDE, previous value of GRAPH$LIBRARY has been superseded

                  ******* Modification to SYS$MANAGER:SYSTARTUP_V5.COM *******

          To complete the DECgraph installation, you MUST add the following line
          to your system startup file (SYS$MANAGER:SYSTARTUP_V5.COM):

              @SYS$STARTUP:GRAPH$START.COM
          %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target
          directories...

             ************************************************************
             *                                                          *
             *                    VAX DECgraph V1.6                     *
             *                                                          *
             *          Installation Verification Procedure             *
             *                                                          *
             *       Copyright 1990, Digital Equipment Corporation      *
             *                                                          *
             ************************************************************

          Please wait for the Installation Verification Procedure to complete.
          The IVP takes from 2 to 20 minutes to complete depending on your
          configuration.

                                                              A-3

 


          Sample Installation



          The VAX DECgraph Installation Verification completed successfully.

           Installation of GRAPH V1.6 completed at 11:55

           VMSINSTAL procedure done at 11:55




































          A-4
