DEC IEZ11 Class Driver for VMS, Version 1.0			SSA 31.41.00-A

HARDWARE REQUIREMENTS

Processors Supported

VAXstation:	   VAXstation 3100 Series

MicroVAX:	   MicroVAX 3100

VAXserver:	   VAXserver 3100

Processors Not Supported

VAX:	      VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 
              6000 Model 400 Series

	      VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500, VAX 8530, 
              VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, VAX 8810, 
              VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 8978

	      VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/780, VAX-11/782, 
              VAX-11/785

MicroVAX:	   MicroVAX I, MicroVAX II, MicroVAX 2000, MicroVAX 3300, 
                   MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, MicroVAX 
                   3800, MicroVAX 3900

VAXstation:	   VAXstation I, VAXstation II, VAXstation 2000, VAXstation 
                   3200, VAXstation 3500, VAXstation 3520, VAXstation 3540, 
                   VAXstation 8000

VAXserver:	   VAXserver 3300, VAXserver 3400, VAXserver 3500, 
                   VAXserver 3600, VAXserver 3602, VAXserver 3800, 
                   VAXserver 3900, VAXserver 6000-210, VAXserver 6000-310, 
                   VAXserver 6000-410, VAXserver 6000-420

Other Hardware Required

SCSI488/D Bus Converter 

The number of supported SCSI488/D bus converters is normally limited by the 
SCSI bus hardware configuration.  This limitation is effected by the number 
of SCSI system devices including disk and tape units. For more information, 
contact your local Digital office.

Block Space Requirements (Block Cluster Size = 1)

Disk space required for installation:

						      1,200 blocks
						      (600K bytes)

Disk space required for use (permanent):

						      850 blocks
						      (425K bytes)

These counts refer to the disk space required on the system disk. The sizes 
are approximate; actual sizes may vary depending on the user's system 
environment, configuration, and software options.

CLUSTER ENVIRONMENT

This layered product is fully supported when installed on any valid and 
licensed VAXcluster * configuration without restrictions. The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and 
System Support Addendum detail any special hardware required by this 
product. 

*   V5.x VAXcluster configurations are fully described in the VAXcluster 
    Software Product Description (29.78.xx) and include CI, Ethernet and 
    Mixed Interconnect configurations. 

SOFTWARE REQUIREMENTS

VMS Operating System V5.3

VMS Tailoring

For VMS V5.x systems, the following VMS classes are required for full 
functionality of this layered product.

VMS Required Saveset

For more information on VMS classes and tailoring, refer to the VMS 
Operating System Software Product Description (SPD 25.01.xx). 

OPTIONAL SOFTWARE

The following optional software is required if applications are to be 
developed using the specified languages. 

VAX C V3.1
VAX FORTRAN V5.4
VAX PASCAL V4.0
VAX Ada V2.1
VAX BLISS-32 Implementation Language V4.6
VAX BASIC V3.4

GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different from the minimum requirements for the current 
version. 

DISTRIBUTION MEDIA

Tape:	 TK50 Streaming Tape
Disk:	 RX23 Diskette

This product is also available as part of the VMS Consolidated Software 
Distribution on CDROM. 

ORDERING INFORMATION

Software Licenses: QL-YEHA*-**
Software Media: QA-YEHAA-**
Software Documentation: QA-YEHAA-GZ
Software Product Services: QT-YEHA*-**

*   Denotes variant fields. For additional information on available 
    licenses, services and media, refer to the appropriate price book or 
    contact your local Digital office.

Note:	 The software can only be ordered in conjunction with the SCSI488/D 
         bus converter. Refer to the systems and options catalog for 
         IEZ11-** ordering information. 

The above information is valid at the time of release. Please contact your 
local Digital office for the most up-to-date information. 

(R)  The DIGITAL Logo is a registered trademark of Digital Equipment 
     Corporation.
(TM) DEC, DECstation, MicroVAX, VAX, VAXserver, VAXstation and VMS are 
     trademarks of Digital Equipment Corporation.

April 1990
AE-NU47A-TE

