 






     System
     Support
     Addendum

     ________________________________________________________________
     ________________________________________________________________

     PRODUCT NAME:  VAX ISDN ACCESS, Version 1.1       SSA 31.24.01-A

     HARDWARE REQUIREMENTS

     Processors Supported

     VAX:        VAX 4000 Model 300

                 VAX 6000 Model 200 Series,
                 VAX 6000 Model 300 Series,
                 VAX 6000 Model 400 Series,
                 VAX 6000 Model 500 Series

                 VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 8500,
                 VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700,
                 VAX 8800, VAX 8810, VAX 8820, VAX 8830, VAX 8840

     MicroVAX:   MicroVAX II, MicroVAX 2000,
                 MicroVAX 3100, MicroVAX 3300,
                 MicroVAX 3400, MicroVAX 3500,
                 MicroVAX 3600, MicroVAX 3800,
                 MicroVAX 3900

     VAXstation: VAXstation II, VAXstation 2000,
                 VAXstation 3100 Series, VAXstation 3200,
                 VAXstation 3500, VAXstation 3520,
                 VAXstation 3540





                                  DIGITAL               December 1990

                                                          AE-NS27B-TE

 


     VAX ISDN ACCESS, Version 1.1                      SSA 31.24.01-A




     VAXserver:  VAXserver 3100, VAXserver 3300, VAXserver 3400,
                 VAXserver 3500, VAXserver 3600, VAXserver 3602,
                 VAXserver 3800, VAXserver 3900

                 VAXserver 4000 Model 300

                 VAXserver 6000-210, VAXserver 6000-220, VAXserver
                 6000-310, VAXserver 6000-320, VAXserver 6000-410,
                 VAXserver 6000-420, VAXserver 6000-510, VAXserver
                 6000-520

     Processors Not Supported

     VAX:        VAXft 3000-310

                 VAX 9000-210, VAX 9000-410

                 VAX-11/725, VAX-11/730, VAX-11/750, VAX-11/780,
                 VAX-11/782, VAX-11/785

     MicroVAX:   MicroVAX I


     VAXstation: VAXstation I, VAXstation 8000

     Processor Restrictions:

     A TK50 Tape drive is required for Standalone MicroVAX 2000 and
     VAXstation 2000 systems.

     Disk Space Requirements (Disk Cluster Size = 1):

     Disk space required for      1,250 blocks
     installation:
                                  (.6 Mbytes)



                                     2

 


     VAX ISDN ACCESS, Version 1.1                      SSA 31.24.01-A




     Disk space required for      1,020 blocks
     use (permanent):
                                  (.5 Mbytes)

     These counts refer to the disk space required on the system
     disk. The sizes are approximate; actual sizes may vary depending
     on the user's system environment, configuration, and software
     options.

     For optional software (DECnet-VAX), the system must, in addi-
     tion, meet the corresponding requirements. Consult the DECnet-
     VAX Software Product Description (SPD 25.03.xx) for a complete
     description.

     Physical memory: at least 1.5 Mbytes

     Non-paged dynamic pool: none

     CLUSTER ENVIRONMENT

     This layered product is fully supported when installed on any
     valid and licensed VAXcluster* configuration without restric-
     tions. The HARDWARE REQUIREMENTS sections of this product's
     Software Product Description and System Support Addendum detail
     any special hardware required by this product.

     *  V5.x VAXcluster configurations are fully described in the
        VAXcluster Software Product Description (29.78.xx) and in-
        clude CI, Ethernet, and Mixed interconnect configurations.

     Though the product's images will exist in the common system di-
     rectory and will be executable by all VAX computers sharing this
     directory, it is essential that all VAX systems of a VAXcluster
     requiring access be licensed.




                                     3

 


     VAX ISDN ACCESS, Version 1.1                      SSA 31.24.01-A



     SOFTWARE REQUIREMENTS

     VMS Operating System V5.2-1-V5.4

     DECnet-VAX (either end-node or full-functional) both on the
     connector node(s) and on the node where installation occurs.

     VAX ISDN V1.1 on at least one of the connector node(s).

     VMS Tailoring

     For VMS V5.x systems, the following VMS classes are required for
     full functionality of this layered product:

     o  VMS Required Saveset

     o  Network Support

     o  Programming Support

     o  Utilities

     For more information on VMS classes and tailoring, refer to
     the VMS Operating System Software Product Description (SPD
     25.01.xx).

     GROWTH CONSIDERATIONS

     The minimum hardware/software requirements for any future ver-
     sion of this product may be different from the requirements for
     the current version.

     DISTRIBUTION MEDIA

     Disk: RX23

     Tape: 9-track 1600 BPI Magtape (PE), TK50 Streaming Tape

     This product is also available as part of the VMS Consolidated
     Software Distribution on CDROM.

                                     4

 


     VAX ISDN ACCESS, Version 1.1                      SSA 31.24.01-A



     ORDERING INFORMATION

     Software Licenses: QL-VZCA*-**
     Software Media: QA-VZCA*-**
     Software Documentation: QA-VZCAA-GZ
     Software Product Services: QT-VZCA*-**

     *  Denotes variant fields. For additional information on avail-
        able licenses, services, and media, refer to the appropriate
        price book.

     The above information is valid at time of release. Please con-
     tact your local Digital office for the most up-to-date informa-
     tion.

     [TM] The DIGITAL Logo, CI, DEC, DECnet, DECnet-VAX, DECsta-
          tion, DECsystem, ISDN, MicroVAX, VAX, VAXcluster, VAXft,
          VAXserver, VAXstation, and VMS are trademarks of Digital
          Equipment Corporation.




















                                     5
