






             ________________________
             Second Edition, 29 October 1990
             __________
             The information in this document is subject to change without
             notice and should not be construed as a commitment by Digital
             Equipment Corporation. Digital Equipment Corporation assumes
             no responsibility for any errors that may appear in this
             document.
             The software described in this document is furnished under a
             license and may be used or copied only in accordance with the
             terms of such license.
             No responsibility is assumed for the use or reliability
             of software on equipment that is not supplied by Digital
             Equipment Corporation or its affiliated companies.
             Restricted Rights: Use, duplication, or disclosure by the
             U.S. Government is subject to restrictions as set forth in
             subparagraph (c)(1)(ii) of the Rights in Technical Data and
             Computer Software clause at DFARS 252.227-7013.
             __________
             Copyright ©1990 by Digital Equipment France

             All Rights Reserved.
             __________

             The following are trademarks of Digital Equipment Corporation:
             DEC            DIBOL          UNIBUS
             DEC/CMS        EduSystem      VAX
             DEC/MMS        IAS            VAXcluster
             DECnet         MASSBUS        VMS
             DECsystem-10   PDP            VT
             DECSYSTEM-20   PDT
             DECUS          RSTS
             DECwriter      RSX            DIGITAL


             This document was prepared using VAX DOCUMENT, Version 1.1


 



 













                                                                   Preface
          ________________________________________________________________



          __________________________________________________________
          Intended Audience

             This manual provides information for system managers and
             DIGITAL software specialists. The manual assumes that readers
             understand and also have some experience of:

              o  Installation of software products on VAX/VMS
              o  Wide Area Networks (WANs)

              o  DECnet-VAX
              o  DIGITAL's VAX ISDN product.

          __________________________________________________________
          Purpose of this Document

             This manual explains how to install VAX ISDN and VAX ISDN
             ACCESS. Information about how to configure and start up
             the VAX ISDN Software is contained in the VAX ISDN Software
             Management Guide.







                                                                       vii


 





          __________________________________________________________
          Associated Documentation



          __________________________________________________________
          Terminology
             Throughout this document, the following terminology has been
             used:

             _____________________________________________________________
             Term__________________Meaning________________________________
             VAX ISDN Software     The VAX ISDN Software in general, i.e.
                                   both VAX ISDN and VAX ISDN ACCESS

             VAX ISDN              The full-function variety of the VAX
                                   ISDN Software

             VAX ISDN ACCESS       The reduced-function variety of the VAX
             ______________________ISDN_Software-see_Section_1.1.1________




















          viii


 











                                                                 Chapter 1


                                                              Introduction
          ________________________________________________________________


             This chapter provides an introduction to the software and its
             installation procedure.
          __________________________________________________________

          1.1  VAX ISDN Software Overview
          __________________________________________________________
          1.1.1  Product Variants

             There are two variants of the VAX ISDN product:

              o  the full-function product "VAX ISDN"
              o  an access-only variant, which is called "VAX ISDN ACCESS".

             VAX ISDN ACCESS allows users to access the VAX ISDN Call
             Control on remote nodes which are connected to an ISDN and
             which have VAX ISDN installed and running. VAX ISDN ACCESS
             uses a DECnet logical link to connect to the node to be con-
             trolled remotely. VAX ISDN ACCESS uses the link to transmit
             ISDN Call Control messages between the remote node and the
             local VAX user.
             VAX ISDN ACCESS only provides an interface to the VAX ISDN
             Call Control, and does not include the VAX ISDN Call Control
             software itself. It is meant to be used only on nodes that
             are not directly connected to the ISDN network.



                                                         Introduction  1-1


 





          __________________________________________________________
          1.1.2  Network Profiles

             Network profiles each contain a description of the character-
             istics of a particular ISDN network.

             The contents of the various Network Profiles for public ISDNs
             appear in the Public ISDN Network Information manual.
                                          NOTE

                 You must use the correct Network Profile for your
                 local ISDN network. Use of an incorrect Network
                 Profile invalidates DIGITAL's support of the VAX ISDN
                 Software.

          __________________________________________________________
          1.2  Installation Overview

             This software is installed by use of the VMSINSTAL utility.
             The procedure can be carried out by the customer himself at
             his own site.

             Whatever variant is used, the VAX ISDN software will re-
             quire DECnet-VAX to operate. The appropriate DECnet license,
             however, is not required for the operation of VAX ISDN on a
             single DECnet node.

          __________________________________________________________
          1.3  What Happens During Installation

             This section introduces the procedures you use when in-
             stalling VAX ISDN and VAX ISDN ACCESS.
             The procedures for installing VAX ISDN and VAX ISDN ACCESS
             are automated as far as possible. Throughout an installation,
             the procedures prompt you with questions that require a
             simple answer such as Yes or No. In many cases defaults
             have been set up. These are indicated in square brackets.
             To accept the default, simply press the <Return> key.


          1-2  Introduction


 






                                          NOTE

                 If you do not understand a prompt or are uncertain
                 about the the information required at any point during
                 the installation, enter a question mark (?) in answer
                 to the prompt. You will be provided with on-line help
                 about that prompt and about the information you should
                 enter.
             Installation involves the following steps:

              1. Executing VMSINSTAL.COM to copy the VAX ISDN Software
                files from the distribution kit to the system disk.
              2. Executing the IVP (this can be done automatically as part
                of the installation procedure).

              3. Adding the VAX ISDN Software startup file, ISDN$STARTUP.COM,
                to the SYSMAN startup database (for VAX ISDN only).
              4. If necessary, updating the SYSGEN system parameters
                database. Note that if the VAX ISDN Software had pre-
                viously been installed on the system, the system parameter
                values may already be correct.

              5. Rebooting the system (not necessary if installing VAX ISDN
                ACCESS and if no system parameters are changed).















                                                         Introduction  1-3


 











                                                                 Chapter 2


                                                Preparing for Installation
          ________________________________________________________________

          __________________________________________________________

          2.1  Distribution Kits

             The software is supplied in two kits:
              o  the ISDN V1.1 kit, which supplies the software for config-
                uring a full-function VAX ISDN system

              o  the ISDN ACCESS V1.1 kit, which supplies the software for
                configuring a VAX ISDN ACCESS system.

             The software is distributed on the following media:

             Table_2-1:_Media_for_Installation_of_VAX_ISDN________________
             Medium________________Quantity_________Volume_Label__________

             TK50 cassette         1                ISDN

             1600 BPI magnetic     1 x 2400 feet    ISDN
             tape

             CDROM                 (part of VMS
                                   CD)
             _____________________________________________________________




                                           Preparing for Installation  2-1


 






             Table_2-2:_Media_for_Installation_of_VAX_ISDN_ACCESS_________
             Medium________________Quantity_________Volume_Label__________

             TK50 cassette         1                ISDN-A

             1600 BPI magnetic     1 x 2400 feet    ISDN-A
             tape

             RX23 floppy disk      1                ISDN-A

             CDROM                 (part of VMS
                                   CD)
             _____________________________________________________________
             The contents of the various kits are listed in Appendix C.

          __________________________________________________________
          2.2  Hardware Requirements

             The hardware requirements for the VAX ISDN Software are
             listed as part of the System Support Addendum for this
             product. Please refer to this document to verify that these
             requirements are met.

                                          NOTE

                 The VAX ISDN Software currently only supports the
                 DEC ISDNcontroller 100 ("DIV32" device) as interface
                 to an ISDN network. The installation of the VAX ISDN
                 software should therefore be performed on a VAX sys-
                 tem that is equipped with a Q-Bus. No error will be
                 reported, however, if this is not the case.








          2-2  Preparing for Installation


 





          __________________________________________________________
          2.2.1  Checking the Disk Space

             Before you install the VAX ISDN products, check that the
             system disk has enough free space by entering the following
             command:

               $ SHOW DEVICE SYS$SYSDEVICE
             The information displayed includes the number of free blocks
             on the disk. Consult Table 2-3 in order to make sure that
             there is enough space to install your system. (If you try
             to install either of the VAX ISDN products with too few free
             blocks, the installation procedure will of course fail.)


             Table_2-3:_Disk_Space_Requirements___________________________
                              For
                              Product     Peak Requirement During
             _________________Itself______Installation____________________

             VAX ISDN         1750        2200 blocks
                              blocks

             VAX ISDN ACCESS  1020        1250 blocks
                              blocks
             _____________________________________________________________
          __________________________________________________________
          2.3  Software Requirements

             The only required software for the installation procedure
             itself is VMS. Please refer to the System Support Addendum
             document to see which VMS version(s) are supported.








                                           Preparing for Installation  2-3


 





          __________________________________________________________
          2.4  Information Required for Installation

             Table 2-4 or Table 2-5 show the information which will be
             required during the installation.


             Table_2-4:_Installation_Information-VAX_ISDN_________________
             Item_____________Value_______________________________________

             Kit name         ISDN

             LMF product      ISDN
             name

             Load device      VMS device name of the device which reads
             name             the kit media, for example DUA1:.

             Network Profile  One of the following:
             Identifier          ATT
                                 AUST
                                 BRITISH
                                 FRENCH
                                 GERMAN
                                 JAPAN
                                 NORTHERN
             _____________________________________________________________

             Table_2-5:_Installation_Information-VAX_ISDN_ACCESS__________
             Item_____________Value_______________________________________

             Kit name         ISDN-ACCESS

             LMF product      ISDN-ACCESS
             name

             Load device      VMS device name of the device which reads
             name             the kit media, for example DUA1:.
             _____________________________________________________________

          2-4  Preparing for Installation


 






             If you do not know the answers to any of these questions,
             obtain the missing values from your system manager, net-
             work administrator, or DIGITAL software specialist, before
             attempting the installation.
          __________________________________________________________

          2.5  Installing VAX ISDN on a Cluster

             In the case of a VAXcluster, VAX ISDN must be installed
             on each node that is going to run the software. One way to
             achieve this is to install VAX ISDN on any systems that are
             connected to the ISDN, and VAX ISDN ACCESS on the other VAX
             systems in the cluster.

                                          NOTE
                 Before you install VAX ISDN or VAX ISDN ACCESS on
                 any system in the cluster, you MUST ensure that VAX
                 ISDN or VAX ISDN ACCESS are not running on any of the
                 other VAXcluster systems during the installation, as
                 described in Section 2.5.1. When you have finished
                 installing the software on all the relevant nodes, you
                 can start the VAX ISDN Software.

             Refer to Appendix C for details of which files are installed
             in the system-specific root area and which are installed in
             the common root area.
          __________________________________________________________

          2.5.1  How to Check if the VAX ISDN Software is Running
             The easiest way to check all the nodes on a cluster to see if
             VAX ISDN or VAX ISDN ACCESS is running, is to use the SYSMAN
             utility to issue an ISDN$NCP command on each node. If the
             message






                                           Preparing for Installation  2-5


 






               %ISDN-W-NOTSTARTED

             is returned from every node (or ISDN$NCP does not exist on
             the node), then it is safe to start the installation. For
             example:
               $ run sys$system:sysman<Return>
               SYSMAN> set environment /cluster<Return>
               %SYSMAN-I-ENV, current command environment:
                       Clusterwide on local cluster
                       Username SYSTEM       will be used on nonlocal nodes

               SYSMAN> do mcr isdn$ncp show line 0<Return>
             The returned messages from each node will be in one of the
             following categories:

              1. The message:

                  %SYSMAN-I-OUTPUT, command execution on node JULIE
                followed by a normal display or error message from
                ISDN$NCP, in which case the node is running the VAX ISDN
                software. In such a case, the VAX ISDN software must be
                shut down before re-installing it.

              2. The message:

                  %SYSMAN-I-OUTPUT, command execution on node JEAN
                  %ISDN-W-NOTSTARTED, VAX ISDN software not loaded
                which means that the VAX ISDN software is installed but
                not started, so it is safe to re-install.

              3. The message:
                  %SYSMAN-I-OUTPUT, command execution on node NICK
                  %SYSTEM-F-NOSUCHOBJ, network object is unknown at remote node

                which means that the VAX ISDN has never been installed, so
                it is safe to install.



          2-6  Preparing for Installation


 





          __________________________________________________________
          2.6  VAX ISDN and the License Management Facility (LMF)

             VAX ISDN and VAX ISDN ACCESS are known by the VMS License
             Management Facility (LMF) as ISDN and ISDN-ACCESS respec-
             tively.

             LMF has two classes of license, Availability and Capacity
             licenses. VAX ISDN and VAX ISDN ACCESS only support
             Availability licensing.
             Before VAX ISDN or VAX ISDN ACCESS can be run on a system,
             you must license the system by running the LICENSE utility.

             To license your system, you enter the information given
             on the Product Authorization Key (PAK), as described in
             Section 2.6.1 below. The PAK contains all the information
             you need to enter during license registration.
             You are recommended to license ISDN or ISDN-ACCESS before you
             run the corresponding Installation Verification Procedure. If
             you do not do this, either of the following messages will be
             displayed, depending on the product:

             Figure 2-1: "No license" Error Messages
             _____________________________________________________________

             %ISDN-W-NOAUTH, DEC ISDN use is not authorized on this node

             %ISDN-W-NOAUTH, DEC ISDN-ACCESS use is not authorized on this node
             _____________________________________________________________











                                           Preparing for Installation  2-7


 





          __________________________________________________________
          2.6.1  Entering the PAK

             To activate the license registration procedure, enter the
             following command:

               $ @SYS$UPDATE:VMSLICENSE

             You will then be prompted for the details contained in the
             ISDN or ISDN-ACCESS PAK. Each question corresponds to a
             heading in the PAK.

             If you are installing on a cluster, you only need to perform
             this procedure on one node. Then enter the following command
             on each of the other nodes in the cluster that will be using
             the same ISDN license:

               $ LICENSE LOAD ISDN

             If you are licensing VAX ISDN ACCESS, enter the following
             command:


               $ LICENSE LOAD ISDN-ACCESS

             You can then install VAX ISDN or VAX ISDN ACCESS on the other
             nodes in the cluster as required.
             Refer to the VMS documentation set for further details on
             using the VMSLICENSE procedure and the LICENSE utility.

          __________________________________________________________
          2.6.2  Using VAX ISDN or VAX ISDN ACCESS

             If you have not licensed VAX ISDN or VAX ISDN ACCESS, and
             you try to start up VAX ISDN or to access the VAX ISDN Call
             Control (using either ISDN$NCP or ISDN$SA), then your re-
             quest will fail, and one of the LMF error messages shown in
             Figure 2-1 will be returned. In such cases you should install


          2-8  Preparing for Installation


 






             the license as detailed in Section 2.6.1 above and then start
             the product.

             At any time, you can check that either license has been
             registered, enabled and loaded by issuing the following
             commands:
               $ LICENSE LIST

             to see if the license is in the license database (which is
             cluster-wide), and

               $ SHOW LICENSE
             to see if the license has been correctly loaded onto the
             local node.

























                                           Preparing for Installation  2-9


 











                                                                 Chapter 3


                                                       Installing VAX ISDN
          ________________________________________________________________


             This chapter guides the reader through the procedure for
             installing VAX ISDN. If you are installing VAX ISDN ACCESS,
             refer instead to Chapter 4.
          __________________________________________________________

          3.1  Installing VAX ISDN Files from the Distribution Volume

             To install the VAX ISDN Software from the distribution vol-
             ume, you should carry out the following procedure at the
             system console.
              1  Log in to the SYSTEM account.

              2  Check that the disk has enough free space for VAX ISDN.
                Refer to Table 2-3 for details of how much free space you
                need on your system disk.
              3  To start the installation procedure, enter the following
                command:

                  $ @SYS$UPDATE:VMSINSTAL<Return>

                The procedure displays:

                          VAX/VMS Software Product Installation Procedure <REFERENCE>(VMS_VER)
                                     It is date at time.

                  Enter a question mark (?) at any time for help.

                                                  Installing VAX ISDN  3-1


 






                If DECnet is currently running on your system, the proce-
                dure warns you with the following message:

                  %VMSINSTAL-W-DECNET, Your DECnet network is up and running.
                  * Do you want to continue anyway [NO]?

                As you do not have to shut DECnet down in order to install
                VAX ISDN, you may answer YES to this question.
              4  The procedure continues with:

                  * Are you satisfied with the backup of your system disk [YES]?

                Make sure you have a good backup copy of the disk, as
                the installation will write to the system disk. If your
                system disk has not been backed up or you wish to make
                a fresh copy, answer NO; the procedure would then exit
                without installing the software. When you have backed up
                your system disk, you can start the installation procedure
                again.
                If you answer YES, the procedure continues.

              5  Next it asks the following question:

                  * Where will the distribution volumes be mounted:
                Enter the name of the device on which the volume contain-
                ing the VAX ISDN Software will be mounted. ddcu: is the
                device name, where dd is the device code, c is the con-
                troller letter, and u is the unit number. For example,
                MUA0:.

              6  Next the procedure displays:
                  Enter the products to be processed from the first distribution
                  volume set.
                  * Products:





          3-2  Installing VAX ISDN


 






              7  Enter:

                  ISDN
                and (as normal) press <Return>.

              8  The procedure responds with:

                  * Enter installation options you wish to use (none):
                Enter n<Return>. This will request the display and/or
                printing of the Release Notes.

                If you specified a device which is not already mounted in
                step 5, then the installation procedure will continue as
                follows, otherwise it will proceed with step number 10

                  Please mount the first volume of the set on device
                  * Are you ready?

              9  Load the distribution volume (labelled ISDN) into the
                corresponding drive.
                Answer YES when you have done so.

                The procedure will then mount the volume on the device,
                and display a message such as this:
                  %MOUNT-I-MOUNTED, ISDN mounted on _MUA0:

              10 VMSINSTAL proceeds with:

                  The following products will be processed:
                    ISDN V1.1
                          Beginning installation of ISDN V1.1 at time

                      Release notes included with this kit are always copied to SYS$HELP.

                      Additional Release Notes Options:




                                                  Installing VAX ISDN  3-3


 






                          1.  Display release notes
                          2.  Print release notes
                          3.  Both 1 and 2
                          4.  None of the above

                  * Select option [2]:
                You should print or display the Release Notes and read
                them before continuing.

              11 VMSINSTAL continues with:
                  %VMSINSTAL-I-RESTORE, Restoring product saveset A ...
                  %VMSINSTAL-I-RELMOVED , The product's release notes have been
                  successfully moved to SYS$HELP.

                          +---------------------------------------------------+
                          |      VAX ISDN Software Installation Procedure.    |
                          +---------------------------------------------------+

                          Product:      ISDN        Producer:     DEC
                          Version:      V1.1
                          Release Date: 30-NOV-1990

                  * Does this product have an authorization key registered and loaded?

              12 Now answer either Y<Return> or N<Return>, depending on
                whether or not you have loaded the appropriate license, as
                described in Section 2.6.
                If you have answered Y and the license is not active, then
                the following warning is displayed:


                  %ISDN-W-NOAUTH, DEC ISDN use is not authorized on this node
                If the license has not been loaded, the installation
                procedure will continue, but the Installation Verification
                Procedure will not be activated. The following message is
                then displayed:



          3-4  Installing VAX ISDN


 






                  %ISDN-W-NOIVP, the Installation Verification Procedure will not be
                  executed

                You should execute the IVP after loading the appropriate
                license, as described in Section 2.6.
              13 If, on the other hand, the license is active, the proce-
                dure continues with:

                  * Do you want to run the IVP [YES]?
                Now press <Return> if you want to the Installation
                Verification Procedure to be run automatically at the
                end of the installation.

              14 The procedure continues with:

                  * Do you want to purge files replaced by this installation [YES]?
              15 Now press <Return> if you want to purge files resulting
                from a previous installation.

                Note that if you are going to use the VAX ISDN Software on
                several nodes in a cluster, and are installing VAX ISDN
                or VAX ISDN-ACCESS on these nodes, the files installed in
                the SYS$COMMON area of the system disk are identical and
                should be purged.
              16 Next the procedure asks you to specify the network identi-
                fier:


                          VAX ISDN Software V1.1 contains network-specific code.
                          In order  to install the software correctly,  you must
                          identify which  network  you will be using by entering
                          one of the following network identifier strings:







                                                  Installing VAX ISDN  3-5


 






                                  ATT
                                  AUST
                                  BRITISH
                                  FRENCH
                                  GERMAN
                                  JAPAN
                                  NORTHERN

                  * Enter network identifier string:

              17 Identify your local implementation of ISDN.
                The procedure responds with:

                          Your country specific network profile has been configured.
                                          Installation continues...

                                          No More Questions.

                There may be a time delay of several minutes at this
                stage in the procedure. As you have now answered all the
                questions required for the installation, there is no need
                to watch the output, which will be like this:

                  %VMSINSTAL-I-RESTORE, Restoring product saveset B ...
                  %VMSINSTAL-I-RESTORE, Restoring product saveset C ...
                  %VMSINSTAL-I-RESTORE, Restoring product saveset D ...
              18 If you had previously installed VAX ISDN (or another
                communication product that makes use of NETTRACE) on
                your system, a series of messages may be displayed. These
                messages tell you that some existing files will not be
                updated. This is done to preserve user modifications to
                these files.







          3-6  Installing VAX ISDN


 






                These are the messages you may see:

                  %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]NETTRACE_SECURITY.COM already
                  exists on system
                  %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]NETTRACE_SECURITY.COM not
                  installed

                  %ISDN-I-FILEXISTS, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT already
                  exists on system
                  %ISDN-I-FILNOTINST, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT not
                  installed

                  %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]ISDN$SECURITY.COM already
                  exists on system
                  %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]ISDN$SECURITY.COM not
                  installed

                  %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]ISDN$STARTUP_SITE.COM already
                  exists on system
                  %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]ISDN$STARTUP_SITE.COM not
                  installed
              19 The procedure checks the system parameter MAXBUF. If it is
                less than 2048 bytes, the procedure issues the following
                warning:

                  %ISDN-W-MAXBUFTOOSMALL, MAXBUF is too small, change from n to 2048.

                where n is the current value of the MAXBUF parameter.
                Change the value of the MAXBUF system parameter after
                you have installed VAX ISDN. See Section 3.2.3 for a
                description of how to do this.

              20 Next the system will display a list of "things to do".
                More details on these are given in Section 3.2. Take heed
                of the advice given, the next time you see the DCL prompt.




                                                  Installing VAX ISDN  3-7


 






                Here is the corresponding display:

          *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *
                  Upon completion of this installation, please follow the instructions
                  below:-

                         - using the following command, add the VAX ISDN product to the
                           database of components to be automatically started when
                           the system is booted:-
                           $ RUN SYS$SYSTEM:SYSMAN
                           SYSMAN> startup add file ISDN$STARTUP.COM [/node=(A,B,C)]

                         - REBOOT the system
          *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *

              21 When the last saveset has been copied, the proce-
                dure copies the distribution files from a subdirectory
                of SYS$UPDATE to their respective directories. (See
                Appendix C for details of which files are installed into
                which directories.) The following message is displayed
                then:

          %VMSINSTAL-I-MOVEFILES, files will now be moved to their target directories...

              22 Now, if the license check at step 12 was successful and if
                you answered "YES" at step 13, the IVP will be run:

                        *****************************************************
                        *                                                   *
                        *   ISDN V1.1 Installation Verification Procedure   *
                        *                                                   *
                        *****************************************************

          %ISDN-W-NOTSTARTED, VAX ISDN software not loaded<Return>
          %ISDN-I-IVPSUCCESS, ISDN V1.1 IVP was successful




          3-8  Installing VAX ISDN


 






                The %ISDN-W-NOTSTARTED message is not necessarily dis-
                played; if it is displayed, ignore it.

                  Installation of ISDN V1.1 completed at time

          Enter the products to be processed from the next distribution volume set.
          * Products:
              23 You can now leave the VMSINSTAL procedure by pressing
                <Ctrl-Z>. You will then be returned to the DCL prompt:

                  * Products: <Ctrl-Z>
                   VMSINSTAL procedure done at time.

                  $
                You may then remove the distribution medium from the
                device.

             See Section 3.2 for what to do next.

          __________________________________________________________
          3.1.1  Installation Failures
          __________________________________________________________
          3.1.1.1  Incorrect Version of Operating System
             During the installation, the procedure checks that the ver-
             sion number of the operating system (VMS) is correct. If
             it is incorrect, the procedure exits after displaying the
             following message:

               This product requires VMS version V5.2-1 or later to install

               %VMSINSTAL-E-INSFAIL, The installation of ISDN V1.1 has failed
             Note that the correct version(s) are shown in the System
             Support Addendum.






                                                  Installing VAX ISDN  3-9


 





          __________________________________________________________
          3.1.1.2  Insufficient Disk Space

             During the installation, the procedure checks that there is
             sufficient space on your disk for the VAX ISDN files. Refer
             to Table 2-3 for details of how many free blocks you need
             on your system to install VAX ISDN. If there is not enough
             space, the procedure exits after displaying the following
             messages:

               %ISDN-E-NOSPACE, this installation requires nnnn blocks of
               disk space.
               %VMSINSTAL-E-INSFAIL, The installation of VAX ISDN V1.1 has
               failed.
             Make sure your system has sufficient free blocks before try-
             ing to install VAX ISDN again, by going through the procedure
             described in Section 2.2.1.

          __________________________________________________________
          3.1.1.3  Insufficient Global Pages
             If you receive the following message during installation:

               %INSTALL-E-FAIL, failed to REPLACE entry for
               DISK$VAXVMSRL052:<SYS0.SYSCOMMON.SYSLIB>DCLTABLES.EXE
               -SYSTEM-F-GPTFULL, global page table is full
               %INSTALL-W-DELETED, previous Known File Entry has been deleted

             then it will be necessary to increase the value of the sys-
             tem parameter GBLPAGES by 354. To do this, edit the file
             SYS$SYSTEM:MODPARAMS.DAT and add the line:

               ADD_GBLPAGES=354
             Then issue the following command sequence:

               $ @SYS$UPDATE:AUTOGEN SAVPARAMS GENPARAMS
               $ @SYS$UPDATE:AUTOGEN SETPARAMS REBOOT
             This will cause AUTOGEN to recompute the system parameters
             and reboot.


          3-10  Installing VAX ISDN


 





          __________________________________________________________
          3.1.1.4  User Interrupt

             If you decide to cancel the installation of VAX ISDN at
             any time by pressing <Ctrl-Y>, after a short time delay the
             following is displayed:

               %VMSINSTAL-F-CTRLY, Installation cancelled via CTRL/Y.
               %VMSINSTAL-F-UNEXPECTED, Installation terminated due to unexpected
               event.
                              VMSINSTAL procedure done at time

             If you enter <Ctrl-Y> after the information message that the
             files are being moved to the target directories, your system
             will have some new and (if previously installed) some old VAX
             ISDN files. Therefore, you should reinstall the product.

          __________________________________________________________
          3.2  Post-Installation Procedure

             This section describes what must be done when the DCL prompt
             has reappeared, after exiting from VMSINSTAL.

          __________________________________________________________
          3.2.1  Setting up the VAX ISDN Software

             Please refer to the chapter entitled "VAX ISDN Operations" in
             VAX ISDN Software Management Guide for a detailed descrip-
             tion of how to configure the various VAX ISDN files on your
             node or cluster. For users in Japan, note also the appendix
             specific to them in said Guide.

          __________________________________________________________
          3.2.2  Updating the SYSMAN Startup Component Database

             After a reboot, the VAX ISDN Software can be started using
             the following command:



                                                 Installing VAX ISDN  3-11


 





          __________________________________________________________
          3.2.3  Updating System Parameters

             Update the system parameters to provide space for the data
             structures required by VAX ISDN.

          __________________________________________________________
          3.2.3.1  MAXBUF Parameter
             Make sure that the value of the MAXBUF parameter is set to at
             least 2048. Note that this is the current default value with
             VMS.

             If necessary, use SYSGEN to change this parameter.
          __________________________________________________________
          3.2.3.2  Using SYSGEN

             Log in under the system manager's account and run
             SYS$SYSTEM:SYSGEN.
             Within SYSGEN, then use the SHOW/MAJOR command to display the
             current values of the most significant system parameters. Use
             the SET command to specify new values for these parameters.
             For example:

               $ RUN SYS$SYSTEM:SYSGEN
               SYSGEN> use ACTIVE
               SYSGEN> show /major
                  .
                  .
                  .
               SYSGEN> set MAXBUF 2048
               SYSGEN> write ACTIVE
               SYSGEN> exit
               $

                                          NOTE
                 If you alter your SYSGEN parameters because of a VAX
                 ISDN installation, you must update SYS$SYSTEM:MODPARAMS.DAT



          3-12  Installing VAX ISDN


 






                 so that subsequent use of the AUTOGEN procedure does
                 not lose your changes.

                 Use of the AUTOGEN procedure and of the file
                 SYS$SYSTEM:MODPARAMS.DAT are described in the VMS
                 documentation set.
             When you have changed the parameter values, reboot your
             system.

          __________________________________________________________
          3.2.4  Disk Backup

             Finally, when you have installed and configured VAX ISDN, and
             checked that the system is installed properly, back up the
             updated system disk and save the distribution kit for future
             updates.

          __________________________________________________________
          3.2.5  Reboot

             The ISDN software that you have installed will not come into
             operation until you have rebooted the system.

          __________________________________________________________
          3.3  Installation Verification Procedure

             This section explains how to check that the application has
             been installed correctly.

          __________________________________________________________
          3.3.1  The Verification Steps

             The Installation Verification Procedure, which is activated
             either automatically by VMSINSTAL or by the user, verifies
             that the various software components have been correctly
             installed on the system disk.



                                                 Installing VAX ISDN  3-13


 






             The IVP can be executed at any time after the installation
             (for troubleshooting purposes, for instance), by entering the
             following command:

               $ @SYS$TEST:ISDN$IVP

          __________________________________________________________
          3.3.2  Communication Verification

             As this requires specific ISDN controller hardware, the IVP
             does not check successful communication between the VAX ISDN
             Software and the ISDN itself.
             Please refer to the Troubleshooting chapter of VAX ISDN
             Software Management Guide for indications on this type of
             verification.
























          3-14  Installing VAX ISDN


 











                                                                 Chapter 4


                                                Installing VAX ISDN ACCESS
          ________________________________________________________________


             This chapter guides the reader through the procedure for
             installing VAX ISDN ACCESS. If you are installing VAX ISDN
             (full-function version), refer to Chapter 3 instead.
          __________________________________________________________

          4.1  Installing VAX ISDN ACCESS Files from the Distribution
               Volume

             To install the VAX ISDN Software from the distribution vol-
             ume, you should carry out the following procedure at the
             system console.

              1  Log in to the SYSTEM account.
              2  Check that the disk has enough free space for VAX ISDN
                ACCESS. Refer to Table 2-3 for details of how much free
                space you need on your system disk.

              3  To start the installation procedure, enter the following
                command:

                  $ @SYS$UPDATE:VMSINSTAL<Return>
                The procedure displays:





                                           Installing VAX ISDN ACCESS  4-1


 






                          VAX/VMS Software Product Installation Procedure <REFERENCE>(VMS_VER)

                                     It is date at time.
                  Enter a question mark (?) at any time for help.

                If DECnet is currently running on your system, the proce-
                dure warns you with the following message:
                  %VMSINSTAL-W-DECNET, Your DECnet network is up and running.

                  * Do you want to continue anyway [NO]?
                As you do not have to shut DECnet down in order to install
                VAX ISDN, you may answer YES to this question.

              4  The procedure continues with:

                  * Are you satisfied with the backup of your system disk [YES]?
                Make sure you have a good backup copy of the disk, as
                the installation will write to the system disk. If your
                system disk has not been backed up or you wish to make
                a fresh copy, answer NO; the procedure would then exit
                without installing the software. When you have backed up
                your system disk, you can start the installation procedure
                again.

                If you answer YES, the procedure continues.
              5  Next it asks the following question:

                  * Where will the distribution volumes be mounted:

                Enter the name of the device on which the volume contain-
                ing the VAX ISDN Software will be mounted. ddcu: is the
                device name, where dd is the device code, c is the con-
                troller letter, and u is the unit number. For example,
                MUA0:.





          4-2  Installing VAX ISDN ACCESS


 






              6  Next the procedure displays:

                  Enter the products to be processed from the first distribution
                  volume set.
                  * Products:
              7  Enter:

                  ISDN-ACCESS

                and (as normal) press <Return>.
              8  The procedure responds with:

                  * Enter installation options you wish to use (none):

                Enter n<Return>. This will request the display and/or
                printing of the Release Notes.
                If you specified a device which is not already mounted in
                step 5, then the installation procedure will continue as
                follows, otherwise it will proceed with step number 10

                  Please mount the first volume of the set on device
                  * Are you ready?

              9  Load the distribution volume (labelled ISDN-A) into the
                corresponding drive.
                Answer YES when you have done so.

                The procedure will then mount the volume on the device,
                and display a message such as this:

                  %MOUNT-I-MOUNTED, ISDN mounted on _MUA0:








                                           Installing VAX ISDN ACCESS  4-3


 






              10 VMSINSTAL proceeds with:

                  The following products will be processed:
                    ISDN-ACCESS V1.1
                          Beginning installation of ISDN-ACCESS V1.1 at time

                      Release notes included with this kit are always copied to SYS$HELP.

                      Additional Release Notes Options:
                          1.  Display release notes
                          2.  Print release notes
                          3.  Both 1 and 2
                          4.  None of the above

                  * Select option [2]:
                You should print or display the Release Notes and read
                them before continuing.

              11 VMSINSTAL continues with:

                  %VMSINSTAL-I-RESTORE, Restoring product saveset A ...
                  %VMSINSTAL-I-RELMOVED , The product's release notes have been
                  successfully moved to SYS$HELP.
                          +----------------------------------------------------------+
                          |      VAX ISDN-ACCESS Software Installation Procedure.    |
                          +----------------------------------------------------------+


                          Product:      ISDN-ACCESS        Producer:     DEC
                          Version:      V1.1
                          Release Date: 30-NOV-1990

                  * Does this product have an authorization key registered and loaded?
              12 Now answer either Y<Return> or N<Return>, depending on
                whether or not you have loaded the appropriate license, as
                described in Section 2.6.



          4-4  Installing VAX ISDN ACCESS


 






                If you have answered Y and the license is not active, then
                the following warning is displayed:

                  %ISDN-W-NOAUTH, DEC ISDN-ACCESS use is not authorized on this node

                If the license has not been loaded, the installation
                procedure will continue, but the Installation Verification
                Procedure will not be activated. The following message is
                then displayed:

                  %ISDN-W-NOIVP, the Installation Verification Procedure will not be
                  executed

                You should execute the IVP after loading the appropriate
                license, as described in Section 2.6.
              13 If, on the other hand, the license is active, the proce-
                dure continues with:

                  * Do you want to run the IVP [YES]?

                Now press <Return> if you want to the Installation
                Verification Procedure to be run automatically at the
                end of the installation.
              14 The procedure continues with:

                  * Do you want to purge files replaced by this installation [YES]?
              15 Now press <Return> if you want to purge files resulting
                from a previous installation.

                Note that if you are going to use the VAX ISDN Software on
                several nodes in a cluster, and are installing VAX ISDN
                or VAX ISDN-ACCESS on these nodes, the files installed in
                the SYS$COMMON area of the system disk are identical and
                should be purged. The procedure responds with:

                                          No More Questions.



                                           Installing VAX ISDN ACCESS  4-5


 






                There may be a time delay of several minutes at this
                stage in the procedure. As you have now answered all the
                questions required for the installation, there is no need
                to watch the output, which will be like this:

                  %VMSINSTAL-I-RESTORE, Restoring product saveset B ...
                  %VMSINSTAL-I-RESTORE, Restoring product saveset C ...
              16 The procedure checks the system parameter MAXBUF. If it is
                less than 2048 bytes, the procedure issues the following
                warning:

                  %ISDN-W-MAXBUFTOOSMALL, MAXBUF is too small, change from n to 2048.

                where n is the current value of the MAXBUF parameter.
                Change the value of the MAXBUF system parameter after you
                have installed VAX ISDN-ACCESS. See Section 4.2.1 for a
                description of how to do this.

              17 When the last saveset has been copied, the proce-
                dure copies the distribution files from a subdirectory
                of SYS$UPDATE to their respective directories. (See
                Appendix C for details of which files are installed into
                which directories.) The following message is displayed
                then:

          %VMSINSTAL-I-MOVEFILES, files will now be moved to their target directories...

              18 Now, if the license check at step 12 was successful and if
                you answered "YES" at step 13, the IVP will be run:
                     ************************************************************
                     *                                                          *
                     *   ISDN-ACCESS V1.1 Installation Verification Procedure   *
                     *                                                          *
                     ************************************************************





          4-6  Installing VAX ISDN ACCESS


 






          %ISDN-ACCESS-I-IVPSUCCESS, ISDN-ACCESS V1.1 IVP was successful

                  Installation of ISDN-ACCESS V1.1 completed at time

          Enter the products to be processed from the next distribution volume set.
          * Products:
              19 You can now leave the VMSINSTAL procedure by pressing
                <Ctrl-Z>. You will then be returned to the DCL prompt:

                  * Products: <Ctrl-Z>
                   VMSINSTAL procedure done at time.

                  $
                You may then remove the distribution medium from the
                device.

             See Section 4.2 for what to do next.

          __________________________________________________________
          4.1.1  Installation Failures
          __________________________________________________________
          4.1.1.1  Incorrect Version of Operating System
             During the installation, the procedure checks that the ver-
             sion number of the operating system (VMS) is correct. If
             it is incorrect, the procedure exits after displaying the
             following message:

               This product requires VMS version V5.2-1 or later to install

               %VMSINSTAL-E-INSFAIL, The installation of ISDN V1.1 has failed
             Note that the correct version(s) are shown in the System
             Support Addendum.







                                           Installing VAX ISDN ACCESS  4-7


 





          __________________________________________________________
          4.1.1.2  Insufficient Disk Space

             During the installation, the procedure checks that there
             is sufficient space on your disk for the VAX ISDN ACCESS
             files. Refer to Table 2-3 for details of how many free blocks
             you need on your system to install VAX ISDN. If there is
             not enough space, the procedure exits after displaying the
             following messages:

               %ISDN-E-NOSPACE, this installation requires nnnn blocks of
               disk space.
               %VMSINSTAL-E-INSFAIL, The installation of VAX ISDN ACCESS V1.1 has
               failed.
             Make sure your system has sufficient free blocks before
             trying to install VAX ISDN ACCESS again, by going through
             the procedure described in Section 2.2.1.

          __________________________________________________________
          4.1.1.3  Insufficient Global Pages
             If you receive the following message during installation:

               %INSTALL-E-FAIL, failed to REPLACE entry for
               DISK$VAXVMSRL052:<SYS0.SYSCOMMON.SYSLIB>DCLTABLES.EXE
               -SYSTEM-F-GPTFULL, global page table is full
               %INSTALL-W-DELETED, previous Known File Entry has been deleted

             then it will be necessary to increase the value of the sys-
             tem parameter GBLPAGES by 354. To do this, edit the file
             SYS$SYSTEM:MODPARAMS.DAT and add the line:

               ADD_GBLPAGES=354
             Then issue the following command sequence:

               $ @SYS$UPDATE:AUTOGEN SAVPARAMS GENPARAMS
               $ @SYS$UPDATE:AUTOGEN SETPARAMS REBOOT
             This will cause AUTOGEN to recompute the system parameters
             and reboot.


          4-8  Installing VAX ISDN ACCESS


 





          __________________________________________________________
          4.1.1.4  User Interrupt

             If you decide to cancel the installation of VAX ISDN ACCESS
             at any time by pressing <Ctrl-Y>, after a short time delay
             the following is displayed:

               %VMSINSTAL-F-CTRLY, Installation cancelled via CTRL/Y.
               %VMSINSTAL-F-UNEXPECTED, Installation terminated due to unexpected
               event.
                              VMSINSTAL procedure done at time

             If you enter <Ctrl-Y> after the information message that the
             files are being moved to the target directories, your system
             will have some new and (if previously installed) some old
             VAX ISDN ACCESS files. Therefore, you should reinstall the
             product.























                                           Installing VAX ISDN ACCESS  4-9


 





          __________________________________________________________
          4.2  Post-Installation Procedure

             This section describes what must be done when the DCL prompt
             has reappeared, after exiting from VMSINSTAL.

          __________________________________________________________

          4.2.1  Updating System Parameters
             Update the system parameters to provide space for the data
             structures required by VAX ISDN ACCESS.

          __________________________________________________________
          4.2.1.1  MAXBUF Parameter
             Make sure that the value of the MAXBUF parameter is set to at
             least 2048. Note that this is the current default value with
             VMS.

             If necessary, use SYSGEN to change this parameter.
          __________________________________________________________

          4.2.1.2  Using SYSGEN
             Log in under the system manager's account and run
             SYS$SYSTEM:SYSGEN.
             Within SYSGEN, then use the SHOW/MAJOR command to display the
             current values of the most significant system parameters. Use
             the SET command to specify new values for these parameters.
             For example:












          4-10  Installing VAX ISDN ACCESS


 






               $ RUN SYS$SYSTEM:SYSGEN
               SYSGEN> use ACTIVE
               SYSGEN> show /major
                  .
                  .
                  .
               SYSGEN> set MAXBUF 2048
               SYSGEN> write ACTIVE
               SYSGEN> exit
               $

                                          NOTE
                 If you alter your SYSGEN parameters because of
                 a VAX ISDN ACCESS installation, you must update
                 SYS$SYSTEM:MODPARAMS.DAT so that subsequent use of
                 the AUTOGEN procedure does not lose your changes.

                 Use of the AUTOGEN procedure and of the file
                 SYS$SYSTEM:MODPARAMS.DAT are described in the VMS
                 documentation set.
             When you have changed the parameter values, reboot your
             system.

          __________________________________________________________
          4.2.2  Disk Backup

             Finally, when you have installed and configured VAX ISDN
             ACCESS, and checked that the system is installed properly,
             back up the updated system disk and save the distribution kit
             for future updates.

          __________________________________________________________
          4.3  Installation Verification Procedure


             This section explains how to check that the application has
             been installed correctly.


                                          Installing VAX ISDN ACCESS  4-11


 





          __________________________________________________________
          4.3.1  The Verification Steps

             The Installation Verification Procedure, which is activated
             either automatically by VMSINSTAL or by the user, verifies
             that the various software components have been correctly
             installed on the system disk.

             The IVP can be executed at any time after the installation
             (for troubleshooting purposes, for instance), by entering the
             following command:
               $ @SYS$TEST:ISDN$IVP_ACCESS

          __________________________________________________________

          4.3.2  Communication Verification
             As this requires specific ISDN controller hardware, the IVP
             does not check successful communication between the VAX ISDN
             Software and the ISDN itself.

             Please refer to the Troubleshooting chapter of VAX ISDN
             Software Management Guide for indications on this type of
             verification.

















          4-12  Installing VAX ISDN ACCESS


 











                                                                Appendix A


                                        Example of a VAX ISDN Installation
          ________________________________________________________________


             The following is an example of a VAX ISDN software installa-
             tion. Text entered by the user is shown in boldface.

          $ @sys$update:vmsinstal<Return>

                  VAX/VMS Software Product Installation Procedure <REFERENCE>(VMS_VER)

          It is 19-DEC-1990 at 11:44.
          Enter a question mark (?) at any time for help.
          * Are you satisfied with the backup of your system disk [YES]? <Return>
          * Where will the distribution volumes be mounted: mua0:<Return>

          Enter the products to be processed from the first distribution volume set.
          * Products: isdn<Return>
          * Enter installation options you wish to use (none): n<Return>
          Please mount the first volume of the set on  MUA0:.
          * Are you ready? yes<Return>
          %MOUNT-I-MOUNTED, ISDN mounted on _MUA0:
          The following products will be processed:
            ISDN V1.1

                  Beginning installation of ISDN V1.1 at 11:50
          %VMSINSTAL-I-RESTORE, Restoring product saveset A ...

              Release notes included with this kit are always copied to SYS$HELP.
              Additional Release Notes Options:

                                   Example of a VAX ISDN Installation  A-1


 






                  1.  Display release notes
                  2.  Print release notes
                  3.  Both 1 and 2
                  4.  None of the above

          * Select option [2]: 1<Return>

          DUA0:[SYS0.SYSUPD.ISDN011]ISDN011.RELEASE_NOTES;1
              Release notes for VAX ISDN, Version V1.1

             At this point, the Release Notes are displayed on the screen;
             the user presses <Return> after reading each screen. Then the
             installation continues:

          End of VAX ISDN V1.1 release notes.

          * Do you want to continue the installation [NO]? yes<Return>
          %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully moved
          to SYS$HELP.
                  +-------------------------------------------------------+
                  |        VAX ISDN Software Installation Procedure.      |
                  +-------------------------------------------------------+

                  Product:      ISDN
                  Producer:     DEC
                  Version:      V1.1
                  Release Date: 30-NOV-1990

          * Does this product have an authorization key registered and loaded? yes<Return>
          * Do you want to run the IVP after the installation [YES]? <Return>
          * Do you want to purge files replaced by this installation [YES]? <Return>

                  VAX ISDN Software V1.1 contains network-specific code.
                  In order  to install the software correctly,  you must
                  identify which  network  you will be using by entering
                  one of the following network identifier strings:



          A-2  Example of a VAX ISDN Installation


 






                          ATT
                          AUST
                          BRITISH
                          FRENCH
                          GERMAN
                          JAPAN
                          NORTHERN


          * Enter network identifier string: french<Return>

                  Your country specific network profile has been configured.
                  Installation continues...

                  No More Questions.
          %VMSINSTAL-I-RESTORE, Restoring product saveset B ...
          %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]NETTRACE_SECURITY.COM already exists on system
          %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]NETTRACE_SECURITY.COM not installed
          %ISDN-I-FILEXISTS, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT already exists on system
          %ISDN-I-FILNOTINST, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT not installed
          %VMSINSTAL-I-RESTORE, Restoring product saveset C ...
          %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]ISDN$STARTUP_SITE.COM already exists on system
          %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]ISDN$STARTUP_SITE.COM not installed
          %ISDN-I-FILEXISTS, VMI$ROOT:[SYSMGR]ISDN$SECURITY.COM already exists on system
          %ISDN-I-FILNOTINST, VMI$ROOT:[SYSMGR]ISDN$SECURITY.COM not installed
          %VMSINSTAL-I-RESTORE, Restoring product saveset D ...

          *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *
                  Upon completion of this installation, please follow the instructions
                  below:-

                         - using the following command, add the ISDN product to the
                           database of components to be automatically started when
                           the system is booted:-
                           $ RUN SYS$SYSTEM:SYSMAN
                           SYSMAN> startup add file ISDN$STARTUP.COM [/node=(A,B,C)]

                         - REBOOT the system

                                   Example of a VAX ISDN Installation  A-3


 






          *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *  *

          %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...
                        *****************************************************
                        *                                                   *
                        *   ISDN V1.1 Installation Verification Procedure   *
                        *                                                   *
                        *****************************************************

          %ISDN-W-NOTSTARTED, VAX ISDN software not loaded
          %ISDN-I-IVPSUCCESS, ISDN V1.1 IVP was successful
                  Installation of ISDN V1.1 completed at 12:02

          Enter the products to be processed from the next distribution volume set.
          * Products: <Ctrl-Z>
                  VMSINSTAL procedure done at 12:20
          $






















          A-4  Example of a VAX ISDN Installation


 











                                                                Appendix B


                                 Example of a VAX ISDN ACCESS Installation
          ________________________________________________________________


             Text entered by the user is shown in boldface.

          $ @sys$update:vmsinstal<Return>

                  VAX/VMS Software Product Installation Procedure <REFERENCE>(VMS_VER)

          It is 20-DEC-1990 at 11:02.
          Enter a question mark (?) at any time for help.
          * Are you satisfied with the backup of your system disk [YES]? <Return>
          * Where will the distribution volumes be mounted: mua0:<Return>

          Enter the products to be processed from the first distribution volume set.
          * Products: isdn-access<Return>
          * Enter installation options you wish to use (none): n<Return>
          Please mount the first volume of the set on  MUA0:.
          * Are you ready? yes<Return>
          %MOUNT-I-MOUNTED, ISDN mounted on _MUA0:
          The following products will be processed:
            ISDN-ACCESS V1.1
                  Beginning installation of ISDN-ACCESS V1.1 at 11:08

          %VMSINSTAL-I-RESTORE, Restoring product saveset A ...
              Release notes included with this kit are always copied to SYS$HELP.

              Additional Release Notes Options:


                            Example of a VAX ISDN ACCESS Installation  B-1


 






                  1.  Display release notes
                  2.  Print release notes
                  3.  Both 1 and 2
                  4.  None of the above

          * Select option [2]: 2<Return>
          * Queue name [SYS$PRINT]: <Return>
          Job ISDN011 (queue SYS$PRINT, entry 257) started on LPA0)
          * Do you want to continue the installation [NO]? yes<Return>
          %VMSINSTAL-I-RELMOVED , The product's release notes have been successfully moved
          to SYS$HELP.
                  +---------------------------------------------------------------+
                  |        VAX ISDN-ACCESS Software Installation Procedure.       |
                  +---------------------------------------------------------------+

                  Product:      ISDN-ACCESS
                  Producer:     DEC
                  Version:      V1.1
                  Release Date: 30-NOV-1990

          * Does this product have an authorization key registered and loaded? yes<Return>
          %ISDN-W-NOAUTH, DEC ISDN-ACCESS use is not authorized on this node
          %ISDN-W-NOIVP, the Installation Verification Procedure will not be executed
             Note that, in this example, a positive answer confirmed the
             license registration when, in fact, the VAX ISDN ACCESS
             license was not active. This is why the "ISDN-W-NOAUTH"
             message above was displayed in addition to the "ISDN-W-NOIVP"
             message.

          * Do you want to purge files replaced by this installation [YES]? <Return>
                  No More Questions.

          %VMSINSTAL-I-RESTORE, Restoring product saveset B ...
          %ISDN-ACCESS-I-FILEXISTS, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT already exists on system
          %ISDN-ACCESS-I-FILNOTINST, VMI$ROOT:[SYSLIB]NETTRACE$KEY.INIT not installed
          %VMSINSTAL-I-RESTORE, Restoring product saveset C ...
          %VMSINSTAL-I-MOVEFILES, Files will now be moved to their target directories...


          B-2  Example of a VAX ISDN ACCESS Installation


 






           Installation of ISDN-ACCESS V1.1 completed at 11:20

          Enter the products to be processed from the next distribution volume set.
          * Products: <Ctrl-Z>
                  VMSINSTAL procedure done at 11:21
          $

































                            Example of a VAX ISDN ACCESS Installation  B-3


 











                                                                Appendix C


                       Contents of the VAX ISDN Software Distribution Kits
          ________________________________________________________________


                                          NOTE

                 Except where otherwise stated, all the files installed
                 as part of the VAX ISDN or VAX ISDN ACCESS installa-
                 tion procedure are copied to the SYS$COMMON area of
                 the system disk.

          __________________________________________________________
          C.1  Contents of the VAX ISDN Distribution Kit

             The following release notes and help libraries are copied to
             the SYS$HELP directory:
              o  ISDN011.RELEASE_NOTES

              o  ISDN$NCP_HELP.HLB
              o  TRACEHLP.HLB

             The following libraries are copied to the SYS$LIBRARY direc-
             tory:

              o  ISDN$SA_DEF.H
              o  ISDN$SA_DEF.L32

              o  ISDN$SA_DEF.MLB
              o  ISDN$SA_DEF.PAS


                  Contents of the VAX ISDN Software Distribution Kits  C-1


 






              o  ISDN$SA_DEF.PEN

              o  ISDN$SA_DEF.R32
              o  ISDN$SA.OLB

              o  NETTRACE$KEY.INIT
             The following images are copied to the SYS$LOADABLE_IMAGES
             directory:

              o  ISDN$DRIV.EXE
              o  ISDN$L2.EXE#

              o  ISDN$L3.EXE#
              o  ISDN$CC.EXE

              o  LES$DECNET.EXE
              o  LES$DECNET_ALT.EXE

              o  LES$LES.EXE
              o  ISDN$NETPRF.EXE#

              o  LES$TRACE.EXE
              o  LES$TRACE_MBX.EXE

              o  SDDRIVER.EXE
              o  SDDRIVER.ULD

             The following DCL command files are copied to the SYS$MANAGER
             directory:

              o  ISDN$NPF_SHOW.COM
              o  ISDN$SECURITY.COM (this file is installed in the
                SYS$SPECIFIC area)

              o  ISDN$SHUTDOWN.COM
          ___________________
              # this file is network-dependent, and is chosen according to
                the operator's answer during the installation procedure

          C-2  Contents of the VAX ISDN Software Distribution Kits


 






              o  ISDN$STARTUP_SITE.COM (this file is installed in the
                SYS$SPECIFIC area)

              o  NETTRACE_INSTALL.COM
              o  NETTRACE_SECURITY.COM

             The following message files are copied to the SYS$MESSAGE
             directory:
              o  ISDN$MESSAGES.EXE

              o  LES$ACP_MESSAGES.EXE
              o  NETTRACE_MESSAGES.EXE

             The following shareable images are copied to the SYS$SHARE
             directory:

              o  ISDN$ACPCODESHR.EXE
              o  ISDN$ACPDATASHR.EXE

              o  LES$ACP_CODE.EXE
              o  NETTRACE$ISDN$L2_ANALYZE.EXE

              o  NETTRACE$ISDN$L3_ANALYZE.EXE
              o  NETTRACE$ISDN$CC_ANALYZE.EXE

             The following DCL command file is copied to the SYS$STARTUP
             directory:

              o  ISDN$STARTUP.COM
             The following files are copied to the SYS$SYSTEM directory:

              o  ISDN$NCP.EXE (this file is installed in the SYS$SPECIFIC
                area)
              o  ISDN$LES_CONTROL.DAT

              o  LES$STARTUP.EXE
              o  LES$ACP.EXE


                  Contents of the VAX ISDN Software Distribution Kits  C-3


 






              o  NETLTC.EXE

              o  NETTRACE.EXE
             The following DCL command file is copied to the SYS$TEST
             directory:

              o  ISDN$IVP.COM

          __________________________________________________________
          C.2  Contents of the VAX ISDN ACCESS Distribution Kit

             The following release notes and help libraries are copied to
             the SYS$HELP directory:

              o  ISDN-ACCESS011.RELEASE_NOTES
              o  ISDN$NCP_HELP.HLB

              o  TRACEHLP.HLB
             The following libraries are copied to the SYS$LIBRARY direc-
             tory:

              o  ISDN$SA_DEF.H
              o  ISDN$SA_DEF.L32

              o  ISDN$SA_DEF.MLB
              o  ISDN$SA_DEF.PAS

              o  ISDN$SA_DEF.PEN
              o  ISDN$SA_DEF.R32

              o  ISDN$SA_ACCESS.OLB
              o  NETTRACE$KEY.INIT

             The following DCL command files is copied to the SYS$MANAGER
             directory:

              o  NETTRACE_INSTALL.COM


          C-4  Contents of the VAX ISDN Software Distribution Kits


 






             The following message file is copied to the SYS$MESSAGE
             directory:

              o  NETTRACE_MESSAGES.EXE
             The following shareable images are copied to the SYS$SHARE
             directory:

              o  NETTRACE$ISDN$L2_ANALYZE.EXE
              o  NETTRACE$ISDN$L3_ANALYZE.EXE

              o  NETTRACE$ISDN$CC_ANALYZE.EXE

             The following files are copied to the SYS$SYSTEM directory:
              o  ISDN$NCP.EXE (this file is installed in the SYS$SPECIFIC
                area)

              o  NETTRACE.EXE
              o  NETLTC.EXE

             The following DCL command file is copied to the SYS$TEST
             directory:

              o  ISDN$IVP_ACCESS.COM
















                  Contents of the VAX ISDN Software Distribution Kits  C-5


 

