DECimage Storage Manager for VMS, Version 1.0		    SSA 31.22.00-A


HARDWARE REQUIREMENTS

Processors Supported

VAX:	      VAX 6000 Model 200 Series, VAX 6000 Model 300 Series, VAX 6000 
              Model 400 Series, VAX 8200, VAX 8250, VAX 8300, VAX 8350, VAX 
              8500, VAX 8530, VAX 8550, VAX 8600, VAX 8650, VAX 8700, VAX 8800, 
              VAX 8810, VAX 8820, VAX 8830, VAX 8840, VAX 8842, VAX 8974, VAX 
              8978

	      VAX-11/750, VAX-11/780, VAX-11/785

MicroVAX:	   MicroVAX II, MicroVAX 2000, MicroVAX 3100, MicroVAX 3300, 
                   MicroVAX 3400, MicroVAX 3500, MicroVAX 3600, MicroVAX 3800, 
                   MicroVAX 3900

VAXstation:	   VAXstation II, VAXstation 2000, VAXstation 3100, VAXstation 
                   3200, VAXstation 3500, VAXstation 3520, VAXstation 3540

VAXserver:	   VAXserver 3100, VAXserver 3300, VAXserver 3400, VAXserver 
                   3500, VAXserver 3600, VAXserver 3602, VAXserver 3800, 
                   VAXserver 3900, VAXserver 6000-210, VAXserver 6000-310, 
                   VAXserver 6000-410, VAXserver 6000-420

Processors Not supported

		   11/725, 11/730, 11/782, MicroVAX I, VAXstation I, VAXstation 
                   8000

Processor Restrictions

A TK50 Tape Drive is required for standalone MicroVAX 2000 and VAXstation 2000 
systems.

Block Space Requirements (Block Cluster Size = 1)

Disk space required for installation				   4,000 blocks
								   (2.0 Mbytes)

Disk space required for use (permanent)				   3,000 blocks
								   (1.5 Mbytes)

These counts refer to the disk space required on the system disk.

CLUSTER ENVIRONMENT

For the server

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration.  It must be installed once on each VAX, 
MicroVAX or VAXstation processor from which usage is planned. In order to 
configure some product specific attributes that must remain unique to each 
system, certain components of the product are stored in the system specific 
environment, SYS_$SPECIFIC:[SYSxxx]. of the VAX, MicroVAX or VAXstation 
processor on which the installation is performed. The remaining components of 
the product, including some or all of the executable images will be installed 
common to all accessing systems. The HARDWARE REQUIREMENTS sections of this 
product's Software Product Description and System Support Addendum detail any 
special hardware required by this product.

For the client

This layered product is fully supported when installed on any valid and 
licensed VAXcluster* configuration without restrictions.  The HARDWARE 
REQUIREMENTS sections of this product's Software Product Description and System 
Support Addendum detail any special hardware required by this product.

*    V5.x VAXcluster configurations are fully described in the VAXcluster 
     Software Product Description (29.78.xx) and include CI, NI, and Mixed 
     Interconnect configurations.

SOFTWARE REQUIREMENTS

Operating System

     VMS Operating System, Version 5.3

Layered Products

     DECnet/VAX V5.3 (Phase IV endnode) required for distributed client access 
     to server.

     VAX Rdb/VMS, Version 3.0 (Runtime Option)


VMS Tailoring

For VMS V5.0 or later systems, the following classes of VMS are required for 
full functionality of this layered product:

     VMS Required Saveset
     Network Support
     Programming Support
     System Programming Support
     Utilities
     Miscellaneous Files

For more information on VMS classes and tailoring, refer to the VMS Operating 
System Software Product Description (SPD 25.01.xx).

OPTIONAL SOFTWARE

DECimage Application Services for VMS, Version 2.0
DECimage Scan Software for VMS, Version 2.0
VAX Rdb/VMS, Version 3.0
DECwrite for VMS, Version 1.0

 
 
GROWTH CONSIDERATIONS

The minimum hardware/software requirements for any future version of this 
product may be different than the minimum requirements for the current version.

DISTRIBUTION MEDIA

Tape:  9-Track 1600 BPI Magtape, TK50 Streaming Tape

This product is also available as part of the VMS Consolidated Software 
Distribution on CDROM.

ORDERING INFORMATION

Software License (Server) - QL-893A*-**
Software License (Client) - QL-YGDA*-**
Software Media and Documentation - QA-893AA-H*
Software Product Services (Server) - QT-893A*-**
Software Product Services (Client) - QTYGDA*-**

*    Denotes variant fields. For additional information on available licenses, 
     services and media, refer to the appropriate price book.

The above information is valid at time of release. Please contact your local 
Digital office for most up-to-date information.

November 1989
AE-PAAAA-TE

(R)   The DIGITAL Logo is a registered trademark of Digital Equipment 
Corporation.

(TM)   DECimage, DECwrite, VMS, MicroVAX, VAX, VAXstation and VAXserver are 
trademarks of Digital Equipment Corporation.

